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CPCCBC4012B 
Read and interpret plans and specifications 
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4012B Read and interpret plans and specifications cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	Corey Passey
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
	Corey Passey

	
	

	Participant signature
	
	
	

	Date
	20/06/2022



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	87
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	




	ASSESSOR COMMENTS

	


Q1.  Plans and specifications are used to inform which of the following processes? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Building contracts
	

	
		Development applications 
	

	
		Estimation
	

	
		Planning
	

	
		Supervisory tasks
	

	
		Tenders
	




Q2.  [bookmark: _Ref532191033]Which compass direction is always shown on plans and drawings?

	Answer
	North
	



Q3.  [bookmark: _Ref427670124]What information is provided on a location plan?

	Answer
	Location Plan
A location plan is required so that you can correctly identify your building site.
A location plan is necessary for a big development so that the relative location of the site in a particular street is clear. 
A location plan details the:
· Lot number/s
· Deposit plan numbers 
· North point
· Scale (usually 1:5000)

	



Q4.  [bookmark: _Ref427670125]What detail does a site or block plan contain?

	Answer
	A Site or Block Plan is usually drawn at 1:500 and gives the following information:
· A datum  - reference height to other site levels
· Building location and orientation to north point
· 
· A Site or Block Plan is usually gives the following information:
· Outline of site boundaries showing location of proposed building and existing dwellings
· Street frontage names
· Major geological and topographical features (trees and vegetation)
· Datum points, contours and slopes 
· Driveways, stormwater drainage, easements and right of carriage
· Soil and surface water drains, pipe sizes
· Service runs from the house to mains - utility services location (sewer, water, gas, electricity)
· Details of paving and retaining walls
· 

	


Q5.  [bookmark: _Ref427670660]What do floor plans identify?

	Answer
	· Floor plans: Shows detail of the proposed structure, such as rooms, positions of fixtures, floor coverings
· the floor plan it shows the size and thickness of structural members and relationships between spaces
· Floor plans have all the dimensions of room sizes

	



Q6.  [bookmark: _Ref427671793]What is a landscape plan and what information might it provide?

	Answer
	· Landscape plan: Shows details of plants, paths, garden layouts and retaining walls 

	



Q7.  [bookmark: _Ref427670661]What are elevation views? What do they provide to the plan reader?

	Answer
	Elevation views 
View of the proposed structure from its sides (i.e. from north, south, east and west). 
Each side is what is called an elevation view. 

	



Q8.  [bookmark: _Ref427670662]What is a section?

	Answer
	Section views 
In most cases elevation and plan views cannot show sufficient information to enable a builder or tradesman to see how various structural parts are to be built or assembled. The section is a view of the house after it has been cut vertically at some point. Like the floor plan it shows the size and thickness of structural members and relationships between spaces. 

	



Q9.  [bookmark: _Ref427670664]What are detailed drawings?

	Answer
	Preliminary and final drawings and plans
Final drawings and plans are drawings that show overall sizes, levels and references to assembly drawings. The location drawings, which can be plans, elevation or sections, are numbered consecutively. 
Typically, final drawings will include: 
· Site plans
· Floor plans 
· Sections through the entire building
· Elevations
· Landscape plans
· Detailed drawings

	



Q10.  [bookmark: _Ref427671414]What are specifications?

	Answer
	General items contained within Building Specifications include a:
· Full description of work 
· Precise list of materials
· Details of all fittings, fixtures and finishes (appliances – make and model)
· Precise list of products (e.g. types, brands, grades, thickness, colour, model) 
· 
· Key features included within building specifications include:
· Levels and survey information
· Materials lists
· Performance data and material technical data
· Schedules of quantities
· Stress, load and bearing calculations
· 

	




Q11.  [bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	ACRYL
	Acrylic
	

	
	AS
	Australian Standard
	

	
	ASSD
	Assumed Datum
	

	
	B
	Basin
	

	
	BN
	Bull nose
	

	
	BTH
	Bath
	

	
	BWK
	Brickwork
	

	
	CB
	Concrete Block
	

	
	CF
	Concrete Floor
	

	
	CG
	Clear Glass
	

	
	CJ
	Ceiling Joist
	

	
	CORR
	Corrugated
	

	
	CWT
	Cold water tank
	

	
	DG
	Double Glazing
	

	
	DH
	Double Hung
	

	
	DPC
	Damp Proof Course
	

	
	DSB
	Distribn Switch Board
	

	
	DW
	Dishwasher
	

	
	EJ
	Expansion Joint
	

	
	FPBD
	Fibrous Plaster Board
	

	
	FFL
	Finished Floor Level
	

	
	FHR
	Fire Hose Reel
	

	
	GPO
	General Purpose Outlet
	

	
	HBD
	Hardboard
	

	
	HTR
	Heater
	

	
	HWD
	Hardwood
	




Q12.  [bookmark: _Ref427675022]Name each of the drawing symbol images shown in the table below.

	Answer
	Name
	Image
	
	
	Double brick walls
	[image: Wall - Cavity brick]
	

	
	Brick and frame wall
	[image: Wall - Brick veneer]
	

	
	Internal Frame wall
	[image: Wall - Timber stud]
	

	
	Window external wall
	[image: Window - In cavity wall]
	

	
	Window
	[image: Window - In single wall]
	

	
	Door
	[image: Door - Swing single]
	

	
	Double doors
	[image: Door - Swing double]
	

	
	Cavity slider
	[image: Door - Sliding into pocket]
	

	
	External slider
	[image: Door - Sliding exposed on wall]
	

	
	Single power point
	[image: Socket outlet (power) - general]
	





Q13.  [bookmark: _Ref427733304]Identify what the following window symbols represent on elevations.

	Answer
	Item
	Drawing
	
	
	Hinged at side
	[image: ]
	

	
	Awning hinged at top
	[image: ]
	

	
	Sliding horizonatally
	[image: ]
	

	
	Fixed 
	[image: ]
	




Q14.  [bookmark: _Ref532192707]What does a clouded area on a plan indicate?






	Answer
	On plans, revisions or amendments are represented by a clouded area

	



Q15.  [bookmark: _Ref532192900]An amendment to specifications could relate to which of the following? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Contact details of all construction crew members
	

	
		Materials or products used
	

	
		Methods of carrying out specified work
	





Refer to the title block below to respond to Q16. to Q18. 
[image: ]
Source: http://www.dtwd.wa.gov.au/sites/default/files/teachingproducts/BC1934_CCBY.PDF 

Q16.  [bookmark: _Ref531861864]On what date was an amendment made to the window details?

	Answer
	5/10/2011
	



Q17.  [bookmark: _Ref532193187]True or False (Tick your response): Details of the window in Q16. should also be reflected in the specifications and confirmed with the client.

	Answer
		True 
	
	
	
		False 
	
	




Q18.  [bookmark: _Ref531862015]What amendment occurred on 08/11/2011?

	Answer
	Bed 3 Robe deleted
	




Refer to the site plan below to respond to Q19. to Q26. 

[image: Site plan for a block of land showing existing building and proposed residence plus other detail]


Q19.  [bookmark: _Ref531861219]What structure is being built on this site? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Residence
	

	
		Road
	

	
		Shed
	

	
		Water meter
	




Q20.  [bookmark: _Ref532193598]What is the Lot number of this site?

	Answer
	16
	



Q21.  [bookmark: _Ref532193601]What is the size of this lot?

	Answer
	3653m2
	



Q22.  [bookmark: _Ref532193617]Is the shed at the north-east of the proposed structure to be removed or retained? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Removed
	

	
		Retained
	




Q23.  [bookmark: _Ref532193558]True or False (Tick your response): The sewer is at the eastern boundary of the property.

	Answer
		True 
	
	
	
		False 
	
	




Q24.  [bookmark: _Ref532193550]True or False (Tick your response): The driveway is located to the south of the proposed property.

	Answer
		True 
	
	
	
		False 
	
	



Q25.  [bookmark: _Ref532193569]What size is the easement on the eastern boundary of the site?

	Answer
	5m
	



Q26.  [bookmark: _Ref531861509]True or False (Tick your response): The stormwater drain is constructed from PVC pipe.

	Answer
		True 
	
	
	
		False 
	
	




Refer to the contour plan below to respond to Q27. to Q28. 

[image: contourplan]

Q27.  [bookmark: _Ref531872622]What is the level at the northernmost point of the site?

	Answer
	3.94
	



Q28.  [bookmark: _Ref532193453]Which end of the site has the lowest level? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		East
	

	
		West
	



Refer to the sectional drawing below to respond to Q29. to Q49. 

[image: cross_section]
Q29.  [bookmark: _Ref427660755][bookmark: _Ref532194571]Give a brief description about the building from the detail available in the sectional drawing. Is it the same structure proposed in Q19. to Q26.?

	Answer
	Yes

Two story dwelling, slab on ground, corrugate iro roof with lightweight cladding to upper floor and brick veneer to lower level.  With verandahs
	



Q30.  [bookmark: _Ref427733756]Who is the client?

	Answer
	H and M Smith
	



Q31.  [bookmark: _Ref427733757]Where is this project to be built?

	Answer
	Lot 16  Glenvalley Road Richmond
	



Q32.  [bookmark: _Ref427733759]What are the contact details for the draftsman?

	Answer
	Joe Foreman
Ph.03 9514 2311
M. 0413 113 113
18 Fairview Road Richmond 3216
	



Q33.  [bookmark: _Ref427733761]What sheet number is this drawing?

	Answer
	5 of 7
	



Q34.  [bookmark: _Ref427660519][bookmark: _Ref427733762]What timber is required for loading and non-load bearing walls?

	Answer
	F5 45x90 Load Bearing and F5 45035 x 90 non load bearing
	


Q35.  [bookmark: _Ref427733763]What spacing is recommended for common studs?

	Answer
	600mm maximum Stud spacing
	



Q36.  [bookmark: _Ref427733765]What type of roof truss is to be installed?

	Answer
	Scissor trusses 
	



Q37.  [bookmark: _Ref427733766]What centres are the trusses positioned at?

	Answer
	900mm spacing
	



Q38.  [bookmark: _Ref427733769]What size are the veranda posts?

	Answer
	90 x 90 DAR Oregon
	



Q39.  [bookmark: _Ref427733771]What timber species are the veranda posts to come from?

	Answer
	DAR Oregon
	



Q40.  [bookmark: _Ref427733773]What pitch is the roof?

	Answer
	30 degree pitch
	



Q41.  [bookmark: _Ref427733774]What size are the noggings and at what spacing?

	Answer
	F5 35 x 70mm and 1350mm spacing
	



Q42.  [bookmark: _Ref427733776]What size are the ceiling joists?

	Answer
	450mm spacing 35 x 70mm
	


Q43.  [bookmark: _Ref427733778]What timber is used for roof battens and what spacing?

	Answer
	35 x 70 FG pine battens at 900mm spacing
	



Q44.  [bookmark: _Ref427733780]What thickness is the plasterboard sheeting?

	Answer
	10mm
	



Q45.  [bookmark: _Ref427733781]What type of flooring is to be installed?

	Answer
	15mm plywood flooring
	



Q46.  [bookmark: _Ref427733783]What is the roof cladding material?

	Answer
	Colorbond corrugated metal roofing
	



Q47.  [bookmark: _Ref427733784]Where will you find information about the footings?

	Answer
	On the foundation plan
	



Q48.  [bookmark: _Ref427733786]What do the letters ‘DAR’ refer when timber ordering?

	Answer
	Dressed all round , finished size of the post
	



Q49.  [bookmark: _Ref427662218]Explain what ‘240 x 63 LVL’ refers to on the sectional drawing. What do the letters ‘LVL’ refer to?

	Answer
	Laminated Veneer Lumber, means the size of the joists
	


Refer to the drawing below to respond to Q50. to Q65. 

[image: ]

Q50.  [bookmark: _Ref427663500]What is the number of the drawing?

	Answer
	2
	



Q51.  [bookmark: _Ref427734104]What is the Job Number?

	Answer
	OOR-112
	



Q52.  [bookmark: _Ref427734106]What is the scale of the drawing?

	Answer
	1:100
	



Q53.  [bookmark: _Ref427733995]What does the drawing show?

	Answer
	Elevations and cross section
	



Q54.  [bookmark: _Ref427734110]Which view shows the front of the house?

	Answer
	East elevation
	



Q55.  [bookmark: _Ref427734113]How many motor vehicles can be parked in the garage?

	Answer
	2
	



Q56.  [bookmark: _Ref427734114]What are the window and doors made from?

	Answer
	Aluminum framed windows and timber door, colourbond roller doors
	



Q57.  [bookmark: _Ref427734116]What is the size of the eaves?

	Answer
	450mm
	


Q58.  [bookmark: _Ref427734119]What are the eaves lined with?

	Answer
	Hardiflex
	



Q59.  [bookmark: _Ref427734120]What type of roof structure is the roof built from?

	Answer
	Timber framed roof trusses 
	



Q60.  [bookmark: _Ref532197046]Which Part of the NCC should be read for more detail about the requirements for the roof structure in Q59.?

	Answer
	Part 3.4.3
	



Q61.  [bookmark: _Ref532197154]Which Australian Standard should be read for more detail about the roof structure in Q59. ?

	Answer
	AS 1720.1
	



Q62.  [bookmark: _Ref427734122]What is the roof cladding materials made from?

	Answer
	Concrete Tile
	



Q63.  [bookmark: _Ref532197156]Which Part of the NCC should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	Part 3.5.2
	



Q64.  [bookmark: _Ref532197157]Which Australian Standard should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	AS 2050
	



Q65.  [bookmark: _Ref427663512]What is the roof pitch?

	Answer
	22.5 degrees
	



Q66.  [bookmark: _Ref531871432]Identify one (1) regulatory body you may need to submit plans to for approval?

	Answer
	Local Council
	



Q67.  [bookmark: _Ref532197251]Briefly describe the approval process and timeframes for an approval through the regulatory body in Q66. 

	Answer
	All plans, specifications and any special soil reports etc and engineering required for the job and forms filled out are submitted.  
The process can take a few weeks to up to 10 months dependant on the size of the job and the shire or councils timing. Also depends on the work load of the councils. 
	



Q68.  [bookmark: _Ref427673788]What is a prime cost (PC) item? Give an example.

	Answer
	A PC item is:
· An amount of money included in a contract sum to purchase a specified item such as tiles, taps, doors or bathroom fittings
· An agreed estimated amount is included at contract signing but the specific products are not selected until a later stage
· A builder must estimate the cost of such items at or above the lowest amount these items could reasonably cost
· For example if a client selects a more expensive door than allowed by the PC item, say a $500 door compared with a $440 PC amount, a variation will be required to cover the additional $60.  If the PC item varies, so will the final contract sum

	



Q69.  [bookmark: _Ref427673790]What is a provisional sum (PS) item? Give an example.

	Answer
	A provisional sum is:
· An amount of money included in contract sum to cover work and/or materials, not detailed when entering the contract
· Typically builders will include a PS for site work costs
· The builder is legally required to take reasonable steps to ensure an accurate site works cost estimate but unforeseen events mean that the provisional sum is exceeded which is added to the contract sum
For example a building site may seem sandy and clean with minimal siteworks required, however, there may be large limestone rocks/tree trunks concealed below the surface which only emerge once siteworks commence, causing cost overrun.

	


Refer to the Bill of Quantities below to respond to Q70. to Q76. 

[image: ]
[image: ]

Source: http://organizedbuilders.com.au/sites/default/files/BOQ-Summary.pdf 



Q70.  [bookmark: _Ref531867328]True or False (Tick your response): This Bill of Quantities represents a job for a two-storey house.

	Answer
		True 
	
	
	
		False 
	
	




Q71.  [bookmark: _Ref532199102]Identify two (2) materials being used for the floors?

	Answer
	Concrete, carpet and vinyl
	



Q72.  [bookmark: _Ref532199110]True or False (Tick your response): A landscaper has been contracted for this job.

	Answer
		True 
	
	
	
		False 
	
	




Q73.  [bookmark: _Ref532199056]How much does the contracted plasterer cost?

	Answer
	$12,900
	



Q74.  [bookmark: _Ref532199058]How much do the kitchen appliances cost?

	Answer
	$2700
	



Q75.  [bookmark: _Ref532199060]What percentage of the total cost does the fixing stage represent of the building contract?

	Answer
	23%
	



Q76.  [bookmark: _Ref531866973]What percentage of the total cost does the completion stage represent of the building contract?

	Answer
	23%
	


Refer to the Purchase Order below to respond to Q77. to Q82. 

[image: ]
Source: http://organizedbuilders.com.au/sites/default/files/Databuild-Bill-of-Quantities.pdf 

Q77.  [bookmark: _Ref531874116]How many Pine F5 90 x 45 studs (2.4m long) are required?

	Answer
	100
	



Q78.  [bookmark: _Ref532199470]If the material in Q77. increased in cost to $2.75 each, what would be the total cost for this material?

	Answer
	$275.00
2.75 / stud
	



Q79.  [bookmark: _Ref532199474]How many sheet of ply are required in total (i.e. all sizes)?

	Answer
	13
	



Q80.  [bookmark: _Ref531874121]What material has the highest total cost?

	Answer
	Pine 90 x 45 MGP10 long lengths
	



Q81.  [bookmark: _Ref531874448]How many metres are required of the material in Q80. ?

	Answer
	322.5m
	



Q82.  [bookmark: _Ref531874565]What beam is identified as being a better option than F17?

	Answer
	E14 beams
	




Refer to the labour chart below to respond to Q83. to Q86. 

[image: ]
Source: https://www.archsd.gov.hk/media/89170/sor2013_vol1_builders_works_2013_11_04.pdf 



Q83.  [bookmark: _Ref531873766]Based on the hourly rates given, which is the least expensive trade to contract?

	Answer
	Asphalter road construction $107.40 per hour
	



Q84.  [bookmark: _Ref532199773]If the trade in Q83. were to be contracted for two (2) hours’ work, how much would this cost?

	Answer
	$214.80
	



Q85.  [bookmark: _Ref531873865]Based on the hourly rates given, which is the most expensive trade to contract?

	Answer
	Bar bender and fixer $214.30
	



Q86.  [bookmark: _Ref531873882]If the trade in Q85. were to be contracted for six (6) hours’ work, how much would this cost?

	Answer
	$1,288.80
	



Q87.  [bookmark: _Ref531691201]Name the building legislation (Act and Regulations) that apply within your jurisdiction and should be referenced when reading plans and building contracts.

	Answer
	· Building Act 1975 (Qld)
· Building Regulation 2021 (Qld)
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Corey Passey

	
	

	Participant signature
	
	
	

	Date
	22/06/2022



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4012B
Read and interpret plans and specifications

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to read and interpret plans and specifications in order to inform estimation, planning and supervisory activities. 

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include:
· [bookmark: _Hlk106622021]Any drawing with a cloud or mark-up you have inserted.
· Copy of the correspondence regarding mark up and any site management/authorising engineer response.

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Drawings (including site plan), Specifications, Tender documentation, Telephone, Facsimile machine, Computer. 

	Assessment of task

	Name of participant:
	Corey Passey

	Name of observer:
	Mark Harris

	Role of observer 
(Confirm suitability to sign)
	GM of Stroud Homes and business owner

	Email address of observer
	Mark.harris@stroudhomes.com.au

	Signature of observer:
	
	Date:
	22/06/2022
	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Interpret drawings

	1.1A.  [bookmark: _Ref531698368]Identify purpose and advantage of different types of drawings.
		
	1.1B.  Identify different aspects of drawings.
		
	1.1C.  [bookmark: _Ref531698394]Identify, understand and apply:
· Commonly used symbols and abbreviations
· Common building and construction terms on drawings
		
	1.1D.  [bookmark: _Ref531698402]Identify building site from location drawings.
		
	1.1E.  [bookmark: _Ref531698498]Identify on the site plan:
· True north
· Building orientation
· Key features in relation to building and other structures
· Levels
· Contours
· Service entry points
· Site features to be removed or retained
		
	1.1F.  [bookmark: _Ref531698586]Identify key features of plans, elevations and sections.
		
	1.1G.  [bookmark: _Ref531698588]Identify client requested variations to standard plans on drawings.
		
	2 Interpret specifications 

	1.2A.  [bookmark: _Ref531698592]Identify and correctly apply Provisional Sum (PS) and Prime Cost (PC) values. 
		
	1.2B.  [bookmark: _Ref531698596]Identify and confirm customer variations to standard specifications and communicate changes to organisational personnel. 
		
	1.2C.  [bookmark: _Ref531698601]Apply and communicate correct interpretations of essential elements to estimation, planning and supervisory tasks (including labour hours/costs and material quantities/costs).
		
	1.2D.  [bookmark: _Ref531698605]Identify Building Codes or standards affecting the work to be undertaken (including references to Australian Standards and the National Construction Code). 
		
	1.2E.  [bookmark: _Ref531698612]Identify key features of products included in the specification, including the design, purpose, aesthetics and cost relationships. 
		
	3 Communicate with others

	1.3A.  [bookmark: _Ref531698617]Consult with industry professionals, clients, organisational personnel and appropriate local authorities.
		
	1.3B.  [bookmark: _Ref530479080]Effectively communicate using the following methods:
· Verbally using language/concepts appropriate to cultural differences
· Non-verbal communication
· Using technology (including telephone, facsimile, email)
		
	The Participant’s performance was:  Satisfactory     Not Satisfactory



	OBSERVER COMMENTS

	Corey understands and has a good knowledge of the tasks in this module.  I have observed him throughout the last year and he is very competent with these topics and knows his way around a set of plans and specifications and also pricing and BOQ’s and getting contracts signed and in and out of council.  Corey has run his own building franchise in NZ for 10 years and has built over 400 homes so it’s clear he knows what he is doing with regards to reading and interpreting plans and specifications.

Kind Regards
Mark Harris
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