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1. PURPOSE
 (
CPB
) (
CPB
 
Contractors
)The purpose of this Plan is to establish and maintain an effective health and safety management system.
(	)
 (
CPB
)is committed to implementing a structured approach to workplace health and safety in order to achieve a consistently high standard of safety performance.
 (
CPB
)This Plan will assist	in meeting its obligations in accordance with work health and safety legislation.
 (
CPB
)This Plan applies to all	officers and workers and to other persons at risk from
work carried out at	workplaces. Failure to comply with the requirements of this Plan may lead to disciplinary action.

2. WORK HEALTH AND SAFETY (WHS) POLICY
 (
CPB
)The Statement of Commitment and the Implementation of Policy Commitment provide the overarching direction
will follow in pursuit of workplace health and safety outcomes. These commitments are

 (
CPB
)Statement of Commitment
is committed to providing a workplace that enables all work activities to be carried out safely.
We will take all reasonably practicable measures to eliminate or minimise risks to the health, safety and welfare of workers, contractors, visitors, and anyone else who may be affected by our operations.
 (
CPB
)We are committed to ensuring we comply with the Work Health and Safety Act 2011 (the Act). We will also comply with any other relevant legislation, applicable Codes of Practice and Australian Standards as far as possible.
 (
CPB
)This WHS Management Plan and	’s WHS Policies and Procedures set out
the safety arrangements and principles which are to be observed by	and its workers to ensure compliance with the WHS Act and to provide appropriate mechanisms for continuing consultation and management of WHS matters.

 (
CPB
)Implementation of Policy Commitment
is committed to ensuring, so far as is reasonably practicable, the health and safety of its workers (employees, contractors, labour hire workers, outworkers, apprentices, students or volunteers) while they are at work, and that the health and safety of other persons (e.g. visitors) is not put at risk from our operations. This will be achieved by:
·  (
CPB
)providing and maintaining a healthy and safe work environment through the implementation of safe work practices, safe systems of work and the provision of safe plant and equipment;
· ensuring that workplaces under the control of	are safe, without risk to health, and have safe means of access and egress;
·  (
CPB
)routinely consulting in order to maintain effective and co-operative relationships between
and its workers, and with other duty holders, on health and safety matters in the
workplace; and
· reviewing, through appropriate mechanisms, the effectiveness of the safety measures taken.
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CPB
)commitment to providing safe and healthy working environments for its workers includes:
· providing relevant, up-to-date WHS information to all workers on matters such as workplace safety and their responsibilities;
· providing expert assistance in WHS matters where necessary;
· providing instruction and/or training in work processes where appropriate;
· developing and implementing strategies which include workplace assessment, hazard identification, and appropriate remedial action to eliminate or control hazards; and
· implementing and maintaining appropriate information, reporting and statistical systems.

3. DEFINITIONS

	Terminology
	Definition

	Person Conducting a Business or Undertaking (PCBU)
	A PCBU has the primary duty of care to ensure, so far as is reasonably practicable:
· the health and safety of its workers while they are at work, and
· that the health and safety of other persons is not put at risk from work carried out as part of the conduct of the PCBU.
CPB
· is a PCBU.

	Officer
	It is an officer’s duty to exercise due diligence to ensure that the PCBU complies with its health and safety obligations under the WHS Act.
CPB
· The Members of the Board for	will usually be Officers under
the WHS Act.
· The Station Manager may be an Officer under the WHS Act
Note: A person is an Officer under the WHS Act only if they “make, or participate in making, decisions that affect the whole, or a substantial part, of the business of the corporation; or who has the capacity to affect significantly the corporation’s financial standing”. Whether a person is an Officer or not under the WHS Act will depend on the facts of the particular situation.

	Worker
	Previously known as ‘employee’.
The term worker includes employees, contractors and sub-contractors and their employees, labour hire employees, outworkers, apprentices and trainees, work experience students and volunteers.

	Health and Safety Representative (HSR)
	A worker elected by members of their work group to represent them in health and safety matters.

	Other persons
	Includes any visitors



4. [bookmark: _bookmark2]RESPONSIBILITIES
 (
CPB
)

 (
CPB
)As the duty holder,	, being the PCBU, must:
· ensure the health and safety of its workers and others in our workplace
· ensure the health and safety of other persons is not put at risk from work carried out as part of its operations
· provide and maintain a work environment that is without risks to health and safety
· provide and maintain safe plant and structures
· provide and maintain safe systems of work
· ensure the safe use, handling and storage of plant, structures and substances
· provide adequate facilities for the welfare of workers
· provide information, training, instruction and supervision
· monitor the health of workers and the conditions of our workplaces. Specific duties as a PCBU also include:
· record and notify Comcare of any notifiable incidents arising out of the conduct of the business or undertaking
· ensure authorisations are in place for any high risk work or plant
· consult so far as reasonably practicable with other PCBUs or persons who have a duty in regard to a work health and safety matter
· consult so far as reasonably practicable with workers, their representatives and Health and Safety Representatives on work health and safety matters.

 (
CPB
)The Chairperson and members of the Board
The Chairperson and members of the Board, as officers, are responsible for ensuring that
complies with any duty or obligation under the WHS Act. This is achieved by these officers exercising due diligence, which means they:
·  (
CPB
)acquire and keep an up to date knowledge of work health and safety matters
· gain an understanding of	’s operations and the hazards and risks involved
· ensure that appropriate resources and processes are provided to enable hazards to be identified and risks to be eliminated or minimised
·  (
CPB
)ensure that information regarding incidents, hazards and risks is received, considered and responded to in a timely way
· ensure that	has, and implements, processes for complying with its WHS duties and obligations
· verify the provision and use of the resources and processes listed above.

This may include:
· having work health and safety as a standing agenda item for each Board meeting
· integrating WHS laws into everyday business through consultation with Managers and all workers
· developing a work health and safety management system framework, which will be reviewed on a regular basis by the Chairperson and Board members
· ensuring that WHS risk management is incorporated into all business activities and that hazard identification, risk assessment and control is an on-going process, including:
· development and maintenance of a WHS risk register
· development and maintenance of WHS policies and procedures
· ensuring an effective injury/incident reporting procedure
· ensuring appropriate processes are in place for WHS issues relating to contractor management
·  (
CPB
)ensuring that the procurement of any equipment takes into account WHS matters
· ensuring that regular hazard inspections of the	workplaces occur
· ensuring that WHS is a standing agenda item at all staff meetings
· incorporating WHS updates and information into regular reporting provided to the Board by Station Managers
·  (
CPB
)ensuring that WHS issues are part of all training provided for staff, including induction
· ensuring that contractors and visitors to	are provided with appropriate and reasonable WHS information at site entry, and
· ensuring that the work environment is a safe environment.

 (
CPB
)Station Manager
The Station Manager, (if an officer), is responsible for ensuring that	WHS policies and procedures are implemented in the workplace and/or systems of work under their control. As an integral part of their normal duties, the Station Manager will:
· consult with their workers on measures to protect their health and safety
· actively follow agreed safety practices and model positive attitudes towards health and safety matters
· arrange for their workers to be instructed in healthy and safe systems of work and procedures and supervise the practice of safe working procedures
· notify the Chairperson and/or other members of the Board of all incidents, hazardous situations, dangerous occurrences or immediate risks to health and safety of any workers
· ensure that all workers are informed of this policy
· undertake consultation with all managers and workers on change that may affect their health and safety
· ensure that WHS is a standing agenda item at all staff meetings
· communicate WHS matters to the Chairperson of the Board.

Managers and Leaders
Managers and leaders are responsible for providing a workplace that is, as far as reasonably practicable, safe and healthy workplace for workers and visitors, in particular in the areas of their control. This includes:
· modelling health and safety leadership
· demonstrating a commitment to good health and safety performance, by:
· talking about safety at regular meetings
· ensuring safe work procedures are followed
· reporting incidents, hazards and safety concerns promptly
· assessing task risk and not allowing an activity to continue until it can be controlled adequately
·  (
CPB
)fostering a strong work health and safety culture where worker input is valued
· Promoting and implementing the	Work Health and Safety Management System
· actively support the identification of hazards and risks and the management of these
· understand and monitor safety performance objectives
· proactively manage other duty holders (e.g. contractors), when required.

Workers
 (
CPB
)Workers must take reasonable care for their own health and safety while they are at work, and take reasonable care that their acts or omissions do not adversely affect the health and safety of other persons. They must comply, so far as they are reasonably able, with any reasonable instruction given by the Station Manager, as well as co-operating with any reasonable
policy or procedure which relates to workplace health and safety. On a day to day basis,
this includes:
· to the extent of the worker’s control or influence over working conditions and methods, take reasonable care to work safely
· making sure that the work area safe when leaving it
· make proper use of all appropriate safeguards, safety devices and personal protective equipment
· follow agreed safe working practices and rules
· report all known hazards, accidents and incidents as soon as possible.
It is acknowledged that, in accordance with the Act, a worker may cease, or refuse to carry out work if they have a reasonable concern the work would expose the worker to a serious risk to their health or safety. The Act requires workers who cease work to notify the relevant manager that they have ceased unsafe work as soon as practicable after doing so. It also requires workers to remain available to carry out ‘suitable alternative work’. This would not however require workers to remain at any place that poses a serious risk to their health or safety.

Contractors
 (
CPB
)Contractors, sub-contractors and self-employed persons are defined as “workers” under the WHS Act if they carry out work in any capacity for	. They are required to:
· comply with the requirements of the WHS legislation
·  (
CPB
) (
CPB
)have in place any work health and safety policies and programs required under State or Territory safety legislation
·  (
CPB
)consult with	about safety matters and comply with	policies
· work safely and to include the safety of	staff and visitors in their safety plans.
If any staff member believes that a contractor may be engaging in an unsafe work practice, they are required to report this issue to their manager.
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CPB
)Visitors
Visitors and other persons to	also have responsibilities to abide by our workplace safety rules and procedures. These responsibilities include to:
· take reasonable care for their own health and safety and for the health and safety of other persons
·  (
CPB
)comply with, so far as they are reasonably able, all reasonable safety directions provided by
 (
CPB
)staff
· report all safety related incidents to	staff
· ensure the adequate supervision of any accompanying children
·  (
CPB
)not enter any restricted area without authorisation or escort
·  (
CPB
)not bring or consume alcohol or illegal drugs at	workplaces
· not wilfully or recklessly interfere with	property.

5. CONSULTATION AND COMMUNICATION ARRANGEMENTS
Open communication between workers and managers is important to ensuring a safe workplace. Therefore, workers are encouraged to:
· ask questions relating to WHS
· bring up safety concerns
· make recommendations regarding WHS
· give regular feedback
· become involved in evaluation of safety issues
· participate in any WHS related problem solving process.
It is important that workers help shape decisions about WHS particularly when:
· identifying hazards and assessing risks
· making decisions about ways to eliminate or minimise those hazards or risks
· proposing business changes that may affect the health and safety of workers
· purchasing of new equipment or substances
· developing or changing job tasks or safety procedures.
All workers belong to a work group and are encouraged to raise any work health and safety concerns they may have with their manager and/or Health and Safety Representative. If the issue identified remains unresolved, it should be raised directly with the Station Manager.

[bookmark: _bookmark4]Health and Safety Representatives (HSR)
HSRs are elected by members of a work group in order to represent the interests of that work group in matters relating to work health and safety. HSRs must undertake approved training to exercise their powers, and may:
· consult with workers on a regular basis
· inspect a work area as required
· participate in workplace accident and incident investigations as required
· participate in any change management discussions that may affect the health and safety of workers
· provide advice to managers on the welfare of workers in their work group.
HSRs cannot exercise their powers under the Act unless they are trained. HSRs are not liable for acts or omissions that are undertaken in good faith. HSRs are not entitled to personal or medical information about a worker without their consent unless that information is of a general form that does not identify workers specifically.

Health and Safety Committee
 (
CPB
)Health and Safety Committees provide the forum for the constructive discussion of measures to assure health and safety in the workplace. At	the Health and Safety Committee will meet quarterly and:
· facilitate co-operation between the PCBU and workers in the instigation, development and implementation of WHS policies and procedures
· assist in developing standards, rules and procedures relating to health and safety
· consult with workers regarding their WHS concerns
· consult with management regarding worker WHS concerns including change that may influence WHS more broadly
· ensure the conduct of regular workplace inspections.
Minutes of the latest Health and Safety Committee meeting will be made available for all workers to review.

6. TRAINING
 (
CPB
)The Station Manager will conduct a training needs analysis and arrange for appropriate WHS training to be undertaken by workers as required.
Where required,	workers are to demonstrate their competencies to perform required tasks safely. In tasks with a high potential for injury, a separate documented assessment of a person’s competency may be undertaken.
As a guide, competency assessments should be signed and dated by the assessor/assessee and contain the following elements:
· task or equipment description
· information on licenses held (or other relevant qualifications)
· a checklist containing the essential competencies that were demonstrated, and
·  (
CPB
)comments or confirmation that the competency was met.
is committed to developing a suite of competencies to deal with all safety sensitive work tasks.

7. [bookmark: _bookmark5]WHS RISK ASSESSMENT
The purpose of any WHS risk assessment is to ensure that, for any identified hazards, appropriate control measures are implemented in order to protect workers, contractors and visitors from risks to their health, safety and welfare.
Control measures for WHS hazards should be implemented as required using the following hierarchy of control, in order of preference these measures relate to:
· elimination (removal of the hazard)
· substitution (substitute the hazard for something which is less hazardous e.g. replace a hazardous chemical with one within is not hazardous)
· isolation (isolate the hazard from people e.g. place a noisy piece of equipment in another location)
· engineering (e.g. guarding on machinery)
· administrative (e.g. provision of training, policies and procedures, signage)
· personal protective equipment (e.g. use of hearing , eye protection, high visibility vests).
 (
CPB
)Outcomes of risk assessments will be documented and the control measures reviewed at least annually or earlier should a task or activity be the subject of a WHS incident or a change of process or requirement. Current risk assessments will ensure that
 (
CPB
)achieves the goal of eliminating or minimising the risk workers may be exposed to.
The list of	policies and procedures in place to manage workplace risk include:
·  (
Procedures
Establish Project Risk Management Undertake
 
Construction
 
Area
 
Risk
 
Review Undertake Work Pack Risk Assessment
Perform
 
Risk
 
Assessment
 
-
 
Basic
 
Plant
 
Operation Conduct Critical Risk Review
Project
 
Risk
 
Management
 
Review
Policies
Risk
 
Management
 
Policy
Capability
 
Integrity
 
and
 
Operation
 
of
 
Plant
 
and
 
Equipment
 
Policy Anti-Bullying, Harassment and Discrimination Policy
Safety
 
and
 
Health
 
Policy Environment Policy
Pre-Contracts
 
Policy Compliance Policy
)

8. [bookmark: _bookmark6]RIGHT OF ENTRY
 (
CPB
)A WHS permit entry holder must also hold a current Fair Work Act 2009 entry permit. Their WHS entry permit and photographic identification must be available at all times for inspection. Where there is a suspected workplace WHS contravention, a permit holder is not required to give prior notice. However, as soon as reasonably practicable they must give notice of their entry and the
suspected contravention to	or the person with management or control of the workplace.
 (
CPB
)The permit holder may, in relation to the suspected contravention, inspect any work system, plant substance or structure; consult
with	and its workers; be allowed to inspect and make copies of relevant documents (unless to do so would contravene a State or Commonwealth law); and warn any person of a serious risk to health and safety if immediate or imminent.
 (
CPB
)Otherwise a permit holder is required to give at least 24 hours notice (and no more than 14 days) to the
before entering a workplace to consult on WHS matters or provide advice on those matters to
 (
CPB
)relevant workers.
must not, without reasonable excuse, refuse or unduly delay a permit holder’s entry into a
workplace or obstruct them from exercising their rights under the WHS Act.
The permit holder must not intentionally and unreasonably delay, hinder or obstruct any person or disrupt any work at a workplace or otherwise act in an improper manner.

9. WHS ISSUE RESOLUTION
Wherever possible, any WHS concerns will be resolved through consultation between workers, their representatives and/or their manager. If the concern cannot be resolved, then it can be referred to the Station Manager for resolution. Ultimately any issue remaining unresolved may be referred to the Board. Where the issue remains unresolved the default procedure for issue resolution set out in the WHS Regulations must be followed.
If reasonable efforts have been made to resolve an issue and it remains unresolved, any party to the issue can ask Comcare to appoint an inspector to assist in resolving the matter.

10. AUTHORITATIVE SOURCES
· Work Health and Safety Act 2011
· Work Health and Safety Regulation 2011
· Approved Work Health and Safety Codes of Practice
Additional information on these sources may be found at www.comcare.gov.au
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1. EMERGENCY PROCEDURES
An emergency evacuation plan has been developed and this plan, together with a list of emergency contacts, is displayed in the following locations:
· Office/reception
· common areas
· workshops
· sheds
· male toilets
· female toilets
The Emergency Contacts List is at Attachment 1. All fire emergency equipment, such as horns, sirens and fire extinguishers, will be tested by an approved provider every 12 months.

2. HAZARD/INJURY/INCIDENT REPORTING
How to Report a Hazard or Injury or Incident:
All managers and workers including contractors are required to complete an incident form if a hazard/injury/incident occurs, and:
· Advise the Station Manager of the incident or injury or hazard
· For recording purposes complete a Hazard/Injury/Incident Report Form
· Complete the relevant sections of the form giving details of the incident. The form should be completed even when an injury has not occurred, that is, in the event of a near miss
· All hard copy forms should be signed by the relevant parties
· The Station Manager or their delegate must record all injuries on the injury register
· Internal reporting of any hazard/injury/incident should occur is separate from reporting of notifiable incidents to Comcare. The Hazard/Injury/Incident Report form is at Attachment 2.
3. REPORTING OF NOTIFIABLE INCIDENTS
Any serious incidents must be notified immediately to the Station Manager. After becoming aware that any such incident has occurred, it is the Station Manager’s responsibility to report ‘notifiable incidents’ to Comcare by the fastest possible means, either:
· by phone—ring Comcare 1300 366 979
· by fax or other electronic means—fax Comcare on 1300 305 916; email notify@comcare.gov.au .
· NOTE: Comcare requires that immediate notification is followed within 48 hours in writing by completing a Notifiable Incident Report Form and forwarding it to Comcare, GPO Box 9905, Canberra, ACT, 2601

 (
Definition
 
of
 
“notifiable
 
incident”:
 
‘Notifiable
 
incidents’
 
include
 
the
 
following:
the
 
death
 
of
 
a
 
person
a
 
serious
 
injury
 
or
 
illness
 
of
 
a
 
person
Serious
 injury or illness includes immediate treatment as an in-patient in a hospital; immediate treatment for certain 
serious injuries; or medical treatment within 48 hours of exposure to a substance
a
 
dangerous
 
incident
A
 
‘dangerous
 
incident’
 
means
 
any
 
incident
 
in
 
relation
 
to
 
a
 
workplace
 
that
 
exposes
 
a
 
worker
 
or
 
any
 
other
 
person
 
to
 
a serious
 
risk
 
to
 
a
 
person’s
 
health
 
or
 
safety
 
caused
 
by
 
incidents
 
such
 
as
 
uncontrolled
 
escape,
 
spillage
 
or
 
leakage
 
of
 
a substance, an uncontrolled implosion, explosion, 
fire;
 or uncontrolled escape of gas or steam.
)
 (
HAZARD/INCIDENT/INJURY
 
REPORTING—SUMMARY
 
FOR
 
THE
 
STATION
 
MANAGER
Ensure
 
that
 
the
 
manager
 
or
 
worker
 
has
 
completed
 
a
 
hazard/incident/injury
 
form.
Review the incident with the manager or worker to determine if any actions need to be taken to eliminate or 
minimise
 
the
 
risk
 
of
 
the
 
incident
 
or
 
hazard
 
recurring.
Complete
 
the
 
injury
 
register.
If
 
the
 
incident
 
results
 
in
 
a
 
death,
 
serious
 
injury
 
or
 
illness
 
or
 
a
 
dangerous
 
incident,
 
notify
 
Comcare
 
IMMEDIATELY
.
Ph:
 
1300
 
366
 
979
Fax:
1300
 
305
 
916
Email:
 
notify@comcare.gov.au
NOTE:
 
Comcare
 
requires
 
that
 
immediate
 
notification
 
is
 
followed
 
within
 
48
 
hours
 
in
 
writing
 
by
 
completing
 
a Notifiable Incident Report Form and forwarding it to Comcare, GPO Box 9905, Canberra, ACT, 2601
Maintain
 
records
 
of
 
all
 
the
 
above.
)

4. FIRST AID
 (
Definitions:
First
 
aid
 
is the immediate treatment or care given to a person suffering from an injury or illness until more advanced
 
care
 
is
 
provided
 
or
 
the
 
person
 
recovers.
First
 
aid
 
officer
 
is
 
a
 
person
 
who
 
has
 
successfully
 
completed
 
a
 
nationally
 
accredited
 
training
 
course
 
or
 
an
 
equivalent level
 
of
 
training
 
that
 
has
 
given
 
them
 
the
 
competencies
 
required
 
to
 
administer
 
first
 
aid.
)

 (
CPB
)has in place the following first aid procedures, as required by First Aid in the Workplace Code
of Practice
· The appointment and training of First Aid Officers (FAO)
· The provision of first aid kits within the workplace
·  (
CPB
)Clear signage with the name of the FAO and the location of the first aid kits
· The provision of a suitable first aid kit in all	vehicles. It is the FAO’s responsibility to ensure that the contents of all first aid kits are maintained First Aid Officer Training:
· The minimum level of training for a FAO is the Senior First Aid Certificate (or equivalent)
· Refresher training should be undertaken every three years.

[bookmark: _bookmark9]First Aid Officer Responsibilities:
· The FAO is approved to render first aid assistance in the workplace.
· The FAO should ensure that they do not administer first aid services beyond their level of training.
·  (
CPB
)A record of any first aid treatment given should be kept by the FAO and reported to the Station Manager on a regular basis to assist with reviewing first aid arrangements.
Contact details for	FAOs are displayed on all noticeboards.
 (
FIRST
 
AID—SUMMARY
 
FOR
 
THE
 
STATION
 
MANAGER
Ensure
 
that
 
a
 
First
 
Aid
 
Officer
 
(FAO)
 
has
 
been
 
appointed
 
and
 
trained.
Keep
 
a
 
copy
 
of
 
the
 
FAO’s
 
qualifications.
Ensure
 
that
 
a
 
first
 
aid
 
kit
 
is
 
provided
 
and
 
maintained
 
by
 
the
 
FAO.
Advise
 
all
 
managers
 
and
 
workers
 
of
 
the
 
name
 
of
 
the
 
FAO
 
and
 
the
 
location
 
of
 
the
 
kit.
Place
 
a
 
sign
 
on
 
the
 
wall
 
where
 
the
 
kit
 
is
 
located.
First
 
Aid
 
in
 
the
 
Workplace
 
Code
 
of
 
Practice
 
[link
 
here]
 
available
 
on
 
the
 
Comcare
 
website.
)

5. WHS TRAINING AND INDUCTION
Training
 (
CPB
) (
CPB
) (
CPB
)is committed to providing appropriate training to ensure workers have the skills and knowledge necessary to fulfil their WHS obligations. WHS training is a fundamental requirement for	to
achieve a safe workplace. The WHS training needs for	will be determined in consultation with managers and workers, as well as through review of the WHS Risk Register, however it can be generally categorised into three kinds:
Generic WHS Training—skills and knowledge which is commonly required, e.g. induction training, WHS risk management training, evacuation procedures.
Risk Specific WHS Training—training required for those persons conducting activities with a specific risk to health and safety or a verification activity, e.g. first aid training, hazardous substances training, manual handling training, confined spaces training, working from heights.
Task Specific WHS Training—skills and licensing which are required depending on the specific hazards and risk, e.g. any farm equipment operation, high risk work licenses such as for driving forklifts, cranes.

Documentation for Training
Training records shall be maintained as evidence of training delivery and assessment of competence.

WHS Induction
All new managers and workers are required to be provided with WHS information regarding the workplace as part of their overall

 (
CPB
)induction and introduction to	. A thorough WHS induction process assists new staff to feel
welcome, become integrated into the organisation and ensure that they are able to work safely.
 (
CPB
)The WHS Induction Checklist at Attachment 3 should be used in conjunction with the general induction training program for land workers to ensure that all new workers are aware of the WHS systems, policies and procedures in place within
.

[bookmark: _bookmark10]Procedure
The Station Manager must ensure a WHS induction is provided on the new team leader or worker’s first day. If the Station Manager is not available, he or she should organise for a replacement to conduct the induction. The Station Manager must:
· use the attached WHS Induction Checklist (Attachment 3) to ensure that all WHS issues are covered
· on completion of the induction, sign the checklist and ensure that the new worker also signs
· file a copy of the induction checklist on the worker’s file
· provide the new worker with access to this WHS Management Plan and the WHS Policies and Procedures Manual. A new Station Manager will be inducted by the outgoing Manager or a Board Member.
 (
CPB
)WHS Induction for Contractors/Visitors
 (
CPB
)All contractors/visitors should be provided with a Safety Briefing prior to entering the	premises.
All contractors/visitors must sign in and be provided with a copy of the	Safety Briefing Handout to read, and to then sign, acknowledging that they have read and understood the information. These documents are included at Attachment 4.

Detailed WHS Induction for Contractors
For contractors (e.g. trade persons) the requirements for induction will depend on the work to the undertaken and the duration of their stay at the workplace. At a minimum, contractors should be advised of emergency procedures and location of facilities. Refer to Attachment 5.
 (
CPB
)All WHS training provided to managers, workers and contractors should be recorded in the WHS Training Register (Attachment 6). Alternatively, this training register can be incorporated into the overall Staff Development and Training Register
which details all professional development and training undertaken by	managers and workers.

6. RISK MANAGEMENT AND THE RISK REGISTER
 (
CPB
) (
CPB
)WHS risk management is a systematic process of hazard identification, risk assessment, and risk control with the aim of providing healthy and safe conditions for managers, workers, visitors and contractors at	.
As required by the WHS Act,	has adopted a risk management approach to underpin its WHS Management System. This approach involves all managers and workers in identifying hazards, assessing and prioritising risks, implementing control measures and reviewing how effective the control measures are.

 (
CPB
) (
CPB
)All workers are responsible for assisting in managing the particular risks associated with their specific work environment. Risk management strategies used by	include:
· regular hazard inspections of the	environment
· a comprehensive risk register detailing all WHS risks associated with the operation and activities of the
 (
CPB
)

· documented WHS policies and procedures
· risk assessments of newly purchased equipment
· risk assessments for any change to work processes
· hazard, injury, incident reporting procedures
·  (
CPB
)incident investigations (at the direction of the Station Manager)
· WHS job safety analysis for specific	activities including:
· mustering
· branding and tagging
· fence tensioning
· changing split rim tyres
· windmill maintenance/working at heights
· refueling.
 (
Definitions:
WHS
 
Hazard:
 
Anything
 
which
 
has
 
the
 
potential
 
to
 
cause
 
injury
 
or
 
illness.
WHS
 
Risk:
 
A
 
WHS
 
risk
 
is
 
the
 
chance
 
of
 
someone
 
becoming
 
injured
 
or
 
ill
 
as
 
a
 
result
 
of
 
a
 
workplace
 
hazard.
 
This significance of the risk is determined by considering the likelihood of it happening and the consequences if it 
does happen.
WHS
 
Risk
 
Control:
 
WHS
 
risk
 
control
 
is
 
action
 
taken
 
to
 
eliminate
 
or
 
reduce
 
the
 
likelihood
 
that
 
exposure
 
to
 
a
 
hazard
 
will result in injury or illness to people or damage to property and the environment.
)

The Risk Management Process
WHS risk management should be undertaken for all activities where there is the potential for harm including:
· before activities commence;
· before the introduction of new equipment, procedures or processes;
· when equipment, procedures or processes are modified.

Step 1: Identify the Hazard
A hazard is a source or potential source of injury, ill health or disease. Hazard identification is the process of identifying all situations and events that could cause injury or illness by examining a work area/task for the purpose of identifying all threats which are ‘inherent in the job’. Tasks can include, but may not be limited to using tools, hazardous chemicals, dealing with people, lifting/moving items and mustering.

Step 2: Assess the Risk
Assessing the risk from a hazard determines its significance. Firstly, consider the consequences should something happen; will it cause a serious injury, illness or death or a minor injury. Secondly, consider how likely is this to occur—very likely, not likely at all or somewhere in between? Some of the things to think about include:
· how often is the task undertaken
· how frequently are people near the hazard
· how many people are near the hazard at a particular time
· has an incident happened before
· have there been any ‘near misses’
 (
CPB
)Use the table below to determine how significant the risk is.
Where a manager, worker, contractor, or visitor to the workplace identifies a hazard,	requires that it is eliminated or reduced in consultation with the relevant stakeholders.
· Step 1: identify the Consequences—or how severely could it hurt someone
· Step 2: identify the Likelihood—or how likely is it for an injury to occur
· Step 3 & 4: identify the Risk Priority Score—to prioritise your actions
· Step 5: apply the hierarchy of hazard control
· Step 6: identify who, how and when the effectiveness of controls will be checked and reviewed

	
Step 1—CONSEQUENCES
How severely could it hurt someone? or
How ill could it make someone?— Circle it
	Step 2—LIKELIHOOD
How likely is it for an injury to occur?—Circle it

	
	
Very likely, could happen frequently
	Likely, could happen occasionally
	
Unlikely, could happen, but rare
	Very unlikely, could happen, probably never will

	
	L1
	L2
	L3
	L4

	Kill or cause permanent disability or ill health
	C1
	Very high risk (1)
	Very high risk (1)
	High Risk (2)
	Substantial Risk (3)

	Long term illness or serious injury
	C2
	Very high risk (1)
	High Risk (2)
	Substantial Risk (3)
	Moderate Risk (4)

	Medical attention and several days off work
	C3
	High Risk (2)
	Substantial Risk (3)
	Moderate Risk (4)
	Acceptable Risk (5)

	First Aid needed
	C4
	Substantial Risk (3)
	Moderate Risk (4)
	Acceptable Risk (5)
	Low Risk (6)



STEP 3: RISK PRIORITY SCORE IDENTIFIES THE NECESSARY ACTION AND RESPONSE

	Step 3—RISK PRIORITY SCORE
	Step 4—ACTION AND RESPONSE

	1 = Very High Risk
	Stop the activity—immediate action is required to ensure safety—safety measures applied must be cleared by the Station Manager before any activity recommences
Proceed with caution—immediate reporting of emerging or ongoing risk exposure at this level to the Station Manager for decision is mandatory

	2 = High Risk
	

	3 = Substantial Risk
	Be aware—action required as soon as possible to prevent injury or illness
Report these risks to the responsible Manager during the current shift or before the next shift

	4 = Moderate Risk
	

	5 = Acceptable Risk
	Do something when possible. Manage by routine procedures.

	6 = Low Risk
	These risks should be recorded, monitored and controlled by the responsible Manager


STEP 4: CONTROL THE HAZARDS
Control the hazards—the aim is to implement the most reliable controls to create a safe workplace rather than simply relying on people to behave safely, following processes or using protective equipment. In many cases, a combination of several control strategies may be the best solution.

Hierarchy of control strategies (in order of preference):
· eliminate the hazard; remove the equipment from use, dispose of unwanted chemicals
· substitute; use a non-hazardous chemical, use a different machine that can do the same task
· isolation; contain noisy machinery within a booth
· engineering controls; design equipment differently, providing lifting devices to minimise manual handling
· administrative processes; task variation, job rotation, training
· personal protective equipment; gloves, hearing protection, eye protection

STEP 5: REVIEW THE PROCESS
Continuously review to monitor and improve control measures and find safer ways of doing things.

Documentation for Risk Assessment
 (
CPB
)The documentation required for a WHS risk assessment will depend on the operation or activity being assessed. The appropriate WHS Risk Assessment Form must be used when undertaking a risk assessment of the various activities of the
. The WHS Risk Assessment Proforma and procedure for conducting an assessment is at
Attachment 7.

The WHS Risk Register
 (
CPB
) (
CPB
)The risk assessment data collected from identifying, assessing and controlling risks should be documented on a centralised risk
register for	. The risk register holds a list of	key risks that need to be monitored and managed. The risk register is to be managed by the Station Manager who should be notified if new hazards are identified and controls implemented so that the risk register can be amended.
The Station Manager is responsible for overseeing the Risk Register, and for ensuring that effective control measures are implemented and that risks are monitored and reviewed on a regular basis.

7. [bookmark: _bookmark11] (
CPB
)WORKPLACE HAZARD INSPECTIONS
is required by WHS legislation to be proactive in identifying hazards in the workplace which may affect the health and safety of its workers and eliminating or minimising the risks arising from those hazards.
In order to ensure a safe and healthy workplace, the Station Manager and/or nominated manager/s accompanied by Health and Safety Representatives (HSRs) should undertake WHS hazard inspections of the workplace regularly and at any other times as required. The hazard inspection should be undertaken by following the principles of WHS risk management and using the attached information and checklists (Attachments 8 and 9).
If any hazards are identified through the hazard inspection process, controls must be implemented to ensure that the risk to health and safety is eliminated or minimised.
In addition to these regular inspections, all managers should also conduct weekly hazard inspections of their work sites in conjunction with HSRs. Any hazards noted during these inspections should immediately be reported to the Station Manager and appropriate remedial action taken.
All hazard inspection documentation should be filed by the Station Manager.

8. PURCHASING
Prior to purchasing any goods or services for the workplace, they should be assessed to determine if there are any associated health and safety hazards. This includes the purchase of equipment such as machinery, tools, furniture, chemicals, as well as contracted services such as maintenance.

9. WHS RECORD KEEPING
The Station Manager should retain all WHS and workers compensation documents. These documents are required to be filed for 30 years in safe storage accessible only to authorised personnel in accordance with the Privacy Amendment (Enhancing Privacy Protection) Act 2012 (Cth).

10. DOCUMENTS TO BE DISPLAYED
· Emergency contacts page (Attachment 1)
· Emergency Evacuation Plan
· Return to Work Policy
· Work Health and Safety Policy
· Accident/Incident Notification details
· Compensation and Return to Work information

11. IMPORTANT CONTACT NUMBERS
· Comcare
· Telephone: 1300 366 979
· Facsimile: 1300 305 916
· Email: notify@comcare.gov.au
· Postal Address: GPO Box 9905, Canberra, ACT 2601
· After Hours Emergencies: In the event of a major incident an on call inspector can be contacted on:
 (
1300
 
362
 
128
 
to
 
be
 
connected
 
to
 
WHSQ's
 
after-hours
 
messaging
 
service.
 
Your
 
notification
 
details
 
will
 
be
 
referred
 
to
 
a
 
WHSQ
 
on-call inspector who will contact you within a time frame that has regard to the seriousness of the incident.
)

[bookmark: _bookmark12]PART C: SPECIFIC WHS REQUIREMENTS
1.  (
CPB
)ASBESTOS
 (
CPB
)It is highly likely that the premises to be occupied by	were built before 31 December 2003
and therefore, there is a requirement for	to comply with these measures outlined including an asbestos management plan and asbestos register. Do not repair or conduct work on any building without first checking the asbestos register. A sample register is included at Attachment 10.

2. INAPPROPRIATE BEHAVIOUR
 (
CPB
) (
CPB
) (
CPB
)Bullying, harassment, discrimination and violence of any form will not be tolerated at	. undertakes to investigate all complaints formally made.		will
take action to resolve the complaint. If the complaint is found to be valid, action may include any combination of the following:
· Asking for an apology
· Creating an agreement with the offender that will stop the behaviour of concern
· Conciliation/mediation conducted by an independent/impartial third party to seek a mutually acceptable solution
· Disciplinary action in the form of verbal, written or final warning or dismissal
· All violence will be reported to the police.
In determining the action to be taken, the following factors will be considered:
· Severity and frequency of the behaviour
· Whether there have been previous incidents or prior warnings.

3. CONTRACTORS
 (
CPB
) (
CPB
)is committed to ensuring that all workers under its control, including contractors and sub- contractors have a safe and healthy environment in which to perform their duties.
 (
CPB
)Contractors are likely to be workers employed by	to undertake a specific task; the
delivery/pickup of goods, tradespeople undertaking repair or maintenance work within the workplace. In order to achieve this objective, it is recognised that contractors need to be:
· suitably experienced to perform the tasks
· in possession of all necessary licenses, permits, registrations and insurance required to perform the works safely and in compliance with appropriate regulations
· notified of any potential hazards associated with the location or use of the area where the works are to be carried out

·  (
CPB
)made aware of	Emergency Procedures

·  (
CPB
)if reasonable, and if the work will involve high risk tasks, have completed the Detailed WHS Induction Checklist for Contractors (Attachment 5).
All contractors must abide by	WHS requirements which will be advised to them before engagement.

4. [bookmark: _bookmark13]DANGEROUS GOODS AND HAZARDOUS SUBSTANCES
Hazardous substances are chemicals, organic matter and other substances which pose a health risk when people are exposed to them. These may include glues, paints, solvents, corrosives, adhesives, thinners, cleaning solutions, chemicals, flammable and Dangerous Goods. Dangerous goods are hazardous substances that are also explosive or flammable in nature with storage required that is fit for purpose.
 (
CPB
)All chemicals will be included in the hazardous substances register and have their current Safety Data Sheet (SDS) present for each chemical on the register. All workers shall have access to information about the chemicals in the event of a spillage or
exposure, even where	workers would not normally use the chemicals directly. Quantities of hazardous substances stored for use shall be kept to a minimum.
 (
CPB
)A hazardous substances register will be developed to record any substances purchased or used by the
(see Attachment 11). This will be reviewed on a regular basis.

5. ELECTRICAL SAFETY
Failure to maintain electrical equipment in a safe condition, or to use equipment in accordance with manufacturer’s instructions may result in injury or death to workers or other parties.
All electrical equipment must be protected from damage, used safely and checked regularly. In addition, there are other requirements that must also be implemented for ‘specified electrical equipment’. These requirements include combinations of testing and recording and connection to safety switches.
Regular inspection and testing of in-service electrical equipment by a competent person is a way to ensure this safety duty is met. The WHS legislation requires that electrical equipment is inspected and tested in accordance with Australian Standard 3760: 2010 In-service safety inspection and testing of electrical equipment. Only authorised electrical personnel are to perform installation, inspection, testing and labelling activities.

1. Testing Frequency:
The frequency of inspections that are outlined in Section 2 of the Standard, AS/NZS 3760:2010 are recommended but can be varied subject to a risk assessment. The Australian standard includes a table that sets out testing and inspection intervals for various types of equipment from 3 months (for equipment that is high use, high risk, or hire equipment) to up to 5 years (for equipment that is not open to abuse, flexing of cords, etc). In addition to the regular testing and inspection, the standard specifies that electrical equipment is to be inspected and tested:
· before return to service after a repair or servicing, which could have affected the electrical safety of the equipment, and
· before return to service from a second-hand sale, to ensure equipment is safe. Generally the following should be followed:
· tools and leads: every 12 months (low use)
· Safety Switches: monthly
· Offices: every 3 to 5 years

2. Residual Current Devices:
The fitting of Residual Current Devices (RCD) on certain equipment can considerably reduce the risk of electrocution. An RCD (also known as a safety switch) works by detecting a current leakage. When RCD detects this current leakage, it turns the power off almost immediately. Whilst an electric shock may still be received, the duration will be shortened reducing the risk of serious injury.

3. [bookmark: _bookmark14]Unsafe Equipment:
 (
CPB
)Equipment that may be unsafe should be withdrawn immediately from service and have a label attached warning against further use. Arrangements should be made, as soon as possible, for such equipment to be disposed, destroyed, or repaired by an authorised repair agent or competent person.
The	Electrical Safety Policy provides further information in relation to this workplace hazard and its management. This Policy is included in the WHS Policies and Procedures Manual.

6. CONFINED SPACES
All confined spaces are placarded with access strictly controlled. Entry requires the issue of a confined spaces permit on each occasion. No employee or contractor will be issued a permit to work in any confined space on the property unless they are trained and supervised. When working in a confined space a trained bystander must be present at all times. A register of identified confined spaces and entry permits is maintained at the office.

7. MUSTERING
Agitated livestock are a risk. Observe the following considerations when mustering:
· Mustering is best done early in the morning or towards nightfall, when temperatures are cooler and livestock have had a long grazing period.
· Prepare the route in advance. Open the gates and be on guard at the places where livestock are most likely to break away.
· All people involved in the muster should be familiar with the property layout.
· Try to maintain visual, radio or routine contact with others involved in musters.
· Have safe working procedures in place for mustering, including an emergency response procedure.
· Stay at the fringe of their flight distance so they don’t scatter.
· When closing a yard gate behind a mob or flock, stand to the side where possible.
· If it is necessary to be behind the gate, hang on with both hands and use your boots to provide further support in case the gate is flung backwards.
Considerations specific for moving cattle:
· Give the cows time to pick up their calves before moving.
· Never trust cows at calving time.
· Cows and calves should be moved slowly. Beware of aggressive cows and avoid mustering beef cows with very young calves.
· If you have to catch a calf, keep it between you and the cow. Considerations specific for moving bulls:
· Move confidently to demonstrate dominance.
· Don’t try to move a dangerous bull on foot or alone; use a vehicle.
· Always carry a long strong cane or stick.
· Keep bulls moving at a trot until they’re well into the paddock and clear of the gate—keep them a good distance apart.
· Troublesome bulls can be moved by being included with a mob. Considerations specific for moving sheep:
· Assume every ram will act aggressively
· Use sheep dogs to control the mob

8. [bookmark: _bookmark15]FALLS FROM HEIGHT
There is a risk of serious injury from falling when working above ground height. No worker will work at height without ensuring that ladders, steps and handrails are secure or fall prevention/arrest harnesses are in place. These structures include, but are not limited to:
· Overhead fuel, water tanks and windmills
· Buildings and roofs
·  (
CPB
)High machinery; cherry pickers, trucks and trailers.
will ensure that:
· Workers working at height are made aware of the hazards and risk management procedures
· Fall arrest or fall prevention harnesses are provided and used
· Workers are instructed in the correct use of fall prevention or fall arrest harnesses. Contractors will ensure that they:
· Observe and apply risk management procedures when working at heights
· Use the required personal protective equipment (PPE) where indicated.

9. MANUAL HANDLING
 (
CPB
)Manual handling is any task that requires you to push, pull, lift, carry, move, hold or lower any object, person or animal. Manual tasks include tasks that have repetitive actions, sustained postures and may involve exposure to vibration. The types of injuries related to manual handling include repetitive strain injuries, muscle injuries, tendon and ligament injuries, bone injuries and injuries from falling objects.
Manual handling hazards are managed at	by a risk management process in order to prevent or minimise the risk of injuries caused by manual tasks.
 (
CPB
)The process involves conducting a risk assessment on manual tasks carried out in the workplace, working out how to address any problems, choosing and implementing appropriate solutions, and following up to check that the solutions work.
Examples of manual handling tasks in the	environment include:
· lifting and moving equipment
· mustering
· fencing
· general repairs

Preventing Manual Handling injuries
· decide what changes can be made to reduce the risks of injury. If possible, select permanent changes (such as workplace layout, tools and equipment)
· avoid double handling of items
· provide mechanical aids (hoists)
· redesign the task (such as rotating workers)
· identify changes that are possible immediately, and those that may take time to implement
· document your risk control decisions for each task assessed, and set timelines for changes
· trial the changes in consultation with workers before making them permanent
· provide training if new equipment is introduced.

[bookmark: _bookmark16]When loading/unloading vehicles
· use lift equipment wherever practicable, otherwise
· prepare by stretching and warming up, especially after prolonged sitting in the vehicle
· slide the item as close as possible to you before lifting
· keep you back straight and bend your knees when lifting
· put loads down in the same manner in which they were picked up
· where possible store frequently used items at a suitable height; between waist and shoulder height, which reduces the need for forward bending when lifting, and
· whenever possible use trolleys for moving larger and heavy items

10. PLANT AND EQUIPMENT
The definition of plant encompasses hand tools either powered or non-powered (electric drills, hammers) and extends to farm machinery, office furniture and any other equipment used for work purposes.

Risk Management
A risk management process is a systematic method for making plant as safe as possible and can also be incorporated into other workplace risk management systems. This risk management approach should be undertaken before purchasing of, or alterations to plant, changing the way it is used, relocating it, or if additional health and safety information becomes available.

Maintenance and repair
Plant must be maintained and cleaned following the procedures recommended by the designer or manufacturer or by a competent person. Only a competent person may inspect and repair damaged plant.
Unsafe and/or malfunctioning plant and equipment can be identified by any manager, worker or contractor by a number of methods such as:
· equipment inspections;
· verbal reporting of equipment malfunction to the appropriate manager
· hazard and incident reporting.
Once identified, the unsafe or malfunctioning plant/equipment should be reported to the appropriate manager in order for repair to be organised. Plant/equipment which has been identified as unsafe should be disconnected from the power supply and clearly labelled as unsafe and not be used. If possible the plant/equipment should be moved to a location where it is not accessible.

 (
CPB
)Record Keeping
Records of inspection, testing and monitoring are required to be maintained by	. As a minimum, records should include details of inspections, maintenance, repair, calibration and alteration of plant.

11. [bookmark: _bookmark17]PERSONAL PROTECTIVE EQUIPMENT
 (
CPB
)Personal Protective Equipment (PPE) may be required to protect managers and workers during general, specific and hazardous tasks. PPE is the least effective way to control risk and is always the last resort to protect workers. The types of PPE used at
might include:
· respirators and masks
· foot protection (safety shoes and boots)
· body protection (high visibility clothing, long sleeves, wide brimmed hats, gloves)
· helmets
· any substance used to protect health, for example, sunscreen.
If required, workers are obliged to use PPE when required and when reasonably practicable. Other requirements include:
· workers should be fully trained in the safe use, storage and maintenance of PPE
· PPE must be checked before use for the correct type, fit and undamaged
· do not reuse disposable, contaminated or damaged PPE
· store PPE correctly.

12. SLIPS, TRIPS AND FALLS
Slips, trips and falls are one of the major types of accidents in workplaces and may be due to poor housekeeping practices such as water or oil spilt. Material placed untidily or using walkways for storage can also be a cause of these types of incidents. When assessing the potential for slips, trips and falls, make sure you look at out of sight areas such as storage rooms, stairways and workshops.

Prevention
Reduce the risk of injury by following these guidelines:
· avoid walking on slippery floors
· keep floors free of water and grease
· clean floors regularly
· post warning signs around spills or wet floors
· install non-slip tiling or other non-slip floor products
· use rubber mats in areas where the floors are constantly wet
· use non-slip footwear
· clean up spills immediately
· install adhesive strips and slip resistant paint to improve slip resistance. The best method will depend on the existing floor surface.
· use floor cleaning products to remove oil and grease.
· agree on written standards with contract cleaners to ensure that any cleaning agents leave the floor in a non-slip condition.
· use storage areas for equipment and be alert to the dangers of leaving boxes, rubbish, bags and furniture in walkways, entrances and exits.

13. [bookmark: _bookmark18] (
CPB
)DRUGS AND ALCOHOL
 (
CPB
)maintains the right to refuse work to any worker or contractor who, in the opinion of management, is in an unfit state to perform their work in a safe manner.
To assist in these requirements,	workers, contractors and visitors shall observe that:
· No alcohol may be consumed or permitted on property at any time unless expressly authorised by management and only when work is completed for the day
· No illegal drugs shall be consumed or permitted on property at any time or under any circumstance
· If, in the opinion of management, a worker is unfit to work safely, they will be sent/taken home
·  (
CPB
)Workers who are taking prescription medication that may affect their safety at work (that cause drowsiness), are to inform management of the circumstances so that appropriate duties may be assigned.
encourages all employees not to smoke. Please do not smoke in any vehicle, tractor
or building.

14. UV RADIATION
Ultraviolet radiation (UV) exposure can cause sunburn, skin and eye damage and skin cancer. UV protective clothing, hats, sunglasses and SPF 30 sunblock will be provided as PPE and are required to be worn for outdoor tasks.

15. VEHICLES
Alcohol and Drugs
 (
CPB
) (
CPB
)managers and workers must not drive a personal or	vehicle
on work related business in circumstances where that member would breach applicable road transport law by driving under the influence of alcohol or drugs.

Licences
 (
CPB
)managers and workers who are required to drive a vehicle on work related business must hold a current valid driver’s licence of the appropriate class and notify the Station Manager if the licence is suspended or revoked. A copy of the current driver’s licence must be provided to the Station Manager or their delegate to be retained on file.

 (
CPB
)Mobile Phones
The use of a hand-held mobile telephone while driving is a safety risk and is against the law.
managers and workers are not to use a hand-held mobile telephone while driving a motor vehicle or other motorised equipment


 (
CPB
)at an

 (
CPB
)Seat Belts
It is a legal and

workplace.



requirement that seat belts are worn at all times in a moving vehicle. The driver

 (
CPB
)is responsible for ensuring that all passengers wear a seat belt when the vehicle is in motion on a public road or at an workplace.
 (
CPB
)Smoking
Smoking in any	vehicle by either drivers or passengers is prohibited.

[bookmark: _bookmark19]Load Restraint in Vehicles
· All equipment in vehicles must be restrained firmly in order to avoid the risk of the items becoming airborne and causing missile injuries in the case of a vehicle collision
· The tension in the load restraining straps should be checked regularly during the journey
· Distribute the load evenly within the vehicle
· Ensure no loose items are within the passenger area as they may become projectiles in the event of an accident. Do not exceed load/weight capacity of the vehicle.
16. WORKING ALONE
 (
CPB
)The risk of injury or harm for people who work alone may be increased because of difficulty contacting emergency services when they are required. Emergency situations may arise because of the sudden onset of a medical condition, accidental work-related injury or disease, attack by an animal, exposure to the elements, or by becoming stranded without food or water.
The consequences of an incident arising when working alone may be very serious so	managers and workers shall implement the following for each alone work task:
· a telephone call to home base on arrival and departure at a remote work site
· development and approval of trip itineraries for extended trips and adherence to the itinerary
· pre-trip agreement on departure and arrival times and accommodation arrangements
· for travel in remote areas an emergency location beacon should be carried in the vehicle
· pre-arranged mobile/satellite phone calls at scheduled times
· appropriate first aid kit
· sufficient water for emergency purposes.

[bookmark: _bookmark20]PART D: FORMS AND CHECKLISTS
ATTACHMENT 1—EMERGENCY CONTACTS LIST
(To be displayed in appropriate location/s)

	CONTACTS
	PHONE

	POLICE (local station)
	Inala (07) 3737 5555

	
EMERGENCY SERVICES (police, fire and RFDS)
	000	Using Land Line
112	Using Mobile
UHF Band

	Comcare
	1300 366 979

	UTILITIES—Electrical
	Stowe Australia (07) 3423677

	UTILITIES—Gas
	Industrial Gas only: BOC 131 262

	UTILITIES—Sewerage and Stormwater
	Urban Utilities 13 26 57

	Doctor’s Surgery Address:
	Sonic Health Plus 169 Seventeen Mile Rocks Rd Oxley

	Physical Site Address:
	67 Bernouilli Steet, Darra QLD

	(07) 3271 2170
	Delta Insulation Systems

	Adjacent Occupants	(07) 3376 3177
Contacts:
	Norm Engineering

	
	

	First Aid Officer/s: (TBA)
	Luke 0488 709 2XX, Andrew 0418 792 3XX



[bookmark: _bookmark21]ATTACHMENT 2—HAZARD/INJURY/INCIDENT REPORT FORM
Notifiable incidents must be reported to Comcare.

	PART A: HAZARD/INJURY/INCIDENT REPORT (to be completed by the involved worker or manager)

	Is this a	Hazard report	Injury report	Incident (i.e. near miss) report?

	Is this a Notifiable Incident?	No	Yes Date Reported to Comcare: 08/03/2023

	Workplace Location: Br
	isbane
	

	Date of Incident: 08/03/
	2023	Date Reported: 08/03/023
	Time of Incident: 2.20	pm

	Name of person reporting the incident/hazard/near miss (print name):
David
	

	Name of person injured (if applicable):
Subcontractor Apprentice Electrician (no name given)
	

	Nature of injury (if applicable):
Thumb laceration
	

	Part of body injured (if applicable):
Thumb
	

	Treatment Outcome (If applicable):
Nil Required	First Aid	Medical treatment from GP	Hospit
	
al

	Location of the hazard/injury/incident:
Brisbane
	

	Description of hazard/injury/incident:
The apprentice electrician was undertaking a cable stripping task using
	

an auto retractable knife. The knife slipped.

	How did the hazard/injury/incident occur (contributing factors)?
	


the hand was in the line of fire - the hand was in front of the knife


	PART B: CORRECTIVE ACTIONS (to be completed by the Station Manager)

	What needs to happen?
(to ensure that similar incidents do not occur in the future or to minimise the risk from the hazard)
	
By when?
	
Person Responsible




As the worker was an apprentice, training needs to be given on the correct way to use a knife and not to keep your hand in the line of fire. Even if we think something is silly and not likely to happen, remembering that all workers are different ages and have different skill sets and that training on the smallest things can save our workers lives.

Conducting a hazard / risk assessment even briefly with the worker before work commenced they might have covered this as an
issue / potential risk

before work commences.	Direct manager - all
relevant stakeholders above the manager. i.e., supervisors, leading hands etc. Depending on who was running that part of the project.















	
	

	PART C: SIGN OFF
	

	Person Reporting (print name):
Andrew
	Station Manager (print name):
Luke

	Signature: [image: ]
	Signature:

	Date: 5/4/2023
	Date:

	Contact Phone Number: 0418 792 356
	Contact Phone Number: 0488 709 242



[bookmark: _bookmark22]ATTACHMENT 3—WHS INDUCTION CHECKLIST FOR NEW WORKERS

	Worker’s Name
	John Smith
	Position/Job Title
	Labour

	Start Date
	3/04/2023
	Supervisor Name
	Andrew



	Introduction
	Date completed

	Introduce other staff and the supervisor
	3/4/23

	Introduce the first aid officer and show location of first aid supplies	3/4/23

	Explain and demonstrate emergency procedures
	3/4/23

	Show location of exits and equipment
	3/4/23

	Show the work area, toilet, drinking water and eating facilities	3/4/23

	Show how to safely use, store and maintain equipment (tools etc) and hazardous substances	3/4/23
(if applicable)

	Work Health and Safety
	

	WHS Induction Training Program for Land Workers (complete copy)	27/03/2023

	On completion of Safety Induction Training Program confirm the following:

	Roles and responsibilities of people in the workplace regarding WHS	27/03/2023

	Hazards in the workplace and how they are controlled	27/03/2023

	How to report hazards
	27/03/2023

	How to report an injury and the importance of immediate reporting of serious injuries.	27/03/2023

	Consultation about WHS—how they will be kept informed about health and safety issues	27/03/2023

	Injury and Return to Work Procedures
	27/03/2023


WHS Induction conducted by:

	Person providing the induction (print name): Andrew

	Signature: [image: ]
	Date: 5/4/23

	Worker’s Signature:
	Date: 5/4/23



[bookmark: _bookmark23]ATTACHMENT 4—WHS INDUCTION FOR CONTRACTORS/VISITORS
 (
CPB
 
Contractors
)WELCOME TO SAFETY BRIEFING
FOR CONTRACTORS AND VISITORS
 (
CPB
) (
CPB
 
Contractors
)(	)
is committed to ensuring the health and safety of our managers, workers, contractors and all other visitors.

For your safety and the safety of others, it is a condition of entry to this Worksite that you take a few minutes to read this briefing.
General Safety Information
· All visitors are required to report to the main office on arrival.
· Observe any posted speed and parking restrictions.
· Obey all safety signs and barricades.
·  (
CPB
)Violent, threatening or other unacceptable behaviour is not tolerated.

·  (
CPB
)Smoking, alcohol and illegal drugs are not permitted on
· Weapons, including knives, are not permitted on

premises. premises.

· Visitors and contractors intending to bring dangerous goods and/or hazardous substances onto the worksite must declare these at the main office prior to entering the site.
· All hazards, incidents and injuries must be reported to the main office. Injuries will be recorded in the Register of Injuries.
First Aid treatment is available on site.

 (
CPB
)Emergency Procedures
 (
CPB
)In a life threatening emergency DIAL 000 For Fire, Police and Ambulance. In all cases advise an staff member.
Follow directions of	staff in the event of an evacuation

Evacuation Alarms
	slow whoop


Evacuation Procedures
When the evacuation alarm sounds:
· Evacuate the building and proceed to the assembly area identified on the site map.
· Remain in the assembly area until advised otherwise.

Contractors
All contractors are to report to the main office to:
·  (
CPB
)indicate the location and duration of the job
· sign in/ out of	Visitor Register
· advise of the status of the job before leaving the site
· remove all job and personal rubbish

Additionally, the contractor may be required to:
· produce a copy of their Safety Management Plan, including use of personal protective equipment and controls for site specific hazards, including signage and removal of job and personal rubbish
· produce Public Liability Insurance documentation before work is commenced
· complete a Prohibited Employment Declaration concerning tasks requiring specific training or licenses

INSERT WORKSITE PLAN SHOWING EMERGENCY EVACUATION ROUTES AND ASSEMBLY POINTS

 (
CPB
 
Contractors
)—CONTRACTORS/VISITORS/SIGN IN SHEET

	IN
	CONTRACTOR/VISITOR DETAILS
	OUT

	

DATE
	

TIME
	

NAME
	
ADDRESS/ ORGANISATION
	
PERSON VISITED
(or purpose of visit if Supplier or Contractor)
	
Safety Briefing Information provided
	
Signature of Contractor/Visitor/ acknowledging Safety Briefing
	
CPB



representative signature
	

TIME

	25/5/2022
	1045
	am
	Michael
	Pirtek
	Andrew
	yes
	
	[image: ]
	1.20
	pm

	25/5/2022
	1245
	pm
	Salesi F
	CPB
	Luke
	yes
	
	
	1250
	pm

	25/05/2022
	1245
	pm
	Trent M
	CPB
	Luke
	yes
	
	
	1250
	pm

	26/5/22
	1.10
	pm
	Daniel
	DK Stainless
	Steve
	yes
	
	
	1.30
	pm

	27/5/22
	9.30
	am
	Rob Ludlow
	Brisbane tyre battery
	Luke
	yes
	
	
	12.30
	pm

	27/05/2022
	11.15
	am
	Daneil K
	DK Stainless
	Luke
	yes
	
	
	1.30
	pm

	28/5/2022
	7.40
	am
	Mark B
	CPB
	Luke
	yes
	
	
	9.30
	am

	29/5/2022
	12.55
	pm
	Jacob
	Coldpack
	Andrew
	yes
	
	
	1.15
	pm

	30/5/2022
	11.45
	am
	Brad Moor
	Clearwaste Pty Ltd
	Andrew
	yes
	
	
	2.15
	pm
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 (
CPB
 
Contractors
)
CONTRACTORS/VISITORS SIGN IN INSTRUCTIONS
 (
CPB
 
Contractors
)All contractors and visitors must be provided with a Safety Briefing prior to coming onto the worksite. Upon arrival to the front office, ensure that:
· a laminated copy of the
Safety Briefing is given to any contractors or visitors who will be coming onto the site
· verbal advice is given regarding evacuation procedures
· an extra map of the worksite is provided to the contractor/visitor, showing the facilities (eg toilets), evacuation routes and assembly points
· the contractor/visitor is advised to report any hazards, incidents or injuries to the front office immediately
· the contractor/visitor is advised where they can seek first aid treatment, if required
 (
CPB
 
Contractors
)The contractor/visitor is required to sign the Sign In sheet acknowledging that they have read and understood the
Safety Briefing.
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[bookmark: _bookmark24]ATTACHMENT 5—DETAILED WHS INDUCTION CHECKLIST FOR CONTRACTORS
1. Contract Details

Contract Name:


John Smith

Contract Duration Dates: 10th Jan 23

to 10th Jan 24


Contractor Name: John Smith tyre fitting	CPB	Contact: John Smith


Contractor Representative: Andrew

2. Information Checklist

Work area to be Inducted: Plant Yard


	Contractor qualification/license:
	

	Contractor qualification/license and public liability/workers compensation cover provided
	Yes

	Safe Work Method Statement (SWMS):
	

	Safe Work Method Statement (SWMS) document/s with risk assessment and detailed controls (may be detailed in an attachment) sighted and discussed with the Station Manager
	Yes
(work will not commence until sighted)

	Site Induction:
	

	
	

	CPB
Provided with	contact numbers: Emergencies ph XXXXXX;
General Enquiries ph XXXXXX
	Yes

	First aid requirements discussed
	Yes

	
	

	CPB
Accident/incident & hazard reporting procedures for	discussed
	Yes

	
	

	CPB
Emergency procedures at	discussed
	Yes

	Discuss building access requirements/hours of work
	Yes

	Identification of restricted access areas
	Yes

	Discuss vehicle access to work site
	Yes

	
	

	CPB
Advised of	Alcohol/Drugs and Smoking policies
	Yes

	Consultation—discussion and agreement reached with contractor regarding:
	

	Asbestos management plan viewed
	Yes

	Location of any barricades to be erected
	Yes

	Access to electricity/use of extension leads
	Yes

	Contractors tools tested & tagged
	Yes

	Delivery/Storage/Removal of building waste
	Yes

	Storage of building material
	Yes

	Excavation sites
	Yes

	Lock out procedures for plant and equipment
	Yes

	Disconnection of utilities
	Yes

	Impact on fire alarm/smoke detection systems
	Yes

	Noise control measures
	Yes



	Chemicals (If applicable):
	

	Will chemicals be used on job?
	Yes

	Safety Data Sheets for the chemicals being used are provided?
	Yes

	Hot Work (If applicable): A Hot Works permit for welding, soldering, acetylene torch, or other related heat or spark producing
CPB
operations must be obtained from the	Station Manager prior to starting any Hot Works. Hot Work signage must be displayed on the site.

	Fire alarm system needs to be isolated or turned off?
	Yes

	Hot Work Permit is required and supplied to worksite?
	
	Yes
Date supplied 24 / 12 /
	
22

	Will appropriate additional firefighting equipment be located next to work site?
	Yes
	

	Working at heights (if applicable):
	

	Has Contractor completed working at height safety training?
	Yes

	Are procedures detailed in the Safe Work Method Statement?
	Yes

	Working in a confined space (if applicable):
	

	Has Contractor completed Confined Space safety training?
	Yes

	Are procedures detailed in the Safe Work Method Statement?
	Yes



4. Sign-Off

By signing this form I, the undersigned, agree that:
·  (
CPB
)I have participated in and understood the WHS Induction.
· I agree to abide by the safety policies and procedures identified above whilst working for

	Responsible
CPB

staff member
	
	
Date
	
24/12/2022

	Contractor Representative
	Andrew
	Date
	24/12/22

	Copy to Contractor, Copy to
	CPB Contractors
	



[bookmark: _bookmark25]ATTACHMENT 6—WHS TRAINING REGISTER
Publication: February 2014
 (
CPB
)Revision: February 2015
This training register records the work health and safety (WHS) training undertaken by
 (
CPB
)managers and workers, as required by the WHS Act 2011. Training can take place by a supervisor on-the-job, or by an instructor
 (
CPB
)outside of the workplace. WHS training will provide	workers with the information and skills they need to perform their duties without risk to their health and safety.
recognises that WHS training may be required when:
· a new person starts work—induction, on the job training
· new machinery/equipment or hazardous chemicals, products or other things are introduced to the workplace
· a worker’s job change
· there are new work health and safety regulations that affect our industry
·  (
CPB
)there has been an incident /near miss or injury at work.

To ensure the training was successful,	will annually review WHS training to ensure that our managers and workers:
· understand what is required of them
· have the knowledge and skills needed to work safely and without risk to their health and safety
·  (
CPB
)are actually working as they have been trained.
 (
CPB
)Additionally,	will use this register as part of regular overall reviews of the WHS management system with the goal of determining if:
· there has been any improvement in	health and safety performance
· the feedback from people who have been trained
· further information and/or training needed
· whether the most suitable training method was used
· improvements that can be made.
Training records will be monitored so that refresher training can be given when needed.

WHS TRAINING REGISTER

	Who was trained/ job title
	
Reason for training
	
Duration of training
	Who provided training
	Method of training eg on the job, theory, practical
	
Location of training
	
Scheduled date
	
Date completed

	
Ben / Leading Hand
	
job requirement
	
5 days
	
Kallibr
	
RTO (RII Cert)
	
Salisbury
	
14th June 2022
	
18th June 2022

	
Andrew / Supervisor
	
job requirement
	
5 days
	
Kallibr
	
RTO (RII Cert)
	
Salisbury
	
11th July 2022
	
15th July 2022

	
Tristram / Fitter
	
job requirement
	
3 days
	
Kallibr
	
RTO (RII Cert)
	
Salisbury
	
19th Oct 2022
	
21st Oct 2022

	
Ron / Boliermaker
	
Job requirement
	
3 days
	
Kallibr
	
RTO (RII Cert)
	
Salsbury
	
23rd Nov 2022
	
25th Nov 2022

	
Kim / Administration
	
Job Requirement
	
1 day
	
Kallibr
	
onsite face to face
	
Darra
	
12th Jan 2023
	
12 Jan 2023

	
Kris / Labour
	
Job Requirement
	
1 day
	
Kallibr
	
Onsite face to face
	
Darra
	
12th Jan 2023
	
12th Jan 2023
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ATTACHMENT 7—WHS RISK ASSESSMENT PROFORMA

	Workplace location:
	Plant Yard

	Name and position of person/s conducting assessment:
	Caroline Jane Administration

	Date:
	31/3/23



	Serial
	Hazard Identification
	Risk Assessment
	Risk Control
	Review

	
	
What is the Hazard?
	
What injury, illness or consequence could occur?
	
List any Control Measures already implemented
	

Risk Level
	
Describe what can be done to reduce the harm further
	
Whom Responsible
	

When By
	Are the Controls
Effective? (Revised Risk Score*)
	

Date Finalised

	1
	water on floor
	slip
	Clean up water immediately.
Place signs on all sides of the water
	 moderate Risk= 3 or 4
	Notify all workers over the PA system to avoid the area until cleaned up. Notify workers once the area is safe to enter
	Manager, workers and HSR
	Immediately
	Acceptable Risk = 5
	11/04/2023

	2
	electrical lead
	trip
	lead stands
	moderate Risk= 3 or 4
	Put away when not in use
	Manager, workers and HSR
	Immediately / when task is complete
	Low Risk = 6
	11/04/2023

	3
	Objects falling
	Hit by object
	Store files / folders away from desk in a secure area
	moderate Risk= 3 or 4
	Once scanned, shred all paperwork
	Manager, workers and HSR
	Immediately and ongoing
	Low Risk = 6
	11/04/2023

	4
	Poor lighting
	Eye strain and fatigue, falls, collisions
	Correct lighting installed
	moderate Risk= 3 or 4
	Open blinds / close blinds depending on the sun. set up your desk correctly, make sure your monitor is not directly below a light fixture 
	Manager, workers and HSR
	immediately
	Low Risk = 6
	11/04/2023

	5
	Ergonomic: sitting to long
	Aches and pains
	Take short breaks, stand up
	moderate Risk= 3 or 4
	Stretch, use ergonomic furniture such as adjustable chairs / stand up desks
	Manager, workers and HSR
	immediately
	Low Risk = 6
	11/04/2023



CONDUCTING A RISK ASSESSMENT

	Step 1: Identify the Consequences—or how severely could it hurt someone

	Step 2: Identify the Likelihood—or how likely is it for an injury to occur

	Steps 3 & 4: Identify the Risk Priority Score—to prioritise your actions

	Step 5: Apply the hierarchy of hazard control

	Step 6: Identify who, how and when the effectiveness of controls will be checked and reviewed



	

Step 1—CONSEQUENCES
How severely could it hurt someone?
	Step 2—LIKELIHOOD

	
	
Very likely, could happen frequently
	Likely, could happen occasionally
	
Unlikely, could happen, but rare
	Very unlikely, could happen, probably never will

	
	L1
	L2
	L3
	L4

	Kill or cause permanent disability or ill health
	C1
	Very high risk (1)
	Very high risk (1)
	High Risk (2)
	Substantial Risk (3)

	Long term illness or serious injury
	C2
	Very high risk (1)
	High Risk (2)
	Substantial Risk (3)
	Moderate Risk (4)

	Medical attention and several days off work
	C3
	High Risk (2)
	Substantial Risk (3)
	Moderate Risk (4)
	Acceptable Risk (5)

	First Aid needed
	C4
	Substantial Risk (3)
	Moderate Risk (4)
	Acceptable Risk (5)
	Low Risk (6)



	Step 3—RISK PRIORITY SCORE
	Step 4—ACTION AND RESPONSE

	1 = Very High Risk
	Stop the activity—immediate action is required to ensure safety—safety measures applied must be cleared by the Station Manager before any activity recommences
Proceed with caution—immediate reporting of emerging or ongoing risk exposure at this level to the Station Manager for decision is mandatory

	2 = High Risk
	

	3 = Substantial Risk
	Be aware—action required as soon as possible to prevent injury or illness
Report these risks to the responsible Manager during the current shift or before the next shift

	4 = Moderate Risk
	

	5 = Acceptable Risk
	Do something when possible. Manage by routine procedures.

	6 = Low Risk
	These risks should be recorded, monitored and controlled by the responsible Manager


CONTROLLING THE RISKS—THE HIERARCHY OF CONTROL
Once the risk assessment process has been completed, those hazards identified as being a VERY HIGH RISK or HIGH RISK should be addressed as a matter of priority. In considering options for controlling the identified risks, the hierarchy of controls helps to ensure that the most effective controls are implemented.

	Risk Control Hierarchy

	Elimination: this is the best control measure. E.g. remove a trip hazard.

	Substitution: e.g. substitute a hazardous chemical with a less hazardous substance.

	Isolation: e.g. barricade off the area where the hazard is present.

	Engineering: e.g. re-design of tools and equipment, provision of load shifting equipment (trolleys etc).

	Administrative: e.g. written procedures, training, warning signs.

	Personal Protective Equipment (PPE): Introduce PPE only when other control measures cannot be implemented or as a supplement.
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[bookmark: _bookmark26] (
CPB
)ATTACHMENT 8—WHS HAZARD INSPECTION PROCEDURE
Identify hazards in	workplaces by
· Conducting regular systematic inspections of the workplace
· Observe what hazards exist in the workplace and ask “what if?”
· Listen to feedback from people working with the task
· Maintain records of processes used to identify hazards

Frequency

	Location
	Frequency
	By whom?

	
	Ongoing
	The relevant manager, HSR or worker

	Buildings
	

	
	Formally—annually
	The relevant manager accompanied by a HSR

	
	Ongoing
	The relevant manager, HSR or worker

	Workshops and Yards
	Formally—quarterly—location or task based
	The relevant manager accompanied by a HSR

	
	Formally—annually—complete
	The relevant manager accompanied by a HSR


Check
· Air quality—extraction systems and ventilation
· Amenities—ventilation, slip/trip hazards, cleaning and hygiene
· Asbestos—register, management plan, condition
· Chemicals/dangerous goods—storage, labeling, spills, safety data sheets, PPE
· Electrical—leads, loading, testing and tagging
· Fire/emergency/first aid—communication, fire extinguishers, first aid kits
· Office/buildings—cleanliness, equipment serviceability, space, ergonomics
· Workshops—walkways, waste, storage, tools
· Lighting—adequacy, glare, cleanliness, repair
· Storage—adequacy, compatible materials, design, repair
· Machinery—guarding, maintenance, calibration
· Manual or mechanical handling—loads, equipment, training
· Stock work—yards, dairy, shearing, mustering, transport
· Noise—noise levels, designated zones, use of PPE
· PPE—availability, purpose, repair
· Premises security—adequacy, lighting
· Miscellaneous issues

At the end of the inspection a report should be drafted detailing all of the safety hazards identified. The report should provide a description of the risk assessment undertaken for each of these items and the risk rating allocated to each. This is done by considering the following:
· The frequency of persons exposed to the hazard—days per week, times per day.
· What the consequences might be—personal injury, environmental damage, associated costs or losses to replace or repair— how severe the outcome.
· What systems are currently in place, how effective are they or what other information is required

[bookmark: _bookmark27]ATTACHMENT 9—WHS HAZARD INSPECTION QUICK CHECKLIST

	Work Health and Safety Hazard Inspection Summary

	Location details: Plant yard
	Date of Inspection: 11/04/2023

	Inspection undertaken by: Andrew
	Accompanying Manager: Luke

Accompanying HSR: N/A

	
Reference Number
	Identified Hazard/ Issue
	
Location
	Recommended Control Measure
	
Priority
	To be endorsed by Station Manager

	
	
	
	
	
	To be actioned by:
	Completion Date:
	Review Date:

	1
	water on floor
	Bay 1 workshop
	Elimination: clean up the water
	Immediately
	Andrew
	11/04/2023
	11/04/2023

	2
	electrical lead
	Office 1 Ground floor
	Engineering: lead stands & Elimination: once finished, remove cord 
	Immediately and ongoing
	Andrew
	11/04/2023
	Daily

	3
	Objects falling
	Office 3 level 1
	Elimination: remove overhead bookcases and designate an area to storage. If scanned, all paperwork to be shredded
	Immediately and ongoing
	Andrew
	11/04/2023
	Monthly

	4
	Ergonomic: sitting to long
	Office 2 level 1
	Engineering: Use a stand up desk and take short breaks and stretch.
	Immediately and ongoing
	Andrew
	11/04/2023
	Weekly to start with and then monthly once the worker is set up and not in any pain. 
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	Quick Hazard Inspection Checklist

	Area Assessed:
	Plant Yard

	Date:
	11/4/2023

	ITEM
	COMMENTS

	Are the following safe and fit for purpose? Answering “No” will require corrective action stated in Comments

	1. Buildings
· air-conditioning
	yes.
All inspections completed quarterly, and registers updated.

	· ventilation
	

	· adequate lighting
	

	· glare problems
	

	· ergonomics
	

	· amenities clean
	

	· amenities serviceable
	

	· slip/trip hazards
	

	· electrical testing/tagging
	

	· smoke alarms
	

	· fire extinguishers
	

	· safety signage/ information
	

	2. Chemicals
· appropriately stored
· excess quantities beyond immediate use
	yes.
Appropriately separated as per compatibility chart. In correct locations. Andrew's shirt ripped today, new shirt PPE ordered 6.4.2023

	· decanted materials labelled
	

	· Safety Data Sheets available
	

	· spills procedure
	

	· first aid
	

	· PPE
	

	3. All Electrical
· leads, plugs, switches in good condition
· leads safely positioned; any temp leads; tagged
· tagging current
· RCD testing
	yes.
All testing and tagging are completed by a registered electrician each quarter and our registers updated.

	4. Fire & Emergencies
· fire extinguishers/hoses checked and serviceable
· exit signage
· exits clear
· signage of HSRs, FAOs, Fire Wardens
· designated assembly areas
	Yes.
All testing of fire extinguishers and hoses are completed each quarter and our register updated.
Signage for all emergency is in multiple areas around the office and dedicated (trained) employees are Fire wardens.
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	Quick Hazard Inspection Checklist

	Area Assessed:
	Plant Yard

	Date:
	11/4/2023

	ITEM
	COMMENTS

	Are the following safe and fit for purpose? Answering “No” will require corrective action stated in Comments

	5. First Aid
· first aid kits adequately stocked
· first aid kits clearly located
· first aid room adequately stocked
· FAO appointed and trained
	Yes.
We have a registered company who comes and restocks our first aid kits each month. This is recorded in the register. Currently there are 6 workers who are appointed and training as first aiders

	6. Workshops
· machine guarding in place
· safety lockout procedures observed
· walkways clear
· waste disposal
· housekeeping
· storage
· maintenance
· electrical
· battery recharging area
· designated noise zones
· PPE
	Yes
These checks are completed daily and one work each week on a rotating basis. This paperwork is scanned into our drive and saved each week in date order.

	7. Walkways, stairs and landings
· surface in good condition
· no clutter, trip hazards
· rails stable
	Yes.
These checks are completed daily and one work each week on a rotating basis. This paperwork is scanned into our drive and saved each week in date order.

	8. Storage and manual handling
· adequate for needs; items appropriately stored
· safe work method statements for hazardous tasks
· loads configured to reduce risk
· lift equipment provided and serviceable
· training in manual tasks
	yes These checks are completed daily and one work each week on a rotating basis. This paperwork is scanned into our drive and saved each week in date order.
SWMS are recorded separately and all workers must sign onto each SWMS before commencing work.



	Quick Hazard Inspection Checklist

	Area Assessed:
	Plant yard

	Date:
	11/4/23

	ITEM
	COMMENTS

	Are the following safe and fit for purpose? Answering “No” will require corrective action stated in Comments

	9. Stock work
· safe access
· protective railing
· stairs, handrails and ramps in good condition
· mustering routes established
· communication
· PPE
· workers trained
· workers supervised
	Yes.
These checks are completed monthly on a rotating basis. This paperwork is scanned into our drive and saved each week in date order. The registers for PPE are updated at the same time.

	10. Noise
· PPE available for designated noise zones
	Yes.
This will be discurssed during prestart when noise works are due to commence. Signs will also be placed at a short distance for the works and all works must wear correct ear protection.

	11. Security
· visitor procedures
· signage
· lighting
	We use Damstra as our database. All workers, visitors, deliver drivers etc must sign into the Damstra terminal before coming onto site. This also has a mandatory breathalyzer and must be zero to enter. 
Signage is updated regularly depending on what is happening e.g., covid-19.
Lighting is maintained as part of our daily checks and recorded in both scanned copies and on our register

	12. Miscellaneous (list)
	As required



[bookmark: _bookmark28]ATTACHMENT 10—SUGGESTED ASBESTOS REGISTER

	ASBESTOS REGISTER

	Work site: Plant Yard
	Name of Competent Person: External Contractor

	Date of Identification
	Type of Asbestos
	Condition of Asbestos
	Specific Location of Asbestos
	Is this an inaccessible area?

	No asbestos on property
	
	
	
	

	Document register closed
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[bookmark: _bookmark29]ATTACHMENT 11—HAZARDOUS SUBSTANCES REGISTER

	
Name of substance
	
Supplier
	
Location of substance
	
Hazardous Y/N
	Current SDS
ie less than 5 years old Date of issue
	Risk Assessment Yes/No
	
Uses

	Engine oil
	Valvoline
	combustibles container
	yes
	yes
	yes
	Engine lubricant

	Yellow OEM (Paint)
	PPG Industries
	Flammable gas cupboard
	yes
	yes
	yes
	Paint

	Epoxy Enamel Flat
	Dulux Group
	Flammable gas cupboard
	yes
	yes
	yes
	Paint

	High performance ename
	Dulux Group
	Flammable gas cupboard
	yes
	yes
	yes
	Paint

	Spraypak gloss
	Dulux Group
	Flammable gas cupboard
	yes
	yes
	yes
	Paint

	Dry enamel topcoat
	Dulux Group
	Flammable gas cupboard
	yes
	yes
	yes
	Paint

	Avagard Antiseptic hand
	3M Australia P/L
	Flammable liquids contai
	yes
	yes
	yes
	Hand sanitiser

	Enamel thinner
	PPG Industries
	Flammable liquids contai
	yes
	yes
	yes
	Paint thinner
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