Supervising the inspection, testing and measuring of the delivered building materials

When it comes to testing and measuring doors and windows materials, there are several relevant industry standards that are referenced to. These standards ensure that the products meet specific requirements for performance, safety, and quality. Some of the key standards used were:
1. ASTM E283/E283M-19: Standard Test Method for Determining Rate of Air Leakage Through Exterior Windows, Curtain Walls, and Doors Under Specified Pressure Differences Across the Specimen.
2. ASTM E330-02(2017): Standard Test Method for Structural Performance of Exterior Windows, Doors, Skylights and Curtain Walls by Uniform Static Air Pressure Difference.
3. ASTM E547-13(2018): Standard Test Method for Water Penetration of Exterior Windows, Skylights, Doors, and Curtain Walls by Cyclic Static Air Pressure Difference.
4. ASTM E2068-18: Standard Test Method for Determination of Operating Force of Sliding Windows and Doors.
5. ASTM E1886-19: Standard Test Method for Performance of Exterior Windows, Curtain Walls, Doors, and Impact Protective Systems Impacted by Missiles and Exposed to Cyclic Pressure Differentials.
6. ASTM F588-19: Standard Test Methods for Measuring the Forced Entry Resistance of Sliding Door Assemblies, Excluding Glazing Impact.
7. ANSI/AAMA/WDMA/CSA 101/I.S.2/A440-17: North American Fenestration Standard/Specification for Windows, Doors, and Skylights.
These standards provide guidelines for various aspects of doors and windows testing, including air leakage, structural performance, water penetration resistance, operating force, impact resistance, and forced entry resistance. Compliance with these standards ensures that the materials meet the necessary performance and safety requirements for their intended use.
NOTES:
· Confirmed the currency of plans and specifications are most recent and up to date.
· Checking the installation of the Windows and Doors as per specifications set out in the plans, to make sure it meets the requirements of the building codes standards, plans and specifications of the contract with high quality.
· Checking the external window and door fittings meet the correct wind loading requirements
· Checking the external window and door flashings are in place
· Checking the correct glass is used in areas of high risk
· Checking the installation certificates and waterproofing certificates are obtained
