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Steelcraft Framing Pty Ltd
1300 141 151 / (07) 3376 4824
12 Forge Close, Sumner QLD 4074
info@steelcraftframing.com.au
www.steelcraftframing.com.au
ABN: 77 606 911 684
QBCC Licence: 131 4735


	
Description of work activity:      INSTALLATION OF STEELCRAFT® FRAMES AND TRUSSES


	
Name: 
	
Steelcraft Framing
ABN: 77 606 911 684
12 Forge Close
Sumner QLD 4074
Ph: (07) 3376 4824

	
High Risk Construction Work:

Select all ‘High Risk Construction Work’ which is applicable to this task/project

	
	Involves a risk of person falling 2 metres

	
	
	
	
	Is carried out on a telecommunication tower 

	
	
	
	
	Involves demolition of a load-bearing element of a structure

	
	
	
	
	Involves, or is likely to involve, the disturbance of asbestos

	Principal Contractor (PC)





Project Address:

	
Various
	
	
	Involves structural alterations or repairs that require temporary support to prevent collapse

	
	
	
	
	Is carried out in or near a confined space

	
	
	
	
	Is carried out in or near a shaft or trench with an excavated depth greater than 1.5m, or a tunnel  

	
	
	
	
	Is carried out on or near pressurised gas distribution mains or piping

	
	
	
	
	Is carried out on or near chemical, fuel or refrigerant lines

	Project Manager:
	Various
	
	
	Is carried out on or near energised electrical installations or services

	Contact Phone:
	
	
	
	Is carried out in an area that may have a contaminated or flammable atmosphere

	Construction Supervisor:
	Gordon Pirret
	
	
	

	Contact Phone:
	0477 726 618
	
	
	

	Person Responsible for ensuring compliance with SWMS
	Name: Gordon Pirret
	
	
	Involves tilt-up or precast concrete

	
	Signature: 
	
	
	Is carried out on, in or adjacent to a road, railway, shipping lane or other traffic corridor that is in use by traffic other than pedestrians

	
	Date: 
	
	
	

	Person(s) Responsible for reviewing the SWMS
	Name:  Brad Althaus (Director)
	
	
	Is carried out in an area at a workplace in which there is any movement of powered mobile plant

	
	Signature:  [image: ]
	
	
	Is carried out in an area where there are artificial extremes of temperature

	
	Date:  28/10/2019
	
	
	

	Date SWMS Provided to PC:
	
	Various
	
	
	Is carried out in or near water or other liquid that involves a risk of drowning

	Last SWMS Review Date:
	
	04/03/2019
	
	
	Involves diving work





PPE REQUIRED
	Hard hat (where required)
	X
	Respirator or Dust mask
	
	Harness
	 
	Erect Access Scaffolding
	
	Fall Arrest systems
	
	UV protection clothing
	X

	Safety Boots
	X
	Hand Protection - Gloves
	X
	Fire Extinguishers
	 
	Erect Warning Signs
	
	Protective Clothing
	X
	Sun Glasses
	X

	Eye Protection
	X
	Full Face Shield
	
	Barricades
	 
	Welding screen
	
	Sun Screen 30+
	X
	
	

	Ear Protection
	X
	High Visibility Shirt or Vest
	X
	Ventilation
	 
	Welding Face Shield
	
	Broad Brim Hat
	X
	
	

	
	
	
	
	
	 
	
	
	
	
	
	

	
	 
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	




 

	RISK TABLE
How bad is the hazard likely to be?
If a hazard is rated Level 1 [Extreme], Level 2 [High] or Level 3 [Moderate]
 Do not start work until the revised risk rating is either 4, 5 or 6
	
	
How to complete this safe work method statement

1) Adjust all details on the front page
2) Consult with the workers who are going to use this SWMS and make the necessary adjustments
3) “Risk Assessment Hazard Identification” - Inspect the site, identify the hazards that may be present and add to this SWMS
4) Job Steps- List the job steps in sequence of tasks required to carry out the work
5) Hazard Identification- List the potential hazards associated with each Job Step
6) Initial Risk- Using the “Risk Table”, rate the identified risks.
7) Control Measures Implemented- List the controls you will implement to reduce the risks to the lowest possible level
8) Revised Risk- Using the “Risk Table”, rate the level of risk once the controls have been implemented. If the revised risk rating is still 1, 2 or 3 do not start work until better control measures are implemented and the revised risk rating is 4, 5 or 6.
9) Person Responsible- List the name or position of the person or persons responsible for ensuring the controls are implemented
10) Ensure this safe work method statement is reviewed and revised if relevant control measures are revised.


	
WHAT DAMAGE COULD IT CAUSE?

	
VERY LIKELY
Could happen anytime.

	LIKELY
Could happen sometimes.
	UNLIKELY
Could happen, but only rarely.
	VERY UNLIKELY
Could happen, but probably never will
	
	

	Death or permanent disability.
	1
	1
	2
	3
	
	

	Long-term illness or serious injury. 
	1
	2
	3
	4
	
	

	Medical attention or several days off work.
	2
	3
	4
	5
	
	

	First Aid Needed
	3
	4
	5
	6
	
	

	1, 2 & 3 Indicates unacceptable hazard/risk that must be eliminated 
4, 5 & 6 Indicates acceptable hazard/risk
	
	




	
Step No
	Job Steps

Break the job down into steps.
List the steps in sequence of activities in this column.
	Hazard Identification

Identify any potential hazards associated with each step – and any related risks. Detail the hazards and risks in this column, and enter the risk rating in the next column.
	Initial Risk Rating [1 – 6]
	Controls Measures Implemented

Decide what control measures to use to eliminate or minimise the risks. Detail the control measures in this column, and enter the revised risk rating in the next column.
Note: If the revised risk rating is still 1, 2 or 3 do not start work until better control measures are implemented and the revised risk rating is 4, 5 or 6.
	Revised Risk Rating [1- 6]
	
Person Responsible

	
1
	Plan the job prior to arriving on site.
	· Inadequate training, consultation & planning
	3
	· Review the principal contractors Site Safety Plan 
· Provide adequate & competent supervision  
· Provide equipment to ensure job is completed safely
	5
	Supervisor &
Sub-Contractors

	

	
	· Lack of competence
	3
	· Ensure all workers are adequately trained and competent to undertake the work
	5
	Supervisor &
Sub-Contractors

	
	
	· Untrained personnel commencing work
	
	· All workers to have current General Induction Card
	
	Supervisor &
Sub-Contractors

	
2
	Entry to Site
	· First day on site, entry to unsafe areas.
	3
	· Report to site office. All workers to undertake site induction
	5
	Supervisor &
Sub-Contractors

	

	
	· Accessing site via other means than the main gate can lead to exposure to site hazards
	3
	· Entry to site to be via gate directed by site management.
· Review site access, parking and delivery area
	5
	Supervisor &
Sub-Contractors

	
3
	General Requirements
Identify site conditions

	· If site management are unaware of work being carried out then workers will be unaccounted for in the event of emergency evacuation
	3
	· Review the site emergency evacuation plan and advise site management of work activity for the day. 

	5
	Supervisor &   
Sub-Contractors       

	

	
	· Failure to follow traffic management plans can lead to injury, damage to vehicle or equipment
	2
	· Ensure Traffic management procedures developed by site management are followed

	5
	  Supervisor &            Sub-Contractors

	

	
	· Ignoring safety signs can lead to exposure to hazards and noncompliance with site safety

	1
	· Become familiar with the site safety signs and follow all instructions (e.g. wearing of appropriate PPE)

	5
	    Supervisor &          Sub-Contractors

	

	
	· Uneven ground can cause slip and fall injuries when moving tools and equipment to work area. 
	3
	· Check for slip and fall hazards and use designated areas to access work area. 
	5
	Supervisor &
Sub-Contractors           

	

	
	· Underground or overhead power can cause electrocution
	1
	· Identify the location of underground or overhead power lines on site
	4
	Supervisor &
Sub-Contractors          

	

	
	· Underground or overhead gas lines can cause serious burns in punctured
	1
	· Identify the location of underground or overhead gas lines on site
	5
	Supervisor &
Sub-Contractors        

	

	
	· Personal Injury
	2
	· Identify where the first aid kit is located.
· Identify who the first aider is on site.
· Identify the location of the toilets and amenities on site
· Each worker is required to wear the required PPE at all times.
· MSDS for any onsite materials are to be registered on site
	5
	Supervisor & 
Sub-Contractors         

	

	
	· Exposure to weather conditions
· UV Radiation when working in the sun
	2
	· Wear a hat 
· Use 30+ sunblock
· Eye and skin protection
	5
	Supervisor &
Sub-Contractors           

	

	
	· Fire
	3
	· Identify where the fire extinguisher is located
	5
	  Supervisor &          Sub-Contractors

	


	
	· Manual handling issues

	2
	· Use correct Manual Handling techniques.
· Utilise mechanical lifting devices where possible to minimise the need for manual work.
· Only lift within your capabilities. Use at least two people to lift heavy or awkward loads when mechanical means are not available. If load is to heavy do not move until mechanical means are available to assist
	5
	Supervisor &
Sub-Contractors          

	

	
	· Possible work at height 

	2
	· If working at heights - Ensure EWP (Elevating Work Platforms) are properly used or scaffold is properly erected for work and certified, Ensure fall protection measures are in place.  Only licensed personnel are to use EWP’s
	5
	Supervisor &           Sub-Contractors

	

	
	· Slips, trips & falls

	3
	· Signs, barricades or secure fencing are to be used to identify the work area.
· Site conditions must be clear, tidy and secure. Sufficient lighting to be in place
	5
	Supervisor &           Sub-Contractors

	

	
	· Risks associated with mobile plant
	2
	· Plan route and work area, keep area clean & tidy, monitor light levels. 
· Secure when transporting.
· Use spotter when reversing and positioning vehicles, observe site speed limit on site.
	6
	Supervisor &
Sub-Contractors

	
	Power Supply
	· Risks associated with using portable electrical equipment, flexible extension leads and portable power tools
	1
	· Ensure that power supply is protected by an RCD device (earth leakage/safety switch)
· All portable electrical equipment, flexible extension leads and portable power tools must be visually inspected for wear and tear before use.
· Ensure portable electrical equipment, flexible extension leads, portable power tools and RCD devices are regularly tested and carry current inspection tagged.
· Testing must be undertaken by a licensed electrician or a trained competent person.
· Use lead stands where required to keep leads elevated.

	5
	Supervisor &
Sub-Contractors

	
4

	Site Establishment
	· Site specific hazard such as traffic, excavations, overhead work, pedestrians
	3
	· Plan out the job with the site supervisor before commencing and ensure that suitable access/hazard control is available for the duration of the works
	5
	Supervisor &
Sub-Contractors



	
	Delivery of Materials
	· Injury from vehicle 
· Injury unloading materials
· Injury stacking materials 
· Materials blocking exits or footpaths
· Moving materials over long distances
· Stacked materials falling
	
	· Plan space and location requirements before materials arrive.
· Ensure delivery time has been pre-arranged.
· Driver to wear PPE
· Driver to ensure clear view is available or a spotter is in place while moving, reversing or unloading the vehicle
· Keep materials inside site boundaries. People must not be forced off footpaths or on to roadways.
· Have materials delivered as close as possible to work areas.
· Ensure materials are stacked safely and appropriately braced
· Use barricades and traffic control as required
	
	Supervisor &
 Sub-Contractors

	
	Unload materials or equipment from vehicle
	· Lifting – back injury
· Load falling on personnel
· Fall From vehicle
· Manual handling injuries
	3
	· Ensure that vehicle is parked on flat even surface
· Use proper lifting technique
· Ensure all employees have undergone manual handling training 
· Use mechanical assistance (crane/hiab)
· No personnel to stand under suspended load
· Only trained operator to use lifting equipment
· Do not exceed SWL of lifting equipment
· Use suitable lifting chains/slings that are in good condition and are related to lift the weight
· Ensure slings are secure
· Only licenced operator to use forklift
· Be mindful of overhead hazards
	5
	Supervisor &
 Sub-Contractors

	
5
	Setting up equipment
	· Slips, trips & falls
· Crush hands, cuts
· Damage to feet
	2
	· Set up equipment on level ground.
· Avoid rough & difficult terrain
· Use P.P.E equipment when required.
· Training in the set up of electrical leads.
· P.P.E equipment such as safety shoes
	5
	Supervisor &
Sub-Contractors

	
6
	Unloading of frames & trusses
	· Being struck by delivery trucks or crane
· Crane or lifting gear failure
	2
	· Site staff to be aware of entry & set up area of trucks & cranes.
· Crane & truck drives to be made aware of location of on-site personnel.
· Training & use of P.P.E equipment such as hard hats, safety vests.
· Only suitably trained personnel to work with plant & equipment.
· Plant & equipment to be maintained & operated by licenced person only.
	5
	Supervisor &
Sub-Contractors

	
7
	Placing of house
frames to ground floor
	· Falls & trips when carrying frames
	2
	· Clear area used for access
· Ensure site is clear of any debris, obstructions.
· Team lifting when required
	5
	Supervisor &
Sub-Contractors

	

	
	· Back & shoulder injury’s when standing frames
· Back injury & missing target when using sledge hammer while positioning frames
· Crushing, hit by falling objects
· Fall from step ladder when connecting frames
· Injury from concrete nail guns
· Electrocution
	2
	· Training in manual handling.
· Training in manual handling, personnel to be trained & shown the correct procedure in using a sledge hammer
· Remove any loose blocking before standing frames
· Ensure ladders are level & stable before using.
· Training in the use of portable ladders.
· Keep hands & limbs clear when firing guns.
· Provide training in the use of concrete nail guns.
	5
	Supervisor &
Sub-Contractors

	
8
	Laying first floor joists
	· Slips, trips & falls when carrying materials
· Fall from heights
	2
	· Clear work area of debris & obstructions
· Avoid rough terrain.
· Ensure team lifting when placement of joists off a ladder.
· Training in the use of portable ladders
	4
	Supervisor &
Sub-Contractors

	

	
	· Injury from impact drivers
· Electrocution
	1
	· Training in the use of impact drivers. 
· Keep hands & limbs clear of tip when fastening.
· Ensure site personnel are clear of the work area.
· Training in the set up of electric leads.
· Test & tagging of all power equipment
	4
	Supervisor &
Sub-Contractors

	

	
	· Cuts from angle grinders/ snips when cutting

	2
	· Training in the use of angle grinders/snips
· Ensure maintenance checks have been carried out on power tools
· Test & tagging of all power equipment
· Adequate PPE to be worn
	5
	Supervisor &
Sub-Contractors

	
9
	Laying of upper floor
sheet flooring
	· Slips & trips when carrying floor to loading position

· Hit by sheet flooring

· Back injury’s


	2
	· Ensure access & loading area is clear of debris and hazards underfoot.
· Full size particleboard sheets must be carried by two persons.
· Ensure correct lifting & carrying techniques are used at all times. 
· Training in manual handling
· Training in general lifting & carrying.
· Ensure team lifting
	5
	Supervisor &
Sub-Contractors

	

	
	· Falls from heights
	1
	· Training in the use of portable ladders
· Erect temporary handrail 
· Erect temporary work platform
· Lay floor sheeting from one corner working off work platform.
	4
	Supervisor &
Sub-Contractors

	
	
	· Electrocution


	1
	· Training in the use of power tools & running of leads
· Testing & tagging of all power equipment
	4
	Supervisor &
Sub-Contractors

	

	
	· Damage to eyes, hands & fumes from glues (long term illness)
	3
	· Use P.P.E equipment safety glasses, gloves when necessary. 
· Training in the use of hazardous substances.
	5
	Supervisor &
Sub-Contractors

	
10
	Installation of upper
floor wall frames
	· Slips, trips, falls when accessing upper floor area
	1
	· Ensure fall protection at floor perimeter & stair void is in place & all ground floor temporary bracing is adequate.
· Secure ladder access to first floor ensuring that ladders are secured.
· Training in the use of portable ladders.
	4
	Supervisor &
Sub-Contractors

	
	
	· Crushing, falling objects, cuts from straps
· Slips, trips, sprains & strains when lifting upper floor frames
	2
	· Ensure frames will not slide or fall when straps are cut. (Use tin snips of strap cutters)
· Straps should be cut so that they are prevented from striking the body.
· Place in waste enclosure immediately.
· Asses the path (clear rubble debris)
· Adjust edge protection to provide sufficient access to allow frames to be passed up to the floor deck.
· Assess the weight of frames. If frames are too heavy for manual handling, deploy mechanical means of lifting (e.g crane).
· If frames can be safely handled manually, persons handling the frames should lift frames using correct lifting techniques.
· Training in manual handling.
· Frames should be carried by the studs so that the frames will be in the correct position (plates at top & bottom) when placed against the side of the house.
· Hand frames up to persons above on upper floor level.
	5
	Supervisor &
Sub-Contractors

	
	
	· Falls from heights
	1
	· Training in working from heights.
· Training in use of portable ladders.
· Persons on top desk must stay back from edge as those on ground lift & tilt frames towards them.
· Persons on the upper floor level must hold the top section of the frames, pull them back towards the centre of the upper floor & lay them flat.
· Ensure floor is swept of sawdust & clear of waste materials to access area.
· Ensure handrails system is in place
	4
	Supervisor &
Sub-Contractors

	
	
	· Manual Handling


	2
	· Training in manual handling
· Training in general lifting & carrying.
· Ensure team lifting
	5
	Supervisor &
Sub-Contractors

	
	
	· Falls, slips, sprains, strains

	2
	· Ensure upper floor deck is clear of waste materials.
· Training in manual handling.
	5
	Supervisor &
Sub-Contractors

	
	
	· Frames over balancing & hitting persons
	1
	· Allocate one person to attend to the temporary braces, which should be ready before standing commences.
· Fit sufficient temporary bracing to hold the frame stable & secure.
	4
	Supervisor &
Sub-Contractors

	
	
	· Leaning on unsecured frames and falling
	1
	· All straps, connectors & fixing to top plates must be carried out using stepladders, (or similar) that are self-supporting and not lent against an unsecured frame.
	4
	Supervisor &
Sub-Contractors

	
	
	· Injury from impact driver
	1
	· Training in the use of impact driver 
· Keep hands & limbs clear when firing.
· Ensure site personnel are clear of firing area.
	4
	Supervisor &
Sub-Contractors

	
11
	Roof truss installation
	· Frames falling over when loading trusses
	1
	· Ensure all trusses are tied down and braced before loading roof.
· Check that all temporary bracing is adequate, as well as additional bracing needed for temporary stacking of trusses.
· Stand clear of trusses being loaded
	4
	Supervisor &
Sub-Contractors

	
	
	· Manual handling injury
	2
	· If trusses are too heavy for manual handling use mechanical means of lifting (i.e crane)
· Use correct lifting technique
· Training in manual handling
· The trusses are to be placed on the top plates in the order that minimises the amount of manual handling.
	5
	Supervisor &
Sub-Contractors

	
	
	· Hit by falling objects
	1
	· External scaffolding is to be erected before accessing roof on external walls.
· No one is to walk top plates or trusses.
· Trusses should be stockpiled by crane onto the top plates, which have been additionally braced to carry the extra temporary load. Work should be planned so that trusses are arranged in sequence to minimise handling during truss standing.
	4
	Supervisor &
Sub-Contractors

	
	
	· Hit by materials when being lifted by crane.
· Crane failure.
	1
	· Only licensed personnel to work plant & equipment
· P.P.E. equipment, such as hard hats, to be worn when working below or under crane
	4
	Supervisor &
Sub-Contractors

	
	
	· Falls, slips, trips, sprains & strains and structural collapse
	
	· Ensure the first truss is securely braced straight and plumb. (Working from a ladder and or scaffold)
· Ensure correct lifting techniques.
· Ensure working conditions are safe (i.e wet weather & excessive wind)
· Install all ties, noggings, binders, trimming, & tie downs to secure trusses.
	4
	Supervisor &
Sub-Contractors

	
	
	· Falls through stair voids
	1
	· Installation of stair void cover to be in place before access or working above
	4
	Supervisor &
Sub-Contractors

	
	
	· Cuts, crush hands
	3
	· Training in manual handling & the use of P.P.E equipment when required.
	5
	Supervisor &
Sub-Contractors

	
	
	· Electrocution
	1
	· Training in the set up of electric leads
· Test & tagging of all power equipment
	4
	Supervisor &
Sub-Contractors

	
	
	· Cuts & abrasions from the use of power tools
	2
	· Training in the use of angle grinders & circular saws
	5
	Supervisor &
Sub-Contractors

	
	
	· Falls, cuts, back injuries from removing work  platforms & unused bracing
	2
	· Remove work platforms in the reverse order that they were erected, working from stepladders from the floor below.
	5
	Supervisor &
Sub-Contractors

	
	
	· Damage to eyes, ears
	2
	· Training in the use of P.P.E eye and ear protection.
	4
	Supervisor &
Sub-Contractors

	
	
	· Frames falling over when loading roof trusses.
	1
	· Ensure that any locations designated for the landing of trusses will not overload the wall frames.
· Check that all bracing is adequate for the temporary stacking of roof trusses
	4
	Supervisor &
Sub-Contractors

	
	
	· Fall from heights
	1
	· Under no circumstances should any person walk the external top plate until the perimeter scaffolding is erected.
	4
	Supervisor &
Sub-Contractors

	
	
	· Truss frames falling over while standing trusses
	1
	· Placement of structural grade or aluminium planks adequately supported across their spans to be used to transport trusses into position.
· Ensure first truss is adequately braced before erecting the next truss.
· Ensure when transporting trusses across roof area that contact is maintained with the truss at all times.
· Do not lift trusses over others which have been erected.
· Always work from one end, standing main truss first and working within each truss as it is being erected.
· When fixing or moving trusses to outside plates, all work to be undertaken from scaffold.
· If scaffold can not be placed then trestle and planks or industrial ladders may be used for this procedure.
	4
	Supervisor &
Sub-Contractors

	
12
	Clean up & leave site
	· Inhale dust when sweeping
· Eye damage
	3
	· Training & use of P.P.E equipment safety glasses & dust masks
	5
	Supervisor &
Sub-Contractors

	
	
	· Hit by on-site vehicles, plant & equipment
	2
	· Ensure work vehicle is in a clear area when loading tools & equipment
	5
	Supervisor &
Sub-Contractors

	
	
	· Cuts, slips, trips when loading waste materials into bins
	3
	· Avoid rough terrain.
· Ensure clear access to waste bin
· Fold/ cut any sharp edges
	5


5
	Supervisor &
Sub-Contractors

Supervisor & Sub-Contractors
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CONSULTATION & SIGN OFF


	Declaration by Workers:
1. I have been consulted with and have assisted in the development of this Safe Work Method Statement.
2. I have been given the opportunity to comment on the content of this Safe Work Method Statement.
3. I have read and understand how I am to carry out the job steps listed, and will abide by the control measures outlined in this Safe Work Method Statement.
4. I have been supplied with the personal protective equipment identified in this SWMS and I have been given training in the safe use of this equipment.
5. I have read and understand the requirements set out in the  mateial safety data sheets for the hazardous substances identified in this Work Method Statement.
6. I will ensure that this safe work method statement is reviewed and revised if relevant control measures are revised.

	
NAME

	
OCCUPATION, QUALIFICATIONS, 
DUTIES, RESPONSIBILITIES
	
SIGNATURE
	
DATE
	
SIGNATURE
	
REVISED DATE
	
SIGNATURE
	
REVISED DATE
	
SIGNATURE
	
REVISED DATE
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