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RIICPL401E 
Supervise the installation of underground services using open excavation 

ASSESSMENT SUMMARY

The assessment activities for RIICPL401E Supervise the installation of underground services using open excavation cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Benjamin Wixon

	Participant signature
	[image: Shape

Description automatically generated with low confidence]



	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable



	Task
	Date completed
	Assessment Results 

	Theory Exam
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for RIICPL401E
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
	 Practical Assessment



	Assessor Name
	

	Assessor Signature
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RIICPL401E 
Supervise the installation of underground services using open excavation

THEORY EXAM


	Participant name
	Benjamin Wixon




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 
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	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	[bookmark: _Hlk82780839][bookmark: _Hlk82780839]




Q1.  [bookmark: _Ref95744510]You have been assigned the task of supervising open excavation for installing services. Complete the table below describing documents you need to review to confirm the work activity and compliance.

	Answer
	Type of document
	Documents required
	

	
	Project documents
	Project plans, specifications, drawings, work method statements (SWMS), job safety and environmental analysis (JSEA), inspection and test plans (ITPs), and site risk assessments. 
	

	
	Guidance documents
	Codes of practice, Australian Standards (e.g. AS 4744 for trenching), manufacturer instructions, and workplace policies or procedures for excavation and service installation. 
	

	
	Legislation
	Work Health and Safety Act and Regulations, Environmental Protection Act, local council permits, and any relevant utility authority requirements (e.g. Dial Before You Dig). 
	




Q2.  [bookmark: _Ref95745058]What type of information are you expecting to locate from the documents listed in Q1. ?

	Answer
	From the project documents, I’d expect to find details like job scope, trench dimensions, alignment of services, safety controls, and inspection requirements — basically, what needs to be done and how it must be done.
From the guidance documents, I’d be looking for safe work methods, trenching standards, and manufacturer instructions to make sure the work follows best practice and is compliant.
From the legislation, I’d check for legal requirements around excavation safety, environmental protection, and utility locating — making sure the site meets all WHS and regulatory obligations.

	[bookmark: _Hlk85785851]




Q3.  [bookmark: _Ref95819177]What are three (3) considerations you make as part of risk assessment processes during the ‘walk-through’ of the work area?

	Answer
	1. Ground conditions – check for soil stability, moisture, or signs of movement that could cause trench collapse.
2. Existing services – locate and mark utilities like gas, water, electrical, and communications before digging.
3. Access and controls – look at how plant, people, and materials will move safely around the area, and check that barriers, signage, and exclusion zones are in place.




	




Q4.  [bookmark: _Ref95819180]How would you divert runoff around stockpiles unavoidably located in drainage paths?

	Answer
	Earth berms, diversion drains, silt fences and rock check to slow down run off
	




Q5.  [bookmark: _Ref95819182]All workers must wear the PPE required by the site. Why is it particularly important for supervisors?

	Answer
	Its important to lead by example
	




Q6.  [bookmark: _Ref95819184]Where does the use of PPE fit in the risk management process?

	Answer
	PPE is the last line of defence. You use it after all other controls have been put in place.
Elimination
Substitution
Isolation
Engineering
Admin
PPE
	




Q7.  [bookmark: _Ref95820646]What would you read in the job plan to confirm the plan meets task requirements?

	Answer
	I’d check the scope of work, drawings, and specifications to make sure the plan matches what needs to be built. I’d also look at the methods, sequence of work, safety controls, and resource requirements to confirm everything lines up with site conditions and project standards. 
	



Q8.  [bookmark: _Ref95395099]Why is it important to understand the relationship of the job to other jobs within the project?

	Answer
	Because every crew’s work affects the next one. Knowing how your job fits in helps you plan around other activities, avoid clashes, and keep the project running smoothly.
	




Q9.  [bookmark: _Ref95822160]How do you confirm that required resources are available to meet job requirements?

	Answer
	I’d check the job plan and resource schedule to make sure all plant, materials, and labour are listed and booked in. Then I’d confirm deliveries, equipment availability, and crew availability
	




Q10.  [bookmark: _Ref95822122]Two (2) labourers assigned to your team have called in sick and are unable to attend site as allocated. How would you respond?

	Answer
	I would review the day’s work plan to see what can still be done safely with the crew I’ve got. If the workload’s too heavy or the task needs extra hands for safety, I’d arrange replacement labour through the site office or adjust the schedule to suit. 
	



Q11.  [bookmark: _Ref95823167]Once your team members have arrived on-site, how do you confirm that they understand their roles and all requirements?

	Answer
	Hold a prestart to run through the day’s tasks, safety points, and any changes, then go through the workpack with them which lists all the major steps of the task. Then when we are at the work face, we would develop a JHA/start card for the site conditions of that exact job to capture any other hazards not identified 
	




Q12.  [bookmark: _Ref95823171]What emergency response information should you be sure your team understands before undertaking work tasks?

	Answer
	What can go wrong
Who to call in case of an emergency (UHF, phone)
Muster points
landmarks, what 3 words etc to help emergency services
	




Q13.  [bookmark: _Ref95823276]How do you encourage workers to adhere to work zone traffic management controls such as exclusion zones and traffic routes?

	Answer
	I remind the crew during prestarts why the controls are in place — to keep everyone safe around machines and trucks. I make sure signs and barriers are clear and in good condition, and I lead by example by following the same rules myself. 
	




Q14.  [bookmark: _Ref95825228][bookmark: _Ref89768019]How can you support sub-contractors to achieve their responsibilities?

	Answer
	I’d start by making sure they fully understand the job scope, safety requirements, and site rules before they begin. I’d check their SWMS and make sure it lines up with our procedures. During the job, I’d keep communication open, checking progress, checking JHAs, giving feedback, and helping sort out any issues that could slow them down or cause safety risks. 
	




Q15.  [bookmark: _Ref95825323][bookmark: _Ref89769346]How do supervisors determine human resources and sub-contractors needed for the job plan?

	Answer
	I look at the job scope, timeline, and the type of work involved — like excavation, pipe laying, or backfilling — to figure out how many workers and what skills are needed. They also review the plan to see if any specialist tasks require subcontractors, such as electrical, drainage, or testing work. From there, they match labour and subcontractors to meet safety, quality, and schedule requirements. 
	




Q16.  [bookmark: _Ref95825718]What is the relationship between various areas of civil work and how are these relationships relevant when developing job plans and work schedules?

	Answer
	All civil works are linked. 
earthworks set up levels and foundations, drainage needs to go in before road layers, and services must be installed before final surfaces go down. If one stage runs late or isn’t coordinated, it holds up the others. Understanding these relationships helps plan the sequence properly, avoid rework, and keep everything moving safely and on schedule. 
	




Q17.  [bookmark: _Ref89775621]Elaborate on four (4) different types of estimates used when developing job plans.

	Answer
	1. Preliminary estimate – a rough early cost based on limited info, used to check if the project is viable before full planning. 

2. Detailed estimate – worked out from final drawings and specs, covering materials, labour, plant, and subcontractors. 

3. Unit rate estimate – based on cost per unit of work (like per metre of trench or per cubic metre of material), often used for comparison or tendering. 

4. Revision or variation estimate – done when changes happen on-site to update costs and schedules accurately. 
	



Refer to the following image and respond to Q18. Q19. and Q20. 
Depth 1.85m
Length 3.725m
Width 1.56m


Q18.  [bookmark: _Ref95826391]What is the total volume of the shape?

	Answer
	LxWxD
=3.725m×1.56m×1.85m
= 10.75 m³ 
	




Q19.  [bookmark: _Ref95826904]Calculate the surface area of the shape.

	Answer
	A = 2(LW + LD + WD)
=2×[(3.725×1.56)+(3.725×1.85)+(1.56×1.85)]
=2×(5.81+6.89+2.89)
=2×15.59
= 31.18 m² 

	




Q20.  [bookmark: _Ref95826914]Calculate the percent grade of the dotted line.

	Answer
	Rise/Run x 100
=1.85/3.725
=49.7%
	


Refer to the following image and respond to Q21. and Q22. 
Depth 1.58m
Length 3.545m
Width 1.34m



Q21.  [bookmark: _Ref95826969]Calculate the volume of the shape.

	Answer
	1.34x3.545x1.58
=7.51m³ 
	




Q22.  [bookmark: _Ref95826894]Calculate the grade of the dotted line as a percentage.

	Answer
	1.58/3.545
=45%
	




Q23.  [bookmark: _Ref95826917][bookmark: _Ref102633881]You need an excavator for 3 days and have been asked to make sure there is enough diesel to last the whole 3 days.  

[bookmark: _Ref95826917]The excavator uses 15 litres per hour and will be operating for approximately 6 hours per day.  The company buys its diesel at cost ($1.10 p/l) and it has a policy that requires all orders to include a contingency of 10%. 

How much diesel will you need to order?

	Answer
	15 L/hr × 6 hr/day × 3 days = 270 litres
10% of 270=27litres
270 + 27 = 297 litres
297 × 1.10 = $326.70 
	



Q24.  [bookmark: _Ref95891933]Clearly explain the steps you undertake when setting out the site for a trench.

	Answer
	Review plans and drawings – check the trench location, depth, width, and service alignment against project specs.

Locate existing services – use “Dial Before You Dig,” service plans, and physical markings to identify and protect any underground assets.
Mark out the trench line – use pegs, spray paint, or string lines to mark the trench centreline and edges according to design measurements.
Confirm levels and alignment – set out levels with a laser or dumpy level to make sure the trench runs to the correct depth and grade.
Install controls and signage – put up barriers, warning signs, and environmental controls (like silt fences or bunds) before excavation starts.

	




Q25.  [bookmark: _Ref95892261]A hold point may be required following the set out. Why would this be necessary?

	Answer
	A hold point is needed so the set-out can be checked and approved before any excavation starts. It gives engineers or supervisors a chance to confirm the trench location, depth, and alignment are correct and that all services have been identified. This prevents costly rework, damage to existing utilities, and safety issues once digging begins. 
	




Q26.  [bookmark: _Ref95826743]Write a description for each of the following trench collapse prevention methods (1) shoring, (2) benching (3) battering.

	Answer
	1. Shoring: Using supports like hydraulic shores, timber, or steel frames to hold up trench walls and stop them from collapsing. 

2. Benching: Cutting the trench sides into horizontal steps or levels. This reduces pressure on the walls and makes it safer for workers to enter. 

3. Battering: Sloping the trench walls back at a safe angle instead of keeping them vertical. It prevents collapse by letting the soil support itself naturally. 
	




Q27.  [bookmark: _Ref95889290][bookmark: _Ref95826745]Why is it important that the slope ratio not exceed the prescribed maximum value?

	Answer
	Because if the slope is too steep, the trench walls can’t support themselves and may collapse. Keeping within the prescribed ratio makes sure the batter angle suits the soil type and depth, keeping workers safe and the trench stable. 
	




Q28.  [bookmark: _Ref95893527]What does it mean, to monitor the excavation and installation process?

	Answer
	It means regularly checking that the work is being done safely, correctly, and according to the plans. This includes watching excavation depth and alignment, checking trench support systems, making sure controls stay in place, and confirming the installation of services meets specs and standards.
	




Q29.  [bookmark: _Ref95893530]What methods do you use to confirm the outcomes are being achieved according to the job requirements?

	Answer
	I’d check progress against the job plan, drawings, and ITPs to make sure everything lines up with the specs. I’d do visual inspections, measure levels and depths, and review test results or checklists. I’d also talk with the crew and subcontractors to confirm the work matches quality, safety, and environmental standards. 
	




Q30.  [bookmark: _Ref95894785]What is one (1) reason you may have to adjust the work practices and (2) what effect can this have on your work plan?

	Answer
	1. Unexpected site conditions/services

2. It can slow progress, change the sequence of tasks, or require extra resources or approvals. The plan might need updating to keep everything safe, compliant, and on schedule. 
	




Q31.  [bookmark: _Ref95895456]How do you record the changes and adjustments made to work practices mentioned in Q30. ?

	Answer
	I’d record any changes in the site diary or daily shift report, noting what changed, why it changed, and who approved it. If the change affects safety or quality, I’d also update the SWMS, ITP, or job plan and make sure the crew is briefed. This keeps everything documented and traceable for compliance and future reference. 
	




Q32.  [bookmark: _Ref95897233]If you come across an unidentified existing service during excavation work, which methods or procedures would you use to identify the service?

	Answer
	Double check the dials, looks for markers that could be overgrown or knocked over, trace/ndd the service
	




Q33.  [bookmark: _Ref95897235]What is the BYDA system and how would you go about getting the information sent out to you and by what means?

	Answer
	BYDA stands for Before You Dig Australia. It’s an online service that provides underground utility plans so you can locate services before starting excavation. To get the info, you submit an enquiry on the BYDA website with your site details and map area. The system then sends plans and service drawings by email, usually within a few hours, from all the relevant utility providers. 
	




Q34.  [bookmark: _Ref95899267]What are some characteristics, technical capabilities and limitations related to one (1) item of plant or equipment you should be monitoring during installation works?

	Answer
	Lifting capacity, lifting radius, ground pressures
	




Q35.  [bookmark: _Ref95899697]How do you, as the supervisor, confirm plant, equipment and tools maintenance requirements are carried out and recorded according to job requirements and manufacturer specifications?

	Answer
	I check that all plant and equipment have current service tags, logbooks, and prestart checklists completed by operators. I make sure any defects are reported and fixed before use, and that maintenance records match manufacturer specs and site procedures. I also keep copies or photos of the paperwork as part of the site documentation to show compliance. 
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RIICPL401E 
Supervise the installation of underground services using open excavation

PRACTICAL ASSESSMENT


	Participant name
	Benjamin Wixon




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1 (Occasion 1)
	Select Date.
	 Workplace
 Simulation
	
	
	

	Task 1 (Occasion 2)
	Select Date.
	 Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 
	Specify documents located, read and applied:



	1.1B. 
	Describe job to be undertaken:



	1.2J. 
	Specify what is set out for the tasks:



	1.3D. 
	Specify where measurements are recorded:



	1.3E. 
	Specify method of communication used with operators:



	1.3F. 
	Specify adjustments made:



	1.4A. 
	Specify reports submitted:



	1.4C. 
	Specify recommended changes:





	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 2

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 
	Specify documents located, read and applied:



	1.1B. 
	Describe job to be undertaken:



	1.2J. 
	Specify what is set out for the tasks:



	1.3D. 
	Specify where measurements are recorded:



	1.3E. 
	Specify method of communication used with operators:



	1.3F. 
	Specify adjustments made:



	1.4A. 
	Specify reports submitted:



	1.4C. 
	Specify recommended changes:







RIICPL401E
Supervise the installation of underground services using open excavation

	Practical Task 1 (2X)

	Description of task:
The participant must demonstrate the ability to supervise the installation of underground service using open excavation on two (2) occasions including:
· plan and prepare for underground service installation
· locate job plan and all associated documentation to confirm work requirements and compliance
· determine all risk controls required to address identified risks and hazards, including wearing PPE
· prepare team members to execute tasks
· check and confirm resource availability including human resources, organising as required
· prepare for and facilitate a pre-start meeting and walk the site with team to confirm roles and responsibilities, provide instruction and clarify questions
· set out task from plans and specifications using control lines, cleared width, batters and off-sets as required
· oversee the execution of tasks
· monitoring, measuring, testing according to task requirements to confirm outcomes are achieved according to job requirements
· perform calculations to confirm volumes, grades, percentages, area and resource consumption figures and supply rates
· initiate adjustments to work practice and job plans as required to meet job requirements
· confirm plant, equipment and tools maintenance requirements are carried out and recorded according to job requirements and manufacturer specifications
· report on execution of tasks
· complete and submit reports as required by organisational, authority and site requirements
· make recommendations related to required changes to confirm task execution meets job requirements

Tasks are at the Assessor’s Discretion, but detail of tasks undertaken must be recorded in the Assessor’s Comments (on the back of the Practical Assessment cover page).

	Resources required: 
Work site, work team, job plan and all associated documents (e.g. SWMS, permit to excavate) all plant, tools and equipment required for the task.



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Plan and prepare for underground service installation

	1.1A.  [bookmark: _Ref95901072]Locate the job plan and all associated documentation to confirm work requirements and compliance.
	
	

	1.1B.  [bookmark: _Ref95902918]Check contents of job plan against related documentation to confirm the installation of underground services using open excavation and any related pavement maintenance meets legislated and industry requirements.
	
	

	1.1C.  [bookmark: _Ref95903685]Read and confirm contents of SWMS and permit (as required) and facilitate implementation of required controls.
	
	

	1.1D.  [bookmark: _Ref95903710]Meet site requirements for personal  protective equipment.
	
	

	2 Prepare team members to execute tasks

	1.2A.  [bookmark: _Ref95903740]Prepare notes or presentation material for prestart meeting.
	
	

	1.2B.  [bookmark: _Ref95903486]Check availability of plant, equipment and tools for the tasks against schedule and potential conflicting requirements.
	
	

	1.2C.  [bookmark: _Ref95903753]Check human resources for availability of competent workers and confirm availability.
	
	

	1.2D.  [bookmark: _Ref95903757]Estimate material requirements using specifications for work and confirm availability onsite when required.
	
	

	1.2E.  [bookmark: _Ref95903767]Facilitate a pre-start meeting and walk the site with team to confirm roles and responsibilities and check for new or unexpected hazards.
	
	

	1.2F.  [bookmark: _Ref95903769]Use appropriate questioning and answering techniques to confirm worker understanding of tasks, roles and responsibilities.
	
	

	1.2G.  [bookmark: _Ref95904177]Clarify emergency response procedures including emergency rescue as required.
	
	

	1.2H.  [bookmark: _Ref95904179]Discuss and confirm worker understanding of work zone traffic management and safety
	
	

	1.2I.  [bookmark: _Ref95903771]Have workers read and sign understanding of SWMS related to tasks as applicable. 
	
	

	1.2J.  [bookmark: _Ref95903628]Set out tasks from plans and specifications.
	
	

	3 Oversee execution of tasks

	1.3A.  [bookmark: _Ref95904519]Confirm workers understand how to respond and refer client or public query.
	
	

	1.3B.  [bookmark: _Ref95905354]Watch work in progress, measuring consistently to ensure outcomes are achieved.
	
	

	1.3C.  [bookmark: _Ref95906253]Ensure trench collapse prevention methods are applied as required.
	
	

	1.3D.  [bookmark: _Ref95904981]Record measurements as taken.
	
	

	1.3E.  [bookmark: _Ref95905011]Assess operational techniques and apply approved method of communication to operators to ensure outcomes are achieved according to job requirements.
	
	

	1.3F.  [bookmark: _Ref95905126]Initiate adjustments to work practice and job plans as required to meet job requirements.
	
	

	1.3G.  [bookmark: _Ref95905401]Adhere to measuring and testing requirements, hold and witness points, recording and reporting as applicable in specifications.
	
	

	1.3H.  [bookmark: _Ref95905408]Check that plant, equipment and tools maintenance requirements are carried out and recorded as required by site and manufacturer requirements.
	
	

	4 Report on execution of tasks

	1.4A.  [bookmark: _Ref95905589]Complete and submit reports according to site requirements.
	
	

	1.4B.  [bookmark: _Ref95906507]Use sector-specific vocabulary, grammatical structures and conventions when writing reports.
	
	

	1.4C.  [bookmark: _Ref95905708]Recommend changes as required to confirm task execution meets job requirements.
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