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Waste Management Plan for 16 Sheehan Street 

Waste Types & Management Methods
	Waste Type
	Source/Activity
	Management Action
	Disposal Method

	Excavated Soil
	Site levelling & footings
	Reuse on-site if suitable or dispose to clean fill
	Local landfill or reuse on-site

	Concrete Offcuts
	Slab pour & finishing
	Minimize offcuts; collect in skip bin
	Construction waste facility

	Timber (formwork)
	Concrete forming
	Reuse where possible; collect offcuts
	Recycle timber where possible

	Colorbond Offcuts
	Cladding and roofing
	Store safely; return large pieces to supplier if viable
	Scrap metal recycler

	Plastic Wrap & Straps
	Material packaging
	Collect in designated bags or bins
	General waste or soft plastic recycling

	Pallets
	Material delivery
	Return to supplier or reuse
	Pallet recovery service or reuse on-site

	General Waste
	Miscellaneous construction waste
	Bin on site; segregate when practical
	Council collection or licensed facility



Bin & Storage Locations On Site
· 1 x 3m³ skip bin – for general construction waste
· 1 x labeled drum/bin – for metal offcuts (Colorbond, fasteners)
· Designated soil stockpile – for reuse or removal
· Pallet stacking area – behind site fence near entry

 Prohibited Practices
· No burning of waste on site
· No burying of materials
· No dumping in council bins or on public land
· All asbestos (if any) must be professionally removed (not expected on this project)

Waste Minimisation Strategies
· Order materials to exact sizes to reduce offcuts
· Use reusable formwork materials where possible
· Store materials properly to prevent weather damage
· Reuse pallets and packaging where safe
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