

	Handout 3 - CPCCBC4001 Apply building codes and standards to the construction process for Class 1 and 10 buildings

Cascade Peaks Construction Quality System: Mandatory Inspections
Mandatory Inspections
Buildings must be properly inspected by qualified certifier at various stages of its construction to ensure that the building meets relevant standards, local regulations, and requirements of the Building Code of Australia (BCA). These inspections ensure the safety of the users of the building when the building is finally completed.
Building Inspections for class 1a and 10 buildings
1. All building certifiers in Queensland must be licensed with the Queensland Building and Construction Commission (QBCC).
2. The Building Regulation 2021 requires mandatory inspections at the following stages for new houses (single detached class 1a buildings):
a. excavation – after excavation of foundation material and before the concrete for the footings, or slab, for the building are poured
b. footings – if the building is to have footings—after the placement of formwork and reinforcement for the footings but before the concrete for the footings is poured
c. slab – if the building is to have a slab—after the placement of formwork and reinforcement for the slab but before the concrete for the slab is poured
d. frame – inspection of the frame (note the breakdown of the framing stage under section 44 of the Building Regulation 2021)
e. final – inspection of any outstanding items and the collection of certificates, such as termite protection, wet area membrane installation, glazing, smoke alarms and energy efficiency.
f. 
3. Under the Building Regulation 2021, the only mandatory stage of inspection for class 10 buildings and structures (other than swimming pools) is the final stage of inspection. However, a building approval may list additional stages that require inspection.
4. Any problem identified during the inspection must be rectified to the satisfaction of the building certifier.
Damp and weatherproofing Inspections
1. Class 1a- single detached dwelling:
a. Weatherproof coating to external face of single-leaf masonry walls
b. Flashing to wall/roof junctions
c. Location and spacing of weepholes to cavity masonry walls
d. Flashing to door and window openings for sheet-clad external walls
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