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BSBOHS201A 
Participate in OHS processes


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
	Lana Lyons

	

	

	Participant signature
	



	Assessor name
	

	

	

	Assessor signature
	



	Date
	21/08/2019



	Number of questions
	Number of questions answered correctly
	Satisfactory?

	24
	
	Yes
	No

	
	
		

	ASSESSOR COMMENTS

	


Match the terms and definitions by writing the appropriate letter next to each number in the centre column.

	Answer
	Terms
	Answers
	Definition
	
	
	1
	PRA
	1 - F
	A
	Outline the requirements of the work to be undertaken.
	

	
	2
	JSA
	2 - E
	B
	Outline what to do in the event of fires and other accidents
	

	
	3
	Plans and specifications
	3 - A
	C
	Contains important information about hazardous materials or chemicals.
	

	
	4
	Manufacturer specifications
	4 - D
	D
	Outlines how tools and equipment should be used (e.g. lubricant levels, maintenance requirements).
	

	
	5
	SDS
	5 - C
	E
	Identifies hazards and potential hazards that may be encountered while working.
	

	
	6
	Emergency procedures
	6 - B
	F
	A personal assessment of risk
	




[bookmark: _Ref424210309][bookmark: _Ref412796746]For each of the hazards identified below, describe the injuries/damage they may cause (i.e. to fellow workers, other people and/or animals) and suggest a suitable control measure.

	Answer
	Hazard
	Injuries or damage
	Control measure
	
	
	Hazardous chemical
	-Respiratory Damage
- Skin Rashes
- Chemical Burns
	- MSDS located with all hazardous chemicals
- Spill Kits
- Eye & Body Wash Kits
- Complete JSA
	

	
	Noise
	-Hearing Damage
-Headaches
-Fatigue
	- Hearing Protection
- Exclusion Zones
	

	
	Manual handling
	-Strains
- Sprains
- Abrasions
	- Gloves
- Prework stretches
- Adhere to lifting limits as per SWMS (i.e 2 person lift etc)

	




[bookmark: _Ref415045277]Who should you speak to if you find problems (e.g. hazards, accidents and emergencies)?

	Answer
	Your Health & Safety Representative
	


[bookmark: _Ref406591713]What should you do if you discover a fault with plant, tools or equipment?

	Answer
	Stop using it, tag it out of service, report it to your supervisor & record the details of the fault
	



[bookmark: _Ref424211517]Which legislation relates to safety in the workplace? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
	☐	Occupational Health and Safety Act 2015 
	

	
	☒	Work Health and Safety Act 2011 
	

	
	☐	Safety Act 1900 
	

	
	☒	Safety and Health Act 2011 
	




[bookmark: _Ref424211632]True or False (Tick your response): Employers are required by legislation to implement safety measures which are reasonably practicable.

	Answer
	☒	True 
	
	
	
	☐	False 
	
	




[bookmark: _Ref424211634]True or False (Tick your response): Workers are required by legislation to follow reasonable employer directives (e.g. to undertake first aid and/or fire safety training).

	Answer
	☒	True 
	
	
	
	☐	False 
	
	





[bookmark: _Ref424213216]The following symbols appear under the heading ‘Required PPE’ on an SDS. What do the symbols represent?

	Answer
	Symbol
	Meaning
	
	
	
[image: ]

	Protective clothing must be warn
	

	
	
[image: ]

	Gloves must be warn
	

	
	
[image: ]

	Eye Protection must be worn
	

	
	
[image: ]

	Respirator Required
	




[bookmark: _Ref408209094]Describe the meaning and use of the signs displayed below.

	Answer
	Sign
	Meaning
	
	
	[image: First aid.jpg]
	First Aid Kit Locatable here
	

	
	[image: Do Not Enter Saftety Sign]
	Restricted work zone, do not enter
	

	
	[image: https://encrypted-tbn3.gstatic.com/images?q=tbn:ANd9GcRfZQGVU3BvP46nBERPIeqexiKuKX8OHW4dEmTYE6j-oAKUgPPkHw]
	Fire extinguisher locatable here
	





Refer to the Risk Matrix below when responding to Q10. to Q12. 

	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low




[bookmark: _Ref408921283]Which rating is designated for the highest risk and which rating is used for the lowest risk?

	Answer
	Highest Risk:  E = Extreme 
Lowest Risk:   L = Low 

	



[bookmark: _Ref408921265]What is the risk rating for the following circumstances: An event which is possible and would require low-level hospital treatment.

	Answer
	L- Low (3.Possible to 5.Very Unlikely
	



[bookmark: _Ref408921287][bookmark: _Ref412797660]What are the factors that would lead to a risk rating of E: Extreme?

	Answer
	The seriousness of the possible consequences of the hazard and the likelihood that those consequences will occur
	



[bookmark: _Ref424212548]When should safety checks be undertaken on machinery and equipment? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
	☐	Before operation
	

	
	☐	After operation
	

	
	☒	Both before and after operation
	



[bookmark: _Ref408921427]Order the elements of the hierarchy of control, from 1 to 6 (i.e. most effective to least effective).


	Answer
	Label (1 – 6)
	Element
	
	
	3
	Isolate the hazard
	

	
	6
	Provide and use Personal Protective Equipment (PPE)
	

	
	1
	Eliminate the hazard
	

	
	4
	Control the hazard by engineering means
	

	
	5
	Control the hazard by administrative means
	

	
	2
	Substitute the hazard
	




[bookmark: _Ref408921430]Why is elimination the best method of hazard control and PPE considered the least effective?

	Answer
	By eliminating the hazard completely there is no risk, the task is re-designed without the hazard.  By using the PPE method this means the hazard is still current and avoiding the risk relies on human behaviour (much higher risk of injury)
	



[bookmark: _Ref408921432]If you were to replace a flammable solvent with a water-based solvent, what category of control measure would that be under the hierarchy of control?

	Answer
	Substitution
	


[bookmark: _Ref401921251][bookmark: _Ref401900343]

[bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	
	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




[bookmark: _Ref415049799][bookmark: _Ref421093133]In a medical emergency, what is the first step in the DRSABCD action plan that you need to follow?

	Answer
	Danger Checked (ensuring no one else can be injured whilst assisting the person requiring medical attention)
	



[bookmark: _Ref421092991]In the event of a fire emergency, what should you do? 
Fill in the table below to explain the acronym R.A.C.E.

	Answer
	Letter
	Meaning
	
	
	R
	Remove People from Immediate Danger
	

	
	A
	Alert People of Emergency
	

	
	C
	Confine fire & smoke
	

	
	E
	Evacuate to the assembly area
	



[bookmark: _Ref414952615]What should you do as part of the clean up process? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
	☐	Store all plant, tools and equipment without cleaning
	

	
	☐	Maintain plant, tools and equipment
	

	
	☒	Dispose of materials that cannot be reused or recycled
	

	
	☒	Report faults in logbook and/or site records
	

	
	☒	Clean all plant, tools and equipment before storage
	




[bookmark: _Ref408921186]Read the scenario below and complete the Hazard Report Form.

SCENARIO
Today at 10:45am a delivery truck reversed into a car park (located at 54 Standish Street, Salisbury) to deliver gardening materials. There was nobody in the car park to guide the driver and he backed into a number of drums of diesel located to the left of the photograph (below).  One drum was pierced and its contents erupted from the container. 

The marked area on the photo represents the diesel spill, measuring 3m x 4m.











HAZARD REPORT FORM

	GENERAL

	Date
	21/8/2019

	Submitted by
	Lana Lyons – Contracts Administrator

	HAZARD DETAILS

	Location
	Car Park of 54 Standish Street, Salisbury

	Description of issue
	Delivery driver reversed into multiple diesel drums located in the carpark causing one of the drums to be pierced and as a result it spilled through the carpark.

	Risk class
	☒  Extreme
	☐  High
	☐  Medium
	☐  Low

	CONTROL MEASURES

	Corrective action required 
	-Driver to immediately switch off, and exit, vehicle to illuminate fire hazard
- Exclusion zone to be set up
- MSDS for the diesel drums to be reviewed and spill to be cleaned up/contained accordingly with required PPE
- When safe to do so the vehicle to be sent to wash out bay to ensure no external diesel is left on the delivery truck 

	Person to action
	Driver / Safety Officer
	When
	☒  Immediately
☐  Within 24 hours
☐  Within 7 days



	Answer
	
	


[bookmark: _Ref412803069]Who would you submit a hazard report form to?

	Answer
	Your health & safety representative and/or your supervisor 
	



[bookmark: _Ref412803089]Who would approve proposed risk controls and organise the required resources for implementation of the risk control?

	Answer
	Site Project Manager and/or Health & Safety Representative
	



[bookmark: _Ref424215038]Identify one (1) way you can assess if risk controls have been effective.

	Answer
	Monitor incident reports relating to the risk, if there was a timeframe relating to the implementation of the risk then review it after its implemented, discuss at team safety meetings and/or directly with those carrying out works in relation to the risk  
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