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CPCCBC4001A 
Apply building codes and standards to the construction process for low rise building projects


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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[bookmark: _Ref5882211]A Performance Solution must abide by which of the following? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Be assessed according to one or more of the Assessment Methods
	

	
		Go beyond the requirements of Deemed-to-Satisfy Provisions
	

	
		Comply with the Performance Requirements
	




[bookmark: _Ref5882213]True or False (Tick your response): The Performance Requirements of the National Construction Code can be achieved by using a Performance Solution, a Deemed-to-Satisfy Solution, or a combination of both.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref5882215]True or False (Tick your response): The term ‘Performance Solution’ in the NCC was formerly known as ‘Alternative Solution’.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref5882219]Where a Performance Solution has been proposed, which of the following documentation should be prepared and retained? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Details of the relevant Performance Requirements 
	

	
		Assessment Methods used to establish compliance with the relevant Performance requirements
	

	
		Details of any Expert Judgement relied upon
	

	
		Details of any tests of calculations used to determine compliance with the Performance Requirements
	

	
		Details of any Standards or other information which were relied upon
	





[bookmark: _Ref5950292]True or False (Tick your response): Where a Deemed-to-Satisfy solution has been proposed, all relevant plans/specifications should be retained.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that outline the Assessment Methods used to determine whether a Performance Solution or a Deemed-to-Satisfy Solution complies with the Performance Requirements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2
	Volume one
	




[bookmark: _Ref536106146]Identify the Australian Standard that relates to artificial lighting needed for safe movement, as noted in the NCC.

	Answer
	Section F health and amenity part  FF4.2 light and ventilation.
	



[bookmark: _Ref5782698]Identify the Volume and Parts of the NCC that outline the requirements for artificial lighting needed for safe movement for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 part 3.8,  3.8.4.3 
	Volume 1 part F4,  FP4.2   
	





[bookmark: _Ref5882620]Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to lighting:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements ____________ to ____________ are satisfied by complying with F4.12
F4.1							
FP4.5
FP4.1

(i) ____________ to ____________; and PartG6

(ii) For a building containing an occupiable outdoor area, ____________; and 
(iii) for farm buildings and farm sheds, ____________. 
Part H3

Where a Performance Solution is proposed, the relevant Performance Requirements must be determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)


	Answer
	

	



[bookmark: _Ref422743346][bookmark: _Ref531682593]Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to light:

Where an alternative light system is proposed as a Performance Requirement to that described in ____________, that proposal must comply with – P2.4.4
Part 3.8.4

(a) Performance Requirement ____________; and 
(b) the relevant Performance Requirements determined in accordance with ____________ and ____________ as applicable.A2.4(3)
A2.2(3)


	Answer
	

	



[bookmark: _Ref5882637]Identify the Australian Standard that relates to each of the listed types of fire fighting equipment, as noted in the NCC.

	Answer
	Equipment
	Australian Standard
	
	
	Fire hydrants
	AS 2419.1
	

	
	Fire hose reels
	AS 2441
	

	
	Portable fire extinguishers
	AS 24444 
	

	
	Smoke alarms
	AS 3786, AS 1670.1 
	



[bookmark: _Ref5882646]For each of the listed types of fire fighting equipment, identify whether they are required by the NCC (if so, identify the relevant Part).

	Answer
	Equipment
	Volume 1
	Volume 2
	
	
	Fire hydrants
	EP1.3, E1.2 
	Table 2.8


	

	
	Fire hose reels
	EP1.1 E1.4
	-
	

	
	Portable fire extinguishers
	EP1.2  E1.6
	-
	

	
	Smoke alarms
	E2.2a
	Part 3.7.5
	




[bookmark: _Ref531682022]Identify the applicable Act in your jurisdiction that outlines the requirements for smoke alarm installation in domestic dwellings. 
Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	


 Building fire and safety (domestic smoke alarms) legislation amendment regulation 2016
Part 3 13AC  
	
	Each smoke alarm must  comply with AS 3786 – 2014 
Contain a photoelectric sensor and not also contain an ionisation sensor.  
	





[bookmark: _Ref5883662]Identify the applicable Act in your jurisdiction that outlines the requirements for testing smoke alarms in domestic dwellings. 
Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Fire and Emergency Services Act 1990
Division 5A
104RD 
	Must be tested within 30 days before the start of tenancy, the lessor must test each smoke alarm in the dwelling in compliance with section 104RAA(3)
	




[bookmark: _Ref5952975]Identify the applicable Act in your jurisdiction that outlines what must occur if smoke alarm in a domestic dwelling does not operate upon testing and when any rectification must occur. Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Fire and Emergency Services Act 1990
Division 5A 104Rc
	If a smoke alarm does not operate upon testing the owner of the dwelling must immediately replace the smoke alarm
	




[bookmark: _Ref5883528]In observation of NCC Volume 2, identify three (3) aspects which should be checked with regards to smoke alarms.

	Answer
	Should be located in class 1a buildings in accordance with 3.7.5.3 and 3.7.5.5
Be powered from the consumers main source where a consumer mains source is supplied to the building and be interconnected where there is more than one alarm.  
	




[bookmark: _Ref5883676]Must all smoke alarms be interconnected in domestic dwellings? Explain your response with reference to legislation.

	Answer
	3.7.5.2 
Smoke alarms must- 
(D) be interconnected where there is more than one alarm. 

	



[bookmark: _Ref5883539]Fill in the blanks for the definition of fire compartments, referring to Volume 1 of the NCC:

Fire compartment means – 
(a) The total space of a building; or
(b) When referred to in –
(i) The Performance Requirements – any part of a building separated from the remainder by ____________ to fire such as _____________ and/or ____________ having an appropriate resistance to the spread of fire with any ____________ adequately protected; orfloors
walls
barriers
Openings 

(ii) The Deemed-to-Satisfy Provisions – any part of a building separated from the remainder by ____________ and/or ____________ each having an ____________ not less than that required for a fire ____________ for that type of construction and where all ____________ in the ____________ construction are protected in accordance with the DtS Provisions of the relevant Part. wall
openings
FRL
floors
walls
Separating 


	Answer
	
	



[bookmark: _Ref5787153]Identify the Volume and Parts of the NCC that outline the requirements for fire compartmentation and separation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 part 3.7.2
	Volume 1 Part C2
	



[bookmark: _Ref5885739]Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to fire compartmentation and separation:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements ____________ to ____________ are satisfied by complying with C2.14
C2.1
C1.14
C1.1
CP9
CP1

(i) ____________ to ____________, ____________ to ____________ and ____________ to ____________; and C3.1
Part G3
C3.17

(ii) in a building containing an atrium, ____________; and Part H1

(iii) for additional requirements for Class 9b buildings, ____________; and Part H3

(iv) for farm sheds, ____________. 
Where a Performance Solution is proposed, the relevant Performance Requirements must be determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)


	Answer
	

	



[bookmark: _Ref5885741]Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to fire separation:

Where an alternative fire separation design is proposed as a Performance Solution to that described in Part ____________ that proposal must comply with Performance Requirement ____________; and the relevant Performance Requirements determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)
P2.3.1
3.7.2


	Answer
	

	



[bookmark: _Ref5885751]Identify the Australian Standard referenced in NCC Volume 1 with regards to compartmentation and separation for electricity supply systems.

	Answer
	C2.13
	




[bookmark: _Ref5886137]Identify the Volume and Parts of the NCC that outline the level of fire resistance required for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 schedule 5  
	Volume 1 C1.14 
	




[bookmark: _Ref5951761]In a building’s specifications, an FRL is stated as being 90 / 60 / -. 
If exposed to a standard fire test, how many minutes can you expect this building element to last for the criteria listed below? 

	Answer
	Minutes
	Criteria
	
	
	-
	Insulation
	

	
	60
	Integrity
	

	
	90
	Structural adequacy
	




[bookmark: _Ref5886138]Fill in the blanks: 
According to NCC Volume 1, an electricity substation located within a building must be separated from any other part of the building by construction having an FRL of no less than ____ / ____ / ____ and have any doorway in that construction protected with a self-closing fire door having an FRL of not less than ____ / ____ / ____. 120
120
120
-
30
120


	Answer
	

	



[bookmark: _Ref5886140]Fill in the blanks: According to NCC Volume 2, if an electrical wire or cable penetrates a separating wall, the service and building element at the penetration must be identical with a prototype assembly which has been tested and achieve an FRL of not less than ____ / ____ / ____. -
60
60


	Answer
	

	




[bookmark: _Ref5886711]Identify the applicable Act in your jurisdiction that outlines the occupier’s requirements for maintaining prescribed fire safety installations (e.g. fire doors). Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Building Fire Safety Regulation 2008 
Division 3
	[bookmark: _GoBack]The occupier must ensure that maintenance of each fire safety installation for the building is carried out by an appropriate qualified person 
	




[bookmark: _Ref5958063]Identify the applicable Regulation in your jurisdiction that outlines the timeframes in which repair or corrective action must be taken when maintaining prescribed fire safety installations. Briefly identify the requirements. 

	Answer
	Regulation name and section(s)
	Requirements
	
	
	Building Fire Safety Regulation 2008
Division 3 

	Corrective action is taken no later than a month after the maintenance of the installation.
	




[bookmark: _Ref5886716]NCC Volume 1 outlines that fire doors must be fitted with smoke seals and the assembly must be tested in accordance with Australian Standards. To which classes of building does this specification apply?

	Answer
	Classes 2-9 
	



[bookmark: _Ref5886719]Do all fire doors require tags? Explain your response with reference to legislation.

	Answer
	Not all doors require fire tags. Under building act 1975 buildings approved after 1 April  1976 all require tags to be fitted, buildings approved before this date are not required to have tags fitted to the fire doors unless required by the local authority at the time of approval. 
	


[bookmark: _Ref5886882]Match the building classifications and their descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Classification
	Answers
	Description
	
	
	1
	Class 1
	1 - E
	A
	A non-habitable building or structure.
	

	
	2
	Class 2
	2 - H
	B
	A laboratory or a building in which a handicraft or process for the production, assembling, altering, repairing, packing, finishing or cleaning of goods or produce is carried on for trade, sale or gain.
	

	
	3
	Class 3
	3 - C
	C
	A residential building other than Class 1 or 2 which is a common place of long term transient living for a number of unrelated persons. 
	

	
	4
	Class 4
	4 - D
	D
	A dwelling in a building that is Class 5, 6, 7, 8 or 9 if it is the only dwelling in the building. 
	

	
	5
	Class 5
	5 - F
	E
	May be a single dwelling or a boarding house, guest hose or hostel with a floor area less than 300m2.
	

	
	6
	Class 6
	6 - G
	F
	An office building used for professional or commercial purposes, excluding buildings of Class 6, 7, 8 or 9.
	

	
	7
	Class 7
	7 - I
	G
	A shop or other building for the sale of goods by retail or the supply of services direct to the public.
	

	
	8
	Class 8
	8 - B
	H
	A building containing 2 or more sole-occupancy units, each being a separate dwelling. 
	

	
	9
	Class 9
	9 - J
	I
	A building which is a carpark or fore storage/display of goods or produce for sale by wholesale. 
	

	
	10
	Class 10
	10 - A
	J
	A building of a public nature.
	




[bookmark: _Ref5886883]What class of building would shops, restaurants and cafes belong to?

	Answer
	Class 6 
	



[bookmark: _Ref5886885]What class of building would a general medical practitioner’s office belong to?

	Answer
	Class 9 
	




[bookmark: _Ref423946303]True or False (Tick your response): At the design stage, it may not be clear who the final tenant will be (or how they will be using their tenancy), so as long as the design meets the minimum requirements of all the classifications, it could be used for any of the purposes.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531681692]Where parts of a building have different purposes, the classification of Class 1 may apply to the whole building if not more than what percentage of the floor area is used for a purpose which is a different classification? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		5%
	

	
		10%
	

	
		25%
	

	
		50%
	




[bookmark: _Ref5965263]The NCC aims to ensure structures appropriately withstand normal forces. Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definitions
	
	
	1
	Bending
	1 - B
	A
	A force which shortens or crushes.
	

	
	2
	Compression
	2 - A
	B
	A fore which stretches and squashes at the same time.
	

	
	3
	Shear
	3 - F
	C
	A force which tries to pull something apart.
	

	
	4
	Strain
	4 - E
	D
	Intensity of the internally distributed forces that resist a change in the form of a body.
	

	
	5
	Stress
	5 - D
	E
	Physical change in the dimensions of a structure that results from applying a load.
	

	
	6
	Tension
	6 - C
	F
	Created where two opposite forces try to cut, tear or rip something in two.
	





[bookmark: _Ref5965264]True or False (Tick your response): When a beam is loaded, the top is compressed and the bottom is in tension.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref5965265]True or False (Tick your response): When a cantilever is loaded, the top surface is in tension and the bottom is in compression.

	Answer
		True 
	
	
	
		False 
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