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RIICPL401E 
Supervise the installation of underground services using open excavation 

ASSESSMENT SUMMARY

The assessment activities for RIICPL401E Supervise the installation of underground services using open excavation cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Joshua Ferguson

	Participant signature
	Joshua Ferguson



	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable



	Task
	Date completed
	Assessment Results 

	Theory Exam
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for RIICPL401E
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
	 Practical Assessment



	Assessor Name
	

	Assessor Signature
	



Theory Exam - RIICPL401E Supervise the installation of underground services using open excavation

	Assessment Summary - RIICPL401E Supervise the installation of underground services using open excavation
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RIICPL401E 
Supervise the installation of underground services using open excavation

THEORY EXAM


	Participant name
	Joshua Ferguson




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref95744510]You have been assigned the task of supervising open excavation for installing services. Complete the table below describing documents you need to review to confirm the work activity and compliance.

	Answer
	Type of document
	Documents required
	

	
	Project documents
	- SWMS
- JSA
- TMP
- EMP
- SDS
- JSEA
	

	
	Guidance documents
	- State or territories codes of practice
- Australian standards on the works being undertaken
- Operation manuals 

	

	
	Legislation
	WHS Act
	




[bookmark: _Ref95745058]What type of information are you expecting to locate from the documents listed in Q1. ?

	[bookmark: _Hlk85785851]Answer
	- Policies & procedures
- legislations with in your state that you must adhere to 
- Codes of practice, WHS act for your state/ work 
- Hazards
- Controls 
- Safe operating procedures 
	




[bookmark: _Ref95819177]What are three (3) considerations you make as part of risk assessment processes during the ‘walk-through’ of the work area?

	Answer
	1. Working Space

2. Existing infrastructure & Utility Services 

3. The Disposal of Soil
	




[bookmark: _Ref95819180]How would you divert runoff around stockpiles unavoidably located in drainage paths?

	Answer
	By using an up-slope perimeter bank to divert runoff around stockpiles located in Drainage paths 
	




[bookmark: _Ref95819182]All workers must wear the PPE required by the site. Why is it particularly important for supervisors?

	Answer
	We set the standard that must be adhered to 
	




[bookmark: _Ref95819184]Where does the use of PPE fit in the risk management process?

	Answer
	PPE is a last resort where there is no other practical control measures lelft
	




[bookmark: _Ref95820646]What would you read in the job plan to confirm the plan meets task requirements?

	Answer
	Scope of works
	



[bookmark: _Ref95395099]Why is it important to understand the relationship of the job to other jobs within the project?

	Answer
	This will help with planning of resources and their availability 
	




[bookmark: _Ref95822160]How do you confirm that required resources are available to meet job requirements?

	Answer
	Through communication with HR & sub contractors. 
	




[bookmark: _Ref95822122]Two (2) labourers assigned to your team have called in sick and are unable to attend site as allocated. How would you respond?

	Answer
	Would thank them for the notification and ask for them to keep me updated so I was aware wether this will effect works the following day aswell.
	



[bookmark: _Ref95823167]Once your team members have arrived on-site, how do you confirm that they understand their roles and all requirements?

	Answer
	Through daily prestarts. Encourage them to speak up and ask any questions that they are unsure of
	




[bookmark: _Ref95823171]What emergency response information should you be sure your team understands before undertaking work tasks?

	Answer
	Evacuation plans
Emergency procedures
Emergency contact numbers
List of site first aiders
	




[bookmark: _Ref95823276]How do you encourage workers to adhere to work zone traffic management controls such as exclusion zones and traffic routes?

	Answer
	Include them in the risk analysis side of this as this will show them the risks involved and associated with this works. Will also help them understand the controls put in place to prevent any risk
	




[bookmark: _Ref89768019][bookmark: _Ref95825228]How can you support sub-contractors to achieve their responsibilities?

	Answer
	use good communication skills and show leadership in encouraging subcontractors to become part of the team. Keep them updated with upcoming works & variations aswell as keeping them notified of achievements and project progress.
	




[bookmark: _Ref89769346][bookmark: _Ref95825323]How do supervisors determine human resources and sub-contractors needed for the job plan?

	Answer
	This is done through the estimate and planning stage. Breakdown the project into major activities and then align them with the resources required to complete them. Create a schedule, find what activites can be completed at the same time maximising the use out of the resources available 
	




[bookmark: _Ref95825718]What is the relationship between various areas of civil work and how are these relationships relevant when developing job plans and work schedules?

	Answer
	various areas of civil work are related and their relationships are crucial for developing effective job plans and work schedules. Understanding these relationships helps ensure that projects are completed efficiently, safely, and within time and on budget
	




[bookmark: _Ref89775621]Elaborate on four (4) different types of estimates used when developing job plans.

	Answer
	1. Approximate estimate

2. Preliminary estimate

3. Detailed estimate

4. Basic cost
	



Refer to the following image and respond to Q18. Q19. and Q20. 
Depth 1.85m
Length 3.725m
Width 1.56m


[bookmark: _Ref95826391]What is the total volume of the shape?

	Answer
	10.75035m3
	




[bookmark: _Ref95826904]Calculate the surface area of the shape.

	Answer
	5.811m2
	




[bookmark: _Ref95826914]Calculate the percent grade of the dotted line.

	Answer
	49.66%
	


Refer to the following image and respond to Q21. and Q22. 
Depth 1.58m
Length 3.545m
Width 1.34m



[bookmark: _Ref95826969]Calculate the volume of the shape.

	Answer
	7.50M3
	




[bookmark: _Ref95826894]Calculate the grade of the dotted line as a percentage.

	Answer
	44.56%
	




[bookmark: _Ref102633881][bookmark: _Ref95826917]You need an excavator for 3 days and have been asked to make sure there is enough diesel to last the whole 3 days.  

The excavator uses 15 litres per hour and will be operating for approximately 6 hours per day.  The company buys its diesel at cost ($1.10 p/l) and it has a policy that requires all orders to include a contingency of 10%. 

How much diesel will you need to order?

	Answer
	297L
	



[bookmark: _Ref95891933]Clearly explain the steps you undertake when setting out the site for a trench.

	Answer
	 - Access site (entry and exit points, designated routes, spoil areas, material storage areas, existing services & Infrastructure, surfaces, levels )
 - Access required resources (look for effiency and effectiveness of resources)
- Mark out trench line so you can see where this runs in correspondence with any service crossings or infrastructure
- Access the site for any hazards that may arise while completing works
- Implement controls to allow the task to be completed safely 
- Start tasks
	




[bookmark: _Ref95892261]A hold point may be required following the set out. Why would this be necessary?

	Answer
	As a quality requirement to ensure that set out is in the right place before any works are started. This will ensure that no works are completed incorrectly leading to reworks and time delays
	




[bookmark: _Ref95826743]Write a description for each of the following trench collapse prevention methods (1) shoring, (2) benching (3) battering.

	Answer
	1. Shoring - A hard barricade inserted in to a trench that cannot be battered or benched. This ensures that in the case of side wall collapse that any working in the trench has a hard barricade eliminating any risk to a worker

2. Benching - Excavating the sides of a trench/excavation creating a serious of horizontal levels/steps. Usually with near vertical walls between levels/steps

3. Battering - where the sides of an excavation are cut on a 45 degree angle to minimise the risk of them collapsing
	




[bookmark: _Ref95826745][bookmark: _Ref95889290]Why is it important that the slope ratio not exceed the prescribed maximum value?

	Answer
	if slopes exceed maximum value (45 degrees) this increase the risk of the walls/sides collapsing as dirt generally breaks away at that 45 degree angel
	




[bookmark: _Ref95893527]What does it mean, to monitor the excavation and installation process?

	Answer
	It means to constantly to check the progress of this work looking for any issues that may arise while also ensuring that works are being completed properly and as per the job plan 
	




[bookmark: _Ref95893530]What methods do you use to confirm the outcomes are being achieved according to the job requirements?

	Answer
	Through hold points and regular inspections/monitoring
	




[bookmark: _Ref95894785]What is one (1) reason you may have to adjust the work practices and (2) what effect can this have on your work plan?

	Answer
	1. Heavy rain

2. This can delay works by minimising the amount of activities that can be completed at this time aswell as the possibility of reworks. 
	




[bookmark: _Ref95895456]How do you record the changes and adjustments made to work practices mentioned in Q30. ?

	Answer
	Through daily dairies and weekly reports
	




[bookmark: _Ref95897233]If you come across an unidentified existing service during excavation work, which methods or procedures would you use to identify the service?

	Answer
	Colour of service pipe, depth, location, markings 
	




[bookmark: _Ref95897235]What is the BYDA system and how would you go about getting the information sent out to you and by what means?

	Answer
	Before you dig Australia is national organistaion created to assist in locating known services/infrastructure with in an area to minimise any disruption or damage to these assets. 

This information can be gained through contacting them or via online services. 
	




[bookmark: _Ref95899267]What are some characteristics, technical capabilities and limitations related to one (1) item of plant or equipment you should be monitoring during installation works?

	Answer
	Excavator installing RCPs

Looking for 
- SWL
- Capabilities of the machine/Lifting equipment (is it the right equipment for the job)
- Lifting equipment in good working order
- Lifting equipment tested and tagged 
- Prestart done on equipment
- Any faults documented & reported
- Maintenance up to date

	




[bookmark: _Ref95899697]How do you, as the supervisor, confirm plant, equipment and tools maintenance requirements are carried out and recorded according to job requirements and manufacturer specifications?

	Answer
	This is done through regular inspection of log books with in the machine aswell as weekly inspections of plant to make sure maintenance is upto date and any issues are reported an not missed.
	



	Theory Exam - RIICPL401E Supervise the installation of underground services using open excavation
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RIICPL401E 
Supervise the installation of underground services using open excavation

PRACTICAL ASSESSMENT


	Participant name
	Joshua Ferguson




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1 (Occasion 1)
	Select Date.
	 Workplace
 Simulation
	
	
	

	Task 1 (Occasion 2)
	Select Date.
	 Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 
	Specify documents located, read and applied:



	1.1B. 
	Describe job to be undertaken:



	1.2J. 
	Specify what is set out for the tasks:



	1.3D. 
	Specify where measurements are recorded:



	1.3E. 
	Specify method of communication used with operators:



	1.3F. 
	Specify adjustments made:



	1.4A. 
	Specify reports submitted:



	1.4C. 
	Specify recommended changes:





	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 2

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 
	Specify documents located, read and applied:



	1.1B. 
	Describe job to be undertaken:



	1.2J. 
	Specify what is set out for the tasks:



	1.3D. 
	Specify where measurements are recorded:



	1.3E. 
	Specify method of communication used with operators:



	1.3F. 
	Specify adjustments made:



	1.4A. 
	Specify reports submitted:



	1.4C. 
	Specify recommended changes:







RIICPL401E
Supervise the installation of underground services using open excavation

	Practical Task 1 (2X)

	Description of task:
The participant must demonstrate the ability to supervise the installation of underground service using open excavation on two (2) occasions including:
· plan and prepare for underground service installation
· locate job plan and all associated documentation to confirm work requirements and compliance
· determine all risk controls required to address identified risks and hazards, including wearing PPE
· prepare team members to execute tasks
· check and confirm resource availability including human resources, organising as required
· prepare for and facilitate a pre-start meeting and walk the site with team to confirm roles and responsibilities, provide instruction and clarify questions
· set out task from plans and specifications using control lines, cleared width, batters and off-sets as required
· oversee the execution of tasks
· monitoring, measuring, testing according to task requirements to confirm outcomes are achieved according to job requirements
· perform calculations to confirm volumes, grades, percentages, area and resource consumption figures and supply rates
· initiate adjustments to work practice and job plans as required to meet job requirements
· confirm plant, equipment and tools maintenance requirements are carried out and recorded according to job requirements and manufacturer specifications
· report on execution of tasks
· complete and submit reports as required by organisational, authority and site requirements
· make recommendations related to required changes to confirm task execution meets job requirements

Tasks are at the Assessor’s Discretion, but detail of tasks undertaken must be recorded in the Assessor’s Comments (on the back of the Practical Assessment cover page).

	Resources required: 
Work site, work team, job plan and all associated documents (e.g. SWMS, permit to excavate) all plant, tools and equipment required for the task.



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Plan and prepare for underground service installation

	[bookmark: _Ref95901072]Locate the job plan and all associated documentation to confirm work requirements and compliance.
	
	

	[bookmark: _Ref95902918]Check contents of job plan against related documentation to confirm the installation of underground services using open excavation and any related pavement maintenance meets legislated and industry requirements.
	
	

	[bookmark: _Ref95903685]Read and confirm contents of SWMS and permit (as required) and facilitate implementation of required controls.
	
	

	[bookmark: _Ref95903710]Meet site requirements for personal  protective equipment.
	
	

	2 Prepare team members to execute tasks

	[bookmark: _Ref95903740]Prepare notes or presentation material for prestart meeting.
	
	

	[bookmark: _Ref95903486]Check availability of plant, equipment and tools for the tasks against schedule and potential conflicting requirements.
	
	

	[bookmark: _Ref95903753]Check human resources for availability of competent workers and confirm availability.
	
	

	[bookmark: _Ref95903757]Estimate material requirements using specifications for work and confirm availability onsite when required.
	
	

	[bookmark: _Ref95903767]Facilitate a pre-start meeting and walk the site with team to confirm roles and responsibilities and check for new or unexpected hazards.
	
	

	[bookmark: _Ref95903769]Use appropriate questioning and answering techniques to confirm worker understanding of tasks, roles and responsibilities.
	
	

	[bookmark: _Ref95904177]Clarify emergency response procedures including emergency rescue as required.
	
	

	[bookmark: _Ref95904179]Discuss and confirm worker understanding of work zone traffic management and safety
	
	

	[bookmark: _Ref95903771]Have workers read and sign understanding of SWMS related to tasks as applicable. 
	
	

	[bookmark: _Ref95903628]Set out tasks from plans and specifications.
	
	

	3 Oversee execution of tasks

	[bookmark: _Ref95904519]Confirm workers understand how to respond and refer client or public query.
	
	

	[bookmark: _Ref95905354]Watch work in progress, measuring consistently to ensure outcomes are achieved.
	
	

	[bookmark: _Ref95906253]Ensure trench collapse prevention methods are applied as required.
	
	

	[bookmark: _Ref95904981]Record measurements as taken.
	
	

	[bookmark: _Ref95905011]Assess operational techniques and apply approved method of communication to operators to ensure outcomes are achieved according to job requirements.
	
	

	[bookmark: _Ref95905126]Initiate adjustments to work practice and job plans as required to meet job requirements.
	
	

	[bookmark: _Ref95905401]Adhere to measuring and testing requirements, hold and witness points, recording and reporting as applicable in specifications.
	
	

	[bookmark: _Ref95905408]Check that plant, equipment and tools maintenance requirements are carried out and recorded as required by site and manufacturer requirements.
	
	

	4 Report on execution of tasks

	[bookmark: _Ref95905589]Complete and submit reports according to site requirements.
	
	

	[bookmark: _Ref95906507]Use sector-specific vocabulary, grammatical structures and conventions when writing reports.
	
	

	[bookmark: _Ref95905708]Recommend changes as required to confirm task execution meets job requirements.
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