Processes & Procedures for the control of hazardous chemicals
Chemical 1: 
Ajax Hydrogen Peroxide 30% 100 VOL
Hazard: flammable, corrosive
Potential worker exposure:
	Activity resulting in exposure to the  substance: 
	As bleaching agent to remove stains 

	 


 
	Frequency of Exposure:  
	​​☒​ 
	Daily 
	​​☐​ 
	Weekly  
	 

	 
	​​☐​ 
	Monthly 
	​​☐​ 
	Other: 
	 


 
	Period of exposure per frequency: 
	1 hour 


 
	Is the substance released or emitted into the work area? 
	​​☐​ 
	Yes 
	​​☒​ 
	No 


	Possible Absorption routes:  
	​​☒​ 
	Inhalation 
	​​☒​ 
	Skin 
	​​☒​ 
	Eyes 

	 
	​​☒​ 
	Ingestion 
	​​☐​ 
	Injection 
	 
	 



 Risk Assessment:	
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Risk Conclusion 
Medium, hydrogen peroxide is a corrosive liquid and can cause chemical burn if accidently spill on skin and lead to lost time injury. But with the appropriate PPE (safety glasses, full face shield, gloves, long sleeve shirt and pants), the chance of getting injury can be minimized.  

Training: All staff know the correct procedure and precautions for handling hydrogen peroxide and understand how to read the safety data sheet. 

Personal Protective Equipment (PPE): gloves, safety goggles, face shield, long sleeve & pants, closed-toe shoes 

Storage: 
- DO NOT repack. Use containers supplied by manufacturer only. 
- Drums and jerricans must be of the non-removable head type. 
- Where combination packages are used, and the inner packages are of glass, there must be sufficient inert cushioning material in contact with inner and outer packages 
- In addition, where inner packagings are glass and contain liquids of packing group I and II there must be sufficient inert absorbent to absorb any spillage 
- Hydrogen peroxide containing/ generating materials requiring rigid packaging.
- Store in: containers with vented lids; properly passivated aluminium containers; properly passivated stainless steel; polyethylene containers; porcelain; vitreous stoneware; Teflon lined containers.
-  Keep material away from light, heat, flammables or combustibles
- Keep cool, dry, and away from incompatible materials

Handling: 
- Ensure that a safety shower and eyewash station are accessible nearby.
- Do not allow clothing wet with material to stay in contact with skin
- Avoid personal contact and inhalation of dust, mist or vapours
- Provide adequate ventilation
- Avoid physical damage to containers
- DO NOT repack or return unused portions to original containers. Withdraw only sufficient amounts for immediate use
- Use only minimum quantity required
- Peroxides should be added slowly and cautiously to the reaction medium. This should be completed prior to heating and with good agitation
Spill Response:
- Have a spill kit accessible that includes absorbent materials and neutralizing agents.
- For small spills: Contain and absorb using appropriate materials.
- For large spills: Evacuate the area, cordon off, and notify emergency personnel.

First Aid:
- Skin Contact: Rinse with plenty of water for at least 15 minutes.
- Eye Contact: Flush eyes with water for at least 15 minutes and seek medical attention.
- Inhalation: Move to fresh air and seek medical attention if symptoms persist.

Disposal: Containers may still present a chemical hazard/ danger when empty. Return to supplier for reuse/ recycling if possible.

Exposure standards: Occupational Exposure Limit: 1ppm/1.4mg/m3 (Australia Exposure Standards)

Transportation & storage (including labelling & signage): 
Land transport: 
Transport hazard class: Class 5.1, subrisk: 8 
Limited quantity: 1L 
Air transport:
Transport hazard class: ICAO/IATA Class 5.1, ICAO/IATA subrisk: 8, ERG code: 5C
Limited quantity: 1L (Passenger and Cargo Maximum Qty / Pack)
Sea transport: 
Transport hazard class: IMDG Class: 5.1, IMDG Subrisk: 8 
Limited quantity: 1L 

Documentation and Record-Keeping:
- Maintain records of training, safety data sheets (SDS), incident reports, and waste disposal

Regular Review and Improvement:
- Periodically review procedures and update training and protocols based on new information or incidents
Processes & Procedures for the control of hazardous chemicals
Chemical 2: 
Esplanade Herbicide 
Hazard: Organ toxicity, Toxic to aquatic life 
Potential worker exposure:
	Activity resulting in exposure to the  substance: 
	As herbicide 

	 


 
	Frequency of Exposure:  
	​​​☐
	Daily 
	​​☐​ 
	Weekly  
	 

	 
	​​​ 
	Monthly 
	​​☐​ 
	Other: 
	 


 
	Period of exposure per frequency: 
	1 hour 


 
	Is the substance released or emitted into the work area? 
	​​☐​ 
	Yes 
	​​☒​ 
	No 


	Possible Absorption routes:  
	​​☒​ 
	Inhalation 
	​​☒​ 
	Skin 
	​​☒​ 
	Eyes 

	 
	​​☒​ 
	Ingestion 
	​​☐​ 
	Injection 
	 
	 



 Risk Assessment:	
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Risk Conclusion 
Medium, esplanade herbicide may cause damage to organs (Nervous system) through prolonged or repeated exposure. But with the appropriate PPE (safety glasses, full face shield, gloves, long sleeve shirt and pants), the chance of getting injury can be minimized.  

Training: All staff know the correct procedure and precautions for handling esplanade herbicide and understand how to read the safety data sheet. 

Personal Protective Equipment (PPE): gloves, safety goggles, face shield, long sleeve & pants, closed-toe shoes 

Storage: 
- Keep containers tightly closed in a dry, cool and well-ventilated place 
- Store in original container
- Store in a place accessible by authorized persons only
- Protect from freezing
- Keep away from direct sunlight
- Keep away from food, drink and animal feedingstuffs

Environmental precaution: Do not allow to get into surface water, drains and ground water

Handling: 
-Use only in area provided with appropriate exhaust ventilation. 
-Advice on protection against fire and explosion 
-Keep away from heat and sources of ignition. 
- Hygiene measures Avoid contact with skin, eyes and clothing. Keep working clothes separately. Wash hands before breaks and immediately after handling the product. Remove soiled clothing immediately and clean thoroughly before using again. Garments that cannot be cleaned must be destroyed (burnt).

Spill Response:
-Soak up with inert absorbent material (e.g. sand, silica gel, acid binder, universal binder, sawdust). Clean contaminated floors and objects thoroughly, observing environmental regulations. Keep in suitable, closed containers for disposal.

First Aid:
- General advice: When possible, have the product container or label with you when calling a poison control center or doctor or going for treatment. Move out of dangerous area. Place and transport victim in stable position (lying sideways). Remove contaminated clothing immediately and dispose of safely. Inhalation Move to fresh air. Keep patient warm and at rest. Call a physician or poison control center immediately.
- Skin contact: Wash off thoroughly with plenty of soap and water, if available with polyethyleneglycol 400, subsequently rinse with water. If symptoms persist, call a physician. 
- Eye contact Rinse immediately with plenty of water, also under the eyelids, for at least 15 minutes. Remove contact lenses, if present, after the first 5 minutes, then continue rinsing eye. Get medical attention if irritation develops and persists. 
- Ingestion: Rinse mouth. Do NOT induce vomiting. Call a physician or poison control center immediately

Disposal: 
-Triple-rinse containers before disposal. Add rinsings to spray tank. Do not dispose of undiluted chemicals on site. If recycling, replace cap and return clean containers to recycler or designated collection point. If not recycling, break, crush, or puncture and deliver empty packaging to an approved waste management facility. If an approved waste management facility is not available, bury the empty packaging 500 mm below the surface in a disposal pit specifically marked and set up for this purpose, clear of waterways, desirable vegetation and tree roots, in compliance with relevant Local, State or Territory government regulations. Do not burn empty containers or product. 

Exposure standards:
[image: ]

Documentation and Record-Keeping:
- Maintain records of training, safety data sheets (SDS), incident reports, and waste disposal

Regular Review and Improvement:
- Periodically review procedures and update training and protocols based on new information or incidents
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