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CPCCBC4013A 
Prepare and evaluate tender documentation


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	ASSESSOR COMMENTS

	


[bookmark: _Ref515968645]Describe each of the listed types of building contract.

	Answer
	Contract
	Description
	
	
	Cost-plus
	 takes two forms:
The builder is entitled to be paid the cost of the work plus a commission 
The builder is paid the cost plus a fixed fee (which also may be reduced if the estimated cost of the work is exceeded by the actual cost)

	

	
	Lump sum
	Where the builder is to complete the works according to specification, within an agreed timeframe and for an agreed sum. Lump-sum contracts can be of two types:
‘Fixed’ or ‘firm’ price – which have no provision for variation on price due to cost fluctuations
‘Subject to rise and fall’ – which allows for price variations

	

	
	Nominated subcontract
	A subcontract within the scope of the main contract for works, whereby the subcontractor is chosen by the architect.
	

	
	Schedule of rates
	The cost of the work is calculated by applying an agreed schedule of rates to the work actually performed, which is measured. This occurs where the extent of the works cannot be specified at the time of letting the contract (e.g. jobs with extensive earthworks)

	




[bookmark: _Ref516047220]Name and describe four (4) documents that may be referred to by a builder considering submitting a tender.

	Answer
	Tender document
	Description
	
	
	Drawings and specifications
	The client will have met with a design consultant (e.g. architect) to interpret their needs by developing drawings and specifications (e.g. specific materials to be used). 

	

	
	Bill of quantities
	Formal quantities determined by a professional quantity surveyor using the architect’s specifications and drawings. By referring to this document, builders should avoid the risk of making errors in measuring such quantities themselves. It also provides a common basis for competitive tendering.

	

	
	Project parameters
	e.g. cost schedules, estimated timeframes
	

	
	Specific terms and conditions
	Terms and conditions that are unique to the particular project
	



[bookmark: _Ref428791704]Identify five (5) risks that should be considered by a builder interested in submitting a tender.

	Answer
	- Breach of contract
- circumstances such as delivery delays, progress payment delays, labour shortages, weather
- disputes over payments
Industrial disputes
Non-performance
	



[bookmark: _Ref496191791]Describe two (2) company policies that may impact on whether a contract is selected for tender.

	Answer
	Policy
	Description
	
	
	1
	Tendering policy
	

	
	2
	Procurement policy
	




[bookmark: _Ref516420356]Identify two (2) financial guidelines and two (2) administrative guidelines that must be observed when considering a tender.

	Answer
	Guidelines
	Description
	
	
	Financial
	Check calculations
Verify costs
	

	
	Administrative
	Ensure documentation meets company quality standards
Check tender documents against contract
	



[bookmark: _Ref497317156]Which of the following are considered direct costs? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Labour costs
	

	
		Material costs
	

	
		Office overheads
	

	
		Plant costs
	

	
		Profit
	

	
		Site overheads
	

	
		Subcontract costs
	




[bookmark: _Ref516237612]Which of the following are considered indirect costs? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Labour costs
	

	
		Material costs
	

	
		Office overheads
	

	
		Plant costs
	

	
		Profit
	

	
		Site overheads
	

	
		Subcontract costs
	




[bookmark: _Ref516420096]Explain how labour costs are established, referring to:
· Labour constant
· Labour quantities
· Labour rates

	Answer
	Labour constant: Anticipated time required for a particular item of work (e.g. 2 hours/m3 to excavate trench)
Labour quantities: Quantity of work required for the item of work in question (e.g. 20m3 to be excavated)
Labour rates: Monetary rate for work performed (e.g. $x per m3 of trench excavated or $y per hour)

	


[bookmark: _Ref516420098]Explain the following types of direct material waste that must be considered when calculating material costs.

	Answer
	Type
	Description
	
	
	Design
	Overestimating the required amount so that there is wastage left over
	

	
	Rejection
	Once delivered to site the quality is not up to standard
	

	
	Mishandling
	Poor handling and/or storage of materials onsite leading to damages and breakages
	




[bookmark: _Ref516420099]Explain the following types of indirect material waste that must be considered when calculating material costs.

	Answer
	Type
	Description
	
	
	Substitution
	Using material in a way other than intended
	

	
	Production
	Construction technique is different to original plan resulting in wastage
	

	
	Negligence
	Mistakes in production or estimating
	

	
	Criminal actions
	Theft or vandalism
	




[bookmark: _Ref516420101]Identify three (3) costs that must be considered when calculating plant costs.

	Answer
	Mobilisation
Plant purchase or hire costs
Running and maintenance
Labour or operator cost
	


[bookmark: _Ref516420103]List the two ways in which subcontractors may provide a price for their work.

	Answer
	An all-inclusive price
A schedule of unit rates

	



[bookmark: _Ref516420106]Identify ten (10) trades that may be required for a residential or commercial building project.

	Answer
	Surveyor
Concreter
Block/brick layer
Carpenter
Electrician
Plumber
Tiler
Plasterer
Roofer
Drainer

	



[bookmark: _Ref497317794]True or False (Tick your response): Each subcontractor is individually responsible to the client for a job tendered by a builder.

	Answer
		True
	
	
	
		False
	
	




[bookmark: _Ref516421466]Name one (1) type of project costing software.

	Answer
	Expert estimation
	




[bookmark: _Ref516420843]True or False (Tick your response): Using costing software can assist builders undertake calculations in short timeframes during the tendering process.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref516420157]True or False (Tick your response): Profit is usually calculated as a percentage of the total, rather than on each item throughout the tender.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref516420161]True or False (Tick your response): Each level of government (i.e. federal, state and local) has its own rules regarding tender submissions.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref516425355]Identify one (1) example of each of the following documents that impacts on building work conducted in Queensland.
[bookmark: _GoBack]
	Answer
	Type
	Description
	
	
	Building and Construction Code
	Building Code of Australia (BCA) (Volumes 1 and 2)
	

	
	Standard
	AS 1684 Residential timber-framed construction
	

	
	Government regulation
	Queensland Building and Construction Commission Regulation 2003
	




[bookmark: _Ref516420166]Identify four (4) types of supporting documentation that you may include with a tender submission.

	Answer
	Artist’s impressions
Organisational information
Product information
Promotional material
	



[bookmark: _Ref516420272]Explain the importance of checking the accuracy of a tender.

	Answer
	A contractual arrangement comes into existence at the moment a tenderer is informed that their tender has been accepted
	



[bookmark: _Ref516420201]Identify an appropriate staff member within an organisation who may approve/endorse/modify a tender prior to submission to the client.

	Answer
	Estimating manager
	



[bookmark: _Ref516421208]True or False (Tick your response): There is a general rule for how long tenders are called for, so specific due dates are not listed.

	Answer
		True 
	
	
	
		False 
	
	





[bookmark: _Ref516423005]You have a formwork job that will take three (3) weeks to complete. 
You are required to hire a range of materials, according to the Bill of Quantities listed below. Allow 15% for loss and damage.

Complete the calculations to determine the costs for the required materials.

	Materials
	Quantity
	Hire rate per week

	Frame 1
	18
	$0.60

	Frame 2
	18
	$0.55

	Brace
	2 x 30
	$0.20

	Base plate
	36
	$0.10

	‘U’ plate
	36
	$0.30

	Pin
	36
	$0.10

	Bearer
	39.6m
	$0.20

	Joints
	165m
	$0.15



	Answer
	Frame 1 18 x $0.60 x 3 = $32.40
Frame 2 18 x $0.55 x 3 = $29.70
Brace 60 x $0.20 x 3 = $36.00
Base Plate 36 x $0.10 x 3 = $10.80
‘U ’plate 36 x $0.30 x 3 = $32.40
Pin 36 x $0.10 x 3 = $10.80
Bearer 39.6 x $0.20 x 3 = $23.76
Joints 165m x $0.15 x 3 = $74.25
Total = $250.11
Total including loss and damage = 115% x $250.11 = $287.63
	


[bookmark: _Ref516423132]For the job in Q24. you must also hire workers to install the plywood for the formwork, at a rate of $15/hour. There is 70m2 of plywood to be installed. Assume the labour constant is 1.10hrs/m2.

Complete the labour calculations.

	Answer
	Hours to complete plywood install = 70m2 x 1.10hrs/m2 = 77hrs
Cost to complete plywood install = $15/hour x 77 hrs = $1155.00
	



[bookmark: _Ref516423607]For the job in Q24. and Q25. you have determined that the overheads and profit will constitute 10% of the materials and labour cost. 

Calculate the total project cost.

	Answer
	Hire costs total = $287.63
Labour cost total = $1155.00
Overheads and profit = 10/100 x ($287.63 + $1155.00) = $144.26
Total project cost = $287.63 + $1155.00 + $144.26 = $1566.89
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