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CPCCBC4012B 
Read and interpret plans and specifications 
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4012B Read and interpret plans and specifications cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 
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	 Satisfactory 
	 Not Yet Satisfactory
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	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
	Lauren McKew

	
	

	Participant signature
	
	
	

	Date
	21/01/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	87
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	




	ASSESSOR COMMENTS

	


Q1.  Plans and specifications are used to inform which of the following processes? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Building contracts
	

	
		Development applications 
	

	
		Estimation
	

	
		Planning
	

	
		Supervisory tasks
	

	
		Tenders
	




Q2.  [bookmark: _Ref532191033]Which compass direction is always shown on plans and drawings?

	Answer
	North.
	



Q3.  [bookmark: _Ref427670124]What information is provided on a location plan?

	Answer
	A location plan sets out the exact location of the site for construction. Information on the location plan includes the Lot Number/s, deposit plan numbers, North Point and Scale to identify exactly where the site is within a location/development area. 
	



Q4.  [bookmark: _Ref427670125]What detail does a site or block plan contain?

	Answer
	A site or block plan contains the information on the block where the proposed building/structure is to be located. It will include a datum which identifies a reference height to other levels on the site. It will also depict where on the site the building is situated and its orientation to the North point. 
	


Q5.  [bookmark: _Ref427670660]What do floor plans identify?

	Answer
	Floor plans identify the details of the proposed building or structure. Floor plans show details such as the rooms, their relative sizes, where fixtures are located, floor covering information and general set out of the internal rooms/areas of the proposed building. 
	



Q6.  [bookmark: _Ref427671793]What is a landscape plan and what information might it provide?

	Answer
	Landscaping plans identify the specific details of exterior items such as details of plants to be installed/planted, paths, garden areas and layouts, retaining walls and other landscaping features to be included as part of the project. 
	



Q7.  [bookmark: _Ref427670661]What are elevation views? What do they provide to the plan reader?

	Answer
	Elevation views of the proposed building/structure provide further detail on the exterior elements of the project with views from the side of the building shown (ie. east, west, north and south. Items such as building heights, levels, finishes, doors, windows and roof types are often depicted on elevation views. 
	



Q8.  [bookmark: _Ref427670662]What is a section?

	Answer
	As section view is a drawings detail which appears as if the building or structure has been cut in half at some point of the build. It shows the internal features and requirements in further detail than what an elevation plan shows. Items such as wall thickness, wall material, structural requirements, wall finishes, wall heights and levels, proposed roof construction and the relationship between different spaces in the building.  
	



Q9.  [bookmark: _Ref427670664]What are detailed drawings?

	Answer
	Detailed drawings depict particular information on a required service or finish relevant to the build. For example, plumbing details, electrical details, wiring details, heating/cooling details, structural details etc. are all specific areas of the build which require exact and detailed information to ensure the build is constructed in accordance with relevant codes and standards. It also assists the relevant trades in preparing their quote for the works and ensuring their scope of works is detailed as required.
	



Q10.  [bookmark: _Ref427671414]What are specifications?

	Answer
	Specifications provide information on all key details relevant to the project. Specifications generally include a full description of the scope of the works, details specific products (including types, brands, models, thickness, colours etc required), materials and finishes to be used, details of all fixtures and fittings to be installed and any other important information relevant to the desired outcome of the project. Specifications are read in conjunction with the plans as they provide specific details on what is to be used throughout the project and what the expected result of the project is.   
	




Q11.  [bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	ACRYL
	Acrylic
	

	
	AS
	Australian Standard
	

	
	ASSD
	Assumed Datum
	

	
	B
	Basin
	

	
	BN
	Bull Nose
	

	
	BTH
	Bathtub
	

	
	BWK
	Brickwork
	

	
	CB
	Concrete Block
	

	
	CF
	Concrete Floor
	

	
	CG
	Clear Glass
	

	
	CJ
	Ceiling Joint
	

	
	CORR
	Corrugated
	

	
	CWT
	Cold Water Tank
	

	
	DG
	Double Glazing
	

	
	DH
	Double Hung
	

	
	DPC
	Damp Proof Course
	

	
	DSB
	Distribution Switch Board
	

	
	DW
	Dishwasher
	

	
	EJ
	Expansion Joint
	

	
	FPBD
	Fibrous Plaster Board
	

	
	FFL
	Finished Floor Level
	

	
	FHR
	Fire Hose Reell
	

	
	GPO
	General Purpose Outlet
	

	
	HBD
	Hardboard
	

	
	HTR
	Heater
	

	
	HWD
	Hardwood
	




Q12.  [bookmark: _Ref427675022]Name each of the drawing symbol images shown in the table below.

	Answer
	Name
	Image
	
	
	Wall – Cavity Double Brick
	[image: Wall - Cavity brick]
	

	
	Wall – Brick Veneer 
	[image: Wall - Brick veneer]
	

	
	Wall – Timber Stud
	[image: Wall - Timber stud]
	

	
	Window in Cavity Wall
	[image: Window - In cavity wall]
	

	
	Window in Single Wall
	[image: Window - In single wall]
	

	
	Single opening door 90deg.
	[image: Door - Swing single]
	

	
	Double door, two leaves. 90deg opening each
	[image: Door - Swing double]
	

	
	Cavity sliding door
	[image: Door - Sliding into pocket]
	

	
	Exposed sliding door/ external door
	[image: Door - Sliding exposed on wall]
	

	
	Power socket outlet - general
	[image: Socket outlet (power) - general]
	





Q13.  [bookmark: _Ref427733304]Identify what the following window symbols represent on elevations.

	Answer
	Item
	Drawing
	
	
	Hinged at side
	[image: ]
	

	
	Hinged at top
	[image: ]
	

	
	Sliding horizontally
	[image: ]
	

	
	Fixed
	[image: ]
	




Q14.  [bookmark: _Ref532192707]What does a clouded area on a plan indicate?






	Answer
	That a change or amendment has been made to the drawing and the pricing/specifications etc. should be checked to see if the change results in the requirement for a variation to be charged or a tradesperson/subcontractor to be notified. 
	



Q15.  [bookmark: _Ref532192900]An amendment to specifications could relate to which of the following? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Contact details of all construction crew members
	

	
		Materials or products used
	

	
		Methods of carrying out specified work
	





Refer to the title block below to respond to Q16. to Q18. 
[image: ]
Source: http://www.dtwd.wa.gov.au/sites/default/files/teachingproducts/BC1934_CCBY.PDF 

Q16.  [bookmark: _Ref531861864]On what date was an amendment made to the window details?

	Answer
	5 October 2011
	



Q17.  [bookmark: _Ref532193187]True or False (Tick your response): Details of the window in Q16. should also be reflected in the specifications and confirmed with the client.

	Answer
		True 
	
	
	
		False 
	
	




Q18.  [bookmark: _Ref531862015]What amendment occurred on 08/11/2011?

	Answer
	The robe in bedroom 3 was removed.
	




Refer to the site plan below to respond to Q19. to Q26. 

[image: Site plan for a block of land showing existing building and proposed residence plus other detail]


Q19.  [bookmark: _Ref531861219]What structure is being built on this site? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Residence
	

	
		Road
	

	
		Shed
	

	
		Water meter
	




Q20.  [bookmark: _Ref532193598]What is the Lot number of this site?

	Answer
	Lot 16
	



Q21.  [bookmark: _Ref532193601]What is the size of this lot?

	Answer
	3,653m2
	



Q22.  [bookmark: _Ref532193617]Is the shed at the north-east of the proposed structure to be removed or retained? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Removed
	

	
		Retained
	




Q23.  [bookmark: _Ref532193558]True or False (Tick your response): The sewer is at the eastern boundary of the property.

	Answer
		True 
	
	
	
		False 
	
	




Q24.  [bookmark: _Ref532193550]True or False (Tick your response): The driveway is located to the south of the proposed property.

	Answer
		True 
	
	
	
		False 
	
	



Q25.  [bookmark: _Ref532193569]What size is the easement on the eastern boundary of the site?

	Answer
	5 meters
	



Q26.  [bookmark: _Ref531861509]True or False (Tick your response): The stormwater drain is constructed from PVC pipe.

	Answer
		True 
	
	
	
		False 
	
	




Refer to the contour plan below to respond to Q27. to Q28. 

[image: contourplan]

Q27.  [bookmark: _Ref531872622]What is the level at the northernmost point of the site?

	Answer
	3.94
	



Q28.  [bookmark: _Ref532193453]Which end of the site has the lowest level? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		East
	

	
		West
	



Refer to the sectional drawing below to respond to Q29. to Q49. 

[image: cross_section]
Q29.  [bookmark: _Ref427660755][bookmark: _Ref532194571]Give a brief description about the building from the detail available in the sectional drawing. Is it the same structure proposed in Q19. to Q26.?

	Answer
	2 storey brick home to be constructed as per sectional plans and in accordance with specifications. Scissor trusses to be utilised for roof construction and finished with corrugated colourbond. The building is the same structure proposed in questions 19 – 26 however the sectional detail provides further information about the construction of the residence.  
	



Q30.  [bookmark: _Ref427733756]Who is the client?

	Answer
	H & M Smith
	



Q31.  [bookmark: _Ref427733757]Where is this project to be built?

	Answer
	Lot 16 Glenvalley Road, Richmond, Victoria, 3216 
	



Q32.  [bookmark: _Ref427733759]What are the contact details for the draftsman?

	Answer
	Joe Foreman
Ph: 0395142311
Mob: 0413 113 113
Address: 18 Fairview Road, Richmond, Victoria, 3216
	



Q33.  [bookmark: _Ref427733761]What sheet number is this drawing?

	Answer
	5 of 7
	



Q34.  [bookmark: _Ref427660519][bookmark: _Ref427733762]What timber is required for loading and non-load bearing walls?

	Answer
	F5 Grade Timber
	


Q35.  [bookmark: _Ref427733763]What spacing is recommended for common studs?

	Answer
	Maximum of 600mm
	



Q36.  [bookmark: _Ref427733765]What type of roof truss is to be installed?

	Answer
	Scissor Truss
	



Q37.  [bookmark: _Ref427733766]What centres are the trusses positioned at?

	Answer
	900mm Spacing
	



Q38.  [bookmark: _Ref427733769]What size are the veranda posts?

	Answer
	90mm x 90mm
	



Q39.  [bookmark: _Ref427733771]What timber species are the veranda posts to come from?

	Answer
	Dar Oregon
	



Q40.  [bookmark: _Ref427733773]What pitch is the roof?

	Answer
	30 degree pitch
	




Q41.  [bookmark: _Ref427733774]What size are the noggings and at what spacing?

	Answer
	Noggins at 35mm x 70mm with maximum 1350mm spacing.
	



Q42.  [bookmark: _Ref427733776]What size are the ceiling joists?

	Answer
	HJ 240mm Joists
	


Q43.  [bookmark: _Ref427733778]What timber is used for roof battens and what spacing?

	Answer
	F5 Timber, 35mm x 70mm at maximum 900mm spacing. 
	



Q44.  [bookmark: _Ref427733780]What thickness is the plasterboard sheeting?

	Answer
	10mm Plasterboard
	



Q45.  [bookmark: _Ref427733781]What type of flooring is to be installed?

	Answer
	15mm Plywood flooring.
	



Q46.  [bookmark: _Ref427733783]What is the roof cladding material?

	Answer
	Corrugated Colourbond roofing to be used (colour not specified)
	



Q47.  [bookmark: _Ref427733784]Where will you find information about the footings?

	Answer
	The foundation plans, usually with the sectional drawings will show information on the required sizes and depths of the footings. 
	



Q48.  [bookmark: _Ref427733786]What do the letters ‘DAR’ refer when timber ordering?

	Answer
	DAR refers to timber being Dressed All Round which means the timber has been machined on all sides to leave a smooth surface. 
	



Q49.  [bookmark: _Ref427662218]Explain what ‘240 x 63 LVL’ refers to on the sectional drawing. What do the letters ‘LVL’ refer to?

	Answer
	It means that a 240mm high x 63mm wide joists are to be used to support level 1 of the build. LVL refers to Laminated Veneer Lumber which is a high strength engineered wood product primarily used for structural purposes in construction.  
	


Refer to the drawing below to respond to Q50. to Q65. 

[image: ]

Q50.  [bookmark: _Ref427663500]What is the number of the drawing?

	Answer
	2
	



Q51.  [bookmark: _Ref427734104]What is the Job Number?

	Answer
	00R-112
	



Q52.  [bookmark: _Ref427734106]What is the scale of the drawing?

	Answer
	1:100
	



Q53.  [bookmark: _Ref427733995]What does the drawing show?

	Answer
	The drawing is showing the elevations and a sectional drawing of the proposed building to provide information on the external treatments and structural elements of the build. 
	



Q54.  [bookmark: _Ref427734110]Which view shows the front of the house?

	Answer
	East Elevation 
	



Q55.  [bookmark: _Ref427734113]How many motor vehicles can be parked in the garage?

	Answer
	2
	



Q56.  [bookmark: _Ref427734114]What are the window and doors made from?

	Answer
	Aluminium
	



Q57.  [bookmark: _Ref427734116]What is the size of the eaves?

	Answer
	450mm
	


Q58.  [bookmark: _Ref427734119]What are the eaves lined with?

	Answer
	Hardiflex
	



Q59.  [bookmark: _Ref427734120]What type of roof structure is the roof built from?

	Answer
	Timber framed roof truss structure. 
	



Q60.  [bookmark: _Ref532197046]Which Part of the NCC should be read for more detail about the requirements for the roof structure in Q59.?

	Answer
	Volume 2 of the NCC, Part 3.4.3 – Timber Framing provides more detail regarding requirements for the roof structure for this build.
	



Q61.  [bookmark: _Ref532197154]Which Australian Standard should be read for more detail about the roof structure in Q59. ?

	Answer
	Australian Standard 1684 will provide further detail regarding roof structure depending on whether or not the proposed building is in a cyclonic or non-cyclonic region. 
	



Q62.  [bookmark: _Ref427734122]What is the roof cladding materials made from?

	Answer
	Concrete roof tiles.
	



Q63.  [bookmark: _Ref532197156]Which Part of the NCC should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	Volume 2 of the NCC, Part 3.5.2 – Roof Tiles and Shingles provides more detail regarding requirements for the roof cladding for this build
	



Q64.  [bookmark: _Ref532197157]Which Australian Standard should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	Australian Standard 2050 will provide details regarding the roof cladding material requirements.
	



Q65.  [bookmark: _Ref427663512]What is the roof pitch?

	Answer
	22.5 degree pitch.
	



Q66.  [bookmark: _Ref531871432]Identify one (1) regulatory body you may need to submit plans to for approval?

	Answer
	Local Council for a Building Approval.
	



Q67.  [bookmark: _Ref532197251]Briefly describe the approval process and timeframes for an approval through the regulatory body in Q66. 

	Answer
	A building certifier is required to certify the building plans for approval and lodge them with Cairns Regional Council. Documents which must be lodged with Council as well as the application fee include the building application (Planning Act Form 2), Notice of engagement (Form 56), decision notice (Form 6), Final inspection certificate, Copy of plans, drawings and specifications and other stamped approved document and any other documents relevant to the building works (ie. fire safety reports, encumbrances or estates etc.). Applications are usually approved within one week provided all documentation is provided and the build meets requirements of Council and relevant standards/codes.  
	



Q68.  [bookmark: _Ref427673788]What is a prime cost (PC) item? Give an example.

	Answer
	A prime cost or PC item is a sum included in a contract for purchasing of specific items – usually fixtures, such as appliances, sanitaryware, tiles or doors. It is an agreed amount included when the contract is entered into before the specific item has been selected for the build. The estimate for the PC item must be at least the lowest amount that the item could reasonably cost. An example of a PC inclusion could be bathroom tapware allowance which are required to be selected after the contract is signed but before construction can start.  

	



Q69.  [bookmark: _Ref427673790]What is a provisional sum (PS) item? Give an example.

	Answer
	A provisional sum or PS item is a sum that is included in a contract to cover works and/or materials which are not specifically detailed at the time of entering into the contract. Estimates to the best of the builder’s ability are required to be provided as part of the provisional sum however sometimes the amount may be exceeded due to unforeseen circumstances. An example of a provisional sum item could be removing existing vegetation from the site prior to works commencing ie. clearing and grubbing of the site. 
	


Refer to the Bill of Quantities below to respond to Q70. to Q76. 

[image: ]
[image: ]

Source: http://organizedbuilders.com.au/sites/default/files/BOQ-Summary.pdf 



Q70.  [bookmark: _Ref531867328]True or False (Tick your response): This Bill of Quantities represents a job for a two-storey house.

	Answer
		True 
	
	
	
		False 
	
	




Q71.  [bookmark: _Ref532199102]Identify two (2) materials being used for the floors?

	Answer
	Carpet and vinyl flooring.
	



Q72.  [bookmark: _Ref532199110]True or False (Tick your response): A landscaper has been contracted for this job.

	Answer
		True 
	
	
	
		False 
	
	




Q73.  [bookmark: _Ref532199056]How much does the contracted plasterer cost?

	Answer
	$12,900
	



Q74.  [bookmark: _Ref532199058]How much do the kitchen appliances cost?

	Answer
	$2,700
	



Q75.  [bookmark: _Ref532199060]What percentage of the total cost does the fixing stage represent of the building contract?

	Answer
	23%
	



Q76.  [bookmark: _Ref531866973]What percentage of the total cost does the completion stage represent of the building contract?

	Answer
	17%
	


Refer to the Purchase Order below to respond to Q77. to Q82. 

[image: ]
Source: http://organizedbuilders.com.au/sites/default/files/Databuild-Bill-of-Quantities.pdf 

Q77.  [bookmark: _Ref531874116]How many Pine F5 90 x 45 studs (2.4m long) are required?

	Answer
	100
	



Q78.  [bookmark: _Ref532199470]If the material in Q77. increased in cost to $2.75 each, what would be the total cost for this material?

	Answer
	$275.00
	



Q79.  [bookmark: _Ref532199474]How many sheet of ply are required in total (i.e. all sizes)?

	Answer
	13
	



Q80.  [bookmark: _Ref531874121]What material has the highest total cost?

	Answer
	Pine 90 x 45 mgp10 (long lengths) for studs over 2.7m long.
	



Q81.  [bookmark: _Ref531874448]How many metres are required of the material in Q80. ?

	Answer
	322.5m
	



Q82.  [bookmark: _Ref531874565]What beam is identified as being a better option than F17?

	Answer
	E14 beams
	




Refer to the labour chart below to respond to Q83. to Q86. 

[image: ]
Source: https://www.archsd.gov.hk/media/89170/sor2013_vol1_builders_works_2013_11_04.pdf 



Q83.  [bookmark: _Ref531873766]Based on the hourly rates given, which is the least expensive trade to contract?

	Answer
	Asphalter 
	



Q84.  [bookmark: _Ref532199773]If the trade in Q83. were to be contracted for two (2) hours’ work, how much would this cost?

	Answer
	$214.80
	



Q85.  [bookmark: _Ref531873865]Based on the hourly rates given, which is the most expensive trade to contract?

	Answer
	Bar Bender and Fixer
	



Q86.  [bookmark: _Ref531873882]If the trade in Q85. were to be contracted for six (6) hours’ work, how much would this cost?

	Answer
	$1,285.80
	



Q87.  [bookmark: _Ref531691201]Name the building legislation (Act and Regulations) that apply within your jurisdiction and should be referenced when reading plans and building contracts.

	Answer
	Australian Standards, National Construction Code, Build Act 1975 (Qld) and the Building Regulation 2006 (Qld) as well as the requirements as per the Cairns Regional Council and the Planning Act 2006 should all be referenced when reading plans and building contracts. 
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Lauren McKew

	
	

	Participant signature
	
	
	

	Date
	20/01/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4012B
Read and interpret plans and specifications

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to read and interpret plans and specifications in order to inform estimation, planning and supervisory activities. 

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include:
· Any drawing with a cloud or mark-up you have inserted.
· Copy of the correspondence regarding mark up and any site management/authorising engineer response.

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Drawings (including site plan), Specifications, Tender documentation, Telephone, Facsimile machine, Computer. 

	Assessment of task

	Name of participant:
	Lauren McKew

	Name of observer:
	Jarryd Londino

	Role of observer 
(Confirm suitability to sign)
	Project Manager

	Email address of observer
	jarryd@fgf.com.au

	Signature of observer:
	
	Date:
	20/01/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Interpret drawings

	1.1A.  [bookmark: _Ref531698368]Identify purpose and advantage of different types of drawings.
		
	1.1B.  Identify different aspects of drawings.
		
	1.1C.  [bookmark: _Ref531698394]Identify, understand and apply:
· Commonly used symbols and abbreviations
· Common building and construction terms on drawings
		
	1.1D.  [bookmark: _Ref531698402]Identify building site from location drawings.
		
	1.1E.  [bookmark: _Ref531698498]Identify on the site plan:
· True north
· Building orientation
· Key features in relation to building and other structures
· Levels
· Contours
· Service entry points
· Site features to be removed or retained
		
	1.1F.  [bookmark: _Ref531698586]Identify key features of plans, elevations and sections.
		
	1.1G.  [bookmark: _Ref531698588]Identify client requested variations to standard plans on drawings.
		
	2 Interpret specifications 

	1.2A.  [bookmark: _Ref531698592]Identify and correctly apply Provisional Sum (PS) and Prime Cost (PC) values. 
		
	1.2B.  [bookmark: _Ref531698596]Identify and confirm customer variations to standard specifications and communicate changes to organisational personnel. 
		
	1.2C.  [bookmark: _Ref531698601]Apply and communicate correct interpretations of essential elements to estimation, planning and supervisory tasks (including labour hours/costs and material quantities/costs).
		
	1.2D.  [bookmark: _Ref531698605]Identify Building Codes or standards affecting the work to be undertaken (including references to Australian Standards and the National Construction Code). 
		
	1.2E.  [bookmark: _Ref531698612]Identify key features of products included in the specification, including the design, purpose, aesthetics and cost relationships. 
		
	3 Communicate with others

	1.3A.  [bookmark: _Ref531698617]Consult with industry professionals, clients, organisational personnel and appropriate local authorities.
		
	1.3B.  [bookmark: _Ref530479080]Effectively communicate using the following methods:
· Verbally using language/concepts appropriate to cultural differences
· Non-verbal communication
· Using technology (including telephone, facsimile, email)
		
	The Participant’s performance was:  Satisfactory     Not Satisfactory



	OBSERVER COMMENTS

	Lauren is competent in reading and interpreting plans and specifications. As part of her role in supporting myself and our other project managers and estimating team, interpreting drawings is a key aspect of her day-to-day requirements. Lauren is confidently able to do take-offs for procurement purposes from interpreting various drawings and is able to effectively communicate proposed changes and subsequent variations. Lauren is also required to undertake extensive document control and preparations of drawing registers and transmittals for all projects and any changes that come through on drawings from clients, engineers and consultants. This requires ability to recognise changes between revisions and accurately record updates as they are received. I believe Lauren has an excellent understanding of reading and interpreting drawings and is able to effectively perform this aspect of her job.  
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