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CPCCBC4053 
Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4053 Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Anya English 

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	12/10/2023
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	20/10/2023
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	10/11/2023
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4053
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Practical Assessment
	 Documentation of design and construction (suitability or evidence of suitability)
 Fire protection inspection checklist



	Assessor name
	

	Assessor signature
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THEORY EXAM


	Participant name
	Anya English




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref127186634]Provide a brief description of the given classes of buildings according to the National Construction Code (NCC). 

	Answer
	Assessment method
	Description
	

	
	Class 2 building
	Class 2 building is a building containing two or more sol-occupancy units. These units must be a separate dwelling. 
	

	
	Class 3 building
	Residential buildings that fall outside class 1 and 2 long term / transient living accommodation for non-related people i.e. boarding home, guest home, dormitory style health care facilities, residential parts of motels, hotels, schools, hospitals and jails.

	

	
	Class 4 building
	A building is the only dwelling or residence within any class 5, 6, 7, 8 or 9 buildings. 
	

	
	Class 5 building
	Office building used for professional or commercial purposes e.g. law office, general medical practitioners fall outside of class 6, 7, 8, 9 buildings. 
	

	
	Assessment method
	Description
	

	
	Class 6 building
	Buildings that directly sell goods by retail or supply services to public i.e. restaurants/cafes, markets, shopping centre/malls, public laundry and hairdressers/barbers. 
	

	
	Class 7a building
	Car parks 
	

	
	Class 7b building
	Warehouse/storage building to display or produce wholesales goods. 
	

	
	Class 8 building
	Buildings used for production assembling, altering, repairing, finishing, packing or cleaning of good or produce. Laboratories. 
	





[bookmark: _Ref128984255]Discuss Class 9 buildings according to the NCC, including the difference between the three (3) Class 9 sub-classifications.

	Answer
	Class 9 buildings are of public nature, class 9a are healthcare buildings that have gone or under-going medical treatment otherwise are in need of physical assistance in case of evacuation emergencies. Class 9b are assembly buildings that are used for social, theatrical, political, religious or arial purposes. Aged care buildings are under 9c where personal care services 24-hour staff assistance to evacuate the building. 
	




[bookmark: _Ref128115391]A client is showing you the plans for a group of four (4) dwellings over two (2) storeys, above a common basement or carpark. Determine what classification would be assigned to this building. Explain your answer.

	Answer
	Class 2 buildings because there is no limitation to what type of dwellings they must be i.e. boarding house or healthcare (class 3) or are not restricted to have another building class – class 7 for the carpark below. 
	




[bookmark: _Ref128115393]Another client would like to build a new doctors surgery. Determine what classification would be assigned to this. Explain your answer.

	Answer
	Class 5 would be assigned due to it being a profession or commercial purposes. 
	



[bookmark: _Ref128119881]Explain why the plans for a warehouse that contains a caretakers residence may have more than one classification.

	Answer
	A warehouse that contains caretakers residence may have more than one class because warehouse falls under class 7b however for a caretakers residence will be under a separate class, class 3. 
	




[bookmark: _Ref128990469]What dictates how buildings must be constructed in Australia and how may this differ in your State or Territory?

	Answer
	Standards, the national code and legislation dictates how buildings must be constructed in Australia and this may differ in different states because each state has a different legislation and must comply with different sections of the NCC. 
	




[bookmark: _Ref127183513]Explain why it is important to understand references the NCC makes to Australian Standards.

	Answer
	Because the standards are sometimes only referenced part while other times entirely. If referenced only partially then the parts not referenced are considered irrelevant and have no authority. To add the new amendments and editions of the standard are nor automatically adopted by the NCC meaning you only need to comply with the edition pf the standard that was referenced. 
	




[bookmark: _Ref128991786]Clarify the purpose of compliance with AS 3600.

	Answer
	The purpose of compliance with AS 3600 is to ensure the projects concrete structures and members as well as pedestal footings are compliant and follow all requirements. 
	




[bookmark: _Ref128995884]Provide a brief explanation of the listed NCC compliance assessment methods used to determine compliance using a Performance Solution pathway.

	Answer
	Assessment method
	Description
	

	
	Evidence of suitability
	Evidence of suitability differs between the three volumes of the NCC, however id showing evidence fit the use of plumbing and drainage materials and design by a Certificate of Accreditation/Conformity, a CodeMark Australia, a report issued by an Accredited Te This is done by doing a comparative analysis to determine whether Performance Solutions provide the superior or same level of health, safety, amenity, or sustainability as using the DTS provisions. sting Laboratory
	

	
	Verification methods
	The three different types of verification methods are test -  on site or at a laboratory , inspections – must be conducted by a qualified person , and calculations – both analytical or mathematical methods
	

	
	Comparison with DTS Provisions
	This is done by doing a comparative analysis to determine whether Performance Solutions provide the superior or same level of health, safety, amenity, or sustainability as using the DTS provisions.
	

	
	Expert Judgement
	An expert person could be a person or an organisations that has the skills and experience necessary to make judgment. The Appropriate Authority is defined differently in every state.

	



[bookmark: _Ref127263388]Discuss the listed levels found in the NCC Performance Hierarchy.

	Answer
	Performance Hierarchy
	Description
	

	
	Objectives
	The objectives are guidance and describe the expectations for the building
	

	
	Functional statements
	The functional statements are also guidance and are how the objectives are going to be achieved.
	

	
	Performance requirements
	These sit at the top of the hierarchy because they are the minimum level of performance for all building plumbing and drainage installation. They are mandatory requirements that need to be met to objectives and functional statements.
	

	
	Building Solutions
	This is a compliance method to achieve commercial buildings through performance based, obtaining mandatory performance requirements
	




[bookmark: _Ref127278250][bookmark: _Ref129067815]Why may you need to use a combination of Performance Solutions and Deemed-to-Satisfy (DtS) solutions to comply with the Performance Requirements of the NCC?

	Answer
	You may need a combination of both because satisfying a single performance requirements is not enough considering that since there are many components inside a building that are protected by performance criteria.
	




[bookmark: _Ref129066894]Discuss the workplace policies and procedures that should be held on-site.

	Answer
	The policy and procedures that should be held on site are Workplace health and safety policies to ensure the workers know the policies and procedures for being safe. All the organisation or workplace related policy and procedures.
	




[bookmark: _Ref129067939]Describe the basic principles of structural design and how these align with large span structures.

	Answer
	Basic principles of structural design are the loads and what loads that the structure need to be able to support. This aligns with large span structures because the structure must be able to withstand and hold against all reasonably design action for a very long period. 
	




[bookmark: _Ref127274757]What type of information is determined from the working drawings and specifications when organising the excavation for a shopping centre with underground parking?

	Answer
	Information – clearly differentiate between the proposed building and other existing structures, include final dimensions of elements, soil information, all standards and requirements that must be followed during the process. 
	




[bookmark: _Ref127253785]Discuss compressive and tensile stresses on buildings.

	Answer
	A tension or tensile stress on a building is where the materials pull apart and on the contrary, compressive stress is where the material squeezes together. 
	




[bookmark: _Ref129070306]Briefly clarify the meaning of ‘water ingress’ when related to waterproofing a building.

	Answer
	Is referred to the process of outside water seeping into a building. This is managed by using concrete mixture and building resources that will prevent water from penetrating the buildings. 
	




[bookmark: _Ref129071735]What do you check for to confirm product compliance with NCC requirements?

	Answer
	To confirm product compliance with NCC requirements is certificate of conformity and accreditation as well as certificates issued by certification bodies. These bodies can be Code Mark or CodeMark Australia. 
	




[bookmark: _Ref129071897]Where do you record checks that you have made on products and materials that have arrived on-site?

	Answer
	You record check that have been made on products/materials under quality management system. 
	




[bookmark: _Ref129075029]What are some indications that a construction company is abiding by environmental protection laws?

	Answer
	An indicator is that a construction company is abiding by environment protection laws is that they follow all the respected state environmental legislation to ensure that they don’t receive any fines or losses of licenses from the respected regulatory authority. 
	



[bookmark: _Ref129075323]Explain your understanding of the following concepts relating to sustainability.

	Answer
	Concept
	Explanation 
	

	
	Ecological footprint
	Ecological footprint is the impact on the environment by a community/person and the amount of land required to sustain natural resources, the quantity of nature it takes to support economies. 
	

	
	Renewable energy
	Renewable energy is energy source that is nor depleted when it is used and derived from natural sources.
	




[bookmark: _Ref128122622]Provide the six (6) bushfire attack level ratings that AS 3959 uses to establish the requirements for construction. Explain each rating.

	Answer
1.



2.



3.



4.



5.



6.
	
Bal-Low – insignificant risk no additional requirements 



Bal-12.5 – Low risk, ember attack, radiant heat 



Bal-19 – increasing levels of ember attack and burning debris ignited by wind bourn embers together with increasing heat flux/between 12.5km2 + 19km2 

Bal-29 – increasing levels of ember attack and burning debris ignited by wind bourn embers together with increasing heat flux/between 19km2 +29km2

Bal-40 – increasing levels of ember attack and burning debris ignited by wind bourn embers together with the increased likelihood of exposure flames.

Bal-FZ – Direct exposure to flames from fire front in addition to heat flux and ember attack. 
	



[bookmark: _Ref128122625]Complete the table below by identifying the type of fire-resisting construction (i.e. Type A, Type B, or Type C) given the following class of building and number of storeys each class of building has.

	Answer
	Rise in Storeys
	Class of building:
2,3,9
	Class of building:
5,6,7,8
	

	
	4 or more
	Class A 
	Class A
	

	
	3
	Class A 
	Class B 
	

	
	2
	Class B
	Class C 
	

	
	1
	Class C 
	Class C 
	




[bookmark: _Ref128129905]Respond to each of the following regarding zero-energy building.

	Answer
	
	Zero energy building
	

	
	Definition
	Zero-energy building is the construction of building that produce as much energy as they consume and it is the difference between the energy produced by the building and the energy consumed by the building is zero.
	

	
	One (1) technique used in zero energy building
	Integrating renewable energy sources that power the building i.e. solar energy, solar panels on the roof.
	

	
	The procedure in implementing the technique you have identified
	Installing solar panels on the roof to create solar energy. 
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WORKBOOK


	Participant name
	Anya English 




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific business context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

	ACTIVITY 1  [bookmark: _Ref35349341]

	Access the National Construction Code (NCC) to:
a) Determine where to locate the technical building requirements for Class 2 to 9 buildings.
b) What is stated in Volume One Amendment 1 – Queensland Part B1 Structural provisions?
c) What is stated in Volume One Amendment 1 – NSW Section A6.6 Class 6 buildings?



	a) Determine where to locate the technical building requirements for Class 2 to 9 buildings.

	Volume one of the NCC for all technical building requirements for class 2 to 9 buildings 

	b) What is stated in Volume One Amendment 1 – Queensland Part B1 Structural provisions?

	This section covers on protecting personnel from injury that is caused by structural failure loss of amenity caused by structural behaviour protection of other property from physical damage as well as to protect personnel from injury caused by glazing. 

	c) What is stated in Volume One Amendment 1 – NSW Section A6.6 Class 6 buildings?

	What class 6 building is which is a shop or other building used for the sale of goods by retail or the supply of services direct to the public including an eating room, café, restaurant or dining room, bar area that is not an assembly building shop part of hotel or motel or a hairdresser or barber shop, public laundry or under takers establishment or market or sale room, showroom or services station. 





	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref128995624]

	Access the National Construction Code (NCC) Volume One Amendment 1 - Section A Governing Requirements - Part A2 Compliance with the NCC and respond to the following:
a) What does this Part explain?
b) What methods are available to achieve the Performance requirements?
c) How is a performance solution shown to comply with the relevant Performance Requirements? 



	a) What does this Part explain?

	This part explains that the governing requirements of the NCC provide the rules and instruction for using and complying with he NCC. 

	b) What methods are available to achieve the Performance requirements?

	Performance solution, Deemed to satisfy, combination of both. 

	c) How is a performance solution shown to comply with the relevant Performance Requirements?

	It is shown by demonstrating compliance with all relevant performance requirements through one or a combination of assessment methods including evidence of suitability a verification method, expert judgement, comparison with deemed to satisfy provision. 




	Satisfactory Outcome
	
	




	ACTIVITY 3  [bookmark: _Ref128134618]

	Some occupants of a brick apartment building have complained about plaster damage, mould build up, damaged skirting and floorboards. The issue seems to affect rooms beside or including bathrooms.

Given the information above:
a) Identify factors that may have contributed to the damage issue.
b) Identify which Part from the NCC Volume 1 Amendment 1 was not properly applied.
c) Briefly explain how the identified Part from the NCC Volume 1 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Briefly explain how the identified Australian standard was not properly applied.
f) Identify what other defect the building may have considering the deviations of the construction from the code and standard.
g) Describe the extent of the work that needs to be done to rectify the issue.



	a) Identify what contributed to the degradation issue.

	The waterproofing/being near or a bathroom, not proper waterproofing or protection would cause these issues. 

	b) Identify which Part from the NCC Volume 1 Amendment 1 was not properly applied.

	Under section F Health and amenity S26C3 shower area. 

	c) Briefly explain how the identified Part from the NCC Volume 1 was not properly applied.

	Because it talks about how a shower area must be water proofed and if the building has damaged from the bathroom it has not been waterproofed properly. 


	d) Identify which Australian standard was not properly applied.

	AS 3740

	e) Briefly explain how the identified Australian standard was not properly applied.

	The parts that were not properly applied are that the all wall of the shower must be waterproofed, waterproof membranes must be graded to the drain waste puddle flange. All products including sealants, adhesives and sheet fastenings must be mould resistance. 

	f) Identify what other defect the building may have considering the deviations of the construction from the code and standard.

	There may be movement in the wall and floor structure as that is caused from by contraction, expansion or settlement and the waterproofing should be prevent this sort of water damage. 

	g) Describe the extent of the work that needs to be done to rectify the issue.

	The skirting, floorboards plaster  will have to be completely replaced, pulled out and reinstalled. Mould will have to be safely removed with appropriate masks and qualifications. Fix the water proofing, the grout must be removed and inject a liquid sealant underneath the tiles and replacing the grout by using an epoxy. 




	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref129007825]

	Access the NCC via the internet to locate the requirements applicable to a building development in the Brisbane area, containing 6 sole-occupancy units, two (2) on each level, each being a separate dwelling. 
This building includes one (1) basement level designated for car parking. 
The proposed building structure requires reinforced concrete floors and columns.
Document your findings or where in the NCC the information can be located. 




Building Description
	Classification

	Class 2 and Class 7

	Rise in Storeys

	4


	Number of Storeys

	4 levels inclusive of the basement level for the carpark. 

	Type of construction

	Type A 

	Climate Zone and description

	Zone 2 a sub-tropical which is warm and mild. 


Fire resistance and stability
	Locate fire resistance information

	A building must have elements which will to the degree necessary maintain structural stability during a fire appropriate to the function or use of the building and the fire load and the protentional fire intensity, the fire hazard, the height of the building, its proximity of other property, any active fire safety systems installed in the building, the size of any fire compartment, fire brigade intervention, other elements they support and the 

	Compartmentation and fire separation

	Class 7 (carpark) must be protected throughout with a sprinkler system and provided with a perimeter vehicular. Ina Type A construction, any part of a window or other opening in an external wall is above another opening on the storey next below and its vertical projection falls no further than 450mm outside the lower opening the opening must be separated by a spandrel which is not less than 900 mm in height and extends not less than 600 mm above the upper surface of the intervening floor and is of non combustible material having an FRL of not less than 60/60/60.

	Fire hazard properties of materials, assemblies, fixtures and linings

	A floor lining must have a critical radiant flux and is a building not protected by a sprinkler system complying with specification E1.5 a maximum smoke development rate of 750 percent-minutes. A wall and ceiling lining must have a smoke growth rate index not more than 100 or an average specific extinction area less than 250m2/kg.




Material requirements
	Reinforced concrete requirements relative to Australian Standards

	Concrete must be to AS 3600 by having a strength at 28 days of not less than 20 MPa and have a 20 mm maximum nominal aggregate size and have a nominal 100 mm slump. Water must not be added to the mix to increase the slump to a value in excess of that specified . Concrete must be placed, compacted and cured in accordance with good building practice. 

	Glazing requirements specifically for windows, sliding doors with frames and balconies.

	Glazing with two horizontal edges unframes shall be grade A safety glass and must be 5mm toughened to a maximum 1000mm span, 6mm toughened to a maximum 1200mm span and 6.38mm laminated to a maximum 750mm span. All windows, sliding and swinging glazed doors with frames must comply with AS 2047. 



	Satisfactory Outcome
	
	



	ACTIVITY 5  [bookmark: _Ref127273569]

	The building discussed in ACTIVITY 2 includes one (1) basement level designated for car parking. 
Provide information required for 
· Bored piling to retain the soil and enable basement walls.
· Work Health and Safety
· Water proofing
· Water ingress

Document your findings or where the information can be located. 



	Bored piling to retain soil and enable basement walls 

	Bored piling has a high load capacity and can be installed into a various range of different soil and rock conditions including soft, compressive or swelling soil and has minimal vibration. 

	Work Health and Safety

	 Excavation work code of practice 2021

	Water proofing

	Carpark for water proofing falls under grade 1 where some seepage and damp areas tolerable Non-habitable spaces. Design options include external drainage, waterproof membrane and dampcourse external structure or internal drainage, sump pump. 

	Water ingress

	Defects to consider are efflorescence which is white staining on the surface of concrete/masonry. Rust stains, concrete cancer/spalling and mould and algae. Rectifying this could include positive / negative waterproofing of walls and slabs, crack injection, additional drainage and larger or additional sump pumps in basement floor. 



	Satisfactory Outcome
	
	



	ACTIVITY 6  [bookmark: _Ref129073248]

	A newly-built hotel needed to have its second-storey elevator lobby renovated, so customers had to take the stairs to get to the second storey of the hotel. On more than one occasion, people with visual impairment have had trouble finding the first step of the stairway, with some even misjudging the first step and falling over. No serious injury has happened yet, but the hotel manager decided something had to be done with the lack of indication of the first step of the stairway. An investigation was made after the third person tripped over the first step, and the investigation revealed that no research on who could possibly use the stairs was done. Respond to the following:
a) Identify one factor that contributed to the failure of the people with visual impairment to find the stairs of the hotel.
b) Identify which clause from the NCC Volume 1 was not properly applied.
c) Briefly explain how the clause from the NCC Volume 1 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Describe the extent of work that needs to be done to rectify the breach.



	a) Identify one factor that contributed to the failure of the people with visual impairment to find the stairs of the hotel.

	That there was no research done on who could possibly use the stairs, which means it wasn’t identified if visually impaired could use the access safely.


	b) Identify which clause from the Building Code of Australia Volume 1 was not properly applied.

	Part D1 Access and Egress 

	c) Briefly explain how the identified clause from the Building Code of Australia Volume 1 was not properly applied.

	It states that any stairways with slip-resistant walking surfaces on ramps and stairway treads or near the edge of the nosing and have suitable handrails to stabilise people, in case of a stairway, suitable safe passage in relation to the nature, volume and frequency of likely usage. 

	d) Identify which Australian standard was not properly applied.

	AS 1657

	e) Describe the extent of work that needs to be done to rectify the breach.

	Research will need to be done on who could use the stairs and ensure everyone is accounted for. The stair will have to be demolished, new stair treads installed and to make sure that the stair treads are now to standard. 



	Satisfactory Outcome
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PRACTICAL ASSESSMENT


	Participant name
	Anya English 




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1 (Occasion 1)
	10/11/2023
	 Workplace
 Simulation
	Cogent Head office
	
	

	Task 1 (Occasion 2)
	10/11/2023
	 Workplace
 Simulation
	Cogent Head office 
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1- Class 2, 3 or 9

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 1.1C. 1.1D. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
 Workplace Quality document  Quality Assurance Template  Other (please specify):

All quality assurance is documented on Procore. 
The criteria requirements were documented and performance solutions were also documented. Report of this was documented on Procore 

 Document attached as evidence

	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson  Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify building checked for compliance with active fire protection requirements:

Building was inspected, all correct PPE was used. 

 Is checklist used attached as evidence





	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 2 - Class 5 to 8

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Details

	1.1A. 1.1B. 1.1C. 1.1D. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
 Workplace Quality document  Quality Assurance Template  Other (please specify):

All quality assurance documented on Procore.
All the criteria and performance solutions were documented correctly and accordingly.


 Document attached as evidence

	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson  Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify building checked for compliance with active fire protection requirements:

All correct PPE was used to safely inspect fire protection requirements

 Is checklist used attached as evidence





CPCCBC4053
Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings

	Practical Task 1 (2X)

	Description of task:
The participant must demonstrate the skills and knowledge to apply building codes and standards to the construction process for Class 2 to 9 Type C buildings. 
· Occasion 1 - Class 2, 3 or 9
· Occasion 2 - Class 5 to 8
Documented evidence of all criteria must be presented (template (HO1) available for use if required) The participant must also inspect one existing buildings for fire protection compliance using workplace or created document (See HO2 for information). Assessor and observer will be looking for evidence including:
· Classify building and document findings.
· Read the plans and specifications to determine the nature of the building, its use and arrangement.
· Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
· Determine and document the classifications applicable to the building. (template available- HO1)
· Identify and interpret multiple classifications from NCC.
· Determine construction compliance requirements.
· Determine NCC Performance Requirements relevant to Class 2 to 9 Type C building projects.
· Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
· Identify and document faults or non-conforming construction methods against NCC Performance Requirements. (template available- HO1) 
· Propose Performance Solution during discussion with design and building professional.
· Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
· Meet the evidence of suitability requirements for building materials and products stated in the NCC.
· Complete documentation demonstrating how the project design and construction will meet NCC requirements (template available- HO1) including:
· Structure
· Access and egress
· Services and equipment
· Health and amenities
· Ancillary provisions
· Energy efficiency
· Determine fire protection requirements.
· Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
· Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
· Inspect one building for compliance with passive and active fire protection requirements.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Construction plans, drawings and specifications of two Type C building projects- one(1) Class 2, 3 or 9 and one (1) Class 5 to 8.; workplace quality policies and procedures; technology to access building and related industry codes, standards and manufacturer product information and materials specifications; Technology to access the NCC and current relevant Acts and Regulations. PPE as required. Documentation of design and construction (suitability or evidence of suitability) (template available- (HO1)). Fire protection checklist (HO2).

	Observer details

	Name of observer:
	Michelle Gomersall 

	Role of observer 
(Confirm suitability to sign)
	Human Resources 

	Email address of observer
	mgomersall@cogentscaffolding.com.au 

	Signature of observer:
	
	Date:
	19/10/2023



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Classify buildings.

	[bookmark: _Ref129077872]Read the plans and specifications to determine the nature of the building, its use and arrangement.
		
	[bookmark: _Ref129077875]Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
		
	[bookmark: _Ref129077878]Determine and document the classifications applicable to the building. (template available- HO1)
		
	[bookmark: _Ref129077882]Identify and interpret multiple classifications from NCC.
		
	2 Determine construction compliance requirements from NCC.

	[bookmark: _Ref129079891]Determine NCC Performance Requirements relevant to Class 2 to 9 Type C building projects.
· Occasion 1- Class 2, 3 or 9
· Occasion 2 - Class 5 to 8
		
	[bookmark: _Ref129079900]Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
		
	[bookmark: _Ref129079909]Identify and document faults or non-conforming construction methods against NCC Performance Requirements. (template available- HO1) 
		
	[bookmark: _Ref129078432]Propose Performance Solution during discussion with design and building professional. 
		
	[bookmark: _Ref129079927]Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
		
	[bookmark: _Ref129079933]Meet the evidence of suitability requirements for building materials and products stated in the NCC.
		
	[bookmark: _Ref129079940]Complete documentation demonstrating how the project design and construction will meet NCC requirements for structure. (template available- HO1)
		
	[bookmark: _Ref129079955]Complete documentation demonstrating how the project design and construction will meet NCC requirements for access and egress. (template available- HO1)
		
	[bookmark: _Ref129079957]Complete documentation demonstrating how the project design and construction will meet NCC requirements for services and equipment. (template available- HO1)
		
	[bookmark: _Ref129079961]Complete documentation demonstrating how the project design and construction will meet NCC requirements for health and amenities. (template available- HO1)
		
	[bookmark: _Ref129079963]Complete documentation demonstrating how the project design and construction will meet NCC requirements for ancillary provisions. (template available- HO1)
		
	[bookmark: _Ref129079964]Complete documentation demonstrating how the project design and construction will meet NCC requirements for  energy efficiency. (template available- HO1)
		
	[bookmark: _Ref129080153]Complete documentation demonstrating how the project design and construction will meet NCC requirements for fire protection. (template available- HO1)
		
	3 Determine fire protection requirements.

	[bookmark: _Ref129079972]Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
		
	[bookmark: _Ref129079978]Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
		
	[bookmark: _Ref129078721]Inspect one building for compliance with passive and active fire protection requirements.
		




	Observer comments:
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