Practical Assessment - CPCCBC4006B Select, procure and store construction materials for low rise projects

	 Practical Assessment - CPCCBC4006B Select, procure and store construction materials for low rise projects

CPCCBC4006B 
Select, procure and store construction materials for low rise projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4006B Select, procure and store construction materials for low rise projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	SAMBARA SERLY




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	BRETT STOWARD

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

1. This exam will occur under standard assessment conditions.
1. An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
2. Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
3. Please fill in the details below, providing your name, signature and date of assessment.
1. Your signature acknowledges that this is your own work.
4. Assessors are to complete marking in pen of a different colour to the Participant.
5. If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
1. If a Participant changes their response in writing, they must put their initials next to the written change.
2. If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	SAMBARA SERLY

	
	

	Participant signature
	
	
	

	Date
	[bookmark: _GoBack]16/07/2019




	Assessor name
	BRETT STOWARD

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	44
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


1. Which of the following documents and/or people would you refer to when selecting materials for a building project? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	Australian Standards
	

	
	
	Contract
	

	
	
	Drawings
	

	
	
	Manufacturer
	

	
	
	National Construction Code
	

	
	
	Specifications
	

	
	
	Tolerances
	




1. [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to suitability of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume Two - Housing Provisions
	Volume One with a gross floor area not exceeding 2000 metre square and not including Type A or Type B construction.
	




1. [bookmark: _Ref535482367]Identify the assessment methods used to verify a performance solution.

	Answer
	Evidence of suitability
A verification method
Expert judgment
Comparison with the deemed to satisfy provisions
	




1. [bookmark: _Ref496611564][bookmark: _Ref536083431]Which of the following solutions for material selection often references the Australian Standards? Tick your response.

	Answer
	Choice
	Possible Answers
	

	
	
	Deemed-to-Satisfy solution
	

	
	
	Performance solution
	




1. [bookmark: _Ref425255684]Identify five (5) materials commonly used for low rise buildings in your region. For each material, identify the following:
11. Its name
12. Properties of the material

	Answer
	#
	Material name
	Properties
	

	
	1
	Concrete
	Concrete is a composite building material made from the combination of aggregate (composite) and a binder such as cement. The most common form of concrete is Portland cement concrete, which consists of mineral aggregate (generally gravel and sand), portland cement and water.
	

	
	2
	Ceramics
	Ceramics are such things as tiles, fixtures, etc. Ceramics are mostly used as fixtures or coverings in buildings. Ceramic floors, walls, counter-tops, even ceilings. Many countries use ceramic roofing tiles to cover many buildings.
Ceramics used to be just a specialized form of clay-pottery firing in kilns, but it has evolved into more technical areas.

	

	
	3
	Glass
	Clear windows have been used since the invention of glass to cover small openings in a building. They provided humans with the ability to both let light into rooms while at the same time keeping inclement weather outside. Glass is generally made from mixtures of sand and silicates, and is very brittle.
Modern glass “curtain walls” can be used to cover the entire facade of a building. Glass can also be used to span over a wide roof structure in a “space frame”.

	

	
	4
	Wood
	Wood is a product of trees, and sometimes other fibrous plants, used for construction purposes when cut or pressed into lumber and timber, such as boards, planks and similar materials. It is a generic building material and is used in building because:
· different structures can be built in most climates
· very flexible under loads, keeping strength while bending
· incredibly strong when compressed vertically
· There are many types so specific species are better for various uses than others

	

	
	5
	Brick and Block

	A brick is a block made of kiln-fired material, usually clay or shale, but also may be of lower quality mud, etc. 
Clay bricks are formed in a moulding (soft mud method), or in commercial manufacture by extruding clay through a die and wire-cutting them to the proper size (the stiff mud process).

	





1. [bookmark: _Ref425323073][bookmark: _Ref425248000]For each of the materials in Q5. identify the following:
14. Quality of the material (i.e. durability, serviceability, cost effectiveness)
15. Compatibility and non-compatibility of the material (i.e. what it would/would not be suitable for)

	Answer
	#
	Quality
	Compatibility 
	

	
	1
	
	Concrete is a composite building material made from the combination of aggregate (composite) and a binder such as cement. The most common form of concrete is Portland cement concrete, which consists of mineral aggregate (generally gravel and sand), portland cement and water

	

	
	2
	ceramics
	
Ceramics are such things as tiles, fixtures, etc. Ceramics are mostly used as fixtures or coverings in buildings. Ceramic floors, walls, counter-tops, even ceilings. Many countries use ceramic roofing tiles to cover many buildings.
Ceramics used to be just a specialized form of clay-pottery firing in kilns, but it has evolved into more technical areas.

	

	
	3
	glass
	Clear windows have been used since the invention of glass to cover small openings in a building. They provided humans with the ability to both let light into rooms while at the same time keeping inclement weather outside. Glass is generally made from mixtures of sand and silicates, and is very brittle.
Modern glass “curtain walls” can be used to cover the entire facade of a building. Glass can also be used to span over a wide roof structure in a “space frame”.
	

	
	4
	wood
	Wood is a product of trees, and sometimes other fibrous plants, used for construction purposes when cut or pressed into lumber and timber, such as boards, planks and similar materials. It is a generic building material and is used in building because:
· different structures can be built in most climates
· very flexible under loads, keeping strength while bending
· incredibly strong when compressed vertically
· There are many types so specific species are better for various uses than others

	

	
	5
	Brick and block
	A brick is a block made of kiln-fired material, usually clay or shale, but also may be of lower quality mud, etc. 
Clay bricks are formed in a moulding (soft mud method), or in commercial manufacture by extruding clay through a die and wire-cutting them to the proper size (the stiff mud process).

	



1. [bookmark: _Ref536083435]Identify five (5) physical characteristics that may be considered when evaluating potential building materials.

	Answer
	1. Density and specific gravity
2. Strength
3. Electrical conductivity
4. Thermal conductivity and capacity
5. Moisture absorption
6. Acoustics

	




1. [bookmark: _Ref536095924]Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definition
	

	
	1
	Carbon footprint
	1 - B
	A
	The amount of energy required to manufacture a product
	

	
	2
	CO2e
	2 - E
	B
	Total GHD emissions produced during manufacture construction and use
	

	
	3
	Embodied energy
	3 - A
	C
	Greenhouse gas emissions
	

	
	4
	Embodied water
	4 - D
	D
	The amount of water required to manufacture a product
	

	
	5
	GHG
	5 - C
	E
	CO2equivalent tonnes emitted into the atmosphere
	




1. [bookmark: _Ref536083463]Which of the following materials would be considered as ‘low energy content’? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	Bricks
	

	
	
	By-products of other industrial processes
	

	
	
	Cement
	

	
	
	Glass
	

	
	
	Metals
	

	
	
	Plastics
	

	
	
	Sand
	

	
	
	Stone
	

	
	
	Timber
	



1. [bookmark: _Ref536099133]Refer to the table below and identify the wall material type that has the smallest embodied energy and emission impact.

[image: ]

	Answer
	Walls timber frame fibro clad
	





1. [bookmark: _Ref536095926]Identify the Volume and Parts of the NCC that relate to energy efficiency of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2, part 3.12
	Volume 1 part J
	




1. [bookmark: _Ref536097820]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses residential slabs and footings.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	QBCC section 2
	2870
	




1. [bookmark: _Ref536097822]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses roof tiles.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	QBCC section 6
	2049
	




1. [bookmark: _Ref536106144]Identify the Volume and Parts of the NCC that relate to safety barriers for swimming pools for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 Part 3.10.10
	Volume 1 Part 61
	




1. [bookmark: _Ref536106145]In some states, barriers and fences for swimming pools are not entirely regulated by the NCC, as noted in the Ancillary Provisions and State and Territory Variations. Identify the applicable Act and Regulation that regulate safety barriers for swimming pools in your jurisdiction.

	Answer
	In Queensland Building Act 1975 and Building Regulation 2006

In NSW Swimming Pools Act 1992 and Swimming Pools Regulations 2008
	



1. [bookmark: _Ref536106146]Identify the Australian Standard that relates to safety barriers for swimming pools.

	Answer
	AS 1926
	




1. [bookmark: _Ref536107455]True or False (Tick your response): According to the Standard in Q16. all gates must be fitted with a self-closing device that will return the gate to a closed position from any position without the use of manual force.

	Answer
	
	True 
	
	

	
	
	False 
	
	




1. [bookmark: _Ref536170034]Identify the Volume and Parts of the NCC that relate to fire-resistance of building elements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	VOLUME 2 schedule 5
	VOLUME 1 schedule 5
	




1. [bookmark: _Ref536170036]Identify the Australian Standard that relates to fire-resistance tests for elements of construction.

	Answer
	AS 1530
	




1. [bookmark: _Ref536169328]For all NCC Classes, where the ground or subfloor space is excessively damp or subject to frequent flooding, which durability class must the subfloor framing must be used where above ground?

	Answer
	Class 1 or 2 timber or H3 preservatives treated timber 
	





1. [bookmark: _Ref536170040]Identify the Australian Standards that must be observed when meeting the requirements for Q20. 

	Answer
	AS 1684.2; AS 1684.3; AS 1986.4
	




1. [bookmark: _Ref536170043]True or False (Tick your response): Where materials are not used as intended (or without considering NCC requirements), this can make a significant difference to the life or serviceability of the structure.

	Answer
	
	True 
	
	

	
	
	False 
	
	




1. [bookmark: _Ref536170044]Explain why durability and serviceability impact on the cost effectiveness of chosen materials.

	Answer
	Materials that are cheap but not durable or have high serviceability costs do not end up being cheaper in the long run. However, spending a little more money on materials that durable and require minimal maintenance will cost less in the long run as they do not need to be replaced as frequently and have low ongoing costs
	




1. [bookmark: _Ref536172033]Provide an example of short term degradation of materials and describe its effects on a building on structure.

	Answer
	Timber is often prone to short term degradation. When exposed to the weather it may suffer from weathering, causing splitting and crumbling or if it is unprotected and remains damp for long periods, it will rot. Some timbers are naturally resistant to rot, for example western red cedar. These timbers form a protective skin on the surface that keeps them relatively intact.

	





1. [bookmark: _Ref536172034]Provide an example of long term degradation of materials and describe its effects on a building on structure.

	Answer
	Stone usually forms a surface skin when exposed to the atmosphere. This can act to protect the stone or in some cases it may cause failure. The failure is usually associated with acid rain, a result of sulphur dioxide pollution in the atmosphere. 

Limestone is particularly vulnerable to this. Some of the softer rocks such as sandstone and limestone also erode with constant exposure to wind and water. This is further exacerbated in cold climates where frost can freeze water in cracks and eventually cause the rock to break. 

	




1. [bookmark: _Ref425327163][bookmark: _Ref425327708]You have spoken to a supplier who has indicated that some of the client’s desired materials are unavailable. When considering alternative building materials what must be taken into consideration (i.e. other than the client’s requirements)?

	Answer
	When selecting building materials you need to be aware of a number of considerations, such as:
· Client requirements
· Material availability or lack of availability
· Environmental issues
· Life Cycle Assessment methodology
An alternative material or building practice should only be considered if it is performance tested, efficient, environmentally sustainable or more cost-effective. You need to evaluate and select alternative materials in the event that specified materials are unavailable or unsuitable, with consideration to:
· Availability
· Transportation
· Handling
· Testing
· Waste reduction
· Reuse/recycling
· Renewable/non-renewable
· Environment impact
· Embedded energy
· Fire resistance rating
· Compatibility
· Acoustic properties
· Life-cycle cost
· Short and long term degradation

	




1. [bookmark: _Ref536177031]Identify two (2) things that you should look for when receiving a delivery of materials.

	Answer
	Quantity and quality
	




1. [bookmark: _Ref536177032]If you encounter issues with delivery, what two (2) options do you have?

	Answer
	Accept the shipment with condition or reject the entire shipment
	




1. [bookmark: _Ref409518704][bookmark: _Ref408838393]Which of the following should be assessed before shifting materials? Tick all that apply. 

	Answer
	Choice
	Possible Answers
	

	
	
	What needs to be relocated (e.g. size, weight)
	

	
	
	The relocation area, site layout and obstacles
	

	
	
	Distance and time to relocate load
	

	
	
	Whether a team is available and/or appropriate
	

	
	
	Whether PPE must be worn (e.g. for hazardous materials)
	




1. [bookmark: _Ref536178585]What document should you refer to for guidance on how to handle and store hazardous chemicals? 

	Answer
	SDS – SAFETY DATA SHEETS
	




1. [bookmark: _Ref408838395][bookmark: _Ref409519364]Name three (3) ways you can reduce the risk of injury if a load is too heavy for one person to carry, push or pull. 

	Answer
	1. Don’t lift heavy objects by yourself, seek help, team lift, lighten the load, use a mechanical aid.
2. Ensure the pathway is clear and no trip hazards are in the way.
3. Do not twist when lifting objects, this is extremely risky.

	





1. [bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




1. [bookmark: _Ref404158235]How should construction materials and components be handled? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	Sorted to suit material type and size, separating hazardous material
	

	
	
	Stacked or stockpiled for ease of identification and retrieval
	

	
	
	Stored in access ways for ease of retrieval
	

	
	
	Stored clear of access ways
	

	
	
	Handled and positioned ready for installation
	




1. [bookmark: _Ref536180244]Identify the Australian Standard that relates to the storage and handling of LP gas.

	Answer
	AS/NZS 1596:2014:
	



1. [bookmark: _Ref536194481]List one (1) testing method for each of the building materials listed below.

	Answer
	Material name
	Properties
	

	
	Concrete
	Concrete cylinders or cubes are normally tested in a hydraulic press. A universal machine for tension, compression and bending is also used
	

	
	Metals
	1. The strength of metals is reduced if they are repeatedly loaded alternately in tension and compression. This test is called ‘repeated loading’ if the load is applied several hundred or thousands of times, and fatigue loading if the load is applied millions of times. 
2. Ductility is tested by bending a bar around a pin over a wide angle. 
3. Hardness is tested by indentation with a diamond or a hardened steel ball. If the tensile strength has been tested, then the hardness of the metal can be deduced.
a. The toughness of a metal can also be deduced from the tension test.Toughness is defined as the energy required to break a material. The greater the area contained under a stress-strain curve up to failure, the greater the toughness of the material.

	

	
	Timber
	1. When timber is used in domestic construction where it is not highly stressed, a visual grading may be a sufficient means of testing the material.
2. Because of imperfections in individual pieces, stress grading is usually more reliable than testing of selected pieces. 
3. A stress grading machine tests every individual piece of timber using a very fast and economical method. The test is based on the relationship between the strength and the deflection of timber. Each piece of timber is deflected at several points along its length, and the deflection category marked by means of a spot of dye. The timber is then classified visually by its colour markings.

	




1. [bookmark: _Ref536181364]What Code gives detailed tables which state the required grade of timber for specific sizes and uses?

	Answer
	AUSTRALIAN TIMBER FRAMING CODE
	




1. [bookmark: _Ref536181366]Name two (2) ways that defects may be seen in timber.

	Answer
	Insect Damage

Pocket of Resin
	




1. [bookmark: _Ref536181368]Identify two (2) tests that may be performed to determine the durability of stone.

	Answer
	Acid emersion test

Water absoption
	



1. [bookmark: _Ref536181370]Name two (2) ways that defects may be seen in stone.

	Answer
	Cracks and fissures in the rock surface
	




1. [bookmark: _Ref536187863]True or False (Tick your response): Under a contract, builders and other specialist tradespersons are the ones most likely to rectify or remedy problems that arise from incorrect installation, application or placement of materials.

	Answer
	
	True 
	
	

	
	
	False 
	
	




1. [bookmark: _Ref536187427]Name two (2) established methods that may be used to preserve timber.

	Answer
	Paint and termite barriers
	




1. [bookmark: _Ref536187429]Identify two (2) established methods that may be used to protect ferrous metals.

	Answer
	Cathodic protection, corrosion inhibitors, panting, and galvanisation
	





1. [bookmark: _Ref536187430]Explain why the corrosion resistance of non-ferrous metals is superior to that of ordinary steel.

	Answer
	This is a result of production of a ceramic coating of oxide or salt on the metal which protects it from further corrosion
	




1. [bookmark: _Ref536187432]When should aluminium be coated with bituminous paint? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	At all times
	

	
	
	When it is buried in soil
	

	
	
	When it comes in contact with chemical materials
	

	
	
	When it is immersed in water
	

	
	
	When it is used on bitumen
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	PRACTICAL ASSESSMENT INSTRUCTIONS

54. The following practical assessment will require the Participant to complete work related activities.
55. The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
56. Please fill in the details below – providing your name, signature and date of assessment.
1. The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
57. The Assessor may substitute a Practical Task with an alternate task of equal value.
1. Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	SAMBARA SERLY

	
	

	Participant signature
	
	
	

	Date
	16/07/2019



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4006B
Select, procure and store construction materials for low rise projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to supervise systems through which materials are selected, acquired and stored on site for the following projects:
58. Occasion 1: Construction classified as Class 1 and 10 construction
59. Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
60. Copy of PO sent to site team for materials.
61. Email correspondence sighting need for materials, delivery of materials and storage of materials (if relevant).

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Computer, Building Contract, Drawings, Specifications, Building materials (including timber, and ferrous and non-ferrous metal).

	Assessment of task

	Name of participant:
	SAMBARA SERLY

	Name of observer:
	INGMAR SOMMER

	Role of observer 
(Confirm suitability to sign)
	SENIOR CONTRACT ADMINISTRATOR

	Email address of observer
	Ingmar.sommer@sydneymetro2.com.au

	Signature of observer:
	
	Date:
	Click here to enter a date.

	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Evaluate building materials

	1. [bookmark: _Ref535842396]Identify suitability of materials commonly used in the region for low rise buildings. 
	
	

	1. [bookmark: _Ref535842402][bookmark: _Ref536020766]Through research and testing, identify properties of different materials, their quality and compatibility and non-compatibility and maintain effective sampling and organisational record-keeping processes.
	
	

	1. [bookmark: _Ref535842408]Identify the environmental impacts of different materials. 
	
	

	1. [bookmark: _Ref535842411]Identify the impact of allowable tolerances on the conversion of naturally occurring materials. 
	
	

	1. [bookmark: _Ref535842424]Identify and check tolerances for installing and assembling materials with regard to the nature of the work being performed and the requirements of relevant construction industry Australian standards. 
	
	

	2 Material selection 

	1.3A.  [bookmark: _Ref535842432]Select materials structurally adequate and appropriate for the building system specified in the contract, drawings and specifications. 
	
	

	1.3B.  [bookmark: _Ref535842436]Select materials after considering:
67. Safety
68. Required fire resistance rating
69. Suitability to the application
70. Durability
71. Serviceability and cost effectiveness
72. Compliance with NCC, legislation, regulations and Australian Standards
	
	

	1.3C.  [bookmark: _Ref535842439]Consider short and long-term degradation of materials in relation to the building’s proposed life cycle. 
	
	

	1.3D.  [bookmark: _Ref535842441][bookmark: _Ref536188601]Select and evaluate alternative materials, if specified materials were unavailable or unsuitable – justifying decisions to regulatory authorities, as necessary
	
	

	1.3E.  [bookmark: _Ref535842446]Finalise selection of materials in accordance with contractual requirements and in consultation with relevant professionals and the client, compiling results in a report.
	
	

	1.3F.  [bookmark: _Ref535842459]Effectively communicate using the following methods:
73. Language/concepts appropriate to cultural differences
74. Non-verbal communication
	
	

	3 Supervising materials on site 

	· [bookmark: _Ref535842490]Determine limitations and effects of transportation on material and components, taking action in potentially damaging circumstances. 
	
	

	· [bookmark: _Ref535842494]Ensure materials were correctly and safely handled on site using appropriate equipment and safe work practices. 
	
	

	· [bookmark: _Ref535842471]Communicate with manufacturers and suppliers to ensure materials are stored in accordance with specifications and Australian standards. 
	
	

	· [bookmark: _Ref535842501]Implement processes for inspecting all materials delivered on site for naturally occurring and/or manufactured defects before installation. 
	
	

	· [bookmark: _Ref535842506]Ensure personnel were aware of actions to be taken in the case of defects caused by incorrect installation, application or placement. 
	
	

	· [bookmark: _Ref535842510]Preserve and protect timber and ferrous and non-ferrous metal used in the construction process.
	
	

	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS
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