4001A Practical Assessment
The classes of building structures being built on site are Class 1 (the house) and Class 10 (the garage). 

In accordance with Volume 2 of the NCC under Part 3.1.4, the requirements for a termite management system are:
· Use of a primary building element not subject to a termite attack;
· A design life of at least 50 years;
· Compliance with Australian Standard 3660 or has been tested and passed the results as required by Australian Standard 3660;
· Have a durable notice installed; and
· Ensure that any chemical termite management system includes use of sanctioned pesticides.
The NCC code which refers to natural light through windows is Part 3.8.4.2 of Volume 2 of the NCC.




















Hi John,

Thanks for sending those colour options over for the exterior of the Design For Place project. 

Unfortunately, we won't be able to use the ones you have identified as they are internal paint options - not external. 

We will need to select an external paint option in order to comply with AS/NZS 2311:2017. See attached screen shot and this link for further detail: https://www.qbcc.qld.gov.au/sites/default/files/Standards_and_Tolerances_Guide_0.pdf 

If you wanted to see a copy of the standard, I can see it can be purchased online via SAI Global.

Can we run with a Dulux Weathershield Exterior Paint and match it to the charcoal option you sent over? 

Let me know what you think.

Regards,
Matt
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Hi Jim,

Just getting in touch with you to discuss the standard of finishes required for the timber flooring at the Design For Place project.

https://www.qbcc.qld.gov.au/sites/default/files/Standards_and_Tolerances_Guide_0.pdf

[bookmark: _GoBack]If you go to section 15 of the link above it will explain the finishing requirements for the timber flooring so we can deliver the project to code.  Please don’t hesitate to contact me if you have any queries.

Regards,
Matt
image1.png
13.1 Standard of painting

Coatings used are to be suitable for the

relevant conditions and relevant wear and tear.
Unless documented otherwise, within the first

12 months from completion of the work, painting
is defective if it does not comply with the
manufacturer’s installation instructions or AS/
NZS 2311 - Guide to the Painting of Buildings.




