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1. PURPOSE
It helps us ensure that we work based on our Policy and Procedures whereby we aim to ensure that building and construction materials and contractors are obtained and managed in an efficient and cost-effective manner, while also ensuring that project timelines and specifications are met including that they meet the required specifications and quality standards we expect.
Our aim is to ensure that we source building and construction materials from reputable and reliable suppliers who share our commitment to quality, sustainability, and ethical business practices and work with contractors who will bring success of our construction projects.
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Scope of works – Residential Build – Kitchen, Pantry and Laundry to design and execute the job. This home kitchen remodelling will begin with a planning and design phase that will ensure all requirements and preferences for the customers, demolition, and construction are met, while being cost-efficient. Includes preliminaries, demolition, plumbing, electrical, carpentry, tiling, window and door installation and removal of debris and site clean-up
Moreover, all materials will be cleared from site on completion of the project, leaving site clean and tidy as we found it.

Any additional jobs will be negotiated and agreed by both parties. 

Preliminaries
Home warranty fees
Contract fees

Site Works – Foundations & Connections
Slabs to be chased to allow for new plumbing
Plumbing and Electricity cap off and reconnections
Plumbing and Electricity dis-connections to existing serviceable connection points and connections
Water dis-connection and connections from pre-tapped water main
Duct work for bench mount exhaust to run through back of drawers and wall to external wall and motor

Energy Efficiency
6 Star Rated as per government regulations
Energy efficient LED lights to dwelling, fluorescent lights 
Power requirements for living area to be determined by client
Cooktop downdraft ventilation system

Windows and Doors
New fixed glass window to existing opening
Enclose wall above and below to match existing 
Window tint to be discussed with client
New doors to match switch opening with screens
New doors to match triple slider with screens
New Laundry door location cavity slider to match existing
Tambour door in kitchen
New Laundry window to suit existing opening width over dishwasher
Requirements as per specification list below

Kitchen 
Demolish existing kitchen and make good
Laminate finish cupboards with manufactured stone bench tops in the standard
Builders range, including waterfall ends
New stud plasterboard wall to be build
Finger pull cupboards
Overhead cupboards with push catch doors
Drawers with integrated tip-on function
Stainless steel kickplate
Coffee nook
Bottom drawer with dividers for baking tray storage
Pull out drawer for bin, top mount 2x35L bucket
Single bowl undermount sink
Secondary drawer with dividers – potential – tbc
Requirements as per specification list below

Pantry
Finger pull cupboards
Double bowl undermount sink
Base mount bin 2x20L bucket
Free standing dishwasher
Pantry with adjustable shelves
Pantry with pull out internal drawers
Requirements as per specification list below

Laundry
Finger pull cupboards
Pull out shelves for washing basket flat top with undermount runners
Plumbing connection to washing machine drain hose
Plumbing connections through cupboard below laundry chute
Laundry chute
Requirements as per specification list below

Flooring and Tiling
New timber look tile flooring to be selected by client
Ceramic tile or colour back glass splashback
Kitchen – timber look tiles to match floors and will be selected by client
Laundry - ceramic tile or colour back glass splashback
Requirements as per specification list below

Electrical
Single phase underground power connection from existing supply point. 
Recessed led strip light under overhead cupboards
Led light strip under island bench
Cooktop isolation switch
Requirements as per specification list below

Plumbing
Water connection for fridge in overhead cupboard 
Plumbing connection to washing machine drain hose
Plumbing connections through cupboard below laundry chute
Requirements as per specification list below
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	Material
	Description

	Demolition – Jack Hammer
	Demolish the 17 sqm of existing storage, supporting walls, wall tiles, flooring, sink etc. at all levels as required carefully and disposing off and clearing away the debris 

	Kitchen 
Elevation
Bench
Drawers
Spice rack
Brushed stainless steel laminate
Ducting
Overheads
Shelves
Caesarstone bench top
Island
Sink cupboard
Paint
Cabinetry - Blum Tandembox antaro h. Fronted pull-out C - DQC5JY, D - DQC69A, DQCB6M
Urbane Castella 192mmCTC handle

	Kitchen elevation 2730x2550Hx600mm diameter or expressed as 2.7mx2.55mx0.6m
Bench height 1000mm with 3 sets of 3 blum tip drawers with 1 of orga line spice rack insert
Brushed stainless steel laminate kick face
Ducting for downdraft cooktop to run behind draws
Overheads 650mm Height with 1 of adjustable shelf with doors hanging below as finger pull and LED strip lighting to underside
Internal 16mm HMR with 1mm ABS PVC match edge
Fronts in 18mm white sating with 2 pac satin finish
40mm Caesarstone bianco drift bench top with cutout for drop in cooktop
Kitchen island 3000x1000Wx1000 D – LH side with pull out drawer with 2x35L bin inserts
Sink cupboard with 1 door housing undermount single bowl sink with 3 sets of 4 blum tip on drawers with 1 of cutlery insert and 2 of utensil insert. Internals 16mmwh HMR with 1mm ABS PVC matching edge. All fronts in 18mm wh sat with 2pac satin finish


	Butlers Pantry
Door sink cupbard
Bins
Dishwasher
Drawers
Shelves
Overheads
Paint
	4480x2550 Hx620mm D pantry or expressed as 4.48m x 2.550m x 0.620m with door sink cupboard and 2x20L bins
Dishwasher opening 600mm
3 sets of 3 blum tip on drawers with 885mm pantyr to RH side
2 door pantry unit with 5 blum soft close internal drawers and 4 adj shelves
Overheads 3595x650 Hx400mm D with 1 adj shelf with doors hanging below as finger pull

	Laundry
Laundry tub unit
Shelves
Bench
Caesartone top 6131 Bianco Drift, 4600 Organic white
Shute cupboard
Overheads
Drawers
Tall cupboard
Brushed SS laminate
Single door cupboard
Paint
	L shaped laundry 2450x2520x2550mm or expressed as 2.45m x 2.52m x 2.55m with 4 door laundry tub unit with 1 adj shelf with bench at 1000mm H
40mm Caesarstone organic white top running wall to wall below laundry shute cupboard and 20mm thick splashback 150mm height
4 door overhead cupboard with 2 adj shelves and dorrs hanging down as finger pull above dryer and washing machine openings with flat pull out shelves and 1 of blum soft close drawer below
2 door Tall broom storage cupboard to right side with 1 of blum soft close drawer below 1 0f internal adj shelf
Brushed stainless steel laminate kick face
Single door cupboard 600x600mm on opposite wall 1000mm height bench top.
All internals 16mm white HMR with 1mm ABS PVCedge.  All fronts in 18mm white sating with 2 pac satin finish
Dryer and washing machine panels, bottoms in 32mm MDF with 2pac finish

	Plumbing
Franke Ancona single bowl undermount sink
Double bowl undermount sink
Mizu drift sink mixer
Mizu smothe sq sink mixer
	Island & laundry - franke ancona single bowl undermount sink – anx 110-48
Pantry - franke ancona double bowl undermount sink - anx 120
Island & pantry - mizu drift mk2 gooseneck sink mixer pull-out
Laundry - mizu soothe square gooseneck sink mixer


	Electrical
Light
LED tape
	Beacon Herman 1 light pendant
14 watt led tape and recess led profile under overhead cupboards
Single phase underground power connection from existing supply point. 
Led light strip under island bench
Cooktop isolation switch


	Tiling
Timber look tile flooring
Ceramic tile splashback – kitchen and laundry
Kitchen timber look tile to match floors
Brushed stainless steel laminate

	New timber look tile flooring 
Kitchen – timber look tiles to match floors 1200x x230mm
Laundry and kitchen - ceramic tile splashback - Snow Brillo Tile Sc19 A7615, Amber Tiles To Match Cabinets. 130mmx130mm
Brushed stainless steel laminate kick face
130 sqm 

	Butlers Pantry - Fixed Glass Window
	New fixed glass window to suit existing opening width frame
1800x600mm
Colour to match exiting and tinted to client requirement (customized)


	French Doors - Triple Slider
	New Triple Slider With Screens To Match Existing Profile & Colour
2710x2100mm


	Dining Room Slider - Reverse Opening
	Slider with reversed opening with screen to match existing profile and colour
1810mmx2100mm

	Removal of Debris
Cleaning material
Skip bin

	Cleaning materials

Skip bins
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	Relevant construction works/services
	Description/scope
	Hrs

	Demolition labour
	Demolish existing kitchen and make good
Dismantling the existing storage, slab platform including supporting walls, wall tiles, flooring, sink etc. at all levels as required carefully and disposing off and clearing away the debris
Slabs to be chased to allow for new plumbing


	16

	Kitchen Labour
	Installation of supply mentioned above
	138.4

	Butlers Pantry Labour
	Installation of supply mentioned above
	35

	Laundry Labour
	Installation of supply mentioned above
	40

	Plumbing
	Installation of supply mentioned above
Slabs to be chased to allow for new plumbing
Plumbing cap off and reconnections
Plumbing dis-connections to existing serviceable connection points and connections
Water dis-connection and connections from pre-tapped water main

	33.3

	Electrical
	Installation of supply mentioned above
Electricity cap off and reconnections
Electricity dis-connections to existing serviceable connection points and connections
Duct work for bench mount exhaust to run through back of drawers and wall to external wall and motor
Cooktop downdraft ventilation system
	29

	Building / Carpentry Labour
	Labour for scopes of work described excluding the installation of above fixtures
New stud plasterboard wall to be build
New fixed glass window to existing opening
Enclose wall above and below to match existing 
Window tint to be discussed with client
New doors to match switch opening with screens
New doors to match triple slider with screens
New Laundry door location cavity slider to match existing
Tambour door in kitchen
New Laundry window to suit existing opening width over dishwasher

	230

	Tiling Labour
	Installation of supply mentioned above
	122

	Butlers Pantry - Fixed Glass Window Labour
	Installation of supply mentioned above
	2

	French Doors - Triple Slider Labour
	Installation of supply mentioned above
	3

	Dining Room Slider - Reverse Opening Labour
	Installation of supply mentioned above
	5

	Removal of Debris
	Labour and clean-up
	8
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As per policy and procedure,  Each business area must maintain its own Contract Register.  The information that must be maintained on the Contract Register. Contract Registers can be further developed with additional information to help suit the individual business area needs. Folders should be labelled with first 6 letters of the address starting with house/lot number, street name then 001 onwards for each stored document
The Contract Register should be used to help manage and plan for contracts and ensure adequate attention and resourcing is applied for ease of reference.
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