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ASSESSMENT SUMMARY

The assessment activities for CPCCBC4010B Apply structural principles to residential low rise constructions & CPCCBC4011B Apply structural principles to commercial low rise constructions cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
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	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
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	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	93
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Q1.  What is the most important aspect in the design of buildings? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Aesthetics
	

	
		Cost
	

	
		Location
	

	
		Stability
	




Q2.  [bookmark: _Ref531083005]Where can the definitive properties of materials used in the building industry be found? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Australian Standards
	

	
		Building journals
	

	
		Practical learning on the job
	

	
		Textbooks on building
	




Q3.  [bookmark: _Ref427229923]Which industry professional would you contact for structural advice? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Architect
	

	
		Draftsperson
	

	
		Engineer
	

	
		Quantity surveyor
	




Q4.  [bookmark: _Ref531353369]Which industry professional would you contact for the preparation of working drawings? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Building surveyor
	

	
		Draftsperson
	

	
		Quantity surveyor
	



Q5.  [bookmark: _Ref427229919]Briefly describe the role of an architect.

	Answer
	Architects design buildings and supervise the projects they designed. They help set a realistic budget, guide you through the construction process, get competitive quotes and manages consultants. 
	



Q6.  [bookmark: _Ref427229924]What is the difference between a building surveyor and a land surveyor?

	Answer
	Land surveyors focus on assessing the surrounding terrain and landscape which will be used for the construction project. The take levels on a site to produce contour plans, Determine location of existing buildings. They set the building lines, and check the vertical alignment of a building during the construction process. A building surveyor’s area of work is providing advice on the property and construction of the project. They assess building plans submitted for approval to ensure compliance with all the legislations, provide advice and assistance to builders/owners before the finalisation of plans. They also inspect buildings during construction and keep records of the progress and if any regulations have been breached. They will stand in court to give evidence when a breach has been made and they issue compliance certification. Building surveyors work across all types of construction; Residential, commercial, industrial, leisure and agriculture projects. 
	



Q7.  [bookmark: _Ref427229926][bookmark: _Ref531353386]Which industry professional would you contact for matters relating to cost? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Architect
	

	
		Building surveyor
	

	
		Engineer
	

	
		Quantity surveyor
	



Q8.  [bookmark: _Ref531353744]A land surveyor is to reinstate survey pegs. Which of the following documents would the surveyor need? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Title
	

	
		Contour plans
	

	
		Project specifications
	




Q9.  [bookmark: _Ref531353745]When preparing a trench a builder digs through a gas pipe which was not shown on the plans. Which report should be used to prove the mistake was not the builder’s? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Engineer’s drawings
	

	
		Condition report
	

	
		Soil report
	




Q10.  [bookmark: _Ref427230180][bookmark: _Ref531353749]Which two (2) of the following can be determined from the contour report? Tick your responses.

	Answer
	Choice
	Possible Answers
	
	
		Extent of cut and fill
	

	
		Height of retaining walls
	

	
		Location of trees
	

	
		Location of windows
	




Q11.  [bookmark: _Ref531353759]The customer has requested a glass balcony. Which document would the builder refer to for information on structural members? 
Tick your response. 

	Answer
	Choice
	Possible Answers
	
	
		Building specifications
	

	
		Condition report
	

	
		Engineering report
	



Q12.  [bookmark: _Ref427230170][bookmark: _Ref531353761]The builder is planning a project and requires information on the location of fixtures and fittings, windows and doors. Which plans show this information? Tick your response. 

	Answer
	Choice
	Possible Answers
	
	
		Cross sections
	

	
		Floor plans
	

	
		Footing designs
	




Q13.  [bookmark: _Ref427230166][bookmark: _Ref531353766]After an inspection, the client believes that what was installed is different to what they had chosen in the contract. What document details the materials the builder was meant to use? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Building specifications
	

	
		Plan of the subdivision
	

	
		Site plan
	




Q14.  [bookmark: _Ref427579066][bookmark: _Ref531353770]What key pieces of information can be found on a site plan? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Location of street frontage
	

	
		Location of proposed building
	

	
		North point
	




Q15.  [bookmark: _Ref427230177]What is the purpose of a footing design?

	Answer
	Footing designs show details about footing depths and widths, slabs and stiffening beams, type and positioning of steel reinforcement. They are made to comply with the legislations.
	



Q16.  [bookmark: _Ref531354185]Why would a pre-commencement site inspection be conducted? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		To ensure all contract documentation clearly reflects the actual site
	

	
		It allows the supervisor to get some fresh air
	

	
		To ensure that the client actually owns the property
	

	
		So that levels can be taken to check the slope of the site
	




Q17.  [bookmark: _Ref531082938]What are the dead loads in a building? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		All stationary materials
	

	
		Permanent materials
	

	
		Roofing materials
	

	
		Use for which the building is intended
	




Q18.  [bookmark: _Ref531082940]What is the formula for calculating a dead load?

	Answer
	Dead load = Volume of member x Unit weight of materials (supplied)
	



Q19.  [bookmark: _Ref531082941]What are the live loads in a building? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Loads arising from the function of the structure
	

	
		Loads due to rain
	

	
		Loads due to wind
	

	
		Utility services
	





Refer to the table shown below to respond to Q20. to Q21.  These values are used to calculate live loads using the formula: Area of floor x Live load rating.

	Live loads for floors as per building usage
	Uniformly distributed load (kPa or kN/m²)

	Houses
	1.5

	Flats, motel bedrooms, apartments
	2.0

	Offices
	3.0

	Workshops
	5.0

	Parking, vehicle >2.5t
	5.0

	Hospitals, school assembly areas with fixed seating
	3.0

	Dance halls, bars, lounges
	5.0




Q20.  [bookmark: _Ref481992592]Calculate the live load of a guest house measuring 23m x 8m. 
Show your calculations.

	Answer
	Area = 23.0m x 8.0m = 192m2
Live load rating = 1.5kPa
Live load = 192m2 x 1.5 kPa
TOTAL = 288 kN
	



Q21.  [bookmark: _Ref427215838]Calculate the live load of a commercial office premises floor measuring 33m x 11m. Show your calculations.

	Answer
	Area = 33.0m x 11.0m = 363m2
Live load rating = 3.0kPa
Live load = 363m2 x 3.0 kPa
TOTAL = 1,089 kN
	



Please refer to the information below in responding to Q22. to Q25. 

There is a building 21m long x 10m wide x 8m high with a 25⁰ pitched gable roof. The rafter line on the metal clad roof measures 5.5m on the rafter line (from the fascia/gutter line up to the ridge line).

The wind load is calculated as Area of surface x Wind load rate. The wind load rates are as follows:
· Windward wall is 21 metres long x 8 metres high with a wind load rate of +1.5KN/m²; 
· Leeward wall is 21 metres long x 8 metres high with a wind load rate of -0.8kN/m²; 
· Windward roof with a wind load rate of +0.8kN/m²; and 
· Leeward roof with a wind load rate of -1.5kN/m²



Q22.  [bookmark: _Ref427218342]What is the wind load of the windward wall? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-252kN
	

	
		134.4kN
	

	
		252kN
	

	
		86.4kN
	




Q23.  [bookmark: _Ref427218344]What is the wind load for the leeward wall? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-134.4kN
	

	
		-94.2kN
	

	
		252kN
	

	
		134.4kN
	




Q24.  [bookmark: _Ref427218346]What is the wind load for the leeward roof? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-173.25kN
	

	
		92.4kN
	

	
		173.25kN
	

	
		-134.4kN
	




Q25.  [bookmark: _Ref427057362]What is the wind load for the windward roof? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		252kN
	

	
		-92.4kN
	

	
		-252kN
	

	
		92.4kN
	





Q26.  [bookmark: _Ref427217924]Explain the term ‘load path’ in reference to a building.

	Answer
	The load path is the direction each consecutive load will passed through connected members. The system will start at the highest point of the structure and work its way down to the footing system. This results in shifting the total load of the structure to the foundation. 
	



Q27.  [bookmark: _Ref427219307]Forces are represented as vectors and have three (3) properties. 
Name these properties.

	Answer
	Magnitude, direction and position.
	



Q28.  [bookmark: _Ref427219642]Name five (5) structural members that a building may consist of.

	Answer
	Structural members in a building may consist of columns, posts and stumps. Retaining walls and wind bracing. Also footings and walls (load-bearing). 
	


Q29.  [bookmark: _Ref427219933]What should be considered when determining the shape and type of material to use?

	Answer
	When choosing the shape and type of materials, you should always consider the mechanical properties such as strength, toughness, elasticity, plasticity, ductility, malleability, brittleness and hardness. Another property to consider is the sections e.g. the mathematical properties of structural shapes.
	



Q30.  [bookmark: _Ref427220471]Match the mechanical properties and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Mechanical properties
	Answers
	Definitions
	
	
	1
	Brittleness
	1 - G
	A
	The resistance the structural member is able to offer the load that will just cause fracture. 
	

	
	2
	Elasticity 
	2 - C
	B
	The resistance to a fracture point of a material by repeated bending or twisting after yield point has passed.
	

	
	3
	Ductility
	3 - E
	C
	Present if a material deforms with loading and then returns to its original shape when the loads are removed.
	

	
	4
	Hardness 
	4 - H
	D
	If a material deforms when loaded and does not return to its original shape when the load is removed, causing permanent deformation. 
	

	
	5
	Malleability
	5 - F
	E
	Enables a material to be drawn out in the direction of its length. 
	

	
	6
	Plasticity
	6 - D
	F
	Can be hammered or otherwise worked into various shapes.
	

	
	7
	Strength
	7 - A
	G
	Causes material to break or snap off without any noticeable lengthening. 
	

	
	8
	Toughness
	8 - B
	H
	The degree of resistance to indentation or abrasion. 
	




Q31.  [bookmark: _Ref427220295]Match the beam types and descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Beam type
	Answers
	Description
	
	
	1
	Cantilevered 
	1 - A
	A
	Overhang their supports.
	

	
	2
	Continuously supported
	2 - C
	B
	Supported at each end only.
	

	
	3
	Simply supported
	3 - B
	C
	Supported by 3+ support points. 
	



Q32.  [bookmark: _Ref427225888]Match the column considerations and explanations by writing the appropriate letter next to each number in the centre column.

	Answer
	Column consideration
	Answers
	Explanation
	
	
	1
	Axially loaded column
	1 - A
	A
	The load is central to the centre of gravity axis. 
	

	
	2
	Buckling
	2 - E
	B
	The load is off-centre, resulting in bending and compressing stress being applied to the column.
	

	
	3
	End fixity and effective length
	3 - C
	C
	The rigid connection to other members at the top and bottom affects the way a column buckles.
	

	
	4
	Non-axially loaded column
	4 - B
	D
	Affects the maximum load a column can be allowed to support.
	

	
	5
	Slenderness ratio
	5 - D
	E
	Occurs at the weakness axis unless a lateral restraint is used to prevent it. 
	




Q33.  [bookmark: _Ref427224602]Explain how a column is in compression.

	Answer
	A column is in compression due to being used as a vertical support member between compressive loads. 
	



Q34.  [bookmark: _Ref427225635]Explain the letters ‘CHS’ and ‘SHS’ with reference to columns.

	Answer
	CHS refers to a circular hollow section and a SHS refers to a square hollow section.
	



Q35.  [bookmark: _Ref427227379]Match the retaining wall types and descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Retaining wall
	Answers
	Description
	
	
	1
	Cantilevered retaining wall
	1 - B 
	A
	Leans into the excavated soil and constructed at an angle between 45 and 80 degrees. Typically constructed from brickwork or pre-cast interlocking concrete units. 
	

	
	2
	Gravity retaining wall
	2 - C
	B
	Relies upon the correct placement of steel reinforcement and varying thickness of concrete to resist the soil pressure. 
	

	
	3
	Inclined retaining wall
	3 - A
	C
	Relies on its own weight to resist soil forces. Typically constructed from stone, brickwork or concrete. 
	




Q36.  [bookmark: _Ref427227493]What is a ground level concrete slab floor?

	Answer
	Ground level concrete slabs are poured directly into excavated trenches in the ground. They rely on the existing ground for support. The ground must be strong enough to support the concrete slab.
	



Q37.  [bookmark: _Ref427227808]What should you consider when selecting the type of slab floor?

	Answer
	When choosing a type of slab floor, you should consider the size, the climate zone which suits the type or slab, and the type of soil.
	



Q38.  [bookmark: _Ref531355302]True or False (Tick your response): Concrete slab floors are popular in the construction of structures because they take less time to construct.

	Answer
		True 
	
	
	
		False 
	
	





Q39.  [bookmark: _Ref427228752]Match the following slab structural performance terms with the descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Description
	
	
	1
	Foundation movement
	1 - C
	A
	Placed along the perimeter of the slab. Design is influenced by the reactivity of the soils. 
	

	
	2
	Slab bending
	2 - B
	B
	Movement is classified as dishing or doming. 
	

	
	3
	Stiffening beams
	3 - A
	C
	Addressed by regulating the moisture content of the soil.
	




Q40.  [bookmark: _Ref531355427]Which of these terms relate to a roof truss? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Chord, knee, web
	

	
		Spider, pitch, chord
	

	
		Ankle, heel, tar
	

	
		Web, heel, pitch
	




Q41.  [bookmark: _Ref427229422][bookmark: _Ref531008635]What are important considerations when undertaking demolition work? Describe relevant legislation, regulations and/or Codes of Practice relating to planning requirements, environmental standards, and safe work practices.

	Answer
	When planning demolition work, you should always go through all relevant legislations. The legislations for demo work are the Work Health and Safety Regulations 2011 QLD, Demolition Code of Practice 2013 QLD and the AS 2601: The demolition of structures. You should always obtain any required licences depending on your local council. A method of demolition should be planned which will also include information regarding temporary fencing and hoardings, protection for properties and public space around the site, disconnection notices for the service authorities. The order in which the building gets demolished in is a key factor, including details of hazardous materials. On-site amenities such as toilets, first aid and fire services will need to be available. Control measures for dust, noise and vibrations and vermin control for rats and mice will need to be considered also. If the demolition is going to affect the public road or pathways, traffic control MUST be organised with your local council and always consider how you can be environmentally friendly e.g. recycling.  
	


Q42.  [bookmark: _Ref531355335]When demolition is being undertaken, which of the following items must be checked daily? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		All boundaries are secured against unlawful entry
	

	
		All hazardous materials are removed or covered as required by OHS legislation
	

	
		All openings and elevated free edges are properly guarded
	

	
		All potential fire and safety hazards are eliminated and disconnected services are secured
	

	
		Asbestos is left on the nature strip for the garbage pickup
	

	
		Demolished materials have not been left on any floor or structure if their weight exceeds the safe carrying capacity of the floor or structure
	

	
		Emergency access routes are clear of debris
	

	
		Footpaths and public access are clear of demolished materials
	

	
		Neighbours have been notified not to hang out their washing
	

	
		No structure or part of a structure is left in such a condition that it may become dangerous, such as collapse due to wind or vibration
	

	
		Partly demolished elements are stabilised and loose materials are secured against bad weather
	

	
		Signs and balloons are in place for the garage sale
	

	
		Tell the demolisher to take a long lunch break as you don't need supervision
	

	
		Temporary hoardings, bracing, shoring and propping is tight and secure and in place as required to protect both workers and public
	




Q43.  [bookmark: _Ref531355737]Identify two (2) requirements under the NCC with regards to construction in bushfire prone areas?

	Answer
	A building that is constructed in a bushfire prone area must be designed to reduce the risk of ignition form a bushfire, appropriate to the potential for ignition caused by embers, radiant heat or flames generated by a bushfire. Also, to be suitable to the intensity of the bushfire attack on the building.
	



Q44.  [bookmark: _Ref427231195]What does AS3959 refer to?

	Answer
	AS3959 – Construction of Buildings in Bushfire-prone Areas
	



Q45.  [bookmark: _Ref531355744]Which of the following can assist with providing sufficient restraint to transfer wind forces to the ground to prevent collapse, uplift or sliding off the footing systems? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Anchorage systems
	

	
		Bracing systems
	

	
		Connecting structural elements together
	




Q46.  [bookmark: _Ref531355745]Which Australian Standard outlines the requirements of high wind areas?

	Answer
	AS 1170.2
	



Q47.  [bookmark: _Ref427232597]The acceleration coefficient is a number which indicates the expected severity of the earthquake ground movement. Which Australian Standard should be referenced for this information?

	Answer
	AS1170.4
	



Q48.  [bookmark: _Ref531355751]True or False (Tick your response): Where the acceleration coefficient is greater than 0.15, there are additional NCC requirements than where the acceleration coefficient is 0.12.

	Answer
		True 
	
	
	
		False 
	
	





Q49.  [bookmark: _Ref531355987]Which of the following areas require specific compliance in alpine areas? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Access bridges
	

	
		Access for emergency vehicles
	

	
		External doorways
	

	
		External ramps
	




Q50.  [bookmark: _Ref531355991]Identify the Volume and Parts of the NCC that relate to each of the following areas for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Topic
	Classes 1 and 10
	Classes 2 to 9
	
	
	Bushfire
	Volume 2 – Part 3.10.5
	Volume 1 -  Part G5
	

	
	High wind
	Volume 2 – Part 3.0
	Volume 1 – Part B1.2, B1.4
	

	
	Earthquake
	Volume 2 – Part 3.10.2
	Volume 1 – Part B1.2
	

	
	Alpine area
	Volume 2 – Part 3.10.4
	Volume 1 – Part G4
	

	
	New technologies
	Volume 2 – Part A2.2, A5
	Volume 1 - Part A2.2, A5
	




Q51.  [bookmark: _Ref427232821][bookmark: _Ref531356004]How are emerging building technologies and methods assessed in the National Construction Code? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Using verification methods
	

	
		With ‘deemed to satisfy’ provisions
	

	
		With documentary evidence
	





Q52.  [bookmark: _Ref531356217]True or False (Tick your response): Footings should be set out in accordance with the building plan.

	Answer
		True 
	
	
	
		False 
	
	




Q53.  [bookmark: _Ref531356194]Name three (3) different types of footing systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	.Columns or stumps, Concrete slab floors or Piers and beams
	Concrete slab floors, Mass concrete piers, Screw piles
	




Q54.  [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to footings (including damp coursing and provision of termite barriers) for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – Part 3.2.2
	Volume 1- Part B1
	




Q55.  [bookmark: _Ref531356170]For each of the following identify two (2) Australian Standards that relate to footings.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	AS 2879-2006
	AS 2904
	





Q56.  [bookmark: _Ref531356390]Name two (2) materials that may be used for damp proof coursing.

	Answer
	Corrosion resistant metal and impact resistant plastics.
	



Q57.  [bookmark: _Ref531356392]Name two (2) termite resistant materials.

	Answer
	Concrete or fibre-reinforced cement.
	



Q58.  [bookmark: _Ref531356575]Name three (3) different types of floor systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Concrete slab, Platform floor or fitted (cut-in) floors.
	Brick bases, engineered timber products or concrete slab floor.
	




Q59.  [bookmark: _Ref427235728]What should be considered when constructing a floor system?

	Answer
	When constructing a floor system, it is important to consider the type of flooring, the laying of pipes and reinforcement.
	



Q60.  [bookmark: _Ref531356610]Which Australian Standard is referenced in Volumes 1 and 2 of the NCC regarding the requirements for slabs and footings?

	Answer
	AS 2870
	



Q61.  [bookmark: _Ref531356630]Name three (3) different types of materials used for wall systems or structures falling under Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Cavity brick, Concrete block or timber
	Earth walls, framed walls or composite walls
	




Q62.  [bookmark: _Ref531356612]Identify the Volume and Parts of the NCC that relate to masonry wall systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – Part 3.3
	Volume 1 – Part B1.4
	




Q63.  [bookmark: _Ref531356616]Which Australian Standard is referenced in Volumes 1 and 2 of the NCC regarding masonry structures?

	Answer
	AS 3700
	



Q64.  [bookmark: _Ref427577558][bookmark: _Ref531356640][bookmark: _Ref427237033]Explain the purpose of bracing. 

	Answer
	Bracing delivers lateral support to wall framing. It allows framework to resist horizontal forces, especially wind loads as buildings must transmit the load through the structure to the foundation. The bracing action requires bracing units to be installed at 90 degrees to the surfaces facing the wind. 
	



Q65.  [bookmark: _Ref531357045]Explain the purpose of fixings and tie-downs. 

	Answer
	Fixings are essential to ensure the structural adequacy of the interconnection of the numerous framing members. Fixings include straps, bolts, screws and framing anchors. Tie-down fixings provide for structural connections to resist uplift and shear forces in the floor, wall and roof framing. Where precise tie-down fixings provide equal or better resistance to gravity or shear loads, nominal nailing is not required.
	



Q66.  [bookmark: _Ref531331115]Which Australian Standard relates to timber frames, bracing and fixings?

	Answer
	AS 1684
	



Q67.  [bookmark: _Ref531357052]For the Australian Standard in Q66. which part relates to cyclonic areas?

	Answer
	AS1684.3 – Part 3
	



Q68.  [bookmark: _Ref531357065]Which of the following should be observed when checking the quality of the frame (whether, factory pre-cut and pre-nailed, factory pre-cut and assembled on site, or cut and assembled on site)? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Fixings must be protected from corrosion
	

	
		Fixings must be protected from termites
	

	
		Provision has been made for plumbing services and fixtures
	

	
		Tie downs and nominal nailing must both be present
	

	
		Top and bottom plates have a tight fit on studs
	

	
		Top plate is to be reinforced when rafters land on top of plates
	

	
		Walls are tied together
	

	
		Walls are plumb
	

	
		Walls are square
	



Q69.  [bookmark: _Ref531357185]True or False (Tick your response): Sarking is a substitute for cladding and is regarded as the principal means of weatherproofing.

	Answer
		True 
	
	
	
		False 
	
	




Q70.  [bookmark: _Ref427237737]What is flashing?

	Answer
	Flashing is usually a piece of thin metal sheet. It is used at corners, vertical joints and openings to ensure that water is prevented from penetrating the wall frame cavity, 
	



Q71.  [bookmark: _Ref531357196]Identify the Volume and Parts of the NCC that relate to wall cladding material requirements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – Part 3.5
	Volume 1 – Part F1
	




Q72.  [bookmark: _Ref531357076]True or False (Tick your response): Timber can stand greater stresses than brickwork.

	Answer
		True 
	
	
	
		False 
	
	




Q73.  [bookmark: _Ref531357077]True or False (Tick your response): Individual timber boards for cladding should be nailed together at the overlap.

	Answer
		True 
	
	
	
		False 
	
	




Q74.  [bookmark: _Ref531357461]When should flashing materials be fixed to plywood cladding? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		After the cladding is fixed
	

	
		Before the cladding is fixed
	

	
		While the cladding is being fixed
	

	
		At any convenient time
	




Q75.  [bookmark: _Ref531357463]What is the purpose of articulation joints? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		They allow for shrinkage in a building
	

	
		They tie the brickwork to the frame
	

	
		They allow for movement in a building
	

	
		They seal the cavities 
	




Q76.  [bookmark: _Ref531357466]When is the most appropriate time for the rough-in to occur for a brick veneer building constructed on a concrete slab Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Before brickwork
	

	
		After brickwork
	

	
		After plasterboard
	

	
		Any time
	




Q77.  [bookmark: _Ref531357473]Apart from plumbing and electrical, name four (4) other services that should be considered at rough-in.

	Answer
	Heating and cooling services, Communication services, Passive and active fire detection and prevention services and powered systems for operating doors and windows.
	


Q78.  [bookmark: _Ref531357478]Identify the Volume and Parts of the NCC that relate to window installation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 -Part 3.6
	Volume 1 – Part B1.4, F1.13, J3.4
	




Q79.  [bookmark: _Ref531357506]Name two (2) Australian Standards that relate to the installation of windows. 

	Answer
	AS1288, AS2047
	



Q80.  [bookmark: _Ref531357537]What is the purpose of a window schedule? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		To help work out the appropriate type of window
	

	
		To work out the appropriate opening size of windows
	

	
		To work out whether to use a timber or aluminium frame
	

	
		To work out the height of a window
	




Q81.  [bookmark: _Ref531357490]Identify the Volume and Parts of the NCC that relate to door installation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – Part 3.6.4.1
	Volume 1 – Part D2.19
	




Q82.  [bookmark: _Ref427238214][bookmark: _Ref531357492]What Australian Standard must the design of a timber roof truss adhere to?

	Answer
	AS1720.1
	



Q83.  [bookmark: _Ref427583793][bookmark: _Ref531357772]What is a roof system? Name three (3) roof types.

	Answer
	A roof system is the structure that forms the roof of a building. Three types of roof systems is gable, hip and skillion.
	



Q84.  [bookmark: _Ref531357774]True or False (Tick your response): Roof trusses can be modified on site to suite different needs.

	Answer
		True 
	
	
	
		False 
	
	




Q85.  [bookmark: _Ref427584594]Devise a checklist for ensuring the quality of an installed roof frame.

	Answer
	To ensure your roof frame is top quality, it is advised to check these things; rise and pitch of roof against plan, correct propping of ridge, hips, valley, rafters and under purlins at correct centres. Also, adequate collar ties, line of rafter, hips and valleys. The support to strutting beams, fascia and barge boards and all the tie-downs and fixings. Ceiling joists and alignment with rafters, hanging beams, trimmers for location and trimming to manhole.
	



Q86.  [bookmark: _Ref531357779]Devise a checklist for ensuring the quality of an installed roof truss.

	Answer
	To ensure the quality of the roof trusses, you should check these things; truss layout plan, manufacturer’s specs for tie-downs, bracings and lateral stability. The roof truss certification, adequacy of supporting structure, dimension and overall width and length of wall for fit. The support to girder trusses, plumb and spacings, all the tie-down and fixings, location of specialised trusses. Ensure the trusses have not been modified on-site, check the eave overhangs and the trimming to the manhole.
	



Q87.  [bookmark: _Ref531357807]Name three (3) roof cladding materials.

	Answer
	Three types of roofing materials are brick veneer, tiles (concrete, clay and metal) and sheeting.
	



Q88.  [bookmark: _Ref427583809]What pitch of roof should roof tiles be applied? Are there exceptions?

	Answer
	Roof tiles should be applied on a 15-degree angle, however, some materials and methods of manufacturer’s require 25 degrees or greater pitch.
	




Q89.  [bookmark: _Ref531358032]When installing corrugated metal roof sheeting, which is the preferred direction of laying sheets to improve side lap effectiveness for minimising leakage? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Away from the prevailing weather
	

	
		Towards the north
	

	
		Towards the prevailing weather
	




Q90.  [bookmark: _Ref531358025]True or False (Tick your response): Sarking is advisable under any roof.

	Answer
		True 
	
	
	
		False 
	
	




Q91.  [bookmark: _Ref531358038]What Australian Standard relates to sarking?

	Answer
	AS/NZS 4256
	



Q92.  [bookmark: _Ref531358043]Name three (3) items that may require roof penetration. 

	Answer
	Roof penetration may be required for services such as ducts, plumbing and electrical service lines.
	



Q93.  [bookmark: _Ref531358046]Identify the sections/parts of NCC Volume 1 that relate to the installation of skylights.

	Answer
	Volume 1 – Section J, Part F4.
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Jessica Manley

	
	

	Participant signature
	
	
	

	Date
	19/04/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1
		
	Task 2
		



	ASSESSOR COMMENTS

	


CPCCBC4010B Apply structural principles to residential low rise constructions

	Practical Task 1

	Description of task:
A suitable observer is to verify the participant’s ability to apply structural principles to the erection and demolition of a low rise residential structure (Classes 1 and 10).

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
· Photographic evidence of projects, including detailed descriptions of all structural elements 
· Documentation from a project structurally designed; for example a garage, small extension, etc. including: 
· A copy of the plans and/or specifications 
· Identification of site classification, uplift forces, wind ratings, 
· Component selection methods – for example; BCA references, Australian Standard references

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Plans, computer, suitable work area appropriate to the construction process. 

	Assessment of task

	Name of participant:
	Jessica Manley

	Name of observer:
	Khyle Glover

	Role of observer 
(Confirm suitability to sign)
	Estimating Manager – superior group

	Email address of observer
	khyle@superiorgroup.com.au

	Signature of observer:
	
	Date:
	19/04/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. Provide comments if left unticked.

	1 Apply structural principles to planning

	1.1A.  [bookmark: _Ref530725761]Identify main structural principles that apply to the erection or demolition of the structure.
	
	1.1B.  [bookmark: _Ref530725767]Describe structural performance in terms of the effect of section properties on various materials. 
	
	1.1C.  [bookmark: _Ref530725780]Explain structural performance characteristics of the slabs, floors, beams, columns and retaining walls – and apply to the planning of the construction work. 
	
	1.1D.  [bookmark: _Ref530725785]Coordinate demolition of existing structures in accordance with safe work practices, legislative, environmental and planning requirements. 
	
	2 Structural integrity of buildings

	1.2A.  [bookmark: _Ref530725788]Consult relevant industry professionals to provide advice regarding the design process and structural integrity of the proposed building – using language and concepts appropriate to cultural differences (including non-verbal communication). 
	
	1.2B.  [bookmark: _Ref530725791]Collect and analyse project documentation to assist with the analysis of plans and specifications. 
	
	1.2C.  [bookmark: _Ref530725796]Analyse project documentation for compliance with National Construction Code requirements for bushfire, high wind, earthquake and alpine environments.
	
	1.2D.  [bookmark: _Ref530725800]Assess new and emerging building technologies, techniques and materials for application to the construction process and their compliance with National Construction Code requirements and Australian standards.
	
	1.2E.  [bookmark: _Ref530725804]Conduct pre-commencement site inspection to confirm analysis. 
	
	3 Footing system

	1.3A.  [bookmark: _Ref530725808]Set out footings in accordance with building plans.
	
	1.3B.  [bookmark: _Ref530725812]Assess structural integrity of the footings specified in the plans for compliance with relevant codes and accepted industry construction principles. 
	
	1.3C.  [bookmark: _Ref530725816]Lay footings specified in building’s plan, checking for compliance with project documentation. 
	
	1.3D.  [bookmark: _Ref530725822]Plan, implement and check damp coursing, provision of termite barriers and other relevant techniques in accordance with codes, standards and industry practice. 
	
	4 Floor system

	1.4A.  [bookmark: _Ref530725827]Assess concrete slab or bearers and joists specified in building plan for structural integrity and compliance with relevant codes and accepted industry construction principles.
	
	1.4B.  [bookmark: _Ref530725949]Supervise laying of floor system specified in building’s plan, checking for compliance with project documentation. 
	
	5 Structural and non-structural wall systems

	2.5A.  [bookmark: _Ref530725953]Identify and analyse technical construction principles and performance of materials to be used in the construction in the planning of the building and construction project. 
	
	2.5B.  [bookmark: _Ref530725957]Plan, implement and check application of bracing requirements, tie-downs, tolerance, allowances and fixing and installation of components for compliance with relevant Australian standards, codes and manufacturer specifications. 
	
	2.5C.  [bookmark: _Ref530725961]Select structural timber members for low rise buildings to conform to AS1684 requirements. 
	
	2.5D.  [bookmark: _Ref530725966]Put processes in place to ensure quality of the frame – whether factory pre-cut and pre-nailed, factory pre-cut and assembled on site, or cut and assembled on site. 
	
	2.5E.  [bookmark: _Ref530725969]Attach and check vapour permeable sarking or a waterproof membrane relevant to the construction method. 
	
	6 Roof system

	2.6A.  [bookmark: _Ref530725974]Assess structural integrity of roof system components specified in building plan for compliance with relevant codes and accepted industry construction principles. 
	
	2.6B.  [bookmark: _Ref530725980]Plan, implement and check erection of roof trusses in accordance with requirements of building plan, type of roof being construction, relevant codes and accepted industry construction principles. 
	
	2.6C.  [bookmark: _Ref530725983]Put processes in place to ensure quality of the manufactured roof trusses or hand-cut roof system. 
	
	2.6D.  [bookmark: _Ref530725987]Plan roof sarking and cladding and supervise installation for compliance with codes, standards and industry practice.  
	
	7 External wall cladding

	2.7A.  [bookmark: _Ref530725992]Assess structural performance of cladding to be used for bracing in the frame construction for compliance with relevant codes, manufacturer specifications and accepted industry construction principles. 
	
	2.7B.  [bookmark: _Ref530725996]Supervise installation of cladding as specified in building plan, and check for compliance with standards and accepted industry construction principles. 
	
	2.7C.  [bookmark: _Ref530725999]Supervise installation of windows and external doors to ensure compliance with relevant codes, manufacturer specifications and accepted industry construction principles. 
	
	The Participant’s performance was:  Satisfactory     Not Satisfactory


	OBSERVER COMMENTS

	Great job Jess, thorough detail in the tasks! - Khyle
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CPCCBC4011B Apply structural principles to commercial low rise constructions

	Practical Task 2

	Description of task:
A suitable observer is to verify the participant’s ability to apply structural principles to the erection and demolition of a low rise commercial structure (Classes 2 to 9 with a gross floor area not exceeding 2000m2, but not including Type A or Type B construction). 

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include:
· Photographic evidence of projects, including detailed descriptions of all structural elements
· Documentation from a commercial works structurally designed; including: 
· A copy of the plans and/or specifications 
· Identification of site classification, uplift forces, wind ratings
· Component selection methods – for example; BCA references, Australian Standard references

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Plans, computer, suitable work area appropriate to the construction process. 

	Assessment of task

	Name of participant:
	Jessica Manley

	Name of observer:
	Khyle Glover

	Role of observer 
(Confirm suitability to sign)
	Estimating Manager – Superior Group

	Email address of observer
	khyle@superiorgroup.com.au

	Signature of observer:
	
	Date:
	19/04/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. Provide comments if left unticked.

	1 Apply structural principles to planning

	2.1A.  [bookmark: _Ref530737028]Identify main structural principles that apply to the erection or demolition of the structure.
	
	2.1B.  [bookmark: _Ref530737033]Describe structural performance in terms of the effect of section properties on various materials. 
	
	2.1C.  [bookmark: _Ref530737038]Explain structural performance characteristics of the slabs, beams, columns and retaining walls – and apply to the planning of the construction work. 
	
	2.1D.  [bookmark: _Ref530737043]Coordinate demolition of existing structures in accordance with safe work practices, legislative, environmental and planning requirements. 
	
	2 Structural integrity of buildings

	2.2A.  [bookmark: _Ref530737047]Consult relevant industry professionals to provide advice regarding the design process and structural integrity of the proposed building – using language and concepts appropriate to cultural differences (including non-verbal communication). 
	
	2.2B.  [bookmark: _Ref530737050]Collect and analyse project documentation to assist with the analysis of plans and specifications. 
	
	2.2C.  [bookmark: _Ref530737054]Analyse project documentation for compliance with National Construction Code requirements for bushfire, high wind, earthquake and alpine environments.
	
	2.2D.  [bookmark: _Ref530737058]Assess new and emerging building technologies, techniques and materials for application to the construction process and their compliance with National Construction Code requirements and Australian standards.
	
	2.2E.  [bookmark: _Ref530737062]Conduct pre-commencement site inspection to confirm analysis. 
	
	3 Footing system

	2.3A.  [bookmark: _Ref530737066]Set out footing systems in accordance with building plans.
	
	2.3B.  [bookmark: _Ref530737070]Assess structural integrity of the footings specified in the plans for compliance with relevant codes and accepted industry construction principles. 
	
	2.3C.  [bookmark: _Ref530737073]Lay footings specified in building’s plan, checking for compliance with project documentation. 
	
	2.3D.  [bookmark: _Ref530737076]Plan, implement and check damp coursing, provision of termite barriers and other relevant techniques in accordance with codes, standards and industry practice. 
	
	4 Floor system

	2.4A.  [bookmark: _Ref530737080]Assess floor system components specified in building plan for structural integrity and compliance with relevant codes and accepted industry construction principles.
	
	2.4B.  [bookmark: _Ref530737083]Supervise laying of structural floor system specified in building’s plan, checking for compliance with project documentation. 
	
	5 Structural wall systems and wall cladding systems

	2.5A.  [bookmark: _Ref530737087]Identify and analyse technical construction principles and performance characteristics of structural wall systems and wall cladding systems in the planning of the building and construction project. 
	
	2.5B.  [bookmark: _Ref530737091]Identify, implement and check processes for erecting wall systems and wall cladding systems for compliance with manufacturer specifications and relevant Australian standards and codes. 
	
	2.5C.  [bookmark: _Ref530737095]Identify and implement building plans and relevant standards and codes to ensure appropriate allowances were made for relevant services to be installed. 
	
	2.5D.  [bookmark: _Ref530737100]Install windows and external doors in compliance with relevant codes, manufacturer specifications and accepted industry construction principles. 
	
	6 Structural roof systems and roof cladding systems 

	2.6A.  [bookmark: _Ref530737103]Assess structural integrity of the structural roof system and roof cladding system components specified in the building’s plan for compliance with relevant codes and accepted industry construction principles. 
	
	2.6B.  [bookmark: _Ref530737107]Plan and implement and check construction of roof system and roof cladding system (including details of service penetrations, skylights and roof ventilators) according to building plan’s requirements, type of roof being constructed, relevant codes and accepted industry construction principles. 
	
	2.6C.  [bookmark: _Ref530737112]Put processes in place to ensure quality of finished roof system. 
	
	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS

	[bookmark: _GoBack]Jess has done an awesome job at navigating the NCC and providing detailed answers.
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