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CPCCBC4053 
Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4053 Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Michael Trott

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4053
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Practical Assessment
	 Documentation of design and construction (suitability or evidence of suitability)
 Fire protection inspection checklist



	Assessor name
	

	Assessor signature
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THEORY EXAM


	Participant name
	Michael Trott




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref127186634]Provide a brief description of the given classes of buildings according to the National Construction Code (NCC). 

	Answer
	Assessment method
	Description
	

	
	Class 2 building
	A building containing two or more sole-occupancy units. Each unit must be a separate dwelling.
	

	
	Class 3 building
	Class 3 buildings are residential buildings other than Class 1 or 2. These are long-term or transient living accommodations for unrelated people.
	

	
	Class 4 building
	A Class 4 building is the only dwelling or residence within any Class 5, 6, 7, 8 or 9 buildings.
	

	
	Class 5 building
	An office building used for professional or commercial purposes, except for buildings of Class 6, 7, 8 or 9.
	

	
	Assessment method
	Description
	

	
	Class 6 building
	Buildings that directly sell goods by retail or supply services to the public
	

	
	Class 7a building
	Carparks
	

	
	Class 7b building
	The following buildings are classified under Class 7b:
· warehouses
· storage buildings
buildings used to display or produce wholesale goods
	

	
	Class 8 building
	These are process-type buildings such as:
· buildings used for production, assembling, altering, repairing, finishing, packing or cleaning of goods or produce
laboratories (classified as such because of their high potential for fire hazard)
	





[bookmark: _Ref128984255]Discuss Class 9 buildings according to the NCC, including the difference between the three (3) Class 9 sub-classifications.

	Answer
	Class 9 buildings are critical for public health, safety, and welfare. Their sub-classifications (9a, 9b, and 9c) reflect their specific uses, occupant needs, and design requirements. Compliance with the NCC ensures these buildings are safe, accessible, and fit for purpose.
	




[bookmark: _Ref128115391]A client is showing you the plans for a group of four (4) dwellings over two (2) storeys, above a common basement or carpark. Determine what classification would be assigned to this building. Explain your answer.

	Answer
	This building would be classified as Class 2 due to the primary use being residential dwellings, with the basement carpark classified separately as Class 7a.This is primarily because the structure is a mixed-use building.
	




[bookmark: _Ref128115393]Another client would like to build a new doctors surgery. Determine what classification would be assigned to this. Explain your answer.

	Answer
	This would be a class 5 building because it is an office used for professional purposes
	



[bookmark: _Ref128119881]Explain why the plans for a warehouse that contains a caretakers residence may have more than one classification.

	Answer
	Because it’s a residence used for dual purposes, warehouse being class 7b and the caretakers residence being class 4
	




[bookmark: _Ref128990469]What dictates how buildings must be constructed in Australia and how may this differ in your State or Territory?

	Answer
	In Australia, the construction of buildings is primarily dictated by the National Construction Code (NCC). The NCC sets out the minimum technical requirements for the design and construction of buildings to ensure safety, health, accessibility, and sustainability. It is a performance-based code that applies uniformly across all states and territories, but local variations may exist like in queensland for example where they may have stricter cyclone-related construction standards.
	




[bookmark: _Ref127183513]Explain why it is important to understand references the NCC makes to Australian Standards.

	Answer
	Understanding references the NCC makes to Australian Standards is crucial because:
1. Detailed Compliance: The NCC provides broad requirements, while Australian Standards offer specific technical details (e.g., materials, testing, and methods).
2. Legal Obligation: Compliance with Australian Standards is often mandatory when referenced in the NCC, ensuring legal adherence.
3. Safety and Quality: Following these standards ensures buildings are safe, durable, and fit for purpose.
4. Consistency: Standards promote uniformity across the industry, ensuring predictable and reliable construction outcomes.
By aligning with referenced standards, builders meet both regulatory and practical expectations for construction quality and safety.

	




[bookmark: _Ref128991786]Clarify the purpose of compliance with AS 3600.

	Answer
	As 3600 is a standard for the design and construction of concrete building structures and members in Australia Compliance with AS 3600 guarantees concrete structures are robust, long-lasting, and conform to Australian regulations and best practices. 
	




[bookmark: _Ref128995884]Provide a brief explanation of the listed NCC compliance assessment methods used to determine compliance using a Performance Solution pathway.

	Answer
	Assessment method
	Description
	

	
	Evidence of suitability
	This is also known as ‘documentary evidence.’ This entails showing evidence that the use of material, plumbing and drainage product or form of construction or design meets the Performance Requirements or a DTS Provision.
	

	
	Verification methods
	Commonly, Verification Methods include quantifiable or predetermined acceptable criteria that must be achieved by the given compliance option.
	

	
	Comparison with DTS Provisions
	This method applies to Performance Solutions. It involves doing a comparative analysis to determine whether Performance Solutions provide the superior or same level of health, safety, amenity, or sustainability as using the DTS provisions.
There must be a defined benchmark provided to the building surveyor. This method is done by subjecting both the DTS Solution and Performance Solution to the same level of analysis using the same methodology.
	

	
	Expert Judgement
	An expert can either be a person or an organisation with the necessary skills and experience to make a judgement concerning NCC compliance. The legal definition of an expert varies per state and territory. In cases where you are unsure who qualifies as an expert, you must consult with an Appropriate Authority.

	



[bookmark: _Ref127263388]Discuss the listed levels found in the NCC Performance Hierarchy.

	Answer
	Performance Hierarchy
	Description
	

	
	Objectives
	High-level goals that outline what the NCC aims to achieve (e.g., ensuring the health and safety of building occupants, sustainability, and protection of property).
	

	
	Functional statements
	Statements that describe the intended purpose or function of a building component or system.
	

	
	Performance requirements
	The core technical specifications that a building must meet. These are the mandatory minimum standards for safety, health, accessibility, and sustainability.
	

	
	Building Solutions
	Methods used to comply with the performance requirements. These can be:
Deemed-to-Satisfy (DTS) Solutions: Prescriptive solutions outlined in the NCC.
	




[bookmark: _Ref127278250][bookmark: _Ref129067815]Why may you need to use a combination of Performance Solutions and Deemed-to-Satisfy (DtS) solutions to comply with the Performance Requirements of the NCC?

	Answer
	Combining Performance Solutions and DtS allows compliance with the NCC’s Performance Requirements while enabling innovation, addressing unique challenges, and ensuring cost-effective, practical outcomes. This hybrid approach ensures both flexibility and adherence to regulatory standards.
	




[bookmark: _Ref129066894]Discuss the workplace policies and procedures that should be held on-site.

	Answer
	Workplace health and safety policies
Environmental policies
Code of conduct
Operational procedures
Emergency procedures
Employment and HR policies
Quality assurance procedures
	




[bookmark: _Ref129067939]Describe the basic principles of structural design and how these align with large span structures.

	Answer
	The principles of structural design ensure safety, functionality, and durability, with specific adaptations for large span structures to address unique challenges like wide load distribution, material efficiency, and environmental factors. These principles, when applied effectively, create resilient, efficient, and visually appealing large span structures.
	




[bookmark: _Ref127274757]What type of information is determined from the working drawings and specifications when organising the excavation for a shopping centre with underground parking?

	Answer
	Working drawings and specifications provide critical details for excavation, including site dimensions, soil conditions, structural requirements, drainage, utilities, and safety measures. This information ensures that excavation for a shopping centre with underground parking is executed efficiently, safely, and in compliance with design and regulatory requirements.
	




[bookmark: _Ref127253785]Discuss compressive and tensile stresses on buildings.

	Answer
	Compressive and tensile stresses play a critical role in building performance. Structural design must balance these forces, leveraging materials and systems that resist compression and tension effectively to ensure safety, stability, and longevity.
	




[bookmark: _Ref129070306]Briefly clarify the meaning of ‘water ingress’ when related to waterproofing a building.

	Answer
	Water ingress is water that penetrates the internal of a building
	




[bookmark: _Ref129071735]What do you check for to confirm product compliance with NCC requirements?

	Answer
	Product labelling and documentation or DTS provisions
	




[bookmark: _Ref129071897]Where do you record checks that you have made on products and materials that have arrived on-site?

	Answer
	Material inspection checklist
	




[bookmark: _Ref129075029]What are some indications that a construction company is abiding by environmental protection laws?

	Answer
	Proper waste management or implementation of EMPs.
	



[bookmark: _Ref129075323]Explain your understanding of the following concepts relating to sustainability.

	Answer
	Concept
	Explanation 
	

	
	Ecological footprint
	The ecological footprint measures the environmental impact of human activities by calculating the amount of land, water, and natural resources needed to produce the goods and services consumed and to absorb the waste generated.
	

	
	Renewable energy
	Renewable energy refers to energy sourced from natural processes that are replenished on a human timescale, such as sunlight, wind, water (hydropower), geothermal heat, and biomass.
	




[bookmark: _Ref128122622]Provide the six (6) bushfire attack level ratings that AS 3959 uses to establish the requirements for construction. Explain each rating.

	Answer
1.



2.



3.



4.



5.



6.
	
BAL-Low



BAL-12.5 Risk of ember attack



BAL-19 Increased level of ember attack and burning debris,increasing heat flux exposure


BAL-29 As above but with variation to vegetation classifications and/or heat flux exposure

BAL-40 As per bal29 and with the increase likelihood of exposure to flames



BAL-FZ Direct exposure to flames from fire front in addition to heat flux and ember attack

	



[bookmark: _Ref128122625]Complete the table below by identifying the type of fire-resisting construction (i.e. Type A, Type B, or Type C) given the following class of building and number of storeys each class of building has.

	Answer
	Rise in Storeys
	Class of building:
2,3,9
	Class of building:
5,6,7,8
	

	
	4 or more
	A
	A
	

	
	3
	A
	B
	

	
	2
	B
	B
	

	
	1
	C
	C
	




[bookmark: _Ref128129905]Respond to each of the following regarding zero-energy building.

	Answer
	
	Zero energy building
	

	
	Definition
	A Zero Energy Building is a structure designed to produce as much energy as it consumes over a year. This is achieved through energy-efficient design, renewable energy generation, and sustainable building practices. The goal is to reduce reliance on external energy sources, minimising environmental impact.
	

	
	One (1) technique used in zero energy building
	Solar power
	

	
	The procedure in implementing the technique you have identified
	Install solar panels on the roof or appropriate outdoor areas
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WORKBOOK


	Participant name
	Michael Trott




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific business context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

	ACTIVITY 1  [bookmark: _Ref35349341]

	Access the National Construction Code (NCC) to:
a) Determine where to locate the technical building requirements for Class 2 to 9 buildings.
b) What is stated in Volume One Amendment 1 – Queensland Part B1 Structural provisions?
c) What is stated in Volume One Amendment 1 – NSW Section A6.6 Class 6 buildings?



	a) Determine where to locate the technical building requirements for Class 2 to 9 buildings.

	Volume One of the NCC

	b) What is stated in Volume One Amendment 1 – Queensland Part B1 Structural provisions?

	This section outlines the structural requirements to ensure buildings can withstand various loads and forces.

	c) What is stated in Volume One Amendment 1 – NSW Section A6.6 Class 6 buildings?

	This section defines Class 6 buildings, which are typically shops or other buildings for the sale of goods by retail or the supply of services direct to the public.





	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref128995624]

	Access the National Construction Code (NCC) Volume One Amendment 1 - Section A Governing Requirements - Part A2 Compliance with the NCC and respond to the following:
a) What does this Part explain?
b) What methods are available to achieve the Performance requirements?
c) How is a performance solution shown to comply with the relevant Performance Requirements? 



	a) What does this Part explain?

	Part A2 explains the possible methods of demonstrating compliance with the NCC. It details the various compliance pathways within the NCC and the appropriate steps that must be taken for each of these pathways.

	b) What methods are available to achieve the Performance requirements?

	Performance solution
DTS Solution


	c) How is a performance solution shown to comply with the relevant Performance Requirements?

	Evidence of Suitability: Documentation that shows the use of a material, product, form of construction, or design meets the relevant Performance Requirements.




	Satisfactory Outcome
	
	




	ACTIVITY 3  [bookmark: _Ref128134618]

	Some occupants of a brick apartment building have complained about plaster damage, mould build up, damaged skirting and floorboards. The issue seems to affect rooms beside or including bathrooms.

Given the information above:
a) Identify factors that may have contributed to the damage issue.
b) Identify which Part from the NCC Volume 1 Amendment 1 was not properly applied.
c) Briefly explain how the identified Part from the NCC Volume 1 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Briefly explain how the identified Australian standard was not properly applied.
f) Identify what other defect the building may have considering the deviations of the construction from the code and standard.
g) Describe the extent of the work that needs to be done to rectify the issue.



	a) Identify what contributed to the degradation issue.

	Waterproofing issues
Plumbing defects
Drainage issues
Building materials
Ventilation

	b) Identify which Part from the NCC Volume 1 Amendment 1 was not properly applied.

	Part F1- Damp and waterproofing

	c) Briefly explain how the identified Part from the NCC Volume 1 was not properly applied.

	The issues (e.g., mould, skirting, and floorboard damage) suggest that waterproofing standards or water management measures were not implemented or installed correctly, allowing water to escape from bathrooms and damage adjoining areas.

	d) Identify which Australian standard was not properly applied.

	AS 3740 – Waterproofing of domestic wet areas

	e) Briefly explain how the identified Australian standard was not properly applied.

	Incomplete membrane application or poor quality control during waterproofing installation

	f) Identify what other defect the building may have considering the deviations of the construction from the code and standard.

	Structural damage 

	g) Describe the extent of the work that needs to be done to rectify the issue.

	Assess damage and rectify waterproofing to bring it to as 3740 standard 




	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref129007825]

	Access the NCC via the internet to locate the requirements applicable to a building development in the Brisbane area, containing 6 sole-occupancy units, two (2) on each level, each being a separate dwelling. 
This building includes one (1) basement level designated for car parking. 
The proposed building structure requires reinforced concrete floors and columns.
Document your findings or where in the NCC the information can be located. 




Building Description
	Classification

	Class 2

	Rise in Storeys

	3 storeys above ground plus 1 basement

	Number of Storeys

	4

	Type of construction

	Type A

	Climate Zone and description

	Climate zone 2 – warm humid summer, mild winter


Fire resistance and stability
	Locate fire resistance information

	Part C of NCC volume 1 - FRLs

	Compartmentation and fire separation

	Part C also details requirements for compartmentation and separation to prevent fire spread between units and other parts of the building. 
Part C also details requirements for compartmentation and separation to prevent fire spread between units and other parts of the building. 
NCC


	Fire hazard properties of materials, assemblies, fixtures and linings

	Part C specifies the fire hazard properties of materials used in construction, ensuring they meet necessary fire performance criteria.



Material requirements
	Reinforced concrete requirements relative to Australian Standards

	AS 3600

	Glazing requirements specifically for windows, sliding doors with frames and balconies.

	Part B1 References AS 1288



	Satisfactory Outcome
	
	



	ACTIVITY 5  [bookmark: _Ref127273569]

	The building discussed in ACTIVITY 2 includes one (1) basement level designated for car parking. 
Provide information required for 
· Bored piling to retain the soil and enable basement walls.
· Work Health and Safety
· Water proofing
· Water ingress

Document your findings or where the information can be located. 



	Bored piling to retain soil and enable basement walls 

	Bored piling involves drilling deep holes into the ground and filling them with reinforced concrete to create strong, vertical structural elements. These piles support the basement walls and retain surrounding soil during excavation and construction.
AS 2159-1995
Volume 2, part 3.2.5

	Work Health and Safety

	Ensuring the safety of workers during construction is paramount. Compliance with WHS regulations helps prevent accidents and health issues on-site.
WHS 2015
Safe work Australia
SWMS

	Water proofing

	Effective waterproofing prevents water ingress, protecting the structural integrity of the basement and ensuring a safe environment.
AS 3740
Volume 2, part 3.8.1

	Water ingress

	Water ingress refers to unwanted water penetration into the building, which can lead to structural damage, mould growth, and other issues.
As 3740



	Satisfactory Outcome
	
	



	ACTIVITY 6  [bookmark: _Ref129073248]

	A newly-built hotel needed to have its second-storey elevator lobby renovated, so customers had to take the stairs to get to the second storey of the hotel. On more than one occasion, people with visual impairment have had trouble finding the first step of the stairway, with some even misjudging the first step and falling over. No serious injury has happened yet, but the hotel manager decided something had to be done with the lack of indication of the first step of the stairway. An investigation was made after the third person tripped over the first step, and the investigation revealed that no research on who could possibly use the stairs was done. Respond to the following:
a) Identify one factor that contributed to the failure of the people with visual impairment to find the stairs of the hotel.
b) Identify which clause from the NCC Volume 1 was not properly applied.
c) Briefly explain how the clause from the NCC Volume 1 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Describe the extent of work that needs to be done to rectify the breach.



	a) Identify one factor that contributed to the failure of the people with visual impairment to find the stairs of the hotel.

	Lack of visual and tactile cues

	b) Identify which clause from the Building Code of Australia Volume 1 was not properly applied.

	Clause D3.8

	c) Briefly explain how the identified clause from the Building Code of Australia Volume 1 was not properly applied.

	The clause mandates the use of appropriate indicators, such as:
Tactile ground surface indicators (TGSI) to alert visually impaired individuals of the stairs' presence.
Visual contrast markings on the edges of steps for improved visibility.
The failure to install these indicators at the stairway entrance violates the clause, as it does not ensure safe access and use for individuals with disabilities.

	d) Identify which Australian standard was not properly applied.

	AS 1428.1:Design for access and mobility

	e) Describe the extent of work that needs to be done to rectify the breach.

	Install tactile ground surface indicators at the landing area leading to the stairs to alert visually impaired users
.



	Satisfactory Outcome
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PRACTICAL ASSESSMENT


	Participant name
	Michael Trott




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1 (Occasion 1)
	17/01/2025
	 Workplace
 Simulation
	
	
	

	Task 1 (Occasion 2)
	10/01/2025
	 Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1- Class 2, 3 or 9

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 1.1C. 1.1D. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
 Workplace Quality document  Quality Assurance Template  Other (please specify):



 Document attached as evidence

	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson  Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify building checked for compliance with active fire protection requirements:



 Is checklist used attached as evidence





	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 2 - Class 5 to 8

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Details

	1.1A. 1.1B. 1.1C. 1.1D. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
 Workplace Quality document  Quality Assurance Template  Other (please specify):



 Document attached as evidence

	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson  Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify building checked for compliance with active fire protection requirements:



 Is checklist used attached as evidence





CPCCBC4053
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	Practical Task 1 (2X)

	Description of task:
The participant must demonstrate the skills and knowledge to apply building codes and standards to the construction process for Class 2 to 9 Type C buildings. 
· Occasion 1 - Class 2, 3 or 9
· Occasion 2 - Class 5 to 8
Documented evidence of all criteria must be presented (template (HO1) available for use if required) The participant must also inspect one existing buildings for fire protection compliance using workplace or created document (See HO2 for information). Assessor and observer will be looking for evidence including:
· Classify building and document findings.
· Read the plans and specifications to determine the nature of the building, its use and arrangement.
· Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
· Determine and document the classifications applicable to the building. (template available- HO1)
· Identify and interpret multiple classifications from NCC.
· Determine construction compliance requirements.
· Determine NCC Performance Requirements relevant to Class 2 to 9 Type C building projects.
· Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
· Identify and document faults or non-conforming construction methods against NCC Performance Requirements. (template available- HO1) 
· Propose Performance Solution during discussion with design and building professional.
· Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
· Meet the evidence of suitability requirements for building materials and products stated in the NCC.
· Complete documentation demonstrating how the project design and construction will meet NCC requirements (template available- HO1) including:
· Structure
· Access and egress
· Services and equipment
· Health and amenities
· Ancillary provisions
· Energy efficiency
· Determine fire protection requirements.
· Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
· Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
· Inspect one building for compliance with passive and active fire protection requirements.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Construction plans, drawings and specifications of two Type C building projects- one(1) Class 2, 3 or 9 and one (1) Class 5 to 8.; workplace quality policies and procedures; technology to access building and related industry codes, standards and manufacturer product information and materials specifications; Technology to access the NCC and current relevant Acts and Regulations. PPE as required. Documentation of design and construction (suitability or evidence of suitability) (template available- (HO1)). Fire protection checklist (HO2).

	Observer details

	Name of observer:
	Dylan Cunningham

	Role of observer 
(Confirm suitability to sign)
	Project manager

	Email address of observer
	dcunningham@cor4service.com

	Signature of observer:
	
	Date:
	10/01/2025



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Classify buildings.

	[bookmark: _Ref129077872]Read the plans and specifications to determine the nature of the building, its use and arrangement.
		
	[bookmark: _Ref129077875]Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
		
	[bookmark: _Ref129077878]Determine and document the classifications applicable to the building. (template available- HO1)
		
	[bookmark: _Ref129077882]Identify and interpret multiple classifications from NCC.
		
	2 Determine construction compliance requirements from NCC.

	[bookmark: _Ref129079891]Determine NCC Performance Requirements relevant to Class 2 to 9 Type C building projects.
· Occasion 1- Class 2, 3 or 9
· Occasion 2 - Class 5 to 8
		
	[bookmark: _Ref129079900]Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
		
	[bookmark: _Ref129079909]Identify and document faults or non-conforming construction methods against NCC Performance Requirements. (template available- HO1) 
		
	[bookmark: _Ref129078432]Propose Performance Solution during discussion with design and building professional. 
		
	[bookmark: _Ref129079927]Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
		
	[bookmark: _Ref129079933]Meet the evidence of suitability requirements for building materials and products stated in the NCC.
		
	[bookmark: _Ref129079940]Complete documentation demonstrating how the project design and construction will meet NCC requirements for structure. (template available- HO1)
		
	[bookmark: _Ref129079955]Complete documentation demonstrating how the project design and construction will meet NCC requirements for access and egress. (template available- HO1)
		
	[bookmark: _Ref129079957]Complete documentation demonstrating how the project design and construction will meet NCC requirements for services and equipment. (template available- HO1)
		
	[bookmark: _Ref129079961]Complete documentation demonstrating how the project design and construction will meet NCC requirements for health and amenities. (template available- HO1)
		
	[bookmark: _Ref129079963]Complete documentation demonstrating how the project design and construction will meet NCC requirements for ancillary provisions. (template available- HO1)
		
	[bookmark: _Ref129079964]Complete documentation demonstrating how the project design and construction will meet NCC requirements for  energy efficiency. (template available- HO1)
		
	[bookmark: _Ref129080153]Complete documentation demonstrating how the project design and construction will meet NCC requirements for fire protection. (template available- HO1)
		
	3 Determine fire protection requirements.

	[bookmark: _Ref129079972]Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
		
	[bookmark: _Ref129079978]Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
		
	[bookmark: _Ref129078721]Inspect one building for compliance with passive and active fire protection requirements.
		




	Observer comments:
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