1. HAZARD AND RISK IDENTIFICATION
Hazardous Chemicals used at Delta
[bookmark: _Hlk181682460]ULTIMATE DIESEL
Re-fuelling heavy plant, pumps, light vehicles
Diesel fuel is classified as a C1 combustible liquid, meaning that it has a closed cup flashpoint between 60 degrees Celsius and 93 degrees Celsius. It is considered hazardous for storage purposes but not dangerous goods for road or rail transport.
LICENCES AND PERMITS
No licence or permits required
SAFE USE, HANDLING, PROCESSING AND DISPOSAL
Keep out of reach of children, use of PPE – gloves, eye/face protection, anti-static clothing and fully enclosed shoes, keep away from flames and hot surfaces, no smoking, use only outdoors or in a well-ventilated area, do not breathe in vapour or spray, wash hands thoroughly after handling.
EXPOSURE STANDARDS AND ASSOCIATED MONITORING
[bookmark: _Hlk181683591]Get medical attention if inhaled or swallowed. Do not induce vomiting if swallowed. Remove contaminated clothing. Wash off skin with plenty of soap and water. Treatment should in general be symptomatic and directed to relieving any effects. Monitor for cardiac dysrhythmias.
TRANSPORTATION AND STORAGE, LABELLING AND SIGNAGE
This product is not regulated as a dangerous good when transported in sizes of <5L or <5kg, provided the packaging meet the general provisions of 4.1.1.1, 4.1.1.2 and 4.1.1.4 to 4.1.18 (IMO – International Maritime Organisation standards and regulations the Australian Code for the Transport of Dangerous Goods by Road and Rail, the Australian Code for the Transport of Explosives by Road and Rail, the International Maritime Dangerous Goods Code, and the Civil Aviation Safety Regulations). All containers must be stored in a segregated and approved area, away from incompatible materials, food and drink. Store in a lock up, well-ventilated place and keep cool. Keep container tightly closed and sealed with appropriate labelling in accordance with the Globally Harmonized System of Classification and Labelling of Chemicals (GHS), as modified under Schedule 6 of the WHS Regulations for mixtures of substances, and Schedule 9 of the WHS Regulations. Dispose of contents and container in accordance with all local, regional, national and international regulations.



WORKER EXPOSURE
Get medical attention if inhaled or swallowed. Do not induce vomiting if swallowed. Remove contaminated clothing. Wash off skin with plenty of soap and water. Follow exposure standards and associated monitoring if exposed.
RISK ASSESSMENT
Identify Hazards: Potential hazards associated with diesel fuel, such as:
Flammability: Diesel fuel is highly flammable and can cause fires or explosions.
Toxicity: Exposure to diesel fumes can lead to health issues like respiratory problems and skin irritation.
Environmental Impact: Spills can contaminate soil and water sources.
Assess Risks: Evaluate the likelihood and severity of these hazards occurring. Consider factors like the amount of diesel stored, frequency of handling, and proximity to ignition sources.
Control Measures: Implement control measures to mitigate identified risks:
Proper Storage: Store diesel fuel in approved containers and storage areas, away from ignition sources.
Ventilation: Ensure adequate ventilation in areas where diesel is handled to reduce fume exposure.
Personal Protective Equipment (PPE): Provide appropriate PPE, such as gloves and safety goggles, to workers handling diesel.
Spill Response Plan: Develop and implement a spill response plan to address potential spills quickly and effectively.
Review and Monitor: Regularly review and monitor the effectiveness of control measures. Update the risk assessment as needed based on new information or changes in handling practices.


GLITZ WATERLESS HAND SANITISER
Waterless hand sanitiser used instead of washing hands with soap and water
This product is classified as flammable. Not classifies as hazardous according to the criteria of SWA. Dangerous according to the Australian Dangerous Goods Code, Class 3 – flammable liquids.
LICENCES AND PERMITS
No licence or permits required
SAFE USE, HANDLING, PROCESSING AND DISPOSAL
Keep out of reach of children, keep away from heat, sparks, open flames and hot surfaces and smoking, do not get into eyes. Dispose of small quantities and empty containers by wrapping with paper and putting in garbage. Larger quantities, use a commercial waste disposal service.
EXPOSURE STANDARDS AND ASSOCIATED MONITORING
If swallowed rinse mouth and do not induce vomiting. Us carbon dioxide, dry chemical foam, water fog in-case of fire.
TRANSPORTATION AND STORAGE, LABELLING AND SIGNAGE
Store in a cool dry place, well-ventilated and in a closed container. Class 3 flammable liquids shall not be loaded in the same vehicle or packed in the same freight container with other dangerous hazardous chemicals. All containers shall be labelled and signage used in area of storage.
WORKER EXPOSURE
In larger quantities, use in a well-ventilated area, use eye protection such as goggles.
RISK ASSESSMENT
Identify Hazards: potential hazards associated with hand sanitiser use, such as skin irritation, allergic reactions, and flammability due to high alcohol content.
Assess Risks: The likelihood and severity of these hazards occurring. Consider factors like frequency of use, concentration of alcohol, and user sensitivity.
Control Measures: Implement control measures such as;
Providing proper training on hand sanitiser use.
Ensuring adequate ventilation in areas where hand sanitiser is used.
Using hand sanitisers with added moisturisers to reduce skin irritation.
Storing hand sanitisers away from ignition sources due to their flammability.
Review and Monitor: Regularly review and monitor the effectiveness of control measures. Update the risk assessment as needed based on new information or changes in usage patterns.

2. DEVELOP PROCESSES AND PROCEDURES

1. Hazard identification – identify potential hazards with storage, handling and usage of diesel and hand sanitizer.
2. Storage – using approved containers, storage facilities for diesel and they are labelled as per legislation. Storing diesel away in well-ventilated areas and away from ignition sources. The same with the hand sanitizer, storing in a well-ventilated area, away from ignition sources.
3. Handling procedures – ensuring all personnel are trained in SOP’s and PPE when transferring diesel into equipment and tanks. Education on correct hand hygiene when using the hand sanitizer.
4. Spill response plan – Have a step-by-step response plan in the event of a spill that details the immediate containment of spill and the clean-up procedures e.g. spill kits located around site.
5. Environmental protection measures – Using drip trays when decanting fuel and inspect containers for leaks.
6. Emergency procedures – establishing emergency procedures in the event of a fire, environmental contamination or health risks.

MONITORING PROCESSESS AND PROCEDURES

1. Conduct regular inspections using checklists of storage facilities, equipment, PPE to ensure compliance.
2. Provide training for all personnel in handling of chemicals and what to do in an emergency.
3. Auditing on the reporting and investigation of incidents involving chemicals.
4. Maintain records of deliveries, stock, usage, spill incidents, training sessions, inspections and track trends for continuous improvement.
5. Conduct audits of chemicals and make sure that regulatory and company standards are being met.



REVIEWING FOR NON-COMPLIANCE

1. Conduct inspections in areas that diesel and hand sanitizer is used or stored and use a checklist to ensure all safety measures are in place.
2. Perform safety walks to observe real-time and identify potential risks.
3. Encourage reporting of any incidents or near-misses by workers.
4. Establish a feedback system for workers to report non-compliance and/or improvements.
5. Provide ongoing training sessions and refresher courses to keep employees updated on lates safety practices and procedures.
6. Analyse data from inspections, audits, incident reports to identify patterns of non-compliance.
7. Establish key performance indicators to measure compliance and effectiveness of control measures.
8. Hold regular meetings to review improvements and/or changes.

Subject: Important Updates: Diesel and Hand Sanitizer Procedures

Dear Team,
Delta is committed to maintaining a safe and healthy work environment for everyone. To this end, Delta have recently developed new processes and procedures regarding the use and handling of diesel and hand sanitizer. You’re understanding and adherence to these guidelines are crucial for our collective safety.
Diesel Handling and Storage Procedures:
Proper Storage: Diesel must be stored in approved, clearly labelled containers. Ensure storage areas are well-ventilated and away from ignition sources.
Handling: Use hand pumps or automatic dispensing systems. Always wear gloves and safety glasses when handling diesel.
Spill Prevention and Response: Follow our spill response plan. Spill kits are accessible on-site for immediate use.
Fire Safety: Fire extinguishers are available near diesel storage and handling areas. Remember, no smoking or open flames are permitted near diesel.
Hand Sanitizer Use:
Application: Use the provided hand sanitizers frequently, especially after touching shared surfaces or before eating. Make sure to apply an adequate amount and rub hands thoroughly until dry.
Storage: Store hand sanitizers in a cool, dry place, away from direct sunlight and heat sources to prevent flammability risks.
Safety Measures: If you experience any skin irritation or allergic reactions, please report it immediately. Use hand sanitizers with moisturizers to reduce skin dryness.

Please review the detailed procedures attached to this email. Adhere to these guidelines in your daily activities. Provide feedback if you notice areas for improvement or have any concerns.
Delta appreciates your cooperation and dedication to maintaining our safety standards. If you have any questions or need further clarification, don't hesitate to reach out.
Thank you for your attention.
Best regards
Kylie Roth, WHSA Delta
