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	[bookmark: _Ref536098285]THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	Assessor signature
	



	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Satisfactory?

	44
	
	Yes
	No

	
	
	
	


	ASSESSOR COMMENTS

	


 Which of the following documents and/or people would you refer to when selecting materials for a building project? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	Australian Standards
	

	
	x
	Contract
	

	
	x
	Drawings
	

	
	x
	Manufacturer
	

	
	x
	National Construction Code
	

	
	x
	Specifications
	

	
	x
	Tolerances
	




[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to suitability of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 part A5.0
	Volume 1 part A5.0
	




[bookmark: _Ref535482367]Identify the assessment methods used to verify a performance solution.

	Answer
	
Evidence of suitability.
A verification method.
Expert judgement.
[bookmark: _GoBack]Comparison with the deemed-to-satisfy provisions.
	




[bookmark: _Ref496611564][bookmark: _Ref536083431]Which of the following solutions for material selection often references the Australian Standards? Tick your response.

	Answer
	Choice
	Possible Answers
	

	
	x
	Deemed-to-Satisfy solution
	

	
	
	Performance solution
	




[bookmark: _Ref425255684]Identify five (5) materials commonly used for low rise buildings in your region. For each material, identify the following:
· Its name
· Properties of the material

	Answer
	#
	Material name
	Properties
	

	
	1
	concrete
	A composite building material made from aggregate (composite) and a binder .Has a low tensil strength, generally strengthened using steel rods and bars. 
	

	
	2
	metal
	Used as structural framework for larger buildings or as external surface covering. Also used in prefabricated structures like stair handles but requires a great deal of human labour to produce metal.
	

	
	3
	glass
	Made from mixture of sand and silicates and is very brittle. It provides covers to small openings and provides the ability of light into rooms; keeps inclement weather outside.
	

	
	4
	ceramic
	Used to be a specialized form of clay -pottery firing in kilns but has evolved into more technical areas. Used in such things as tiles and fixtures, including walls, counter tops and ceilings.
	

	
	5
	foam
	Synthetic polystyrene or polyutherane. It is light weight, easily shaped and excellent insulator . Used as part of a structural insulated panel where foam in sandwiched between wood or cement.
	





[bookmark: _Ref425323073][bookmark: _Ref425248000]For each of the materials in Q5. identify the following:
· Quality of the material (i.e. durability, serviceability, cost effectiveness)
· Compatibility and non-compatibility of the material (i.e. what it would/would not be suitable for)

	Answer
	#
	Quality
	Compatibility 
	

	
	1
	Durability
	Low tensile strength, generally compatible in using with bars and steel rods, lasts years.
	

	
	2
	Physical 
	Used mostly on Prefabricated structures, larger buildings and external surface coverings. Can stain and discolorating effects. Shrinkage and expansion effects.
	

	
	3
	Application
	Can be used in spaced frame. If light and weather needs to be controlled, this should be used.
	

	
	4
	Flexibility
	Can be used on walls, floors, ceilings and counter tops. 
	

	
	5
	Density
	Easily shaped and light, mostly only used for insulation in walls as part of a structural panel.
	



[bookmark: _Ref536083435]Identify five (5) physical characteristics that may be considered when evaluating potential building materials.

	Answer
	
Gravity 
Strengh
Flexibility
Durability
Acoustic

	




[bookmark: _Ref536095924]Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definition
	

	
	1
	Carbon footprint
	1 - B
	A
	The amount of energy required to manufacture a product
	

	
	2
	CO2e
	2 - E
	B
	Total GHD emissions produced during manufacture construction and use
	

	
	3
	Embodied energy
	3 - A
	C
	Greenhouse gas emissions
	

	
	4
	Embodied water
	4 - D
	D
	The amount of water required to manufacture a product
	

	
	5
	GHG
	5 - C
	E
	CO2equivalent tonnes emitted into the atmosphere
	




[bookmark: _Ref536083463]Which of the following materials would be considered as ‘low energy content’? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	Bricks
	

	
	X
	By-products of other industrial processes
	

	
	
	Cement
	

	
	
	Glass
	

	
	
	Metals
	

	
	
	Plastics
	

	
	
	Sand
	

	
	X
	Stone
	

	
	X
	Timber
	



[bookmark: _Ref536099133]Refer to the table below and identify the wall material type that has the smallest embodied energy and emission impact.

[image: ]

	Answer
	Wall timber frame and fibro clad 
	





[bookmark: _Ref536095926]Identify the Volume and Parts of the NCC that relate to energy efficiency of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volue 2 part 3.12
	Volume 1 part j
	




[bookmark: _Ref536097820]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses residential slabs and footings.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Section 3.2 of AS2870
	AS2870
	




[bookmark: _Ref536097822]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses roof tiles.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Section 6.0 of AS2049
	AS2049
	




[bookmark: _Ref536106144]Identify the Volume and Parts of the NCC that relate to safety barriers for swimming pools for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 part 3.10.1.0
	Volume 1 part G1.1.G1.3
	




[bookmark: _Ref536106145]In some states, barriers and fences for swimming pools are not entirely regulated by the NCC, as noted in the Ancillary Provisions and State and Territory Variations. Identify the applicable Act and Regulation that regulate safety barriers for swimming pools in your jurisdiction.

	Answer
	(NSW) Swimming pools Act 1992 and Swimming pools regulation 2008
	



[bookmark: _Ref536106146]Identify the Australian Standard that relates to safety barriers for swimming pools.

	Answer
	As 1926
	




[bookmark: _Ref536107455]True or False (Tick your response): According to the Standard in Q16. all gates must be fitted with a self-closing device that will return the gate to a closed position from any position without the use of manual force.

	Answer
	x
	True 
	
	

	
	
	False 
	
	




[bookmark: _Ref536170034]Identify the Volume and Parts of the NCC that relate to fire-resistance of building elements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 schedule 5
	Volume 1 schedule 5
	




[bookmark: _Ref536170036]Identify the Australian Standard that relates to fire-resistance tests for elements of construction.

	Answer
	AS 1530.4
	




[bookmark: _Ref536169328]For all NCC Classes, where the ground or subfloor space is excessively damp or subject to frequent flooding, which durability class must the subfloor framing must be used where above ground?

	Answer
	Class 1 or 2 Timbers or H3 preservative treated timbers
	





[bookmark: _Ref536170040]Identify the Australian Standards that must be observed when meeting the requirements for Q20. 

	Answer
	AS 1684.2 
	




[bookmark: _Ref536170043]True or False (Tick your response): Where materials are not used as intended (or without considering NCC requirements), this can make a significant difference to the life or serviceability of the structure.

	Answer
	x
	True 
	
	

	
	
	False 
	
	




[bookmark: _Ref536170044]Explain why durability and serviceability impact on the cost effectiveness of chosen materials.

	Answer
	
By choosing building materials wisely, such as considering the complete life cycle of the materials, you can reduce the impact on the project and on the environment. Cheap does not mean cost effective when the question of durability is unsatisfied. The more durable a material is, the longer it lasts and less serviceability which is cost effective.
	




[bookmark: _Ref536172033]Provide an example of short term degradation of materials and describe its effects on a building on structure.

	Answer
	
Weather such as sun, heat, rain and wind can adversely affect the physical structure, look, strength and durability of a material.
	





[bookmark: _Ref536172034]Provide an example of long term degradation of materials and describe its effects on a building on structure.

	Answer
	When choosing an alternative material or building practice, it should only be considered if is performance tested, efficient, environmentally sustainable and cost effective then what hs been recommended in the specification as a natural or man made product or material.

	




[bookmark: _Ref425327163][bookmark: _Ref425327708]You have spoken to a supplier who has indicated that some of the client’s desired materials are unavailable. When considering alternative building materials what must be taken into consideration (i.e. other than the client’s requirements)?

	Answer
	It is important to consider the cost, environmental efficiency, project efficiency, availability of the material, origin of the material in relation to distance of the project/building.
	




[bookmark: _Ref536177031]Identify two (2) things that you should look for when receiving a delivery of materials.

	Answer
	Check the quantity and the quality of the material and reject if incorrect or reject with conditions.
	




[bookmark: _Ref536177032]If you encounter issues with delivery, what two (2) options do you have?

	Answer
	Reject the shipment.
Reject and give conditions.
	




[bookmark: _Ref409518704][bookmark: _Ref408838393]Which of the following should be assessed before shifting materials? Tick all that apply. 

	Answer
	Choice
	Possible Answers
	

	
	x
	What needs to be relocated (e.g. size, weight)
	

	
	x
	The relocation area, site layout and obstacles
	

	
	x
	Distance and time to relocate load
	

	
	x
	Whether a team is available and/or appropriate
	

	
	x
	Whether PPE must be worn (e.g. for hazardous materials)
	




[bookmark: _Ref536178585]What document should you refer to for guidance on how to handle and store hazardous chemicals? 

	Answer
	Safety data sheets
	




[bookmark: _Ref408838395][bookmark: _Ref409519364]Name three (3) ways you can reduce the risk of injury if a load is too heavy for one person to carry, push or pull. 

	Answer
	Lighten the load
Team lift
Mechanical lift
	





[bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




[bookmark: _Ref404158235]How should construction materials and components be handled? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	x
	Sorted to suit material type and size, separating hazardous material
	

	
	x
	Stacked or stockpiled for ease of identification and retrieval
	

	
	
	Stored in access ways for ease of retrieval
	

	
	x
	Stored clear of access ways
	

	
	x
	Handled and positioned ready for installation
	




[bookmark: _Ref536180244]Identify the Australian Standard that relates to the storage and handling of LP gas.

	Answer
	AS/NZS 1596
	



[bookmark: _Ref536194481]List one (1) testing method for each of the building materials listed below.

	Answer
	Material name
	Properties
	

	
	Concrete
	SLUMP TEST
	

	
	Metals
	STRESS TEST
	

	
	Timber
	STRESS GRADING MACHINE
	




[bookmark: _Ref536181364]What Code gives detailed tables which state the required grade of timber for specific sizes and uses?

	Answer
	AUSTRALIAN TIMBER FRAMING CODE
	




[bookmark: _Ref536181366]Name two (2) ways that defects may be seen in timber.

	Answer
	WARPING, CRACKS 
	




[bookmark: _Ref536181368]Identify two (2) tests that may be performed to determine the durability of stone.

	Answer
	ACID TEST WATER ABSORBTION
	



[bookmark: _Ref536181370]Name two (2) ways that defects may be seen in stone.

	Answer
	CRACKS AND FRACTURES
	




[bookmark: _Ref536187863]True or False (Tick your response): Under a contract, builders and other specialist tradespersons are the ones most likely to rectify or remedy problems that arise from incorrect installation, application or placement of materials.

	Answer
	X
	True 
	
	

	
	
	False 
	
	




[bookmark: _Ref536187427]Name two (2) established methods that may be used to preserve timber.

	Answer
	PAINTING AND TERMITE BARRIER

	




[bookmark: _Ref536187429]Identify two (2) established methods that may be used to protect ferrous metals.

	Answer
	CORROSION INHIBITORS, PAINTING, GALVANISATION
	





[bookmark: _Ref536187430]Explain why the corrosion resistance of non-ferrous metals is superior to that of ordinary steel.

	Answer
	This is a result of the production of a ceremic coating of oxide or salt on the metal which protects it from further corrosion.
	




[bookmark: _Ref536187432]When should aluminium be coated with bituminous paint? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
	
	At all times
	

	
	x
	When it is buried in soil
	

	
	x
	When it comes in contact with chemical materials
	

	
	x
	When it is immersed in water
	

	
	
	When it is used on bitumen
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o2l
COMPONENT Wwm2 | m2
indoor | indoor
floor area | floor area
Floor suspended slab 114 - 117 mm 208 68
Floor suspended timber on stumps 76 2
ROOF
Roof steel frame colorbond steel or tile 200 7
Roof imber frame colorbond steel or tile 143 a7
WALLS
‘Walls double brick; s/b interior 312 103
‘Walls brick vencer timber frame 204 67
‘Walls timber frame fibro clad 61 2
‘Walls steel frame fibro clad % 30
‘Walls Timber frame timber clad 68 3
‘Walls pre-cast concrete 264 88
‘Walls conerete block 160 53
OTHER , APPLICABLE TO ALL HOMES REGARDLESS
OF TYPE
Construction, admin, transport, other materials such as copper
pipes, glass, aluminium 406 144
Floor coverings assume approx. 50% ceramic tile 50%
polypropylene carpet 61 20
Fittings, fixed appliances built in § bathroom, kitchen, wirobes % I
Kg
ADDITIONS Wi/ m2 | COZe/
areaorm | m2area
length | orm
length
Roofed open areas - lfresco / porch / verandah / carport 352 n7
Garage single brick or cavity walls, conerete slab, steel or tile oof | 75 219
Open Carport 352 n7
Fence brick or metal (per metre length, assuming 1.5 m height) 186 61
Paving (brick or concrete) 9% 32
Pool (conerete below ground) 534 198
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