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CPCCBC4012 
Read and interpret plans and specifications 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4012 Read and interpret plans and specifications cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Harrison Buswell

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	11/08/2023
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	15/08/2023
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	18/08/2023
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4012
	23/08/2023
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Hand out 3 - Slab Plan for Activity 3
	 Practical Assessment
 Cost estimation sheet (HO5 template available)



	Assessor name
	Jared Francis

	Assessor signature
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THEORY EXAM


	Participant name
	Harrison Buswell




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref130817641]What is the significance of concept drawing/sketches?

	[bookmark: _Hlk85785851]Answer
	Concept drawings are simple however outline the main building principles allowing for ideas to be put on paper to give an idea of what will be built

	




[bookmark: _Ref130817651]Discuss when you may come across concept drawings/sketches.

	Answer
	Concept drawing and sketches will be seen in the very early planning stage in a construction building
	




[bookmark: _Ref130818166]Explain what is meant by architectural plans.

	Answer
	Architectual plans show details of the building from an architectural perspective, showing windows and door schedules, a site plan, elevations and sections 
	




[bookmark: _Ref130818168]Provide four (4) plans that are considered part of the architectural plans.

	Answer
1.

2.

3.

4.
	1. site plan
2. Window schedule
3. elevations
4. sections 
5. detail views

	



[bookmark: _Ref130818385]Describe what structural plans are.

	Answer
	Structural plans show structural aspects of a plan like materials, wall types and ceiling types. They give the builder knowledge on how the building will look structurally.
	




[bookmark: _Ref130818387]How is a structural plan different from an architectural plan?

	Answer
	A structural plan gives structural advice for a builder with what materials will be used for the job, whereas an architectural plan gives a floor plan with windows and door schedules. 
	




[bookmark: _Ref130819696]Explain what a civil plan is.

	Answer
	Civil plans are showing an overview of the entire construction site and how the different aspects will come together.
	




[bookmark: _Ref130819697]Discuss how civil plans may be similar to other plans.

	Answer
	Civil plans can be similar to other plans as they give a full overview of everything involved in the job and how it all comes together.
	




[bookmark: _Ref130820127]What is the purpose for mechanical plans?

	Answer
	Mechanical plans are useful as they give a layout of all mechanical objectgs in the building and can give insight as to where ducting and many other mechanical items will be placed.
	




[bookmark: _Ref130820129]Discuss three (3) details you may find in mechanical plans.

	Answer
1.



2.



3.
	1. Heating and cooling
2. Ventilation
3. Lifts or escalators
	




[bookmark: _Ref130822249]When would electrical plans be used?

	Answer
	Electrical plans will be used when finding out how many lights will be in a building or to see the wiring layout of a building.

	




[bookmark: _Ref130822251]Provide three (3) examples of details contained in electrical plans.

	Answer
1.

2.

3.
	1.Wiring layout
2. Lighting layout
3. Locations of switches
	



[bookmark: _Ref130822998]What are plumbing and drainage plans used for?

	Answer
	Plumbing and drainage plans give the a representation of where plumbing will be run throughout the building
	




[bookmark: _Ref130822999]Discuss what may be needed when plans display council pipework.

	Answer
	If plans display council pipework the council will need to give clearance on where you can or cannot work on, a utilities plan should give insight of where and if the council pipework will be involved in the construction phase
	




[bookmark: _Ref130881039]Why is it important to check and ensure that the plans you are using are the current version?

	Answer
	The current version of plans will show any variations made in the phases before, using an outdated plan can force you to make errors in the construction phase due to variations not being shown. This can then cost a construction company a lot of money due to variations not being seen.
	




[bookmark: _Ref130881993]What can occur if an outdated version of the plans is used?

	Answer
	If an outdated plan is used there are many things that can go wrong however one example would be in the estimation phase, variations may not be shown and when pricing the job you don’t price the variations therefore costing the company money to implement that. Or in the construction phase building something that was meant to be different due to variations on newer plans.
	




[bookmark: _Ref77849989][bookmark: _Ref130883061]Discuss what site plans are drawn to reflect.

	Answer
	Site plans are drawn to give an overview of the property and sow all elements required for construction.
	




[bookmark: _Ref130883068]Discuss the purpose of reading the floor plan.

	Answer
	A floor plan shows the internal arrangement and allows builders to see elements such as walls, doors and windows.
	



[bookmark: _Ref130883412]Discuss two (2) key differences between elevation view and section view.

	Answer
1.











2.
	1. Elevations show the vertical side view of he building whereas sections shows the interior of a building from a side vertical view
2. Elevations allow the reader to see the outside view of as building from all sides whereas sections allow the reader to see the inside objects through the building  
	




[bookmark: _Ref130884038]Discuss the purpose of reading detail drawings.

	Answer
	Detail drawings focus on specific points that are required to show more detail, they are shown in a very deep and small scale so the specifics of a point are highlighted
	




[bookmark: _Ref130884676]Why is it important to measure from a datum point?

	Answer
	A datum point is a point which allows accurate measurement. It is important to use so that the result of your measurement is accurate.
	




[bookmark: _Ref130885229]Discuss what reduced levels (RL) are and how these are established in construction drawings.

	Answer
	Reduced levels can be established by using the datum and finding vertical measurements which are then “Reduced Levels”

	




[bookmark: _Ref130886686]Describe the purpose of the title block and what it contains.

	Answer
	The Title block gives general information about the drawings aswell as specific information about the particular drawing sheet.
	




[bookmark: _Ref130886688]Where is the title block usually located on the plans?

	Answer
	The Title block is usually located on the bottom of a plan or to the right side of a plan
	




[bookmark: _Ref130887510]Describe the purpose of using scale drawings in construction.

	Answer
	Scale plans allow the person reading plans to see a full picture of the plan on smaller paper. The scale then gives them the ability to see the buildings true size.
	




[bookmark: _Ref130552834]Describe each ratio of standard scale ranges below.

	Answer
	Ratio
	Description
	

	
	1:100
	A 1:100 ratio is for every one unit you will multiply that by 100 to get the true scale, this ratio is usually found on full drawings
	

	
	1:2
	A 1:2 ratio shows that or every 1 unit you multiply it by 2, this can be used on a lot smaller drawers such as detail drawings.
	

	
	1:50
	A 1:50 ratio is used in some detail drawings aswell as some section drawings, this shows that for every 1 unit it is 50 units.
	



[bookmark: _Ref130888097]Describe why examining detail drawings is important.

	Answer
	Detail drawings enlarge bits of a site plan that may be hard to see through a full-size drawing. Detail drawings give the reader a chance to see materials and small details through the construction phase
	




[bookmark: _Ref130888441]What is the difference between utilities plans and specifications and services plans and specifications in the context of building construction?

	Answer
	A ultilities plan will show what is needed during the construction phase such as supply of electricity whereas a specification and services plan shows the systems necessary such as fire protection or security for the property 
	




[bookmark: _Ref130889173]Describe what is meant by each of the following drawing descriptions.

	Answer
	Drawing description
	Meaning
	

	
	Isometric drawings
	Isometric drawings are 3D drawing but viewed on a 2D surface, Isometric drawings show a scaled non distorted version of a drawing.
	

	
	Oblique drawings
	Oblique drawing are 3D drawing that are projected on a 2D scale and show the drawing from the viewers desired point. These are used to see certain features of an object.
	

	
	Perspective drawings
	Perspective drawings are 3D drawings that give someone a look at what the building will look like at completion. They give the viewer a realistic look at what the building will look like upon completion.
	

	
	Orthographic drawings
	Orthographic drawings are like floor plan or elevation drawings they are used for examining the building and finding building elements.
	



[bookmark: _Ref130889385]What are CAD drawings? Explain how CAD is used in building and construction?

	Answer
	CAD drawing are computer- aided design drawings and are made using computer software. CAD drawings come in 2D and 3D and allow for very precise drawings. They are mostly used by Engineers, architects and construction employees. 
	




[bookmark: _Ref130889897]Provide a brief description of the given classes of buildings according to the National Construction Code.

	Answer
	Building Class
	Description
	

	
	Class 1a building
	Class 1a buildings are usually residential houses that are just a single dwelling. 
	

	
	Class 2 building
	Class two buildings are apartments usually multi-unit residential buildings where people live.
	

	
	Class 4 building
	Class 4 building are usually a single dwelling in a commercial building and are in a class 5-9 building.
	

	
	Class 5 building
	Class 5 buildings are buildings used for professional use or commercial. One example could be a lawyer building
	

	
	Class 7b building
	Class 7b buildings are storage type buildings like warehouses or display of goods buildings.
	

	
	Class 10a building
	Class 10 buildings are non-liveable buildings, 10a Buildings are sheds, carports or private garages which are not habitable.
	




[bookmark: _Ref130975341]What is building information modelling (BIM)?

	Answer
	BIM is a computer generated technology similar to CAD however BIM allows conflicts to be seen and outlined so the viewer can make changes easily.
	




[bookmark: _Ref130890045]Explain how the NCC is relevant to construction drawings.

	Answer
	The NCC is relevant to construction drawings as it gives the viewer the rules in which the building will be governed by and allows them to find the rules and laws they need to follow when constructing the building.
	




[bookmark: _Ref130890248]Discuss the importance of complying with standards during a building and construction project.

	Answer
	Complying with standards during building and construction phase is extremely important. If standards are not met then the governing body can shut down construction or not allow the builder to continue with the project. Complying with standards also allows for the building to be built to a high standard.
	




[bookmark: _Ref130910187]Discuss how you would identify wind bracing and tie-down requirements from construction plans.

	Answer
	To identify Wind bracing and tie-down points the roof plans in the structural plans will set out the requirements for the wind bracing and also tie down points in the building. 
	




[bookmark: _Ref130969649]Discuss why you would access AS 1684.2 Residential timber-framed construction Non-cyclonic areas, when reading plans and specifications.

	Answer
	Accessing 1484.2 residential timber-framed construction non-cyclonic areas will outline the requirements needed for a residential dwelling in a non-cyclonic area. This will show how the house needs to be built and the requirements that need to be met. 
	




[bookmark: _Ref130970244]Reasonable allowances are made by builders for the different construction items in a building project. Discuss what Prime Cost (PC) items are.

	Answer
	Prime cost (PC) are reasonable allowance that a builder will make for different items in the construction process. PC items are items that cannot be specified at the time of the contract being entered
	




[bookmark: _Ref130970247]Explain what Provisional Sum (PS) items are.

	Answer
	Provisional Sums (PS) are items that refer to particular works or services cost of carrying out related works that are not yet defined into detail for builders. The builder will make a reasonable allowance for the work itself.
	




[bookmark: _Ref130971979]Explain how to locate installation points of the services to the building from the plans.

	Answer
	The floor plan will be used to locate installation of the services to the building. Looking closely at a floor plan will show the installation points. This will outline drainage points, water waste points etc. 
	




[bookmark: _Ref130971981]Explain how to locate connection points of services to the building from the plans.

	Answer
	To find connection points you will look at the site plan and read labels and the legend schedule. This will show connection points utility poles, sewer connection etc.
	




[bookmark: _Ref130972216]Explain how to locate fixtures from the plans.

	Answer
	To locate fixtures from a plan, you use the same process as finding installation points. The fixtures will be found in the construction plans using the labels ad legends.
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WORKBOOK


	Participant name
	Harrison Buswell




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific business context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

For the following activities, name the State/Territory you will base your research on. 

	State/ Territory
	Queensland




	ACTIVITY 1  [bookmark: _Ref35349341]

	Research and document your findings regarding legislation and codes that apply in your state/territory relevant to the following three (3) items. Summarise the requirements relevant to building drawings and sketches you identified and provide the URL where you sourced your responses.
a) Smoke alarms in a new building
b) Pool fences
c) Protection of waterways



a) Smoke alarms
	Name of Legislation (Commonwealth or State) 

	Part 5A Building and fire safety regulation, Australian standard AS 3786:2014


	Summary of relevant excerpt/requirement 

	Smoke alarms Must be of Australian standard, The smoke alarms in building must be interconnected and in each room of a building, they must be hardwired and have a 10 year non removeable battery. Where buildings do not have individual rooms on a storey the smoke alarms are required to be placed on most common path of travel. Smoke alarms are not to be placed in prescribed exclusion zones.

	Source (URL or web source)

	https://www.legislation.qld.gov.au/view/pdf/asmade/sl-2016-0221                    https://ablis.business.gov.au/service/ag/australian-standard-as-3786-2014-smoke-alarms/31032 



b) Pool fence installation
	Name of Legislation (Commonwealth or State) 

	Australian standard. 
Section 14 of Building Act 1975, Building regulation 2006, and Building code of Australia (Pool Barriers legislation)  AS1926.1:2007

	Summary of relevant excerpt/requirement 

	Pools Must have a Barrier that is continuous for the full extent of the hazard which must be of strength to withstand the foreseeable impact of people. The pool fence must restrict the access of young children and have an automatic latch

	Source (URL or web source)

	https://www.hpw.qld.gov.au/__data/assets/pdf_file/0015/4812/qdcmp3.4swimmingpoolbarriers.pdf 



c) Protection of waterways
	Name of Legislation (Commonwealth or State)

	Queensland legislation Environmental Protection (Water and Wetland Biodiversity) Policy 2019 

	Summary of relevant excerpt/requirement

	The protection of waterways is a Queensland legislation act that  The act will protect Queensland’s waterways while allowing for development that is ecologically sustainable.


	Source (URL or web source)

	https://environment.des.qld.gov.au/management/water/policy 



	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref35349352]

	Access Handout 1 (HO1- Floor Plan with dimensions) and respond to the following:
a) What is used for the internal wall lining?
b) What is used for the external cladding?
c) What roofing cladding is required?
d) How do you identify the smoke alarm installation points?



	a) What is used for the internal wall lining?

	Clay bricks to all internal walls

	b) What is used for the external cladding?

	Painted Render finish to external walls

	c) What roof cladding is required?

	Colourbond custom ORB Sheeting

	d) How do you identify the smoke alarm installation points?

	Smoke Alarms are denoted by an S in a circle on Ground Floor plan




	Satisfactory Outcome
	
	





	ACTIVITY 3  [bookmark: _Ref130909754]

	Access Handout 2 (HO2- Footing Plan) and Handout 3 (HO3- Slab Plan) and respond to the following:
a) Specify the size and type of reinforcing to be used for BP.1 in Handout 2 (HO2-footing plan)
b) How do you determine where each BP.1 footing pier should be placed?
c) Mark each of the load bearing points in Hand out 3 (HO3- Slab Plan)



	a) Specify the size and type of reinforcing to be used for BP.1

	Reinforcement 25MPa  Vetical 5.N12 Ligs R6 Helix – 200mm Pitch

	b) How do you determine where each BP.1 footing pier should be placed?

	BP.1 will be shown on sections drawings on where footing pier should be placed

	c) Mark each of the load bearing points in Hand out 3 (HO3- Slab Plan)

	All positions marked in Handout 3 as C1 are load Baring points 




	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref130974558]

	Access Handout 4 (HO4- Residential Floor Plan) and respond to the following:
a) Which drawings are shown in these plans?
b) Which Australian Standard must be referenced when installing termite protection?
c) Make a list of the finishes noted on the document.




	a) Which drawings are shown in these plans?

	Floor Plan and Elevation plans

	b) Which Australian Standard must be referenced when installing termite protection?

	 3660.1-1995 is the Australian standard required when installing Termite protection

	c) Make a list of the finishes noted on the document.

	Schedule of Finishes
Roof – Custom ORB Deep Ocean Colourbond
Gutter/Fascia – Deep Ocean Colourbond
Walls – Dulux Cargo River
Corbells – Dulux Calf Skin
Window Frame – Powder coat Anotech Grey
Paving – Lifestyle Paving Liquid Limestone




	Satisfactory Outcome
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PRACTICAL ASSESSMENT


	Participant name
	Harrison Buswell




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1
	14/08/2023
	 Workplace
 Simulation
	10 Auscan crescent Garbutt 4814
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	Participant satisfactory 



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 
	Specify type of plan and NCC class determined: 
Architectural Commercial unit Plans  Class 2 building

	1.1A. 1.1C. 
	Specify how currency of documents was confirmed:
Confirming the currency of plans was done with the construction manager who spoke to the architect. Then going through the title block to ensure it is the most current date. Confirmed that all variations have been added to the current plan.   

	1.1D. 
	Specify environmental controls determined from plans/specifications.
The site is located in Queensland and will be governed by the Queensland Environmental offsets act 

	1.2B. 1.2C. 
	Specify how building layout, material requirements spaces and dimensions were determined from plans and specifications.
The floor plan was used to determine the building layout through examination of particular all areas.
The Details and schedules were used to determine material requirements by looking at parts of the building and what materials were required.


	1.2G. 
	Specify services identified on site:
Drainage for bathrooms, water waste, Electrical cabling

	1.2H. 
	Specify site features located to be removed/ retained:
Replacing kerbs and gutters, New Crossover to council requirements, make good to footpath, fix any damaged road surfaces damaged during construction.
Excavation to flatten block of land ready for construction.
Existing tree to remain in front of house.

	1.2J. 
	Specify variations found:
Kitchen and living areas variation to wall types.
Kitchen length extended by 1.2 metres.


	1.3A. 
	Specify concrete footing and slab information identified:
Blockwork walls outlined. Driveway slab plan. Therapy pool pathway FFL.
Levels of all slab work. Details of thickness.

	1.3B. 
	Specify how load bearing points were recognised:
Roof plan was examined and load bearing points were found throughout with labels showing what type of load bearing was required

	1.3C. 
	Specify how wind bracing and tie down requirements were confirmed:
Wind bracing and tie down points were found in the elevation drawings 

	1.4B. 1.4C. 
	Specify how installation points and fixtures were determined:
Section drawings were used to find both installation points and fixtures

	1.4B. 
	Specify how connection points were determined:
Services plan was used to find the connection points in the building

	1.4C. 
	Specify where finishing details were located:
Finishes details were found in the architectural finishes schedule as well as in the details section





CPCCBC4012
Read and interpret plans and specifications

	Practical Task 1 

	Description of task:
The participant must demonstrate skills and knowledge to identify and interpret building and construction information from plans and specifications in a workplace (or a similar environment) in the context of a construction project including:
· Identify types of plans.
· Check and confirm that the current version of plans, specifications and amendments is being used.
· Use the appropriate plans and aspects of drawings for relevant purposes.
· Confirm that the details on plans comply with the specifications.
· Identify environmental controls from plans/specifications.
· Read and interpret the plans.
· Read and confirm standards of work and tolerances from job specifications.
· Determine building layout, spaces and dimensions from floor plan.
· Determine material sizes, thickness and construction methods from detail drawings for estimates. (Template available for use HO5_ Cost Estimation)
· Recognise and confirm job specifications located in drawings, notes, and descriptions.
· Determine internal linings, external cladding and roof materials needed for estimates from plans and specifications. .(Template available for use HO5_ Cost Estimation)
· Apply information from plans to estimation, planning and supervisory tasks.(Template available for use HO5_ Cost Estimation)
· Gain access to the site, achieve orientation and identify services, datum and reduced levels.
· Locate site features to be removed or retained.
· Determine the building location from the site plans to actual.
· Verify plans recognising variations between the plans and the actual site, reporting findings as required.
· Appropriately communicate with others to be understood.
· Adhere to site safety requirements, including requirements relating to hazard identification.
· Identify structural details.
· Identify concrete footing and slab sizes and position and type of reinforcing required.
· Identify structural load bearing points of the building and compare information from specification.
· Identify wind bracing and tie-down requirements checking for accuracy against the wind bracing table.
· Identify non-structural details.
· Identify provisional sum (PS) and prime cost (PC) items when estimating costs.(Template available for use HO5_ Cost Estimation)
· Locate installation and connection points of services to the building.
· Identify location of fixtures from plans and details of finishes from specifications.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Work site; plans and specifications, quality documentation; access to the internet/access legislation, current building and construction codes and standards and the NCC. PC applications and software to access CAD. Templates for estimating.

	Observer details

	Name of observer:
	Jared Francis

	Role of observer 
(Confirm suitability to sign)
	Director of Iconic Construction Industries

	Email address of observer
	Jared.Francis@iconiccon.net

	Signature of observer:
	
	Date:
	16/08/2023



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	1 Identify types of plans

	[bookmark: _Ref130979481]Check and confirm that the current version of plans, specifications and amendments is being used.
	
	[bookmark: _Ref130979484]Use the appropriate plans and aspects of drawings for relevant purposes.
	
	[bookmark: _Ref130979803]Confirm that the details on plans comply with the specifications.
	
	[bookmark: _Ref130979521]Identify environmental controls from plans/specifications.
	
	2 Read and interpret the plan

	[bookmark: _Ref130984040]Read and confirm standards of work and tolerances from job specifications.
	
	[bookmark: _Ref130980146]Determine building layout, spaces and dimensions from floor plan.
	
	[bookmark: _Ref130980150][bookmark: _Ref130984245]Determine material sizes, thickness and construction methods from detail drawings.(Template available for use HO5_ Cost Estimation)
	
	[bookmark: _Ref130980260]Recognise and confirm job specifications located in drawings, notes, and descriptions.
	
	[bookmark: _Ref130984259]Determine internal linings, external cladding and roof materials from plans and specifications. (Template available for use HO5_ Cost Estimation)
	
	[bookmark: _Ref130984400]Apply information from plans to estimation, planning and supervisory tasks.(Template available for use HO5_ Cost Estimation)
	
	[bookmark: _Ref130982305]Gain access to the site, achieve orientation and identify services, datum and reduced levels.
	
	[bookmark: _Ref130982340]Locate site features to be removed or retained.
	
	[bookmark: _Ref130982465]Determine the building location from the site plans to actual.
	
	[bookmark: _Ref130982550]Verify plans recognising variations between the plans and the actual site, reporting findings as required.
	
	[bookmark: _Ref130984197]Appropriately communicate with others to be understood.
	
	[bookmark: _Ref130984226]Adhere to site safety requirements, including requirements relating to hazard identification.
	
	3 Identify structural details

	[bookmark: _Ref130983367]Identify concrete footing and slab sizes and position and type of reinforcing required.
	
	[bookmark: _Ref130983503]Identify structural load bearing points of the building and compare information from specification.
	
	[bookmark: _Ref130983514]Identify wind bracing and tie-down requirements checking for accuracy against the wind bracing table.
	
	4 Identify non-structural details

	[bookmark: _Ref130984299]Identify provisional sum (PS) and prime cost (PC) items when estimating costs.
	
	[bookmark: _Ref130983670]Locate installation and connection points of services to the building.
	
	[bookmark: _Ref130983805]Identify location of fixtures from plans and details of finishes from specifications.
	




	Observer comments:

	Competent, very well done.
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