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CPCCBC4004A 
Identify and produce estimated costs for building and construction projects


	[bookmark: _Ref396827952]THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Toni Thomsen 

	

	

	Participant signature
	



	Assessor name
	

	

	

	Assessor signature
	



	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Satisfactory?

	24
	
	Yes
	No

	
	
		



	[bookmark: _Ref424108804]ASSESSOR COMMENTS

	


What is the critical aspect of identifying and interpreting plans, drawings and specifications for a building project?

	Answer
	It shows all parties involved in a building project the proposed structure and what it will look like when completed 
	



[bookmark: _Ref424109148]What is the purpose for date stamping of plans, drawings and specifications?

	Answer
	If any changes are made to the plans after they have been stamped then quotes etc will need to be amended. 
	



[bookmark: _Ref424109264]Nominate at least six (6) people and/or entities that would use plans drawings and specifications on a building project.

	Answer
	Engineers
Carpenters
Painters
Concreters
Landscapers
Electrical/gas and cable supply companies

	


[bookmark: _Ref424109443]Plans and drawings usually hold many and varied features. 

Name some of the types of drawings and details you would expect to see on plans and drawings for a building project.

	Answer
	Floor plans: horizontal sections through the building viewed from above.
Elevations: An elevation is a view you see when standing in front of that wall
Location Plan: will show lot numbers, deposit plan numbers and a north point. 

	



[bookmark: _Ref424109842]It is necessary to acquire all building plans and specifications at the beginning of the negotiation period so we know all building project details prior to commencing work (including dimensions, construction materials, door and window schedules, masonry control joint locations and smoke alarm locations). 

What else would be expected to be provided?

	Answer
	Architectural plans and elevations 
Building Specs 
Framing Plans 
Roof truss computations 
Energy efficiency report 
Footing Construction report and foundation soil assessment
	


[bookmark: _Ref424110143]Drawings are usually arranged in the approximate order of construction. What might a set of drawings consist of?

	Answer
	Civil
Structural 
Architectural 
Electrical 
Mechanical 
Plumbing
	



[bookmark: _Ref424118636]Explain how to access the Building Code of Australia (BCA) and its relevance to estimating costs for building and construction projects.

	Answer
	BCA can be accessed online and it is relevant in estimating costs as there are certain guidelines that need to be followed that may need further allowance for. 

	



[bookmark: _Ref424118637]Explain how to access the Plumbing Code of Australia (BCA) and its relevance to estimating costs for building and construction projects.

	Answer
	PCA can be accessed online and it is relevant in estimating costs as there are certain guidelines that need to be followed that may need further allowance for. 

	


[bookmark: _Ref424118642]Explain how to access Australian Standards and their relevance to estimating costs for building and construction projects.

	Answer
	Australian Standards can be found via the Master Builders website and they are used to help maintain the safety, efficiency and cost effectiveness of building in Australia. 
	



[bookmark: _Ref424119846]Identify two (2) standards that would be relevant to the industry sector. 

	Answer
	[bookmark: _GoBack]Plumbing and smoke alarm standards are relevant to the building industry.  
	



[bookmark: _Ref424118643]Explain the impact of WorkCover requirements on costs to the project. 

	Answer
	Workcover needs to be included in project costs and can be included in the “labour” section of the project. 
	




[bookmark: _Ref424118645]Explain the impact of Environmental Protection Agency requirements on costs to the project. 

	Answer
	Environmental costs to the project can be incurred such as seeking approvals and waste management fees. More information can be found at ehp.qld.gov.au for estimators. 
	



[bookmark: _Ref424110395]Calculate and cost the lineal timber order for 93 x 19 DAR Meranti and allow 5% wastage. The cost per lineal metre is $6.40. 

The requirements are: 22 @ 2400; 30 @ 3600; 10 @ 4800; 12 @ 1880 
Show your calculations.

	Answer
	22*2.4 = 52.8
30*3.6=108
10*4.8=48
12*1.88=22.56
Total area = 231.36 + 5% waste
=242.92
242.92 * $6.40 = $1554.68
	


[bookmark: _Ref424110619]A building floor plan measures 24000 x 14000 and the specification states the sheet flooring is 3.6 x 0.9 x 19mm Yellow TERMIFLOR T&G H2 at $58.38 per sheet. 

Calculate the area of floor sheeting required when an allowance of 2% is made for waste and cutting. Determine the number of sheets to order to the nearest whole sheet and calculate the cost for the flooring. 

Show your calculations.

	Answer
	Area of floor sheeting required is 336m2
The number of sheets required is 107 
Total cost is $6,246.66

	



[bookmark: _Ref424110902]If a solid cavity brick wall is to be built 23000mm long and 2400mm high (no windows and no doors), how many bricks would be required if the number of bricks per square metre is 50? Show your calculations.

	Answer
	23m x 2.4 = 55.2m2
55.2m2 * 50 = 2760 Bricks 
	




[bookmark: _Ref424113087]You are a QBCC licensed plasterer and a client (Owner Builder) Davey Jones-Locker of 100 Reef Avenue, Brisbane, Queensland wants you to quote for plastering an internal wall of his house build and has described to you the following information over the phone:

The Client tells you the Council approved plans and drawings state the finished ceiling height from the top of slab floor is 2400mm. There is one external solid timber door (D4) is 2340 x 870 x 35 in this wall and no other openings. The length of this house end wall is 11 metres. 

The house is of brick veneer construction and includes a 50mm cavity and the load bearing external framing is 70 x 45 MGP12 (a Boral product “Pineguard Blue”). The bricks are standard bricks 230 x 76 x 100mm. (L x H x W). 

The Client tells you that the door is positioned 2100mm from an internal corner (RHS in aerial view) and as seen from inside the house looking out. The specification and drawings state 10mm regular internal plasterboard. You know from experience regular plasterboard is supplied in the following sizes lengths 6M, 4.8M, 4.2M, 3.6M, 3M, 2.7M and 2.4M with recessed edge and widths of 1200mm and 1350mm. 

The Client wants a quote to fix and finish this internal wall with plasterboard. 


Your labour and on-costs are charged at $51.50 an hour per tradesman plus materials including sheets, fixing, finishing and sanding. You estimate ancillaries including stud glue, screws, base coat, top and finish coats at $315.00 and that there is two (2) days’ work. 

Your business works a 38 hour week you allow workers a 15 minute morning tea break and half hour for lunch. You will need two (2) tradesmen first day and one (1) tradesman second day including materials and equipment supply, fixing, finishing and sanding. 

You are to research or acquire plasterboard sheet prices and attach this price list to your email. You are not required to supply or fix cornice.

Sketch the wall in Plan View (not to scale), dimension it with relevant measurements, and position the door on the right side of your plan view sketch and then calculate the plasterboard required and approximate waste expressed as a percentage (%) for internally lining this wall.

Estimate the cost of the job, including supplying plasterboard materials fixing setting, finishing and sanding plus labour. Then write a covering email to be sent to the client. You must show your methods for calculating cost of sheets, waste, plus fixing, setting, finishing and sanding. 

Attach your quote, sketch, calculations and pricing list and email this to your Trainer/Assessor (details provided by them).

DRAFT AREA





DRAFT AREA




	Answer
	
	


[bookmark: _Ref424113617]There are many different ways of estimating project costs. You can use your past experience, or ‘square metre’ rates but if you are unfamiliar with estimating and pricing then you should resort to the materials and labour method of costing using an item-by-item approach which is considered as the best industry approach to estimating. 

What are at least three of the nominated methods for estimating?

	Answer
	Costing by area
Costing by material and labour 
Costing by a costing guide or estimating manual 
	



[bookmark: _Ref424114325]Name some of the circumstances to consider in relation to labour adjustment factors when estimating a project for construction.

	Answer
	Add 10% to 15% when working temperatures are below 40 degrees 
Add 5% to 50% for tradesmen with below average skills 
Add 30% to 50% on small jobs where fitting and matching of materials is required, adjacent surfaces have to be protected and the job site is occupied during construction. 
	


[bookmark: _Ref424114569]If a bricklayer lays 600 bricks in an eight (8) hour day, what is the average number of bricks laid per hour by the bricklayer? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
	☐	65
	

	
	☐	70
	

	
	☐	55
	

	
	☐	90
	

	
	☒	75
	

	
	☐	105
	

	
	☐	85
	




[bookmark: _Ref424114881]What and where are some of the potential sources you could go to in choosing your suppliers for goods and services?

	Answer
	Online is one of the best ways to locate suppliers such as manufacturers and wholesalers  
	



[bookmark: _Ref424114882]What are some of the primary (key) factors for choosing your suppliers?

	Answer
	Price and reliability are some of the main factors to consider when choosing your supplier
	


[bookmark: _Ref424114994]What are some of the ways you could communicate with your suppliers for gaining quotes?

	Answer
	There are a number of ways to communicate with suppliers, some of them are: 
Written request 
Email request
Fax
Telephone or verbal.  
	



[bookmark: _Ref424115147]Explain the concept of a ‘Labour Only’ quote?

	Answer
	Labour only relates to just the labour on the project, the sub-contractor can charge out an hourly rate without a specific timeframe to finish the job. 
	


You will be provided an allocated period by your instructor to complete this task. 
You may use appropriate costing software programs in completing this task.

[bookmark: _Ref424115434]Referring to the supplied set of house plans, you must do the following scheduling and costing: 

a. Identify and nominate a supplier/s and schedule the materials and cost the internal and external timber wall framing.
b. Identify and nominate a supplier/s and schedule the materials and cost the foundations and lower floor concrete slab including the schedule and costing for reinforcement.
c. Identify and nominate a supplier/s and schedule the materials and cost for the sub floor framing and the flooring for the upper floor plan. 
d. Calculate the architrave and skirting required for the fit out of the upper floor only in lineal metres.
e. Calculate the wet area tiles for the upper floor only which are client chosen for both floors and walls with the wall tiles 250 x 100 and floor tiles 300 x 300.
f. Estimate the labour only cost to tile all the wet areas only in the home. The tiler charges labour only $44.00 per square metre.
g. Determine the roofing material and number of square metres of it that are required.
h. Complete the aluminium windows and doors schedule and other external doors schedule for the lower floor only.
i. Complete a full internal doors schedule for the lower floor only. 
N.B. Assume all doors are flush panel 2040mm in height and 35mm thick.
j. Estimate the labour only cost for hanging all doors on the lower floor – if a tradesman takes 2 hours to jamb an opening, hang the door, fit the door furniture, door stops, architrave and fit a door-open-restraint. The hourly rate is $27.80 plus 20% on costs.

	Answer
	
	



	Answer
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