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Daily Pre-Start Form
	Project: 
	Rockpool Pelican Waters

	Approximate Duration:
	10 Minutes

	Date:
	04/05/2023
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Please ensure that all personnel sign in via Hammertech before commencing work on site
[image: image3.png]


[image: image4.png]&R




	[image: image5.png]&0




[image: image6.png]



[image: image7.jpg]Amcnab

nship builder












	Subcontractors Daily Activities (Review Site Board for Locations)
1. DYFA – Level 4 stack work – Level 4 Rough in – Level 1 Fit Off
2. AR Coastal –Level 5.5 Roof Adjustments for suffet cladding.
3. Monteur – Level 5 High Level Services, level 4 Rough in – 
4. Aspire crane – Tower Crane lifts for Apex and Fit Out Glass. – Hoist Operations
5. TK formwork –Concrete Ptching – As per Silica COP
6. Apex ground floor Sheeting. Level 3, set and sand. Level 3 walls and ceiling Sheeting., Level 5 set out,       top and bottom track Zone A
7. Fire boar : Level 5 High Level Wet Fire Install & Level 3 Dry Fire Rough in, Level 4 high level – 
8. Applied Air : Level 5 – Fit out units and pipe install – Level 2 Fit off.
9. Fit Out Glass – Level 5 Frames and glass install –– 
10. Universal Coatings – Render to Level 5 Balconies – Sheer Walls to Stair Core 2. – Painting Level 5          External          
11. Undercover Roofing – Roof Section – Zone A, B & C - Flashings
12. 6 Star Tling – Level 2 Zone A – Tiling Ensuite’s 

13. Scozia – Joinery Install – Level 2 Zone A

14. Fazen Scaffolding – Install Roof Edge Protection

	Permits, Trades Expiry Date
All Permit Expired.
Hot works - DYFA  EXP 08/05/2023
Hot works - Applied Air EXP – 08/05/2023
Work at Heights

UnderCover Roofing EXP 29/04/2023 (Reviewed Daily)

	

	Site Notices, Risks & Restricted Work Areas

	· Roof Edge Protection Installed Today.

· Scaffold Dismantle Commencing Monday – Be prepared for exclusion zones to be in place with temporary closures     around the façade.

· Lead Management – Leads to be on stands until McNab install hooks after sealer coat.

· McNab Respirable Dust Management Hazard Control Sheet – McNab systems to align with Code of Practise.

· Incident – Injury – Circular blade contact with finger – 3 stitches – Review cutting benchesto ensure they are suitable, ensure matreials are secured when cutting. McNab auditing cutting benches today.

· Internal Stair 1, 2 & 3 full operational for emergency procedures and access egress.

· No materials or tools to be stored in corridors must be clear at all times.

· No materials to be stored infront of electrical boards. 1.2m clearance required

· Strictly no access to roof section – Undercover roofing only unless authorised.

· Final Warning – PPE needs to be better – Re – Inductions to follow for failing to meet site requirements. Glasses, gloves

· Strictly no altering of scaffolding components – notify McNab of alterations required to schedule with AR Coastal Scaffolding
· Exclusion zones for work at heights – ensure drop zone is in place prior to works commencing.

· Task Specific gloves to be worn as per SWMS. Need support see Mcnab.

· Initial review of work area this morning – set up for another successful week – electrical equipment review.

· Apex setting to level 3 with the use of stilts, keep out of their exclusion zones.

· Report any Incidents, injuries, near misses or property damage immediately to Mcnab to allow incident investigations and preventing the same incident from repeating with potential injury.

· Strictly authorised personel to enter loading zone. Forklift Operating and Crane overhead, approval required before    entering from Ric or Jack please respect these high risk activities.

· Strictly no EWP Operations Within 1M of slab edges, ensure timbers are installed and spotters in place. EWP to be positioned horizontally across the live edge.

· High Visibility Clothing Required – Jumpers must be high visibility or high visibility vests worn.
· Roof access for authorised personel – See McNab to complete required permits and review SWMS
· Ensure you sign in, If you don’t sign in you are putting yourself, supervisor, employer and McNab at risk. IPad is outside office at 6:00AM !

· Waterproofing exclusion zones ongoing – keep out if you see signage and tape. Zone 1A & 1C
· Task Lighting required for all works within bedrooms and ensuites – 160 Lux minimum.

· Concrete drilling requires mechanical extraction and fit test mask to be worn.
· Hoist restriction – No access to level 5 – Access to level 4 up external stair 1,2 and 3 or internal stair 3 

· Temporary Lighting Live – Ground, Level 1, 2, 3 and 4 – Strictly no altering or touching lights / distribution boards. Notify McNab for alterations or damage to be rectified by Monteur.

· Dust generating activities require controls in place. Extraction, Containment, signage and RPE

· Fire system live – Ground, one, two and three
· Striclty no removing penetration without McNab authorisation

· Strictly no materials stored on scaffold.

· All work platforms must be industrially rated 150kg SWL – 450mm minimum width.

· Hygiene reminder – clean hands before using the ice machine

· Site toilets operational Level 4 & Level 2 by lift shaft / hoist.

· Green Line walkways clear at all times – no tools, ladders, EWP’s or materials stored in walkways.

· Loading docs to be cleared ASAP for next trade with rubbish in bins.

· Aluminium finished product for window frames – Strictly no standing.

· Ensure you sign in, If you don’t sign in you are putting yourself, supervisor, employer and McNab at risk. IPad is outside office at 6:00AM !

· Strictly no tools stored in lunch rooms, reaching 75+ workers onsite need to keep clean and hygienic.
· PPE –Glasses and Gloves to be maintained as per SWMS and McNab requirements.

· Strictly no altering or shifting backpropping without TK Formbuild approval.

· Scaffold is not to be used as a storage zone, keep clean.. 
· Housekeeping to be completed progressively – Managing Silica dust with controls referenced in SWMS

· Aspire Tower Crane Radios to remain on charge in lunch room, strictly no other personel to use these power points for phone charges etc, Strictly no charging or storage of tools in the lunch rooms.
· EWP & Mobile Plant Operations – ensure licensed operator at all times completing daily checks and log books.
· COVID-19 – Any flu like symptoms stay home, maintain 1.5m physical.

· Ensure all Hazardous Chemicals used onsite have SDS available and on Hazardous chemical register.

· Keep lunchroom amenities clean and tidy, respect the site facilities.

· Ensure all electrical equipment is tested and tagged up to date.

· Report all injuries, accidents, near missies to McNab site management.

NO CONSTRUCTION NOISE PRIOR TO 7:00AM
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