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Lana Place – Upper Podium Tile Works

All residents will not be allowed to access the works area, including residents that

Scope of Works

Demolition
· Skip to be provided by the demolition contractor. Location of skip to be provided by Core4. As this location will be in a traffic path of the carpark, appropriate site protection should be present around the skip while maintaining a single car lane access to the carparks.  
· Temporary remove the existing balustrades to stairs allow demolition works (balustrade to be stored onsite, location to be confirmed by Core4). Ensure balustrade are stored so that no damage will occur during the works period.  
· Demolish and remove:
· Totally remove the existing timber awning/patio structure
· [bookmark: _Hlk83888922]Totally remove floor tiles to podium deck area (ensure care not to damage any existing downpipes or posts)
· Totally remove skirting tiles 
· Totally remove screed level and grind any residue to concrete slab (ensure care not to damage any existing downpipes or posts)
· Cut out drains to allow installation of puddle flange and waterproof membrane (co-ordinate with service and waterproofing contractor on works required for the installations)
· Secure all doors to patio during works and safety protection to stair while balustrade is down.
· Ensure SWMS in place and being followed
· Adequate signage and exclusion zones

Waterproofing
· Repairs to concrete cracks using a suitable polyurethane product such as a Fosroc PU400 or similar.
· Install anchor bolts to the concrete to allow the reinstation of the existing balustrade prior to applying the membrane and seal with a suitable epoxy. These bolts are to be a suitable size to allow the balustrade reinstation after the waterproofing, screed and flooring products are applied. 
· [bookmark: _Hlk83886397]Rust treatment to all bolts that remain from the removal of the timber awning structure, rust treat each bolt before sealing with a 2-part epoxy resin 
· Rust treatment to the bases of the steel posts and any associated bolts and brackets (contractor to select product and approved by Core4)
· Cut out drains to allow installation of puddle flange
· Install waterproof membrane to total works area, including 100mm upturns to all walls, posts and balustrading bolts
· Ensure waterproofing is installed in drains, post-puddle flange installation (Co-ordination with service contractor). Provide options for the following for final selection by Core4
· Sandwich membrane with the top level being a trafficable membrane
· Sandwich membrane with applying a stencilled spray resurfacing to the top 
· Membrane to the concrete slab only (no layer of membrane to the top of the screed)
· [bookmark: _Hlk83966273]Secure all doors to patio during works and safety protection to stair while balustrade is down.
· Ensure SWMS in place and being followed
· Adequate signage and exclusion zones



Plumbing
· Allow to temporary relocate any drain lines or air conditioning lines that are on the ground
· Install puddle flanges to all drains where required. Co-ordinate with demolition contractor.
· Allow for any drain lines to accommodate the outdoor A/C units being lifted on the ground and wall mounted (approximately 300mm from ground) co-ordinate with the electrician. 

Electrical
· Allow to relocate all required A/C outdoor units off the ground to allow tiles works to occur
· Some units will be fixed to the wall as a permanent location and some units will need to be temporally disconnected and reconnected once the ground works are completed (Core4 to confirm which units upon receiving clarification from the client)
Flooring 
· Apply resurfacing product to the total works area:
· Stencilled spray resurfacing (contractor to select product and Core4 to approve colour and stencil pattern) – Please note, client may choose to go with solid colour and not have a stencil pattern. Provide specs and application process for both options as per below: 
· Applying the resurfacing to the screed (Contractor to advise on screed requirements for the resurfacing product to be applied
· Applying the resurfacing product to a sandwich membrane 
· Reinstate existing balustrade to the works area post flooring works being completed
· [bookmark: _Hlk84486996]Secure all doors to patio during works and safety protection to stair while balustrade is down.
· Ensure SWMS in place and being followed
· Adequate signage and exclusion zones

Screeding
· Pour screed to total works area, ensuring falls are achieved to all drains. 
· Two membrane/flooring finishes are being investigated for best applications. Provide screed consistency options for both options as per below:
· Screeding to suitable accept stencilled spray resurfacing application
· Screeding suitable to have a trafficable membrane applied
· Secure all doors to patio during works and safety protection to stair while balustrade is down.
· Ensure SWMS in place and being followed
· Adequate signage and exclusion zones

Control Joints
· Cut control joints to all walls required to surrounding podium, approximately control joints 6 in total to be installed. 
· Repairs to existing control joints, where required. 


Carpark Concrete Soffit Repairs
· Spalling repairs to underside of carpark once new puddle flange is installed. Co-ordinate with the service contractor. 
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