WHS FORM 04: SITE SPECIFIC RISK ASSESSMENT


	[bookmark: _GoBack]If you have identified any of the listed or other potential hazards on the site, you will need to enter a suitable control below to show how you have controlled the hazard(s). If any further hazards are introduced, record them and update the table at the bottom on this page. If you identify any high-risk construction work, you require a Safe Work Method Statement. See form 05 (Safe Work Method Statement).

	
#
	
Items to consider when conducting a risk assessment

	1
	Can parking arrangements at the site cause incidents and injuries to any persons?
· Cars parked in a safe and easy to access location with no hazards preventing the vehicle leaving the site in case of an emergency.

	2
	Are there any slips, trips and falls impacting on the safe access and egress?
· There was multiple trip hazards that where not flagged such as; 90mm storm water outlet, earth cable (not live), scraps of building products, sharp objects tossed on ground and holes.



	3
	Are there any other trades or activities that may impact on my work safety?
· There were no trades there that could’ve have impacted me at that time as they were cleaning.

	4
	Have I communicated with other trades/workers in this area?
· Before entering the site, I had a brief conversation with the builder, and whilst at the location I talked to the workers about their jobs.

	5
	Are there any amenities for the site? Can the use of amenities affect workers’ health due to poor maintenance?
· On site they have access to portable water and a clean portable toilet. With cleaning products available and cleaned regularly.

	6
	Is there a risk of injury due to fall zones and penetrations not being protected? (e.g. stair voids, roof areas, balconies)
· There were some small holes and covered as above mentioned.


	7
	Can something fall on me or can I cause something to fall onto someone else?
No ask all workers where on the ground and walking paths where clear.

	8
	Is there a risk of workers or pedestrians being hit by moving plant and/or motor vehicles?
· There were no moving vehicles on the site besides the workers cars and they were at the gate so the chance is almost nil.

	9
	Is there a risk of injury due to impaling hazards not being appropriately protected in the work area? (e.g. star pickets, reo bars, stacked pallet stack)
There was small off cuts and broken objects of this matter around the site which were tossed in the skip upon inspection

	10
	Is there a risk of injury due to open trenches or excavations?
No trenches or excavations only small holes from water erosion.

	11
	Is there a risk of workers meeting the overhead or underground services?
nil

	12
	Am I using correct manual handling techniques?
Worker where using the appropriate techniques to lift and not overloading themselves.



