Draft Processes and Procedures for the Control of Each Chemical
Paint (Solvent-Based): Implement measures like ventilation, PPE (e.g., respirators, gloves), proper storage, and safe disposal procedures.
Process:
1. Storage and Handling: Store in a well-ventilated area away from heat sources.
2. Risk Assessment: Conduct an assessment before starting work to evaluate the exposure risks (e.g., during spray painting).
3. PPE: Ensure workers use appropriate PPE (e.g., respirators, gloves, goggles).
4. Training and Supervision: Provide workers with training on safe handling and emergency procedures.
Acid Cleaner: Control measures may include using spill containment kits, providing PPE, and storing the acid in corrosion-resistant containers.
Process:
1. Storage: Store in tightly sealed, corrosion-resistant containers.
2. Spill Response: Provide workers with spill kits and training on neutralizing acids.
3. PPE: Require workers to wear protective gloves, goggles, and aprons.
4. Disposal: Dispose of used acid according to environmental guidelines and regulations.

Communicate with the PCBU and Seek Feedback
Subject: Hazardous Chemicals Control Procedures Feedback
Dear Kent, 
I have reviewed the chemical register and identified two hazardous chemicals in the workplace: Solvent-Based Paint and Hydrochloric Acid Cleaner. I have drafted control processes and procedures for both chemicals to ensure worker safety and compliance with WHS regulations. I would appreciate your feedback and approval on these processes.
Attached are the procedures for both chemicals for your review.
Best regards,
Elise Painter
HSSE
