	Organisation Name
	Matt Greenwood Constructions 
	ABN
	92163040186

	Organisation Address
	Lot 202 Gillies Range Rd, Gordonvale 4865



	Project
	Sarah Close, Gordonvale 4865



	Task / Operation / High Risk Activity
	Install Roof Trusses	Number
	

	Applicable Legislation, Standards or References
	QLD WH&S Act, QLD WH&S Regulation, QLD Mobile Crane COP, QLD Electrical Safety Act, QLD Electrical Safety Regulation, QLD How to Manage WH&S Risks COP, AS 4440 Installation of Nailplated Timber Trusses, AS 1576 Scaffolding, AS 2550 Cranes, Hoists and Winches

	High Risk Construction Work
	· Falls of more than 2 metres
· Powered mobile plant

	Required Licences, Certificates, Competencies, Permits or OHS Authorities
	DG ( Dogger ),  CN ( Non Slew Crane) or C2 ( 20t Slew Crane )

	Personal Protective Equipment
(Tick PPE required)
Ensure that all workers are trained in the use and maintenance of all PPE required for task by site supervisor
		 Safety Footwear
	 Safety Helmet
	 Respirator*
	* Provide specific details of PPE required
Harness and Lanyard as required.

	
	 Hearing Protection
	 High Vis
	  Other*
	

	
	 Eye Protection*
	 Gloves
	
	

	Plant, Equipment or Tools
	Crane
	Maintenance Checks
	Responsibility of subcontractor

	Special/Hazardous Materials
	(Ensure MSDS for hazardous Materials are available to workers)  Mobile Scaffold, Bond Beam Trestles.

	Emergency Procedures/Resources
(Specific to this JSA-SWMS)
Ensure that all workers are trained in these emergency procedures by site supervisor
	General Emergency procedures are available in the Site Health and Safety Plan.
First Aid procedures are as per site specific induction and Health and Safety Plan.


	Environmental Impacts and Controls
	Impacts
	Controls  ( If there is a potential impact define controls)

	
	 Hydro Carbons (oil and fuel spills)
	 Spill Kits
	 Designated Refueling and Servicing Areas
	 Other (specify)

	
	 Sediment Run Off
	 Silt Fences (Erection and Monitor)
	 Drainage
	 Containment Ponds

	
	 Dust
	 Watering
	 Site Speed Limits
	 Dust Containment Fences
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Job Sequence
	Risk levels: VH – Very High, H – High, M – Medium, L- Low

	Sequence of job steps 
(What to do in the right order) 
	Potential hazards
to people or the environment  
for each step
(eg. Manual Handling)
	Risk Level
(each hazard)
	Control Measures
(How to do it) 

Elimination  Substitution  Engineering  Administration  PPE
	Risk Level after Control 
	Person Responsible

	1. 
	Truss delivery truck access and truss unloading.
	Blocking Traffic and Pedestrian Flow outside site.
	M
	Traffic controllers and signage are positioned in accordance with the MUTCD Part 3.
	L
	Site Supervisor

	2. 
	
	Persons being stuck by falling objects.
	M
	The unloading area is to be barricaded to deny access of other workers and pedestrians.
Hard Hats are to be worn by all workers involved in the unloading process.
High Vis clothing is worn by all workers.
	L
	Site Supervisor

	3. 
	Truss storage
	Stored trusses blocking pedestrian flow and site access / egress.
	M
	Trusses stored in suitable area, if trusses block footpaths suitable barricading and signage to be erected.
	L
	Site Supervisor

	4. 
	Crane set up
	Blocking Traffic and Pedestrian Flow outside site.
	H
	Traffic controllers and signage are positioned in accordance with the MUTCD Part 3.
	L
	Site Supervisor

	5. 
	
	Soft ground/underground services.
	H
	Assessment of the ground condition and location of underground services to be undertaken prior to crane set up. Suitable outrigger packing to be positioned on set up.
	L
	Site Supervisor/ Crane operator

	6. 
	
	Proximity to Power Lines.
	VH
	The location of power lines to be identified prior to operation.
Authorised spotters or visual markers to be used after consultation with Power entity if the operation is closer than specified in the Code of Practice (SWNELP) 3m LV, 6m HV, 8m HV.
Dry natural fibre rope tag lines are to be used when working near powerlines.
	M
	Site Supervisor/ Crane operator

	7. 
	Slinging of trusses
	Faulty or damaged lifting gear.
	M
	All lifting gear to be inspected by a competent person (dogger, rigger) prior to use. 
	L
	Dogger

	8. 
	
	Incorrect slinging method.
	M
	A licenced dogger or rigger must sling the truss. Slinging points must be in accordance with the manufactures’ recommendations.
	L
	Dogger

	9. 
	Lifting of trusses
	Falling trusses
	M
	The work area must be barricaded and signed off to deny access to all other workers.
Workers must not stand under load where possible
	L
	Site Supervisor

	10. 
	
	Controlling the truss
	M
	A tag line must be used to control the truss as it is lifted.
	L
	Dogger

	11. 
	
	Incorrect crane signals whilst directing the truss
	M
	A licenced dogger or rigger must direct the crane.
	L
	Dogger

	12. 
	Access work area
	Persons falling from heights
	H
	All workers to maintain three points of contact when climbing ladders.

	L
	Site Supervisor, Carpenter

	13. 
	Position truss
	Persons falling from heights
	H
	Workers to remain on bond beam scaffold when landing roof trusses. 
	M
	Site Supervisor, Carpenter

	14. 
	Conduct work at height
	Persons falling from heights
	H
	The following controls will be used either together or individually 
Where the trusses are erected at up to 900mm centres work can be performed off the bottom cord if;
· The trusses are braced
· Only competent, trained persons to perform work.
· No damage to bottom cord
· Person completing work take extra precaution
And/ OR
	M
	Site Supervisor, Carpenter

	15. 
	
	· 
	H
	A mobile scaffold is used as a catch platform below the work area or as a work platform where ever possible.
OR
	L
	Site Supervisor, Carpenter

	16. 
	
	· 
	H
	Scaffold planks are laid across the bottom cord to create a work platform
	L
	Site Supervisor, Carpenter

	17. 
	Fix Truss
	Use of Electric drill
	M
	Only trained and competent workers to use.
Drill lead checked for any damage prior to use.
Correct safety features to be correctly installed. i.e drill handle
	L
	Site Supervisor, Carpenter

	18. 
	
	Truss collapse.
	M
	Install temporary bracing
	M
	Site Supervisor, Carpenter

	19. 
	
	Falling objects
	M
	Barricade & sign post area below when working at height above others.
Hard hats to be worn 
	L
	Site Supervisor, Carpenter

	20. 
	Un-slinging of crane
	Persons falling from heights
	M
	Access lifting sling by either;
· Standing on scaffolding
· Standing on bottom cord if the cord has been inspected for defects and a catch platform (mobile scaffold) is used.
· Use a step ladder.
	L
	Dogger

	21. 
	Filling in remaining trusses 
	Persons falling from heights
	M
	Workers to remain on bond beam scaffold supplied where possible
Correct footwear to be worn 
Extra precaution when climbing around on top of trusses 

	L
	Site Supervisor, Carpenter

	22. 
	 Strapping, Batten screwing and speedy bracing to complete job
	Persons Falling from heights
	M
	Correct footwear to be worn
Extra precaution when climbing around trusses
Use mobile scaffold where possible

	L
	Site Supervisor, Carpenter

	23. 
	
	Use of coil gun
	M
	Ensure correct PPE are worn. (Safety Glasses, Ear protection)
Only trained and competent workers to use
Precaution taken when using coil gun on top cords of trusses
Straps to be shot on when standing on scaffold or bottom cord where possible 
	L
	Site Supervisor, Carpenter

	24. 
	
	Use of electric drill
	M
	Only trained and competent workers to use
Screw Batten screws whilst standing on bottom cord or scaffold where possible
	L
	Site Supervisor,
Carpenter

	25. 
	Exiting the roof
	Persons falling from height
	M
	Ensure workers use ladders supplied with bond beam scaffold
Maintain three points of contact when climbing down the ladder
	L
	Site Supervisor,
Carpenter





	Task / Operation / Activity: Install Roof Trusses
	Version: V1.0

	Organisation: Matt Greenwood Constructions
	ABN: 92163040186
	Page 7 of 9



[image: ]



	LIKELIHOOD
How likely could it happen?
	CONSEQUENCES: How severely could it affect health and safety?

	
	Insignificant
No medical treatment required
	Minor
Minor lost time injury or illness
	Moderate
Moderate lost time injury or illness
	Major
Serious lost time injury or illness
	Catastrophic
Death or permanent disablement

	Almost Certain
Is expected to occur in most circumstances
	Medium
	High
	Very High
	Very High
	Very High

	 Likely
Will probably occur in most circumstances
	Medium
	Medium
	High
	Very High
	Very High

	 Possible
Might occur at some time
	Low
	Medium
	High
	High
	Very High

	 Unlikely
Could occur but doubtful
	Low
	Low
	Medium
	Medium
	High

	 Rare
May occur but only in exceptional circumstances
	Low
	Low
	Low
	Medium
	Medium


Based on Table 6.6 HB436-2004 Risk Management Guidelines Companion to AS/NZS4360:2004
	Risk Level
	Action

	VH - Very High 
	ACT NOW – Urgent - Do something about these risks immediately

	H – High
	Highest management action required urgently

	M – Medium
	Manage by specific monitoring or management  procedures

	L – Low
	These risks may not need immediate action – manage by routine procedures



Consequence scales for environmental hazards and risks
	Consequence
	Description

	Catastrophic
	Catastrophic long term environmental impairment of eco systems functions

	Major
	Very serious long term environmental impairment of eco systems functions

	Moderate
	Serious medium term environmental effects

	Minor
	Moderate short term effects not affecting eco system functions

	Insignificant
	Minor effects on biological or physical environment
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