Inspection checklist 
Scaffold vicinity 
1. Has public protection been provided? 
2. Have enough safeguards against electric powerlines been provided? 
3. Do you need control over vehicle movement? 
4. Are scaffolds erected a safe distance away from trenches or excavations? 
Supporting structure 
1. Is the supporting structure in good condition? 
2. Does the supporting structure have satisfactory strength? 
3. Are there controls to prevent deterioration of the supporting structure? 
4. Is the scaffold built on solid ground? If built on soft ground, are soleboards used to properly distribute the load? 
Soleboards and baseplates 
1. Are there enough soleboards? 
2. Are the soleboards of suitable material?
3. Are the soleboards secure? 
4. Are there enough baseplates? 
5. Are the baseplates serviceable and of suitable dimensions? 
6. Are the baseplates secure? 
Scaffold structure 
1. Are the standards bearing firmly? 
2. Are the standards plumb (or as designed)? 
3. Are the longitudinal standard spacings correct? 
4. Are the transverse standard spacings correct? 
5. Are the joints in standards correctly positioned? 
6. Are the joints in standards correctly secured (special duty or hung scaffold)? 
7. Are the ledgers level (or as designed)? 
8. Are the ledgers continuous (or as designed)? 
9. Are the lift heights correct? 
10. Are the horizontal ledger spacings correct? 
11. Are the ledgers correctly secured? 
12. Are ledger joints correctly positioned (tube and coupler scaffold)? 
13. Are the joints in ledgers correctly secured (tube and coupler scaffold)? 
14. Are there sufficient transoms/putlogs? 
15. Are the transoms/putlogs correctly positioned and secured? 
16. Is the bracing adequate? 
17. Is the scaffold sufficiently stable? 
18. Are the ties correctly positioned and correctly fixed? 

Platforms 
1. Does the scaffold have the required number of working platforms? 
2. Are the working platforms at the required locations? 
3. Are the platforms and supporting scaffold constructed for the appropriate duty live loads? 
4. Are the platform dimensions suitable for the intended work? 
5. Is there adequate edge protection? 
6. Are the platforms correctly constructed? 
7. Are planks secured against wind? 

Access and egress 
1. Is there safe access and egress to every scaffold platform? 
2. Are portable ladders of an industrial grade, serviceable and correctly installed? 
3. Are access ways and access platforms correctly installed? 

Containment sheeting 
1. Has the scaffold been designed for wind loading on any containment sheeting? 
2. Are the fixing ties secure? 
3. Are there any rips or tears? 
4. Are the overlap joints satisfactory? 

General fitness for purpose 
1. Is there adequate provision for material handling? 
2. Are the clearances between the scaffold and adjacent structures correct? 
3. Is there adequate protection from falling debris? 
4. Has the scaffold been adequately designed to support all attachments? 
5. Are all approaches and platforms effectively lit? 


Notes:
· The person with management or control of a scaffold at a workplace must ensure that the scaffold and its supporting structure are inspected by a competent person:
a) before the scaffold is used
b) before use of the scaffold is resumed after an incident occurs that may reasonably be expected to affect the stability of the scaffold
c) before use of the scaffold is resumed after repairs
d) at least every 30 days.

Inspection records

[bookmark: _GoBack]Inspections need to be completed by both the site manager AND the scaffolder.
Please fill in the table below once you have completed the checklist.

	Name
	Date & Time
	Location
	Comments
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