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CPCCBC4001 
Apply building codes and standards to the construction process for Class 1 and 10 buildings 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4001 Apply building codes and standards to the construction process for Class 1 and 10 buildings cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Anya English 

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable



	Task
	Date completed
	Assessment Results 

	Theory Exam
	28/09/2023
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	6/10/2023
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	9/10/2023
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4001
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Practical Assessment
	 Fire protection inspection checklist
 Documentation of design and construction (suitability or evidence of suitability)



	Assessor name
	Michelle Gomersall

	Assessor signature
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THEORY EXAM


	Participant name
	Anya English 




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref127183513]Explain why it is important to understand references the NCC makes to Australian Standards.

	Answer
	It is important to understand references made in the NCC to Australian Standards because the standards are sometimes only referenced in one part while other times it is referenced entirely. If referenced only partially then the parts not referenced are considered irrelevant and have no authority. To add, the new amendments/editions of the standards are not automatically adopted by the NCC, meaning you only need to comply with edition of the standard that was referenced. 
	




[bookmark: _Ref127184725]You have been asked to develop a tender proposal for a housing development taking State/Territory. Discuss in depth any legislation and Codes your submission must comply with?

	Answer
	To develop a tender proposal for a housing development you must comply with the National Construction Code specifically Volume 2 of the construction code as this for housing and dwellings. The plans and specifications must be relevant to the requirements stated in the NCC and the standards that are referenced in them. If the plans and specifications are not compliant then the tender disposal will not be compliant meaning that the building will not be safe and that is will not pass all inspections and approvals.  
	




[bookmark: _Ref127186634]Describe the listed NCC compliance assessment methods used to determine compliance using a Performance Solution pathway.

	Answer
	Assessment method
	Description
	

	
	Evidence of suitability
	Evidence of suitability differs between the three volumes of the NCC, however id showing evidence fit the use of plumbing and drainage materials and design by a Certificate of Accreditation/Conformity, a CodeMark Australia, a report issued by an Accredited Testing Laboratory. 
	

	
	Verification methods
	The three different types of verification methods are test -  on site or at a laboratory , inspections – must be conducted by a qualified person , and calculations – both analytical or mathematical methods. ,
	

	
	Comparison with DTS Provisions
	This is done by doing a comparative analysis to determine whether Performance Solutions provide the superior or same level of health, safety, amenity, or sustainability as using the DTS provisions. 
	

	
	Expert Judgement
	An expert person could be a person or an organisations that has the skills and experience necessary to make judgment. The Appropriate Authority is defined differently in every state.

	




[bookmark: _Ref127263388]Discuss the listed levels found in the NCC Performance Hierarchy.

	Answer
	Performance Hierarchy
	Description
	

	
	Objectives
	The objectives are guidance and describe the expectations for the building.
	

	
	Functional statements
	The functional statements are also guidance and are how the objectives are going to be achieved.
	

	
	Performance requirements
	These sit at the top of the hierarchy because they are the minimum level of performance for all building plumbing and drainage installation. They are mandatory requirements that need to be met to objectives and functional statements.
	

	
	Building Solutions
	This is a compliance method to achieve commercial buildings through performance based, obtaining mandatory performance requirements.
	




[bookmark: _Ref127278250]Why may you need to use a combination of Performance Solutions and Deemed-to-Satisfy (DtS) solutions to comply with the Performance Requirements of the NCC?

	Answer
	You may need a combination of both because satisfying a single performance requirements is not enough considering that since there are many components inside a building that are protected by performance criteria. 
	




[bookmark: _Ref128115391]The client is showing you the plans for them to build a duplex on their site. Determine what classification would be assigned to this building. Explain your answer.

	Answer
	Class 1, specifically class 1a because it is a single building having more than one dwelling that is separated by a fire wall.  
	




[bookmark: _Ref128115393]Another client would like to install a swimming pool. Determine what classification would be assigned to this. Explain your answer.

	Answer
	Class 10 specifically Class 10b as it is a non-habitable building or structure. 
	



[bookmark: _Ref128119881]Explain why the plans for a residential building with landscaping features may have more than one classification.

	Answer
	Plans for residential building with landscaping features may have more than one classifications because in the landscaping features could be buildings or structures that are not habitable, i.e. a swimming pool. 
	




[bookmark: _Ref128118928]AS 2870 is referenced in both NCC Volumes One and Two. Respond in the table, what the Australian Standard is referenced in relation to.

	Answer
	NCC Volume
	Referenced in relation to
	

	
	Volume One
	AS 2870 is referenced in V1 under damp-proofing of floors on the ground where the insertion of vapour barrier needs to be accordance with the AS 28710
	

	
	Volume Two
	AS 2870 is referenced in V2 under Site Preparations for the subsoil drainage system. 
	




[bookmark: _Ref128120840]Outline workplace policies and procedures that should be held on-site.

	Answer
	The policy and procedures that should be held on site are Workplace health and safety policies to ensure the workers know the policies and procedures for being safe. All the organisation or workplace related policy and procedures. 
	



[bookmark: _Ref127188238]Why is it important to document quality assurance and quality control processes relevant to the build?

	Answer
	It is important to document quality assurance because it clarifies the standards and requirements. It minimises misunderstandings and potential conflict. Satisfies the requirements of the client and instilling confidence in the organisation, meets workplace requirements against relevant regulations, a provision of product and services in the most cost effective an resource efficient way, lower costs by reducing waste, minimising potential error, defining, controlling and improving processes.
	




[bookmark: _Ref127863024]Discuss the basic principles of structural design that must be considered in any building design.

	Answer
	The basic principals of structural design are the basic concepts and components you must be familiar with. The principles are line-line between two links, a mark, shape-geometric organic, direction – horizontal, obique or vertical, size – in relation to another feature, texture – consists of surface and colour. 
	



[bookmark: _Ref128124628]Provide five conformity assessment pathways that can be used individually, or in combination, to demonstrate product compliance.

	Answer
1.



2.



3.



4.



5.
	Discover document relating to the existing building. 




Undertake a site inspection a record description of building, characteristics addressed by performance requirements. 


Identify potential deficiencies with respect to performance requirements.



Determine whether potential deficiencies are actual deficiencies. 


Alleviate actual deficiencies.  
	




[bookmark: _Ref128122622]Provide the six (6) bushfire attack level ratings that AS 3959 uses to establish the requirements for construction. Explain each rating.

	Answer
1.



2.



3.



4.



5.



6.
	
BAL-LOW – insignificant risk no additional requirements 



BAL-12.5 – Low risk, ember attack, radiant heat



BAL-19 – increasing levels of ember attack and burning debris ignited by wind bourn embers together with increasing heat flux/between 12.5km2 + 19km2 

BAL-29 – increasing levels of ember attack and burning debris ignited by wind bourn embers together with increasing heat flux/between 19km2 + 2 

BAL-40 – increasing levels of ember attack and burning debris ignited by wind bourn embers together with the increased likelihood of exposure to flames 

BAL-FZ – Direct exposure to flames from fire front in addition to heat flux and ember attack. 
	




[bookmark: _Ref128122625]Complete the table below by identifying the type of fire-resisting construction (i.e. Type A, Type B, or Type C) given the following class of building and number of storeys each class of building has.

	Answer
	Rise in Storeys
	Class of building:
2,3,9
	Class of building:
5,6,7,8
	

	
	4 or more
	Class A 
	Class A 
	

	
	3
	Class A 
	Class B
	

	
	2
	Class B
	Class C 
	

	
	1
	Class C 
	Class C
	




[bookmark: _Ref128125400]Provide a brief explanation of each step of the development of Performance Solutions.

	Answer
	Steps in Developing Performance Solutions
	Brief explanation of each step
	

	
	Prepare a performance-based design brief
	Serves as a record of all the fundamental activities and outcomes of the performance solution. Must adequately demonstrate that after designing the solutions and conducting assessment methods that NCC performance requirements have been achieved .
	

	
	Carry out analysis, modelling, or testing
	Some tool to evaluate the proposed performance solution include; comparative or absolute analysis, deterministic or probabilistic analysis, empirical calculations 
	

	
	Collate and evaluate results
	From the previous step the results must be collated for analysis after they have been analysed to form conclusions for the final reporting must meet the criteria agreed in the PBDB.
	

	
	Prepare a final report
	Mandatory document that must clearly demonstrate compliance with NCC performance requirements. Normally includes overview of PBDB outline of the analysis modelling or testing carried out evaluation of results. 
	



[bookmark: _Ref127265454]Discuss two (2) properties, two (2) characteristics and two (2) limitations of concrete when used for buildings. 

	Answer
	
	Concrete
	

	
	Properties
	1. Fire resistant 
	

	
	
	2. Thermal acoustic installations
	

	
	Characteristics 
	1. Very strong in compression stress handling capabilities 
	

	
	
	2. Long lasting 
	

	
	Limitations
	1. very weak in expansion stress - needs reinforcement
	

	
	
	2. Very weak in tensile stress needs pre or post tensioning. 
	




[bookmark: _Ref127265456]Discuss three (3) benefits of using glass in buildings.

	Answer
1.





2.





3.
	
To provide natural light 





To provide natural ventilation 





Rust and weather resistance will not be effected by corrosion or other effects.
	



[bookmark: _Ref128129905]Respond to the following items regarding zero-energy building.

	Answer
	Item
	Zero energy building
	

	
	Definition
	Zero-energy building is the construction of building that produce as much energy as they consume and It is the difference between the energy produced by the building and the energy consumed by the building is zero. 
	

	
	One (1) technique used in zero energy building
	Integrating renewable energy sources that power the building i.e. solar energy, solar panels on the roof. 
	

	
	The procedure in implementing the technique you have identified
	Installing solar panels on the roof to crate solar energy. 
	





	Theory Exam - CPCCBC4001 Apply building codes and standards to the construction process for Class 1 and 10 buildings



CSTC Pty Ltd_RTO#0699_v2-0_23/02/2023	Page 3 of 12
CPCCBC4001 
Apply building codes and standards to the construction process for Class 1 and 10 buildings

WORKBOOK


	Participant name
	Anya English 




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

	ACTIVITY 1  [bookmark: _Ref35349341]

	Access the National Construction Code (NCC) to:
a) Briefly explain what the General Requirements of buildings are.
b) Briefly explain what the Performance Requirements of buildings are.
c) Briefly explain the relationship between a building’s Performance Requirements and compliance options (e.g. performance solutions, deemed-to-satisfy solutions).



	a)  Briefly explain what the General Requirements of buildings are.

	General requirements cover the other aspects off the NCC that performance requirements including its interpretation, referenced documents, the acceptance of design and construction.

	b) Briefly explain what the Performance Requirements of buildings are.

	Performance requirements are the minimal level of compliance a building must comply with and can be satisfied with either performance solutions or deemed to satisfy or both.

	c) Briefly explain the relationship between a building’s Performance Requirements and compliance options (e.g. performance solutions, deemed-to-satisfy solutions).

	The relationship between performance requirements and compliance options are that to achieve the performance requirements it must be through one of the compliance options or both.



	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref35349352]

	Provided in the table below are different building elements of Class 1 and Class 10 buildings. For each building element, provide one performance requirement according to the National Construction Code (NCC) Volume 2.
a) Structural stability and resistance.
b) Weatherproofing.
c) Automatic fire warning for occupants.
d) Personal hygiene and other facilities.
e) Movement to and within a building.



	a) Structural stability and resistance

	By resisting the actions to which it may reasonably expected to be subjected, a building or structure during construction and used with ‘appropriate degree of reliability’ must perform adequately under all reasonably expected design actions.

	b) Weatherproofing

	A roof and external wall must prevent the penetration of water that could cause unhealthy or dangerous conditions or loss of amenity occupants.

	c) Automatic fire warning for occupants

	Occupants must be provided with automatic warning on the detention of smoke with an efficiency greater than 0.95 and a reliability greater than 0.95, so that they may evaluate in the event of a fire to a place of safety appropriate to the function and use of the building.  

	d) Personal hygiene and other facilities

	Suitable sanitary facilities for personal hygiene must be provided in the convenient location within or associated with a building appropriate to its function or use. 

	e) Movement to and within a building

	So that people can move safely to and within a building walk and surfaces must have safe gradients. 



	Satisfactory Outcome
	
	




	ACTIVITY 3  [bookmark: _Ref128058640]

	Provided in the table below are different building elements of Class 1 and Class 10 buildings. Describe the how the verification method for each building element of the buildings must be implemented.



	a) Structural robustness

	Compliance with structural reliability and resistance verified for structural robustness if the structure assess that the building remains stable and the resulting collapse does not extend further than the adjacent storeys upon the notional removed in isolation of any supporting column or beams support one or more column or segment of a load bearing wall length equal to the height of the wall is complied with. 

	b) Room space or height

	Compliance wi3th the room height is verified where the height of a room or space provide an appropriate activity support level that does not unduly interfere with its intended function for a room space in the above activity support level must consider the dimensions of doors, ramps, barriers, stairs and windows and fixed fitting and domestic services and fixed moveable equipment or furniture and occupant circulation spaces. 



	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref128127326]

	Access and review the following documents included with this workbook regarding quality management systems of Cascade Peaks Construction:
Handout 2 (HO2) Cascade Peaks Construction Quality System – Beginning Construction
Handout 3 (HO3)Cascade Peaks Construction Quality System – Mandatory Inspections

Once you have accessed and reviewed the documents above, answer the following questions:
a) Briefly explain why proper procedures for demolition and temporary fencing is needed during construction. 
b) Briefly explain why mandatory inspections are needed during the construction of new buildings.
c) Identify two (2) tasks that should be done before demolition starts.
d) Identify two (2) characteristics that temporary fencing around a construction site should have.
e) Identify two (2) inspections that must be done by a building certifier.
f) Identify two (2) areas in a building that must be inspected for weatherproofing by a building certifier.



	a) Briefly explain why proper procedures for demolition and temporary fencing is needed during construction. 

	Proper procedures for demolition and temporary fencing is needed during construction because there is usually requirements for heavy machinery and equipment there is a need to ensure that the public cannot access and are protected from these works as well as the workers are protected when demolishing. 

	b) Briefly explain why mandatory inspections are needed during the construction of new buildings.

	This is to ensure that the building complies with relevant standards, local regulations and requirements of the building code to ensure the safety of the users of the building when the building is finally complete. 

	c) Identify two (2) tasks that should be done before demolition starts.

	Disconnect existing utilities, power, drainage, gas and water

Establish protective measures to protect nearby properties and structures. 

	d) Identify two (2) characteristics that temporary fencing around a construction site should have.

	Be between 1.8m and 2m tall

Have gates and doors that swing only inwards 

	e) Identify two (2) inspections that must be done by a building certifier.

	Excavation after. Excavation of foundation material and before the concrete for the footings or slab for the building are poured.

Frane – inspection of the frame 

	f) Identify two (2) areas in a building that must be inspected for weatherproofing by a building certifier.

	Weather proofing coating to external face of sing-leaf masonry walls

Flashing to wall/roof junctions



	Satisfactory Outcome
	
	




	ACTIVITY 5  [bookmark: _Ref128128349]

	Access and review: 
Handout 4 (HO4) Cascade Peak Construction’s Safety Policies and Procedures 

After reviewing the policies and procedures, provide the following information below:
a) Cascade Peaks Construction’s safety policy.
b) Cascade Peaks Construction’s field standard safety clothing and equipment policy.
c) Four (4) registers that Cascade Peaks Construction should keep regarding the safety of its workers.
d) Five (5) safety clothing that workers must wear regardless of their task.



	a) Cascade Peaks Construction’s safety policy.

	Committed in creating a workplace environments that is conducive to safety as well as to productivity. Management and employees will comply with all the relevant legislation and safety regulations that are in force both in office and in the client work environment. 

	b) Cascade Peaks Construction’s field standard safety clothing and equipment policy.

	Is that cascade peaks constructions puts the safety of it worker before everything else therefore are expected to wear safety clothing including steel cap boots, wide brim hat, sunscreen, long sleeve shirts, collared shirt for all tasks. 

	c) Four (4) registers that Cascade Peaks Construction should keep regarding the safety of its workers.

	Phone/contact details – staff medical advisors/ambulance/police
Accident – minor/major
Inductions 
Safety training courses staffed attended. 

	d) Five (5) safety clothing that workers must wear regardless of their task.

	Steel cap boots ‘wide brim hat’
UV protection sunscreen 
Long sleeve button down shirt
Collared shirt 



	Satisfactory Outcome
	
	



	ACTIVITY 6  [bookmark: _Ref128131028]

	Consider the columns in the photo below and answer the following questions:
[image: ]

a) What kind of stress is being applied on the columns by the ceiling?
b) Describe the deformation that the columns are possibly undergoing due to the stress that the ceiling is applying on them.
c) Describe what would happen to the columns if the ceiling were too heavy to be supported.



	a) What kind of stress is being applied on the columns by the ceiling?

	Compression stress.

	b) Describe the deformation that the columns are possibly undergoing due to the stress that the ceiling is applying on them.

	A decline in the integrity of the column could cause the column to buckle or break and fail to support themselves and serve their purpose.

	c) [bookmark: _Ref128134604]Describe what would happen to the columns if the ceiling were too heavy to be supported.

	The columns would buckle/collapse. 



	Satisfactory Outcome
	
	




	ACTIVITY 7  [bookmark: _Ref128134618]

	The handrail of a staircase in a two-storey house located in a termite-risk area broke off while a resident was climbing down the stairs. The handrail was hollow and was infested with termites. Upon further inspection, most of the staircase was constructed from untreated timber, and the project plans made no mention of the fact that the house was made in a termite-risk area. 

Given the information above:
a) Identify two factors that contributed to the degradation of the house’s staircase.
b) Identify which Part from the NCC Volume 2 was not properly applied.
c) Briefly explain how the identified clause from the Building Code of Australia Volume 2 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Briefly explain how the identified Australian standard was not properly applied.
f) Identify one practice endorsed by Safe Work Australia was not properly applied.
g) Briefly explain how the identified practice endorsed by Safe Work Australia was not properly applied.
h) Identify what other defect the house would have considering the deviations of the construction from the code and standard.
i) Describe the extent of the work that needs to be done to rectify the termite infestation.



	a) Identify two (2) factors that contributed to the degradation of the house’s staircase.

	Untreated timber 
No mention of being a termite risk area on project plans 

	b) Identify which Part from the NCC Volume 2 was not properly applied.

	Part H1 structure under termite management measures 

	c) Briefly explain how the identified Part from the NCC Volume 2 was not properly applied.

	It did not have a design life of 50 years.

	d) Identify which Australian standard was not properly applied.

	AS 1640 Timber preservation treatment. 

	e) Briefly explain how the identified Australian standard was not properly applied.

	Because the timber was untreated when the standard states to prevent termites the wood must be treated specifically.

	f) Identify one practice endorsed by Safe Work Australia was not properly applied.

	Treated timber with creosote to prevent termites invasion.

	g) Briefly explain how the identified practice endorsed by Safe Work Australia was not properly applied.

	Because it was identified that it was untreated timber.

	h) Identify what other defect the house would have considering the deviations of the construction from the code and standard.

	Because the timber is untreated the house would have fungi through its timber.

	i) Describe the extent of the work that needs to be done to rectify the termite infestation.

	To rectify you will need to scrape off the damaged timber and replace with fillers. The timber will then need to be treated to prevent future termite issues. 



	Satisfactory Outcome
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PRACTICAL ASSESSMENT


	Participant name
	Anya English




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1
	10/10/2023
	 Workplace
 Simulation
	Cogent Headoffice 
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 1.1C. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
 Workplace Quality document  Quality Assurance Template  Other (please specify): 


 Document attached as evidence


	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson  Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify existing building checked for compliance with active fire protection requirements:


 Is checklist used attached as evidence





CPCCBC4001
Apply building codes and standards to the construction process for Class 1 and 10 buildings

	Practical Task 1 

	Description of task:
The participant must demonstrate the skills and knowledge to apply building codes and standards to the construction process one Class 1 or 10) building or structure project to a maximum of two storeys. Documented evidence of all criteria must be presented (template (HO1) available for use if required)The participant must also inspect one existing buildings for fire protection compliance using workplace or created document (See HO5 for information). Assessor and observer will be looking for evidence including:
· Classify building and document findings.
· Read the plans and specifications to determine the nature of the building, its use and arrangement.
· Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
· Determine and document the classification applicable to the building and all ancillary buildings and structures. (template available- HO1)
· Determine construction compliance requirements.
· Determine NCC Performance Requirements relevant to Class 1 and 10, up to two storeys, building projects.
· Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
· Identify and document non-conforming construction methods against NCC Performance Requirements. (template available- HO1)
· Propose and discuss Performance Solution with design and building and construction professionals. Document consultation. (template available- HO1)
· Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
· Meet the evidence of suitability requirements for building materials and products stated in the NCC.
· Complete documentation demonstrating how the project design and construction will meet NCC requirements (template available- HO1) including:
· energy efficiency
· damp and weatherproofing
· fire safety
· health and amenity
· structure
· safe movement and access
· ancillary provisions
· Determine fire protection requirements.
· Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
· Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
· Inspect one existing building for compliance with passive and active fire protection requirements.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Construction plans, drawings and specifications for one (1) building Class 1 or 10) building or structure project to a maximum of two storeys; workplace quality policies and procedures; technology to access building and related industry codes, standards and manufacturer product information and materials specifications; Technology to access the NCC and current relevant Acts and Regulations. PPE as required. Documentation of design and construction (suitability or evidence of suitability) (template available- (HO1).Fire protection checklist.

	Observer details

	Name of observer:
	Michelle Gomersall 

	Role of observer 
(Confirm suitability to sign)
	Human Resources

	Email address of observer
	mgomersall@cogentscaffolding.com.au 

	Signature of observer:
	
	Date:
	10/10/2023



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	1 Classify building

	[bookmark: _Ref128141140]Read the plans and specifications to determine the nature of the building and ancillary provisions, use and arrangement.
	
	[bookmark: _Ref128141144]Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
	
	[bookmark: _Ref128141148]Determine and document the classification applicable to the building and all ancillary buildings and structures. (attach evidence -template available- HO1)
	
	2 Determine construction compliance requirements

	[bookmark: _Ref128143424]Determine NCC Performance Requirements relevant to Class 1 and 10, up to two storeys, building projects. (attach evidence -template available- HO1)
	
	[bookmark: _Ref128143430]Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements. (attach evidence -template available- HO1)
	
	[bookmark: _Ref128143438]Identify and document non-conforming construction methods against NCC Performance Requirements. (attach evidence -template available- HO1)
	
	[bookmark: _Ref128141784]Propose and discuss Performance Solution with design and building and construction professionals. Document consultation. (attach evidence -template available- HO1)
	
	[bookmark: _Ref128143579]Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (attach evidence -template available- HO1)
	
	[bookmark: _Ref128143590]Meet the evidence of suitability requirements for building materials and products stated in the NCC.
	
	[bookmark: _Ref128143524]Complete documentation demonstrating how the project design and construction will meet NCC requirements for energy efficiency (attach evidence -template available- HO1).
	
	[bookmark: _Ref128143527]Complete documentation demonstrating how the project design and construction will meet NCC requirements for damp and weatherproofing (attach evidence -template available- HO1).
	
	[bookmark: _Ref128143529]Complete documentation demonstrating how the project design and construction will meet NCC requirements for fire safety (attach evidence -template available- HO1)
	
	[bookmark: _Ref128143531]Complete documentation demonstrating how the project design and construction will meet NCC requirements for health and amenity. (attach evidence -template available- HO1).
	
	[bookmark: _Ref128143533]Complete documentation demonstrating how the project design and construction will meet NCC requirements for structure. (attach evidence -template available- HO1).
	
	[bookmark: _Ref128143536]Complete documentation demonstrating how the project design and construction will meet NCC requirements for safe movement and access. (attach evidence -template available- HO1).
	
	[bookmark: _Ref128143539]Complete documentation demonstrating how the project design and construction will meet NCC requirements for ancillary provisions. (attach evidence -template available- HO1).
	
	3 Determine fire protection requirements.

	[bookmark: _Ref128143628]Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
	
	[bookmark: _Ref128143542]Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
	
	[bookmark: _Ref128142062]Inspect one existing building for compliance with passive and active fire protection requirements (attach checklist as evidence)
	




	Observer comments:
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