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CPCCBC4006B 
Select, procure and store construction materials for low rise projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4006B Select, procure and store construction materials for low rise projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	Carly Dyson




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Carly Dyson

	
	

	Participant signature
	
	
	[bookmark: QuickMark]

	Date
	17/09/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	44
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Q1.  Which of the following documents and/or people would you refer to when selecting materials for a building project? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Australian Standards
	

	
		Contract
	

	
		Drawings
	

	
		Manufacturer
	

	
		National Construction Code
	

	
		Specifications
	

	
		Tolerances
	




Q2.  [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to suitability of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2, Part 1
	Volume 1, Part A
	




Q3.  [bookmark: _Ref535482367]Identify the assessment methods used to verify a performance solution.

	Answer
	Evidence of suitability
A verification method
Expert judgement
Comparison with the Deemed-to-Satisfy provisions
	




Q4.  [bookmark: _Ref496611564][bookmark: _Ref536083431]Which of the following solutions for material selection often references the Australian Standards? Tick your response.

	Answer
	Choice
	Possible Answers
	

	
		Deemed-to-Satisfy solution
	

	
		Performance solution
	




Q5.  [bookmark: _Ref425255684]Identify five (5) materials commonly used for low rise buildings in your region. For each material, identify the following:
· Its name
· Properties of the material

	Answer
	#
	Material name
	Properties
	

	
	1
	Wood
	Very flexible under loads
Can be built in most climates
Strong

	

	
	2
	Brick
	Cheap to produce
Flame retardant
	

	
	3
	Concrete
	Low tensile strength
Long life
Easy to form
	

	
	4
	Glassl
	Brittle
	

	
	5
	Plastic
	All vary in heat tolerance, hardness and resiliency
Can be moulded
	





Q6.  [bookmark: _Ref425323073][bookmark: _Ref425248000]For each of the materials in Q5. identify the following:
· Quality of the material (i.e. durability, serviceability, cost effectiveness)
· Compatibility and non-compatibility of the material (i.e. what it would/would not be suitable for)

	Answer
	#
	Quality
	Compatibility 
	

	
	1
	Durable, cost effective, low serviceability
	Compatibility: Structural framework and cladding

Non-compatibility: 
	

	
	2
	Durable, cost effective, low serviceability
	Compatibility: Internal / external walls

Non-compatibility: Windows and doors
	

	
	3
	Durable, cost effective, low serviceability
	Compatibility: Slabs and external roofing tiles

Non-compatibility: Windows and doors
	

	
	4
	Durable, cost effective, low serviceability
	Compatibility: Windows / doors / light sources

Non-compatibility: Structural framework 
	

	
	5
	Durable, cost effective, low serviceability
	Compatibility: Fixtures and fittings

Non-compatibility: structural framework 
	



Q7.  [bookmark: _Ref536083435]Identify five (5) physical characteristics that may be considered when evaluating potential building materials.

	Answer
	Strength
Density 
Electrical conductivity
Thermal conductivity
Acoustics
	




Q8.  [bookmark: _Ref536095924]Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definition
	

	
	1
	Carbon footprint
	1 -B
	A
	The amount of energy required to manufacture a product
	

	
	2
	CO2e
	2 -E
	B
	Total GHD emissions produced during manufacture construction and use
	

	
	3
	Embodied energy
	3 -A
	C
	Greenhouse gas emissions
	

	
	4
	Embodied water
	4 -D
	D
	The amount of water required to manufacture a product
	

	
	5
	GHG
	5 -C
	E
	CO2equivalent tonnes emitted into the atmosphere
	




Q9.  [bookmark: _Ref536083463]Which of the following materials would be considered as ‘low energy content’? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Bricks
	

	
		By-products of other industrial processes
	

	
		Cement
	

	
		Glass
	

	
		Metals
	

	
		Plastics
	

	
		Sand
	

	
		Stone
	

	
		Timber
	



Q10.  [bookmark: _Ref536099133]Refer to the table below and identify the wall material type that has the smallest embodied energy and emission impact.

[image: ]

	Answer
	Walls timber frame fibro clad
	





Q11.  [bookmark: _Ref536095926]Identify the Volume and Parts of the NCC that relate to energy efficiency of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 1, Pat J
	Volume 1, Part J
	




Q12.  [bookmark: _Ref536097820]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses residential slabs and footings.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Section 3
	AS 2870
	




Q13.  [bookmark: _Ref536097822]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses roof tiles.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Section 7
	AS 2050-1995
	




Q14.  [bookmark: _Ref536106144]Identify the Volume and Parts of the NCC that relate to safety barriers for swimming pools for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2, Part 3.
	Volume 2, Part 3
	




Q15.  [bookmark: _Ref536106145]In some states, barriers and fences for swimming pools are not entirely regulated by the NCC, as noted in the Ancillary Provisions and State and Territory Variations. Identify the applicable Act and Regulation that regulate safety barriers for swimming pools in your jurisdiction.

	Answer
	The Building Act 1975
	



Q16.  [bookmark: _Ref536106146]Identify the Australian Standard that relates to safety barriers for swimming pools.

	Answer
	AS 1926.1-2007
	




Q17.  [bookmark: _Ref536107455]True or False (Tick your response): According to the Standard in Q16. all gates must be fitted with a self-closing device that will return the gate to a closed position from any position without the use of manual force.

	Answer
		True 
	
	

	
		False 
	
	




Q18.  [bookmark: _Ref536170034]Identify the Volume and Parts of the NCC that relate to fire-resistance of building elements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2, Part 3
	Volume 1, Part C
	




Q19.  [bookmark: _Ref536170036]Identify the Australian Standard that relates to fire-resistance tests for elements of construction.

	Answer
	AS 1530.4-2005
	




Q20.  [bookmark: _Ref536169328]For all NCC Classes, where the ground or subfloor space is excessively damp or subject to frequent flooding, which durability class must the subfloor framing must be used where above ground?

	Answer
	Class 1 or 2 durability timbers or Class H3 preservative treated timbers 
	





Q21.  [bookmark: _Ref536170040]Identify the Australian Standards that must be observed when meeting the requirements for Q20. 

	Answer
	AS 1684
	




Q22.  [bookmark: _Ref536170043]True or False (Tick your response): Where materials are not used as intended (or without considering NCC requirements), this can make a significant difference to the life or serviceability of the structure.

	Answer
		True 
	
	

	
		False 
	
	




Q23.  [bookmark: _Ref536170044]Explain why durability and serviceability impact on the cost effectiveness of chosen materials.

	Answer
	Materials that are not durable and will need to be replaced in a shorter timeframe will cost more money for the client in ongoing servicing or material replacement 
	




Q24.  [bookmark: _Ref536172033]Provide an example of short term degradation of materials and describe its effects on a building on structure.

	Answer
	Materials may deteriorate due to weathering such as timber which may split and crumble if it is unprotected
	





Q25.  [bookmark: _Ref536172034]Provide an example of long term degradation of materials and describe its effects on a building on structure.

	Answer
	Materials may deteriorate due to weathering such as limestone that erodes with constant exposure to wind and water
	




Q26.  [bookmark: _Ref425327163][bookmark: _Ref425327708]You have spoken to a supplier who has indicated that some of the client’s desired materials are unavailable. When considering alternative building materials what must be taken into consideration (i.e. other than the client’s requirements)?

	Answer
	Availability
Environmental issues
Life cycle assessment methodology
	




Q27.  [bookmark: _Ref536177031]Identify two (2) things that you should look for when receiving a delivery of materials.

	Answer
	Confirm quantity correct
Confirm condition of delivery
	




Q28.  [bookmark: _Ref536177032]If you encounter issues with delivery, what two (2) options do you have?

	Answer
	Accept shipment with conditions
Reject entire shipment
	




Q29.  [bookmark: _Ref409518704][bookmark: _Ref408838393]Which of the following should be assessed before shifting materials? Tick all that apply. 

	Answer
	Choice
	Possible Answers
	

	
		What needs to be relocated (e.g. size, weight)
	

	
		The relocation area, site layout and obstacles
	

	
		Distance and time to relocate load
	

	
		Whether a team is available and/or appropriate
	

	
		Whether PPE must be worn (e.g. for hazardous materials)
	




Q30.  [bookmark: _Ref536178585]What document should you refer to for guidance on how to handle and store hazardous chemicals? 

	Answer
	Safety Data Sheet
	




Q31.  [bookmark: _Ref408838395][bookmark: _Ref409519364]Name three (3) ways you can reduce the risk of injury if a load is too heavy for one person to carry, push or pull. 

	Answer
	Team lift
Mechanical aid
Lighten load before lifting
	





Q32.  [bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




Q33.  [bookmark: _Ref404158235]How should construction materials and components be handled? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Sorted to suit material type and size, separating hazardous material
	

	
		Stacked or stockpiled for ease of identification and retrieval
	

	
		Stored in access ways for ease of retrieval
	

	
		Stored clear of access ways
	

	
		Handled and positioned ready for installation
	




Q34.  [bookmark: _Ref536180244]Identify the Australian Standard that relates to the storage and handling of LP gas.

	Answer
	AS/NZS 1596:2002
	



Q35.  [bookmark: _Ref536194481]List one (1) testing method for each of the building materials listed below.

	Answer
	Material name
	Properties
	

	
	Concrete
	Hydraulic press
	

	
	Metals
	Repeated loading 
	

	
	Timber
	Stress grading machine tests
	




Q36.  [bookmark: _Ref536181364]What Code gives detailed tables which state the required grade of timber for specific sizes and uses?

	Answer
	NCC
	




Q37.  [bookmark: _Ref536181366]Name two (2) ways that defects may be seen in timber.

	Answer
	Knots
Insect damage
	




Q38.  [bookmark: _Ref536181368]Identify two (2) tests that may be performed to determine the durability of stone.

	Answer
	Acid immersion test
Measure water retention rate
	



Q39.  [bookmark: _Ref536181370]Name two (2) ways that defects may be seen in stone.

	Answer
	Visible cracks and fissures in the surface
Non- conformity in colour an dgrain

	




Q40.  [bookmark: _Ref536187863]True or False (Tick your response): Under a contract, builders and other specialist tradespersons are the ones most likely to rectify or remedy problems that arise from incorrect installation, application or placement of materials.

	Answer
		True 
	
	

	
		False 
	
	




Q41.  [bookmark: _Ref536187427]Name two (2) established methods that may be used to preserve timber.

	Answer
	Soil poisoning
Preservative treatments
	




Q42.  [bookmark: _Ref536187429]Identify two (2) established methods that may be used to protect ferrous metals.

	Answer
	Galvanising
Painting
	





Q43.  [bookmark: _Ref536187430]Explain why the corrosion resistance of non-ferrous metals is superior to that of ordinary steel.

	Answer
	Result of the production of ceramic coating of oxide or salt on the metal which protects it from further corrosion
	




Q44.  [bookmark: _Ref536187432]When should aluminium be coated with bituminous paint? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		At all times
	

	
		When it is buried in soil
	

	
		When it comes in contact with chemical materials
	

	
		When it is immersed in water
	

	
		When it is used on bitumen
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	

	
	

	Participant signature
	
	
	

	Date
	Click here to enter a date.



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4006B
Select, procure and store construction materials for low rise projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to supervise systems through which materials are selected, acquired and stored on site for the following projects:
· Occasion 1: Construction classified as Class 1 and 10 construction
· Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
· Copy of PO sent to site team for materials.
· Email correspondence sighting need for materials, delivery of materials and storage of materials (if relevant).

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Computer, Building Contract, Drawings, Specifications, Building materials (including timber, and ferrous and non-ferrous metal).

	Assessment of task

	Name of participant:
	

	Name of observer:
	

	Role of observer 
(Confirm suitability to sign)
	

	Email address of observer
	

	Signature of observer:
	
	Date:
	Click here to enter a date.

	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Evaluate building materials

	1.1A.  [bookmark: _Ref535842396]Identify suitability of materials commonly used in the region for low rise buildings. 
	
	

	1.1B.  [bookmark: _Ref535842402][bookmark: _Ref536020766]Through research and testing, identify properties of different materials, their quality and compatibility and non-compatibility and maintain effective sampling and organisational record-keeping processes.
	
	

	1.1C.  [bookmark: _Ref535842408]Identify the environmental impacts of different materials. 
	
	

	1.1D.  [bookmark: _Ref535842411]Identify the impact of allowable tolerances on the conversion of naturally occurring materials. 
	
	

	1.1E.  [bookmark: _Ref535842424]Identify and check tolerances for installing and assembling materials with regard to the nature of the work being performed and the requirements of relevant construction industry Australian standards. 
	
	

	2 Material selection 

	1.2A.  [bookmark: _Ref535842432]Select materials structurally adequate and appropriate for the building system specified in the contract, drawings and specifications. 
	
	

	1.2B.  [bookmark: _Ref535842436]Select materials after considering:
· Safety
· Required fire resistance rating
· Suitability to the application
· Durability
· Serviceability and cost effectiveness
· Compliance with NCC, legislation, regulations and Australian Standards
	
	

	1.2C.  [bookmark: _Ref535842439]Consider short and long-term degradation of materials in relation to the building’s proposed life cycle. 
	
	

	1.2D.  [bookmark: _Ref535842441][bookmark: _Ref536188601]Select and evaluate alternative materials, if specified materials were unavailable or unsuitable – justifying decisions to regulatory authorities, as necessary
	
	

	1.2E.  [bookmark: _Ref535842446]Finalise selection of materials in accordance with contractual requirements and in consultation with relevant professionals and the client, compiling results in a report.
	
	

	1.2F.  [bookmark: _Ref535842459]Effectively communicate using the following methods:
· Language/concepts appropriate to cultural differences
· Non-verbal communication
	
	

	3 Supervising materials on site 

	1.3A.  [bookmark: _Ref535842490]Determine limitations and effects of transportation on material and components, taking action in potentially damaging circumstances. 
	
	

	1.3B.  [bookmark: _Ref535842494]Ensure materials were correctly and safely handled on site using appropriate equipment and safe work practices. 
	
	

	1.3C.  [bookmark: _Ref535842471]Communicate with manufacturers and suppliers to ensure materials are stored in accordance with specifications and Australian standards. 
	
	

	1.3D.  [bookmark: _Ref535842501]Implement processes for inspecting all materials delivered on site for naturally occurring and/or manufactured defects before installation. 
	
	

	1.3E.  [bookmark: _Ref535842506]Ensure personnel were aware of actions to be taken in the case of defects caused by incorrect installation, application or placement. 
	
	

	1.3F.  [bookmark: _Ref535842510]Preserve and protect timber and ferrous and non-ferrous metal used in the construction process.
	
	

	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS
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Floor suspended slab 114 - 117 mm 208 68
Floor suspended timber on stumps 76 2
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Roof steel frame colorbond steel or tile 200 7
Roof imber frame colorbond steel or tile 143 a7
WALLS
‘Walls double brick; s/b interior 312 103
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‘Walls pre-cast concrete 264 88
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length
Roofed open areas - lfresco / porch / verandah / carport 352 n7
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Open Carport 352 n7
Fence brick or metal (per metre length, assuming 1.5 m height) 186 61
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