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	Organisation
	
	Location
	
	Date: 					Time: 		am/pm

	Name the space:
	Person Conducting Assessment:

	
	PHOTO TO BE INSERTED

	Primary Function:

	

	Activities undertaken in space:
	



	No.
	CONFINED SPACE CRITERION – 
Is an enclosed or partially enclosed space which:-
	YES / NO
	COMMENTS
Provide comment supporting response

	1.1. 
	Is not designed or intended primarily to be occupied by a person (e.g. it is not a normal place that people conduct work in)?
	 
	

	1.2. 
	Is, or is designed or intended to be, at normal atmospheric pressure while any person is in the space
	 
	

	1.3. 
	Is or is likely to be a risk to health and safety from:
	Provide details of any identified atmospheric, contaminant or engulfment hazards which may occur in the space, including those which may occur as a result of an introduced activity.

	1.4. 
	· an atmosphere that does not have a safe oxygen level (e.g. too low or too high)
	 
	

	1.5. 
	· contaminants, including airborne gases, vapours and dusts, that may cause injury from fire or explosion
	 
	

	1.6. 
	· harmful concentrations of any airborne contaminants
	 
	

	1.7. 
	· engulfment
	 
	



	SECTION 2 CONFINED SPACE CONCLUSION
	YES / NO

	The space is a Confined Space (For the space to be confined all points, 1.1 to 1.3, must be answered with a yes) 
	 

	The space should be classified as a restricted space
The space would not be defined as a confined space, however if certain hazards are introduced (gas flame brazing torches or flammable solvents), then a risk to health and safety from atmospheric contamination may arise and the space could be classified as a confined space. Anyone planning to enter the space should consider what hazards might be present or introduced when they enter. Appropriate procedures are required for management for restricted spaces with the space being classified accordingly taking into account the activity to be carried out.
	 



	SECTION 3 CONFINED SPACE HAZARD IDENTIFICTATION

	· Access (restricted entry and/or exit)
· Airborne contaminants
· Activity/task performed in the space
· (e.g. use of paints, adhesives, solvents)
· Biological hazards (e.g. contact with micro-organisms, viruses, bacteria or fungi associated with a sewer, grain silo)
· Communication
· Crushing, cutting, piercing or shearing of parts of a person’s body if exposed to plant such as augers, agitators, blenders, mixers and stirrers
· Electrical hazards (e.g. potential for electric shock)
· Emergency management (including evacuation)
· Engulfment (e.g. swallowed up or immersed by sand, liquids, grain, animal feed)
· Entanglement in moving parts
· Entry of natural contaminants such as groundwater and gases from the surrounding land, soil or strata
· Environment - dirty
	· Environment - wet
· Fire hazard/naked flame, fire explosion
· Guarding/barriers inadequate
· Hazardous substances/chemicals
· Hazards outside the confined space
· Ignition source such as a sparking or electrical tool, including from static on a person being introduced into a space containing a flammable atmosphere
· Located near a footpath or road
· Lighting inadequate
· Manual handling – lifting
· Manufacturing process
· Medical emergency – first aid
· Mobile confined space
· Noise (e.g. > 85dBA (8 hrs), or 140dB peak)
· Permits, licenses and registration required, (e.g. asbestos removal)
· Residue left in tanks, vessels etc or remaining on internal surfaces
	· Skin contact with hazardous substances which could cause a burn, irritation or allergic dermatitis)
· Slip, trip hazards or uneven surfaces
· Steam, water or other liquids, gases or solids may result in drowning, or being overcome by fumes
· Temperature extremes (cold)
· Temperature extremes (hot), heat stress
· Uncontrolled introduction of substances
· Unsafe oxygen level
· (less than 19.5% or greater than 23.5%)
· Vertical opening adjacent to or within the confined space
· Workplace/surface is unstable or uneven
· Restricted movement (e.g. space restricted by size or requirement to wear personal protective equipment)
· Personal protective equipment – grip is compromised
· Physiological and psychological demands (e.g. physical ability of the person to conduct the work, possibility of a person being claustrophobic, ability to wear
· the person protective equipment required to do the work (e.g. respirators)
· Powered equipment
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