BSBWHS510 – Practical Task 

Identifying hazards and Workplace Safety Audit
Consulting with specialist advisors (Safe Work Queensland) and emergency services including fire and ambulances will be performed to assist in identifying potential fire hazards/emergencies in the workplace. The main hazards/emergencies found through this process included faulty electronic equipment resulting in a fire in the workplace, spraying methylated spirits onto cut glass to break laminate layer, with a hot lamp that is also used to break laminate barrier, flammable storage cabinet mixed with an ignition source, grinding metal glass storage frames, causing sparks which can ignite a fire in the workplace and cigarette buts being thrown into the large bin out at the front of the workplace.
A safety audit was than completed in the workplace. This safety audit was used to identify if all required resources are available for an immediate response including evacuations maps that have been placed at all emergency exits entrances to the workplace. Than all emergency equipment in the workplace was checked to ensure serviceability that all equipment was in date, equipment can be easily accessed during an emergency and is not blocked, overall cleanliness of the equipment ensuring its in good working condition and finally in correct locations in areas where they will needed to be used in an emergency with enough equipment for the workplace. This workplace was completed using the Business Fire Safety Checklist written by Wormald to ensure all required areas were focused on.

Fire Drill Debrief
After the fire drill has been performed the emergency evacuation checklist was filled out to organize and monitor the information found the fire fire drill. The hazards that arisen from the fire drill include a customer who was at the workplace during the dire drill had parked their car in front of the main door to move into and out of the office. This meant the two other doors in the office had to be used. Another hazard was that two workers operating the glass polisher were using a suction lift the lift glass into the polisher. When the alarm sounds the workers have lifted a piece of glass a few inches off the trolley, it was than lowered back down with the workers evacuating straight after. In a situation where the workers had the panel of glass lifted in mid air it might take more time to return the panel of glass back to the trolley and additional measures and training should be given to prepare for this situation. Another improvement that was discussed is while workers are workers are calmly leaving the build as they walk past toilets to quickly check the toilet block for everyone, this can also be applied the to other areas throughout the workplace.
The information that has been obtained from the fire drill will than be debriefed to the PCBU to make the fully aware of the situation so they can fulfill their WHS obligations. The WHS trainer/assessor will also be debriefed also to source expect feedback to further improve the emergency procedures and finally workers and workplace supervisors will be debrief to keep everyone informed to how well the drill was performed, issues that have arisen and feedback from the workers to incorporate into the procedures.
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