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Documentation of design and construction (suitability or evidence of suitability)
	Project Name: Paddington heights

	Project address: 68 Latrobe terrace
	Site Plans attached: 

	Prepared by: Michael Trott

	Date: 08/11/24

	Description of project:
Spalling repairs

	Site Classification/s, Class and Climate Zone Compliance (NCC bushfire, high wind, earthquake and alpine environment requirements.)
The structure is a 4-storey multi-residential dwelling, it has been constructed with suspended slab floors, walkways & balconies; which are supported by double skin brick walls. Built in the early 1980s, the building is approximately 43 years old, nearing the end of its typical residential 50-year design lif.
Climate zone 2
Class 2 building

	Documentation of design and construction (suitability or evidence of suitability)

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earthworks
	N/A
	

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earth retaining structures
	N/A
	

	Drainage
	NCC PART 3.3.3
AS 4654
	Water testing

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Termite risk management
	N/A
	

	Materials
	N/A
	

	Footings and slabs

	Site classification

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Footings and slabs
	AS 2870
AS 3600
	Slab and footing durability

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Moisture Barrier
	Section 3.2
AS 2870
	Minimise moisture penetration

	Materials
	UV membrane
	

	Concrete and reinforcement

	Concrete and reinforcement
	NCC / Australian Standards requirements
	Compliant Performance solution

	Concrete and reinforcement
	AS 3600
AS 4671
AS 1480
	SAFETY
DURABILITY
STRUCTURAL ADEQUACY 

	Materials
	SIKA MONOTOP-352 NFG CONCRETE REPAIR MORTAR
SIKAGARD-680 S BETONCOLOUR
SikaTop Armatec -110 EpoCem
	

	Masonry

	Masonry
	NCC / Australian Standards requirements
	Compliant Performance solution

	Masonry
	N/A
	

	Moisture Barrier
	N/A
	

	Materials
	N/A
	

	Framing/Structure

	Framing/Structure
	NCC / Australian Standards requirements
	Compliant Performance solution

	Framing
	N/A
	

	Materials
	N/A
	

	Roof and Wall Cladding

	Roof and wall cladding
	NCC / Australian Standards requirements
	Compliant Performance solution

	Roof and wall cladding
	N/A
	

	Materials
	N/A
	

	Glazing

	Glazing
	NCC / Australian Standards requirements
	Compliant Performance solution

	Glazing
	N/A
	

	Materials
	N/A

	

	Fire Safety

	Fire Safety
	NCC / Australian Standards requirements
	Compliant Performance solution

	Fire Safety
	Section c
Part d
AS 1530.4
AS 3745
AS 3600
	

	
	
	

	
	
	

	Access/Stairs/Lifts/Ramps

	Access/Stairs/Lifts/Ramps
	NCC / Australian Standards requirements
	Compliant Performance solution

	Access
	NCC PART D1
AS 1743
	

	
	
	

	Materials
	
	

	Ancillary Provisions

	Ancillary Provisions
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	N/A
	

	
	
	

	
	
	

	Energy Efficiency

	Energy Efficiency
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	N/A
	

	
	
	

	
	
	

	Health and Safety

	



	Issues to be addressed and consultation

	Issue
	Who to consult
	Improvements for consideration
	Feedback following consideration
	Supporting Resources
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