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CPCCBC4012B 
Read and interpret plans and specifications 
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4012B Read and interpret plans and specifications cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 
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	Junquan Chen
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	 Not Yet Satisfactory
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
	Junquan Chen

	
	

	Participant signature
	
	
	

	Date
	6/11/2020



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	87
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	




	ASSESSOR COMMENTS

	


Q1.  Plans and specifications are used to inform which of the following processes? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
	þ	Building contracts
	

	
	þ	Development applications 
	

	
	þ	Estimation
	

	
	þ	Planning
	

	
	þ	Supervisory tasks
	

	
	þ	Tenders
	




Q2.  [bookmark: _Ref532191033]Which compass direction is always shown on plans and drawings?

	Answer
	North
	



Q3.  [bookmark: _Ref427670124]What information is provided on a location plan?

	Answer
	Lot number/s
Deposit plan numbers 
North point
Scale (usually 1:5000)

	



Q4.  [bookmark: _Ref427670125]What detail does a site or block plan contain?

	Answer
	Outline of site boundaries showing location of proposed building and existing dwellings
Street frontage names
Major geological and topographical features (trees and vegetation)
Datum points, contours and slopes 
Driveways, stormwater drainage, easements and right of carriage
Soil and surface water drains, pipe sizes
Service runs from the house to mains - utility services location (sewer, water, gas, electricity)
Details of paving and retaining walls

	


Q5.  [bookmark: _Ref427670660]What do floor plans identify?

	Answer
	Shows detail of the proposed structure, such as rooms, positions of fixtures, floor coverings

	



Q6.  [bookmark: _Ref427671793]What is a landscape plan and what information might it provide?

	Answer
	Shows details of plants, paths, garden layouts and retaining walls 

	



Q7.  [bookmark: _Ref427670661]What are elevation views? What do they provide to the plan reader?

	Answer
	View of the proposed structure from its sides (i.e. from north, south, east and west). Each side is what is called an elevation view. 
Elevations indicate:
Finish to external walls and
Size of windows, doors and balconies


	



Q8.  [bookmark: _Ref427670662]What is a section?

	Answer
	A section is a vertical view (slice) through the building. The direction of section lines or arrows is usually shown on the plan to help interpret the sectional view.

	



Q9.  [bookmark: _Ref427670664]What are detailed drawings?

	Answer
	
	



Q10.  [bookmark: _Ref427671414]What are specifications?

	Answer
	Specifications set out the minimum standards or codes required for all structural components and provide details of building materials and fittings, such as:
Windows, frame material and type of glass
Doors, size, material and the swing on the door
Finishes/colours to walls, floors and ceilings
Door types and models of locks, latches, hinges, push plates and pull handles 

	




Q11.  [bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	ACRYL
	Acrylic
	

	
	AS
	Australian Standard
	

	
	ASSD
	Assumed Daturn
	

	
	B
	Basin
	

	
	BN
	Bull Nose
	

	
	BTH
	Bath
	

	
	BWK
	Brickwork
	

	
	CB
	Concrete Block
	

	
	CF
	Concrete Floor
	

	
	CG
	Clear Glass
	

	
	CJ
	Ceiling Joist
	

	
	CORR
	Corrugated
	

	
	CWT
	Cold Water Tank
	

	
	DG
	Double Glazing
	

	
	DH
	Double Hung
	

	
	DPC
	Damp Proof Course
	

	
	DSB
	Distribution Switchboard
	

	
	DW
	Dish Washer
	

	
	EJ
	Expansion Joint
	

	
	FPBD
	Fibrous Plaster Board
	

	
	FFL
	Finish Floor Level
	

	
	FHR
	Fire Hose Reel
	

	
	GPO
	General Purpose Outlet
	

	
	HBD
	Hard Board
	

	
	HTR
	Heater
	

	
	HWD
	Hard Wood
	




Q12.  [bookmark: _Ref427675022]Name each of the drawing symbol images shown in the table below.

	Answer
	Name
	Image
	
	
	Wall - Cavity brick
	[image: Wall - Cavity brick]
	

	
	Wall - Brick veneer
	[image: Wall - Brick veneer]
	

	
	Wall - Timber stud
	[image: Wall - Timber stud]
	

	
	Window - In cavity wall
	[image: Window - In cavity wall]
	

	
	Window - In single wall
	[image: Window - In single wall]
	

	
	Door - Swing single
	[image: Door - Swing single]
	

	
	Door - Swing double
	[image: Door - Swing double]
	

	
	Door - Sliding into pocket
	[image: Door - Sliding into pocket]
	

	
	Door - Sliding exposed on wall
	[image: Door - Sliding exposed on wall]
	

	
	Socket outlet (power) - general
	[image: Socket outlet (power) - general]
	





Q13.  [bookmark: _Ref427733304]Identify what the following window symbols represent on elevations.

	Answer
	Item
	Drawing
	
	
	Hinged at side
	[image: ]
	

	
	Hinged at top
	[image: ]
	

	
	Sliding horizontrally
	[image: ]
	

	
	Fixed 
	[image: ]
	




Q14.  [bookmark: _Ref532192707]What does a clouded area on a plan indicate?






	Answer
	revisions or amendments
	



Q15.  [bookmark: _Ref532192900]An amendment to specifications could relate to which of the following? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
	þ	Contact details of all construction crew members
	

	
	þ	Materials or products used
	

	
	þ	Methods of carrying out specified work
	





Refer to the title block below to respond to Q16. to Q18. 
[image: ]
Source: http://www.dtwd.wa.gov.au/sites/default/files/teachingproducts/BC1934_CCBY.PDF 

Q16.  [bookmark: _Ref531861864]On what date was an amendment made to the window details?

	Answer
	5/10/2011
	



Q17.  [bookmark: _Ref532193187]True or False (Tick your response): Details of the window in Q16. should also be reflected in the specifications and confirmed with the client.

	Answer
	þ	True 
	
	
	
		False 
	
	




Q18.  [bookmark: _Ref531862015]What amendment occurred on 08/11/2011?

	Answer
	Bed 3 robe deleted
	




Refer to the site plan below to respond to Q19. to Q26. 

[image: Site plan for a block of land showing existing building and proposed residence plus other detail]


Q19.  [bookmark: _Ref531861219]What structure is being built on this site? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
	þ	Residence
	

	
		Road
	

	
		Shed
	

	
		Water meter
	




Q20.  [bookmark: _Ref532193598]What is the Lot number of this site?

	Answer
	16
	



Q21.  [bookmark: _Ref532193601]What is the size of this lot?

	Answer
	3653 ㎡
	



Q22.  [bookmark: _Ref532193617]Is the shed at the north-east of the proposed structure to be removed or retained? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Removed
	

	
	þ	Retained
	




Q23.  [bookmark: _Ref532193558]True or False (Tick your response): The sewer is at the eastern boundary of the property.

	Answer
		True 
	
	
	
	þ	False 
	
	




Q24.  [bookmark: _Ref532193550]True or False (Tick your response): The driveway is located to the south of the proposed property.

	Answer
	þ	True 
	
	
	
		False 
	
	



Q25.  [bookmark: _Ref532193569]What size is the easement on the eastern boundary of the site?

	Answer
	5m
	



Q26.  [bookmark: _Ref531861509]True or False (Tick your response): The stormwater drain is constructed from PVC pipe.

	Answer
		True 
	
	
	
	þ	False 
	
	




Refer to the contour plan below to respond to Q27. to Q28. 

[image: contourplan]

Q27.  [bookmark: _Ref531872622]What is the level at the northernmost point of the site?

	Answer
	3.94
	



Q28.  [bookmark: _Ref532193453]Which end of the site has the lowest level? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		East
	

	
	þ	West
	



Refer to the sectional drawing below to respond to Q29. to Q49. 

[image: cross_section]
Q29.  [bookmark: _Ref427660755][bookmark: _Ref532194571]Give a brief description about the building from the detail available in the sectional drawing. Is it the same structure proposed in Q19. to Q26.?

	Answer
	It is a two story residential house. Lower story is Brick veneer. Upper story is timber wall. It is the same structure proposed in Q19. to Q26. 
	



Q30.  [bookmark: _Ref427733756]Who is the client?

	Answer
	H&M SMITH
	



Q31.  [bookmark: _Ref427733757]Where is this project to be built?

	Answer
	LOT 16 Glenvally Road, Richmond
	



Q32.  [bookmark: _Ref427733759]What are the contact details for the draftsman?

	Answer
	Joe foreman
Ph:0395142311
Mob:0413113113

	



Q33.  [bookmark: _Ref427733761]What sheet number is this drawing?

	Answer
	5 of 7
	



Q34.  [bookmark: _Ref427660519][bookmark: _Ref427733762]What timber is required for loading and non-load bearing walls?

	Answer
	90*45 for loading walls
90*35 for non-load bearing walls

	


Q35.  [bookmark: _Ref427733763]What spacing is recommended for common studs?

	Answer
	600mm
	



Q36.  [bookmark: _Ref427733765]What type of roof truss is to be installed?

	Answer
	Scissor truss
	



Q37.  [bookmark: _Ref427733766]What centres are the trusses positioned at?

	Answer
	Ceiling joists
	



Q38.  [bookmark: _Ref427733769]What size are the veranda posts?

	Answer
	90*90 mm
	



Q39.  [bookmark: _Ref427733771]What timber species are the veranda posts to come from?

	Answer
	DAR OREGON
	



Q40.  [bookmark: _Ref427733773]What pitch is the roof?

	Answer
	30°
	



Q41.  [bookmark: _Ref427733774]What size are the noggings and at what spacing?

	Answer
	90*35mm 600mm max spacing
	



Q42.  [bookmark: _Ref427733776]What size are the ceiling joists?

	Answer
	HJ240
	


Q43.  [bookmark: _Ref427733778]What timber is used for roof battens and what spacing?

	Answer
	35*70 FG pine at 900 spacing
	



Q44.  [bookmark: _Ref427733780]What thickness is the plasterboard sheeting?

	Answer
	10mm
	



Q45.  [bookmark: _Ref427733781]What type of flooring is to be installed?

	Answer
	15mm plywood flooring
	



Q46.  [bookmark: _Ref427733783]What is the roof cladding material?

	Answer
	Colorbond corrugated metal
	



Q47.  [bookmark: _Ref427733784]Where will you find information about the footings?

	Answer
	Section a-a
	



Q48.  [bookmark: _Ref427733786]What do the letters ‘DAR’ refer when timber ordering?

	Answer
	Dressed All Round
	



Q49.  [bookmark: _Ref427662218]Explain what ‘240 x 63 LVL’ refers to on the sectional drawing. What do the letters ‘LVL’ refer to?

	Answer
	240mm*63mm Laminated Veneer Lumber
	


Refer to the drawing below to respond to Q50. to Q65. 

[image: ]

Q50.  [bookmark: _Ref427663500]What is the number of the drawing?

	Answer
	s
	



Q51.  [bookmark: _Ref427734104]What is the Job Number?

	Answer
	OOR-112
	



Q52.  [bookmark: _Ref427734106]What is the scale of the drawing?

	Answer
	1:100
	



Q53.  [bookmark: _Ref427733995]What does the drawing show?

	Answer
	FOUR ELEVATION VIEW OF THE HOUSE
	



Q54.  [bookmark: _Ref427734110]Which view shows the front of the house?

	Answer
	EAST ELEVATION
	



Q55.  [bookmark: _Ref427734113]How many motor vehicles can be parked in the garage?

	Answer
	2
	



Q56.  [bookmark: _Ref427734114]What are the window and doors made from?

	Answer
	Aluminum and timber
	



Q57.  [bookmark: _Ref427734116]What is the size of the eaves?

	Answer
	450mm
	


Q58.  [bookmark: _Ref427734119]What are the eaves lined with?

	Answer
	Hardiflex cement board
	



Q59.  [bookmark: _Ref427734120]What type of roof structure is the roof built from?

	Answer
	timber framed with concrete tiles covering
	



Q60.  [bookmark: _Ref532197046]Which Part of the NCC should be read for more detail about the requirements for the roof structure in Q59.?

	Answer
	 NCC 2019 Volume Two Amendment 1 Part 3.3.6

	



Q61.  [bookmark: _Ref532197154]Which Australian Standard should be read for more detail about the roof structure in Q59. ?

	Answer
	AS 4773.1 and AS 4773.2
	



Q62.  [bookmark: _Ref427734122]What is the roof cladding materials made from?

	Answer
	Concrete roof tiles
	



Q63.  [bookmark: _Ref532197156]Which Part of the NCC should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	NCC-2019-Volume-Two,Part 3.5 Roof and wall Cladding 
	



Q64.  [bookmark: _Ref532197157]Which Australian Standard should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	-Roofing tiles: AS 2049 and AS 2050
-Metal roofing: AS 1562.1
-Plastic sheet roofing: AS/NZS 4256 Parts 1, 2, 3 and 5; and AS/NZS 1562.3
-Corrugated fibre-reinforced cement sheet roofing: AS/NZS 1562.2
-Asphalt shingles: ASTM D3018-90
-Pliable membrane and underlay: AS/NZS 4200 Parts 1 and 2

	



Q65.  [bookmark: _Ref427663512]What is the roof pitch?

	Answer
	22.5°
	



Q66.  [bookmark: _Ref531871432]Identify one (1) regulatory body you may need to submit plans to for approval?

	Answer
	City Council for building approvals
	



Q67.  [bookmark: _Ref532197251]Briefly describe the approval process and timeframes for an approval through the regulatory body in Q66. 

	Answer
	Building approvals require assessment against the Building Code of Australia (forming Volumes 1 and 2 of the National Construction Code) and Queensland’s building and plumbing regulations.
While building approvals are usually only issued once for a specific structure or building, building legislation may require various technical inspections at different stages of the building process, including completion. 
	



Q68.  [bookmark: _Ref427673788]What is a prime cost (PC) item? Give an example.

	Answer
	A PC item is:
An amount of money included in a contract sum to purchase a specified item such as tiles, taps, doors or bathroom fittings
An agreed estimated amount is included at contract signing but the specific products are not selected until a later stage
A builder must estimate the cost of such items at or above the lowest amount these items could reasonably cost
For example if a client selects a more expensive door than allowed by the PC item, say a $500 door compared with a $440 PC amount, a variation will be required to cover the additional $60.  If the PC item varies, so will the final contract sum.


	



Q69.  [bookmark: _Ref427673790]What is a provisional sum (PS) item? Give an example.

	Answer
	A provisional sum is:
An amount of money included in contract sum to cover work and/or materials, not detailed when entering the contract
Typically builders will include a PS for site work costs
The builder is legally required to take reasonable steps to ensure an accurate site works cost estimate but unforeseen events mean that the provisional sum is exceeded which is added to the contract sum

For example a building site may seem sandy and clean with minimal siteworks required, however, there may be large limestone rocks/tree trunks concealed below the surface which only emerge once siteworks commence, causing cost overrun.
	


Refer to the Bill of Quantities below to respond to Q70. to Q76. 

[image: ]
[image: ]

Source: http://organizedbuilders.com.au/sites/default/files/BOQ-Summary.pdf 



Q70.  [bookmark: _Ref531867328]True or False (Tick your response): This Bill of Quantities represents a job for a two-storey house.

	Answer
	þ	True 
	
	
	
	¨	False 
	
	




Q71.  [bookmark: _Ref532199102]Identify two (2) materials being used for the floors?

	Answer
	Floor trusses
Carpet, vinyl&floating floors
	



Q72.  [bookmark: _Ref532199110]True or False (Tick your response): A landscaper has been contracted for this job.

	Answer
	þ	True 
	
	
	
		False 
	
	




Q73.  [bookmark: _Ref532199056]How much does the contracted plasterer cost?

	Answer
	$12900.00
	



Q74.  [bookmark: _Ref532199058]How much do the kitchen appliances cost?

	Answer
	$2700.00
	



Q75.  [bookmark: _Ref532199060]What percentage of the total cost does the fixing stage represent of the building contract?

	Answer
	23%
	



Q76.  [bookmark: _Ref531866973]What percentage of the total cost does the completion stage represent of the building contract?

	Answer
	17%
	


Refer to the Purchase Order below to respond to Q77. to Q82. 

[image: ]
Source: http://organizedbuilders.com.au/sites/default/files/Databuild-Bill-of-Quantities.pdf 

Q77.  [bookmark: _Ref531874116]How many Pine F5 90 x 45 studs (2.4m long) are required?

	Answer
	100
	



Q78.  [bookmark: _Ref532199470]If the material in Q77. increased in cost to $2.75 each, what would be the total cost for this material?

	Answer
	$2750.00
	



Q79.  [bookmark: _Ref532199474]How many sheet of ply are required in total (i.e. all sizes)?

	Answer
	13
	



Q80.  [bookmark: _Ref531874121]What material has the highest total cost?

	Answer
	90*45 KDHW F17
	



Q81.  [bookmark: _Ref531874448]How many metres are required of the material in Q80. ?

	Answer
	189.3M
	



Q82.  [bookmark: _Ref531874565]What beam is identified as being a better option than F17?

	Answer
	E14
	




Refer to the labour chart below to respond to Q83. to Q86. 

[image: ]
Source: https://www.archsd.gov.hk/media/89170/sor2013_vol1_builders_works_2013_11_04.pdf 



Q83.  [bookmark: _Ref531873766]Based on the hourly rates given, which is the least expensive trade to contract?

	Answer
	ASPHALTER(ROAD CONSTRUCTION) 
	



Q84.  [bookmark: _Ref532199773]If the trade in Q83. were to be contracted for two (2) hours’ work, how much would this cost?

	Answer
	$214.8
	



Q85.  [bookmark: _Ref531873865]Based on the hourly rates given, which is the most expensive trade to contract?

	Answer
	Carpenter(foam work - building construction)
	



Q86.  [bookmark: _Ref531873882]If the trade in Q85. were to be contracted for six (6) hours’ work, how much would this cost?

	Answer
	$1206.60
	



Q87.  [bookmark: _Ref531691201]Name the building legislation (Act and Regulations) that apply within your jurisdiction and should be referenced when reading plans and building contracts.

	Answer
	Building Act 1975
Building Regulation 2006
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Junquan Chen

	
	

	Participant signature
	
	
	

	Date
	7/11/2020



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4012B
Read and interpret plans and specifications

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to read and interpret plans and specifications in order to inform estimation, planning and supervisory activities. 

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include:
· Any drawing with a cloud or mark-up you have inserted.
· Copy of the correspondence regarding mark up and any site management/authorising engineer response.

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Drawings (including site plan), Specifications, Tender documentation, Telephone, Facsimile machine, Computer. 

	Assessment of task

	Name of participant:
	Junquan Chen

	Name of observer:
	Yixu Zhang

	Role of observer 
(Confirm suitability to sign)
	Project Manager

	Email address of observer
	Zhangyixu1015@gmail.com

	Signature of observer:
	
	Date:
	8/11/2020
	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Interpret drawings

	1.1A.  [bookmark: _Ref531698368]Identify purpose and advantage of different types of drawings.
	þ	þ
	1.1B.  Identify different aspects of drawings.
	þ	þ
	1.1C.  [bookmark: _Ref531698394]Identify, understand and apply:
· Commonly used symbols and abbreviations
· Common building and construction terms on drawings
	þ	þ
	1.1D.  [bookmark: _Ref531698402]Identify building site from location drawings.
	þ	þ
	1.1E.  [bookmark: _Ref531698498]Identify on the site plan:
· True north
· Building orientation
· Key features in relation to building and other structures
· Levels
· Contours
· Service entry points
· Site features to be removed or retained
	þ	þ
	1.1F.  [bookmark: _Ref531698586]Identify key features of plans, elevations and sections.
	þ	þ
	1.1G.  [bookmark: _Ref531698588]Identify client requested variations to standard plans on drawings.
	þ	þ
	2 Interpret specifications 

	1.2A.  [bookmark: _Ref531698592]Identify and correctly apply Provisional Sum (PS) and Prime Cost (PC) values. 
	þ	þ
	1.2B.  [bookmark: _Ref531698596]Identify and confirm customer variations to standard specifications and communicate changes to organisational personnel. 
	þ	þ
	1.2C.  [bookmark: _Ref531698601]Apply and communicate correct interpretations of essential elements to estimation, planning and supervisory tasks (including labour hours/costs and material quantities/costs).
	þ	þ
	1.2D.  [bookmark: _Ref531698605]Identify Building Codes or standards affecting the work to be undertaken (including references to Australian Standards and the National Construction Code). 
	þ	þ
	1.2E.  [bookmark: _Ref531698612]Identify key features of products included in the specification, including the design, purpose, aesthetics and cost relationships. 
	þ	þ
	3 Communicate with others

	1.3A.  [bookmark: _Ref531698617]Consult with industry professionals, clients, organisational personnel and appropriate local authorities.
	þ	þ
	1.3B.  [bookmark: _Ref530479080]Effectively communicate using the following methods:
· Verbally using language/concepts appropriate to cultural differences
· Non-verbal communication
· Using technology (including telephone, facsimile, email)
	þ	þ
	The Participant’s performance was: þ Satisfactory     Not Satisfactory



	OBSERVER COMMENTS

	Junquan Chen is very good at identifying all types of drawing. He can  read the site plan properly.
[bookmark: _GoBack]He also did well on arranging materials  and labour, communicating with customers about variations. He is familiar with Building Codes or standards . 
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