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CPCCBC4001A 
Apply building codes and standards to the construction process for low rise building projects


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	Date
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	Number of questions
	Number of questions answered correctly
	Satisfactory?

	35
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	[bookmark: _Ref396827952]ASSESSOR COMMENTS

	


[bookmark: _Ref423932567]The diagram below represents an external house wall, shows part of roof and eave and a window in the wall and the vertical boundary line fence is shown a prescribed measurement of 900mm from the house wall to allow light from the sun to reach the window. 

[image: ]

What type of regulation could allow a lesser distance to be used if appropriate justification was provided?

In what document/s might you find the appropriate information?

	Answer
	A performance-based regulation could allow a lesser distance to be used if appropriate justification was provided. You would find the appropriate information in the performance based regulations of the BCA.
	



[bookmark: _Ref423933353]In regard to the above 900mm distance from house wall to boundary fence and in using or referencing performance-based regulations in the BCA what else should you be aware of and consider? 

	Answer
	Fire separation, fire resistance levels and external walls and boundaries that may be subject to govern planning laws.
	


[bookmark: _Ref423934890]Who has responsibility for producing and maintaining The Building Code of Australia (BCA) and who is it done on behalf of? 

	Answer
	It is produced and maintained by the Australian building codes board on behalf of the commonwealth government and each state and territory government.
	



[bookmark: _Ref423934988]Fill in the missing words to complete the following two sentences. 
provisions
technical

a. The BCA is a uniform set of ___________ ______________ for the __________ and ______________ of buildings and other structures throughout Australia. Design		
construction
document
Performance based document

b. It is a ______________________ ________________ that is referenced so that your building system or material can demonstrate that it meets certain performance requirements in order to meet __________________ ____________________.legislative
requirements


	Answer
	
	



[bookmark: _Ref423935105]What is the principal goal of the Building Code of Australia (BCA)?

	Answer
	BCA’s goal is to enable the achievement of nationally consistent, minimum necessary standards of safety, health, amenity and sustainability objectives.
	



[bookmark: _Ref423935280]How many volumes are there in the BCA and to what do the volumes refer?

	Answer
	There are two volumes and they refer to access requirements for people with a disability in class 1b and 10a buildings. Structures including access requirements for people with a disability in class 10b swimming pools. Class 1 and 10a buildings, certain class 10b structures other than access requirements for people with a disability in class 10b. class 10c.
	


[bookmark: _Ref423935639]Explain the BCA performance requirements for low rise projects from the diagram below.
[image: ]

	Answer
	The performance requirements are the core of the BCA, they outline a suitable level of performance for building materials, design factors and construction methods so a building can meet the relevant functional statements and the relevant objectives.
	


[bookmark: _Ref423936447]What is the intent of the ‘Relevant Performance Requirements’ in the BCA?

	Answer
	The intent of the relevant performance requirements is to set out the method of determining the appropriate performance requirements to be used when an alternative solution is used to prove that a building solution complies with the BCA.
	



[bookmark: _Ref423936842]Building solutions set out the means of achieving compliance with the performance requirements. The BCA provides for two methods that can be followed to develop a building solution. Explain these two methods.

	Answer
	1.Deemed to satisfy provisions, these include examples of materials, components, design factors, and construction methods which if used will result in compliance with the performance requirements of the BCA.  2.Alternative solutions, the key to performance-based is there is no obligation to adopt a particular material, design factor or construction method. An approval authority may still issue approval if a building proposal differs in whole or in part from deemed to satisfy provisions described in the BCA and if it can be demonstrated that the design complies with the relevant performance requirements.

	



[bookmark: _Ref423937248]The deemed-to-satisfy building solution establishes a clear and concise process for compliance for a builder, building surveyor or the like (building certifier) who does not want to develop a new means of achieving performance requirements; what does ‘deemed-to-satisfy’ mean?

	Answer
	If a builder does not want to develop a new means of achieving performance requirements may choose to adopt the deemed to satisfy building solution as outlined in the BCA. This means that the building solution complies with an equivalent or superior way to a deemed to satisfy provision.
	


[bookmark: _Ref423937619]Write an example of a ‘deemed-to-satisfy’ provision for a class 1 building including deemed-to-satisfy requirements for kitchen, bathroom, laundry and sanitary facilities.

Nominate where you found the information in the BCA.

	Answer
	A class 1 building must provide a kitchen sink and facilities for the preparation and cooking of food, a bath or shower, clothes washing facilities with at least one wash tub and space in the same room for at least one washing machine, a closet pan and wash basin. Found in volume 2 page 2, facilities.
	


[bookmark: _Ref423937984]Who and what is Standards Australia?

	Answer
	Standards Australia is Australia’s peak standards body recognised through a memorandum of understanding with the commonwealth government. It is an independent, non- profit, non- government organisation. In consultation with government, business, industry, community, academia and consumers, standards Australia develops internationally aligned Australian standards and related publications to help ensure the safety, reliability and performance of a range products, services and systems.
	



[bookmark: _Ref423937985]What are Australian Standards?

	Answer
	They are published documents setting out specifications and procedures designed to ensure products, services and systems are safe, reliable and consistently perform the way they were intended to.
	


[bookmark: _Ref423939945]The classification of a building or part of a building is determined by the purpose for which it is designed, constructed or adapted to be used. Please summarise the 10 building classifications below.

	Answer
	Class
	Summary
	
	
	1
	One or more buildings in association constitute, class 1a single dwelling, class 1b boarding house, hostel.
	

	
	2
	A building containing two or more sole-occupancy unit each being a separate dwelling.
	

	
	3
	A residential building, other than a building of class 1 or 2, which is a common place of long term or transient living for a number of unrelated persons, e.g boarding house, school. 
	

	
	4
	A dwelling in a building that is class 5, 6, 7, 8 or 9 if it is the only dwelling in the building.
	

	
	5
	An office building used for professional or commercial purposes, excluding building of class 6, 7, 8, or 9.
	

	
	6
	AA shop or other building for the sale of goods by retail or the supply of services direct to the public.
	

	
	7
	Abuilding which is class 7a (a car park) or class 7c (the storage or display of goods or produce for sale.
	

	
	8
	A laboratory or building for the production, assembling, altering, repairing, packing, finishing or cleaning of goods for sale.
	

	
	9
	A building of public nature, class 9a, health care building, Class 9b assembly building. Class 9c aged care building.
	

	
	10
	A non-habitable building or structure. Class 10a, non-habitable building. Class 10b post, pool, fence. Class 10c, shelter.
	




[bookmark: _Ref423940316]Other than the 10 BCA building classifications (A3.2), there are also multiple classifications (A3.3) where each part of a building is classified separately. 

Where would you find a full list of Past A3 classification of Buildings and Structures?

	Answer
	It can be found within the BCA.
	



[bookmark: _Ref423946303]True or False (Tick your response): If a building or part of a building has more than one classification applying to the whole building or part in accordance with, that building or part must comply with all the relevant provisions of the BCA for each classification.

	Answer
	☒	True 
	
	
	
	☐	False 
	
	




[bookmark: _Ref423941205]Familiarity with plans and specifications for a project when interpreting a building solution and therefore trying to interpret clauses and other referenced documents in the BCA is important.

What do plans and specifications include?

	Answer
	They include floor level plans, elevation plans, sectional drawing and all specifications.
	



[bookmark: _Ref423941402]You must have a clear picture of the building to be constructed and be able to identify the criteria that you will need to compare to the Deemed-To-Satisfy (DTS). What is it you must also consider when constructing complex buildings?

	Answer
	When constructing complex buildings you must consider that requirements of one BCA clause may have an impact of the requirements of another.
	




[bookmark: _Ref423941611]Complete the missing words from the sentence below and explain the difference between these points. 
mandatory

BCA Performance Requirements are _________________ and Deemed-to-Satisfy provisions are ______________. optional


	Answer
	BCA performance requirements are procedures you must follow to comply with the BCA standards and deemed-to-satisfy provisions are changes made that meet or exceed the BCA standards.
	 




[bookmark: _Ref423941845]What is a Building Solution?

	Answer
	A building solution means a solution which complies with the performance requirements and is an alternative solution or a solution that complies with deemed-to-satisfy provisions, or a combination of both.
	



[bookmark: _Ref423942068]Referring to the BCA, what are the objectives of Section C Fire Resistance?

	Answer
	The objective is to ensure that during a fire the risk to people is minimised, evacuation routes are provided, emergency services personnel can undertake search and rescue operations, the risk of fire spreading is minimised, structural failures (buildings, allotment, roads) does not occur.
	



[bookmark: _Ref423942460]Why is it necessary to identify and document performance-based solutions?

	Answer
	In order to comply with organisational quality procedures and processes, apply and interpret relevant documentation and codes, acuratley apply national state and territory OHS requirements relating to construction workplace, identify faults and problems impacting on OHS proposing appropriate action to rectify.
	



[bookmark: _Ref423942735]In the context of the Building Code of Australia what are Assessment Methods used to determine?

	Answer
	Assessment methods are used to determine whether a building solution complies with the relevant BCA performance requirements. 
	



[bookmark: _Ref423943044]Explain the importance of maintaining detailed documentation for a building project.

	Answer
	It is important that you maintain a detailed level of documentation to ensure that the building is compliant and can pass assessment. The ability to a detailed documentation provides a vital reference tool required for inspections of key building elements, this ensures they are not inadvertently overlooked.  
	


[bookmark: _Ref423943211]With regard to detailed documentation what are some of the documents that must be provided and maintained by contractors?

	Answer
	Clearly document in the plans all calculations of building areas, site areas, site coverage, floor areas, building heights, habitable rooms. Contain full details of any alternative solutions proposed. Contain all submissions necessary in support of the exercise of discretionary under either national, state or territory regulations.
	



[bookmark: _Ref423943524]Other than the Builder maintaining detailed documentation, who will also have responsibility to resolve and correct errors for any ambiguity identified in the plans?

	Answer
	A building certifier. 
	



[bookmark: _Ref423943842]The threat of an accidental fire in a building and to prevent it are important to understanding fire and taking all steps to prevent or confine fire and to prevent fire spreading within the structure as well as to adjoining or adjacent buildings. 

In this regard Fire Protection Systems are paramount and are subject to?

	Answer
	Building regulations, fire regulations, insurance regulations, local government regulations, other regulatory authorities.
	



[bookmark: _Ref423943887]Briefly explain the following fire definitions:

	Answer
	Term
	Explanation
	
	
	Fire
	Fire is the rapid oxidation of a gas, liquid or solid substance.
	

	
	Passive Fire Protection
	Is an integral component of the three components of structural fire protection and safety in the building.Passive fire protection is an integral component of the 3 componants of structural fire protection and fire safety of a building. 
	

	
	Active Fire Protection
	Is an integral part of fire protection and is characterised by items and systems which require a certain amount of motion and response in order to work.Is an integral part of fire protection and is characterised by items and systems which require a certain amount of motion and response in order to work.
	



[bookmark: _Ref423944362]The purpose of fire protection is to: 
1. Prevent/reduce the possibility of fire and 
2. Reduce the spread of fire within and around a building

Name the two categories or systems that provide measurement and arrangements for fire protection.

	Answer
	Active systems, which are portable fire extinguishers, fire hydrants, sprinkler systems, smoke alarms. Passive systems which are fire isolated stairs and passageways, fire resistant materials, fire doors, fire curtains, fire rated ceilings and fire stop collars.
	



[bookmark: _Ref423944529]With respect to the general level of fire protection explain separately the terms ‘Fire Load’ and ‘Fire Load Density’?

	Answer
	Fire load refers to the amount of potential heat that can be liberated during the fire of the combustible contents of a given enclosure. It is expressed that a numerical value represented as kj/kg kilojoule per kilogram, or as mj/mk megajoules per kilogram. Fire load density is the fire load of a given enclosure or building divided by floor area. It is expressed as a fire load per unit area of floor space (the greater the fire load the more severe the fire. 
	


[bookmark: _Ref423944839]Using Volume 2 of the BCA respond to the following:
a) Where in the BCA would you look to find requirements for building in bushfire prone areas for Class 1 and 10 buildings? 
b) Where in the BCA would you look to find requirements for building in bushfire prone areas for Class 2-9 buildings? 
c) What Australian Standard must be complied with to satisfy the Deemed to Satisfy Provisions for construction of Class 2 and 3 buildings in bushfire prone areas?

	Answer
	a)
	In part 2.3.4 page 289. Volume 2
	
	
	b)
	Section C, volume1
	

	
	c)
	Steel frame construction.
	




[bookmark: _Ref423945259]What is a Fire Safety Schedule and its relationship to the approval of development of a class 2 – 9 building?

	Answer
	[bookmark: _GoBack]Upon approval of development of a class 2-9 building, a fire safety schedule is issued, which lists all the general fire safety measures that should be in stalled in the building and the performance standard which each of these measures must capable of operating.
	



[bookmark: _Ref423945523]What are building certifiers responsible for?

	Answer
	Building certifiers are responsible for ensuring specific compliance is achieved and they do this by conducting visual inspections.
	



[bookmark: _Ref423945524]What are building certifiers not responsible for?

	Answer
	Building certifiers are not responsible for the workmanship on the building.
	



[bookmark: _Ref423945635]Where in the BCA would you determine the level of fire resistance required for the construction of buildings?

	Answer
	Volume one, section C and volume two part 3.7.
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