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Documentation of design and construction (suitability or evidence of suitability)
	Project Name: Card Street 

	Project address: 14 card street 
	Site Plan attached: no

	Prepared by: Jerremy Tydd

	Date: 10-01-2024

	Description of project:
New house Build


	Site Classification/s:
class 1a 

	Documentation of design and construction (suitability or evidence of suitability)

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earthworks
	National Construction Code Part 3.1.1 earthworks 
	The provisions in Part 3.1.1 will enable earthworks associated with the construction of a building to be carried out safely and to avoid potential damage to the subject building, adjoining structures and property through the soil collapsing or subsiding.

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earth retaining structures
	National Construction Code Part 3.1.2 Earth retaining structures 
	Where an alternative earth retaining structure design is proposed as a Performance Solution to that described in Part 3.1.2

	Drainage
	Part 3.1.3 Drainage 
	Where an alternative drainage system is proposed as a Performance Solution to that described in Part 3.1.3

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Termite risk management
	Part 3.1.4 Termite risk management 
	Compliance with this acceptable construction practice satisfies Performance Requirement P2.1.1 for termite risk management.

	Materials
	termite management systems
	for wood protection against termites, chemicals with active ingredients like borate, fipronil, or bifenthrin are commonly used

	Footings and slabs

	Site classification: 

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Footings and slabs
	Part 3.2 Footings and slabs 
	Where an alternative footing system is proposed as a Performance Solution to that described in Part 3.2

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Moisture Barrier
	Part 3.2.2 Preparation
	Excavation for footings, including thickenings for slabs and pads must be clean cut with vertical sides, wherever possible.

	Materials
	Damp course 
	The vapour barrier must be VCM Class 1 to AS/NZS 4200.1 and be classified as Water Barrier to AS/NZS 4200.1 and provide moisture proofing, including at laps, at edges and at penetrations through the vapour barrier membrane.

	Concrete and reinforcement

	Concrete and reinforcement
	NCC / Australian Standards requirements
	Compliant Performance solution

	Concrete and reinforcement
	Part 3.2.3 
	Concrete must be manufactured to comply with AS 3600; and— Materials used for reinforcing steel must comply with AS 2870.

	Materials
	Concrete, mesh 
	Concrete must be placed, compacted and cured in accordance with good building practice.

	Masonry

	Masonry
	NCC / Australian Standards requirements
	Compliant Performance solution

	Masonry
	Part 3.3 masonry 
	Must comply with part 3.3 NCC 

	Moisture Barrier
	Part 3.3.4
	

	Materials
	
	

	Framing/Structure

	Framing/Structure
	NCC / Australian Standards requirements
	Compliant Performance solution

	Framing
	Part 3.4.4 Timber Framing 
	Where an alternative timber framing design is proposed as a Performance Solution to that described in Part 3.4.3, that proposal must comply with—
a. Performance RequirementP2.1.1


	Materials
	timber framing, including the use of concrete floors, structural steel support beams,
	

	Roof and Wall Cladding

	Roof and wall cladding
	NCC / Australian Standards requirements
	Compliant Performance solution

	Roof and wall cladding
	Part 3.5 Roof and wall cladding 
	This Part contains requirements including weatherproofing and structural requirements, for roof and wall systems. Gutter and downpipe requirements are also contained in this Part.

	Materials
	Gutter 
Roof batten
Sheet roofing 
	

	Glazing

	Glazing
	NCC / Australian Standards requirements
	Compliant Performance solution

	Glazing
	Part 3.6 Glazing 
	Glazing used in areas where the potential for human impact could occur must comply with the appropriate provisions listed in 3.6.4.

	Materials
	Glass 
	

	Fire Safety

	Fire Safety
	NCC / Australian Standards requirements
	Compliant Performance solution

	Fire Safety
	Part 3.7 Frie Safety 
	The fire hazard properties of materials used in a Class 1 building, including floor or ceiling spaces common with a Class 10 building

	
	Smoke alarms. 
Plaster board 
	

	
	
	

	Access/Stairs/Lifts/Ramps

	Access/Stairs/Lifts/Ramps
	NCC / Australian Standards requirements
	Compliant Performance solution

	Access
	Part 3.9
	Room heights:
3.8.2.2 contains the required height for a ceiling above a stairway, ramp or landing, measured vertically above the nosing line of stairway treads or the floor surface of a ramp or landing.


	
	
	Alpine areas:
The requirements of this Part are to be read in conjunction with Part 3.10.4 where a building is located in an alpine area and contains an external stairway or ramp.


	Materials
	Timber 
Steel 
	

	Ancillary Provisions

	Ancillary Provisions
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	Part 3.10.1 
	Performance RequirementP2.7.1 is satisfied for a swimming pool with a depth of water more than 300 mm and which is associated with a Class 1 building, if it has safety barriers installed in accordance with AS 1926.1 and AS 1926.2

	
	
	

	
	
	

	Energy Efficiency

	Energy Efficiency
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	Part 3.1.2 Energy Efficiency 
	in the case of a new Class 1 building, having either a rainwater tank connected to all sanitary flushing systems, or a solar water heater system, installed in accordance with the Plumbing Regulations 2018.

	
	
	

	
	
	

	Health and Safety

	Part 3.8 Health and Amenity 



	Consultation

	

	Policies

	In Queensland, the Work Health and Safety Act 2011, Work Health and Safety Regulation 2011, and industry specific Codes of Practice set out the minimum rules for managing health and safety in a workplace.

	Procedures

	Follow all work place procedures 

	Issues to be addressed and consultation

	Issue
	Who to consult
	Improvements for consideration
	Feedback following consideration
	Supporting Resources

	No issues 
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