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ASSESSMENT SUMMARY

The assessment activities for CPCCBC4010B Apply structural principles to residential low rise constructions & CPCCBC4011B Apply structural principles to commercial low rise constructions cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 
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	THEORY EXAM INSTRUCTIONS

1. This exam will occur under standard assessment conditions.
1. An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
2. Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
3. Please fill in the details below, providing your name, signature and date of assessment.
1. Your signature acknowledges that this is your own work.
4. Assessors are to complete marking in pen of a different colour to the Participant.
5. If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
1. If a Participant changes their response in writing, they must put their initials next to the written change.
2. If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
	Callum Quinn

	
	

	Participant signature
	
	
	

	Date
	1/12/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	93
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


1. What is the most important aspect in the design of buildings? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Aesthetics
	

	
		Cost
	

	
		Location
	

	
		Stability
	




1. [bookmark: _Ref531083005]Where can the definitive properties of materials used in the building industry be found? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Australian Standards
	

	
		Building journals
	

	
		Practical learning on the job
	

	
		Textbooks on building
	




1. [bookmark: _Ref427229923]Which industry professional would you contact for structural advice? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Architect
	

	
		Draftsperson
	

	
		Engineer
	

	
		Quantity surveyor
	




1. [bookmark: _Ref531353369]Which industry professional would you contact for the preparation of working drawings? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Building surveyor
	

	
		Draftsperson
	

	
		Quantity surveyor
	



1. [bookmark: _Ref427229919]Briefly describe the role of an architect.

	Answer
	Architects are people who design buildings and in many cases also supervises their construction. They help you to set a viable and realistic budget, guide you through the planning process and obtain competitive quotes and manage consultants. 

	



1. [bookmark: _Ref427229924]What is the difference between a building surveyor and a land surveyor?

	Answer
	Building surveyors provide professional advice on property and construction, which spans across residential, commercial, industrial, leisure and agriculture projects whereas land surveyors specifically survey terrain and landscape for the purpose of development 
	



1. [bookmark: _Ref427229926][bookmark: _Ref531353386]Which industry professional would you contact for matters relating to cost? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Architect
	

	
		Building surveyor
	

	
		Engineer
	

	
		Quantity surveyor
	



1. [bookmark: _Ref531353744]A land surveyor is to reinstate survey pegs. Which of the following documents would the surveyor need? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Title
	

	
		Contour plans
	

	
		Project specifications
	




1. [bookmark: _Ref531353745]When preparing a trench a builder digs through a gas pipe which was not shown on the plans. Which report should be used to prove the mistake was not the builder’s? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Engineer’s drawings
	

	
		Condition report
	

	
		Soil report
	




1. [bookmark: _Ref427230180][bookmark: _Ref531353749]Which two (2) of the following can be determined from the contour report? Tick your responses.

	Answer
	Choice
	Possible Answers
	
	
		Extent of cut and fill
	

	
		Height of retaining walls
	

	
		Location of trees
	

	
		Location of windows
	




1. [bookmark: _Ref531353759]The customer has requested a glass balcony. Which document would the builder refer to for information on structural members? 
Tick your response. 

	Answer
	Choice
	Possible Answers
	
	
		Building specifications
	

	
		Condition report
	

	
		Engineering report
	



1. [bookmark: _Ref427230170][bookmark: _Ref531353761]The builder is planning a project and requires information on the location of fixtures and fittings, windows and doors. Which plans show this information? Tick your response. 

	Answer
	Choice
	Possible Answers
	
	
		Cross sections
	

	
		Floor plans
	

	
		Footing designs
	




1. [bookmark: _Ref427230166][bookmark: _Ref531353766]After an inspection, the client believes that what was installed is different to what they had chosen in the contract. What document details the materials the builder was meant to use? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Building specifications
	

	
		Plan of the subdivision
	

	
		Site plan
	




1. [bookmark: _Ref427579066][bookmark: _Ref531353770]What key pieces of information can be found on a site plan? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Location of street frontage
	

	
		Location of proposed building
	

	
		North point
	




1. [bookmark: _Ref427230177]What is the purpose of a footing design?

	Answer
	To ensure that the concreting contracting or carpenter installs the correct quantity of the correct material in a way that an engineer has designed them to safely handle all load requirements. 
	



1. [bookmark: _Ref531354185]Why would a pre-commencement site inspection be conducted? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		To ensure all contract documentation clearly reflects the actual site
	

	
		It allows the supervisor to get some fresh air
	

	
		To ensure that the client actually owns the property
	

	
		So that levels can be taken to check the slope of the site
	




1. [bookmark: _Ref531082938]What are the dead loads in a building? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		All stationary materials
	

	
		Permanent materials
	

	
		Roofing materials
	

	
		Use for which the building is intended
	




1. [bookmark: _Ref531082940]What is the formula for calculating a dead load?

	Answer
	Dead load = Volume of member x Unit weight of materials (supplied)
	



1. [bookmark: _Ref531082941]What are the live loads in a building? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Loads arising from the function of the structure
	

	
		Loads due to rain
	

	
		Loads due to wind
	

	
		Utility services
	





Refer to the table shown below to respond to Q20. to Q21.  These values are used to calculate live loads using the formula: Area of floor x Live load rating.

	Live loads for floors as per building usage
	Uniformly distributed load (kPa or kN/m²)

	Houses
	1.5

	Flats, motel bedrooms, apartments
	2.0

	Offices
	3.0

	Workshops
	5.0

	Parking, vehicle >2.5t
	5.0

	Hospitals, school assembly areas with fixed seating
	3.0

	Dance halls, bars, lounges
	5.0




1. [bookmark: _Ref481992592]Calculate the live load of a guest house measuring 23m x 8m. 
Show your calculations.

	Answer
	28*8= 224m2 Assuming a guest house is motel it has live load rating of 2 

So 2*224 =488kN
	



1. [bookmark: _Ref427215838]Calculate the live load of a commercial office premises floor measuring 33m x 11m. Show your calculations.

	Answer
	33*11 = 363m2 Offices have a live load rating of 3 so 363*3=1089kN
	



Please refer to the information below in responding to Q22. to Q25. 

There is a building 21m long x 10m wide x 8m high with a 25⁰ pitched gable roof. The rafter line on the metal clad roof measures 5.5m on the rafter line (from the fascia/gutter line up to the ridge line).

The wind load is calculated as Area of surface x Wind load rate. The wind load rates are as follows:
1. Windward wall is 21 metres long x 8 metres high with a wind load rate of +1.5KN/m²; 
1. Leeward wall is 21 metres long x 8 metres high with a wind load rate of -0.8kN/m²; 
1. Windward roof with a wind load rate of +0.8kN/m²; and 
1. Leeward roof with a wind load rate of -1.5kN/m²



1. [bookmark: _Ref427218342]What is the wind load of the windward wall? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-252kN
	

	
		134.4kN
	

	
		252kN
	

	
		86.4kN
	




1. [bookmark: _Ref427218344]What is the wind load for the leeward wall? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-134.4kN
	

	
		-94.2kN
	

	
		252kN
	

	
		134.4kN
	




1. [bookmark: _Ref427218346]What is the wind load for the leeward roof? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-173.25kN
	

	
		92.4kN
	

	
		173.25kN
	

	
		-134.4kN
	




1. [bookmark: _Ref427057362]What is the wind load for the windward roof? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		252kN
	

	
		-92.4kN
	

	
		-252kN
	

	
		92.4kN
	





1. [bookmark: _Ref427217924]Explain the term ‘load path’ in reference to a building.

	Answer
	The load path is the direction in which each consecutive load will pass through connected members. The sequence commences at the highest point of the structure, working all the way down to the footing system – ultimately transferring the total load of the structure to the foundation. So the lowest structural member must be strong enough to support all the members above it. 

	



1. [bookmark: _Ref427219307]Forces are represented as vectors and have three (3) properties. 
Name these properties.

	Answer
	1. Magnitude – the size of the force
2. Direction – the direction of the force
3. Position – the place where the force acts

	



1. [bookmark: _Ref427219642]Name five (5) structural members that a building may consist of.

	Answer
	Beams
Columns
Retaining walls
Concrete slabs
Roof trusses
	


1. [bookmark: _Ref427219933]What should be considered when determining the shape and type of material to use?

	Answer
	Section properties involve the mathematical properties of structural shapes and must be considered when analysing and designing structures. 

	



1. [bookmark: _Ref427220471]Match the mechanical properties and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Mechanical properties
	Answers
	Definitions
	
	
	1
	Brittleness
	1 - G
	A
	The resistance the structural member is able to offer the load that will just cause fracture. 
	

	
	2
	Elasticity 
	2 - C
	B
	The resistance to a fracture point of a material by repeated bending or twisting after yield point has passed.
	

	
	3
	Ductility
	3 - E
	C
	Present if a material deforms with loading and then returns to its original shape when the loads are removed.
	

	
	4
	Hardness 
	4 - H
	D
	If a material deforms when loaded and does not return to its original shape when the load is removed, causing permanent deformation. 
	

	
	5
	Malleability
	5 - F
	E
	Enables a material to be drawn out in the direction of its length. 
	

	
	6
	Plasticity
	6 - D
	F
	Can be hammered or otherwise worked into various shapes.
	

	
	7
	Strength
	7 - A
	G
	Causes material to break or snap off without any noticeable lengthening. 
	

	
	8
	Toughness
	8 - B
	H
	The degree of resistance to indentation or abrasion. 
	




1. [bookmark: _Ref427220295]Match the beam types and descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Beam type
	Answers
	Description
	
	
	1
	Cantilevered 
	1 - A
	A
	Overhang their supports.
	

	
	2
	Continuously supported
	2 - C
	B
	Supported at each end only.
	

	
	3
	Simply supported
	3 - B
	C
	Supported by 3+ support points. 
	



1. [bookmark: _Ref427225888]Match the column considerations and explanations by writing the appropriate letter next to each number in the centre column.

	Answer
	Column consideration
	Answers
	Explanation
	
	
	1
	Axially loaded column
	1 - 
	A
	The load is central to the centre of gravity axis. 
	

	
	2
	Buckling
	2 - 
	B
	The load is off-centre, resulting in bending and compressing stress being applied to the column.
	

	
	3
	End fixity and effective length
	3 - 
	C
	The rigid connection to other members at the top and bottom affects the way a column buckles.
	

	
	4
	Non-axially loaded column
	4 - 
	D
	Affects the maximum load a column can be allowed to support.
	

	
	5
	Slenderness ratio
	5 - 
	E
	Occurs at the weakness axis unless a lateral restraint is used to prevent it. 
	




1. [bookmark: _Ref427224602]Explain how a column is in compression.

	Answer
	When a beam carries loads, complex stresses build up and the bending that results from the loading causes beam fibres to:
carry tension - these are called tensile forces
carry compression - these are called compressive forces
take shear forces.
Structural engineers consider bending, shear and deflection

The top till be subject to compressive tension and the bottom will be having it’s tensile strength tested. 
	



1. [bookmark: _Ref427225635]Explain the letters ‘CHS’ and ‘SHS’ with reference to columns.

	Answer
	Circular Hollow Section & Square Hollow Section 
	



1. [bookmark: _Ref427227379]Match the retaining wall types and descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Retaining wall
	Answers
	Description
	
	
	1
	Cantilevered retaining wall
	1 - B
	A
	Leans into the excavated soil and constructed at an angle between 45 and 80 degrees. Typically constructed from brickwork or pre-cast interlocking concrete units. 
	

	
	2
	Gravity retaining wall
	2 - C
	B
	Relies upon the correct placement of steel reinforcement and varying thickness of concrete to resist the soil pressure. 
	

	
	3
	Inclined retaining wall
	3 - A
	C
	Relies on its own weight to resist soil forces. Typically constructed from stone, brickwork or concrete. 
	




1. [bookmark: _Ref427227493]What is a ground level concrete slab floor?

	Answer
	A ground level concrete slab is a structural element of the building for the flooring. It is boxed up over a damp proof course and steel fixed by concreters with reinformed materials on chairs and that are supported by chairs. The N20 N25 N30 Concrete is then placed into the boxing of the slab usually via concrete pump and then concrete is vibrated into place and finessed to achieve falls and the required finish. Once the concrete is set the boxing is removed. A ground level slab usually is resting on natural ground or bored concrete or screw piers if the ground isn’t good enough. In other cases where there is a basement underground the ground level slab is poured on formwork supported by temp propping and is known as a suspended slab. Once these slabs cue the boxing and temp support are removed and the building rest on columns and load baring walls only. 

	



1. [bookmark: _Ref427227808]What should you consider when selecting the type of slab floor?

	Answer
	Soil reactivity and bearing capacities. 
	



1. [bookmark: _Ref531355302]True or False (Tick your response): Concrete slab floors are popular in the construction of structures because they take less time to construct.

	Answer
		True 
	
	
	
		False 
	
	





1. [bookmark: _Ref427228752]Match the following slab structural performance terms with the descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Description
	
	
	1
	Foundation movement
	1 - C
	A
	Placed along the perimeter of the slab. Design is influenced by the reactivity of the soils. 
	

	
	2
	Slab bending
	2 - B
	B
	Movement is classified as dishing or doming. 
	

	
	3
	Stiffening beams
	3 - A
	C
	Addressed by regulating the moisture content of the soil.
	




1. [bookmark: _Ref531355427]Which of these terms relate to a roof truss? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Chord, knee, web
	

	
		Spider, pitch, chord
	

	
		Ankle, heel, tar
	

	
		Web, heel, pitch
	




1. [bookmark: _Ref427229422][bookmark: _Ref531008635]What are important considerations when undertaking demolition work? Describe relevant legislation, regulations and/or Codes of Practice relating to planning requirements, environmental standards, and safe work practices.

	Answer
	The following need to be considered before demolition commences:
· Method of demolition - either manual or mechanised
· Extent of temporary fencing and hoardings
· Protection of adjoining properties, existing buildings and infrastructure
· Disconnection notices for the service authorities, electricity, water, gas and telecommunications
· The order in which the structural systems will be removed (the sequence of operations)
· Details of any hazardous materials and notification of these to relevant authorities
· On-site amenities such as toilet, first aid, fire services
· Control measures for dust, noise and vibration
· Vermin control for rats and mice
· Traffic control on and off the site
· Truck wash bays
· Environmental considerations, such as recycling
All demolition operations are to be in accordance with Australian Standards and Codes of Practices including:
· Work Health and Safety Regulations 2011 (Qld)
· Demolition Code of Practice 2013 (Qld)
· AS 2601: The demolition of structures


	


1. [bookmark: _Ref531355335]When demolition is being undertaken, which of the following items must be checked daily? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		All boundaries are secured against unlawful entry
	

	
		All hazardous materials are removed or covered as required by OHS legislation
	

	
		All openings and elevated free edges are properly guarded
	

	
		All potential fire and safety hazards are eliminated and disconnected services are secured
	

	
		Asbestos is left on the nature strip for the garbage pickup
	

	
		Demolished materials have not been left on any floor or structure if their weight exceeds the safe carrying capacity of the floor or structure
	

	
		Emergency access routes are clear of debris
	

	
		Footpaths and public access are clear of demolished materials
	

	
		Neighbours have been notified not to hang out their washing
	

	
		No structure or part of a structure is left in such a condition that it may become dangerous, such as collapse due to wind or vibration
	

	
		Partly demolished elements are stabilised and loose materials are secured against bad weather
	

	
		Signs and balloons are in place for the garage sale
	

	
		Tell the demolisher to take a long lunch break as you don't need supervision
	

	
		Temporary hoardings, bracing, shoring and propping is tight and secure and in place as required to protect both workers and public
	




1. [bookmark: _Ref531355737]Identify two (2) requirements under the NCC with regards to construction in bushfire prone areas?

	Answer
	Metal Screens to window openings may be required. Metal screening to vented soffits and ember protection to garage doors with special brush kits. 
	



1. [bookmark: _Ref427231195]What does AS3959 refer to?

	Answer
	Australian Standard AS3959:2018 Construction of buildings in bushfire-prone areas is an Australian standard for construction of buildings in bushfire-prone zones. The latest release of AS3959 has significant changes, bringing major changes to
	



1. [bookmark: _Ref531355744]Which of the following can assist with providing sufficient restraint to transfer wind forces to the ground to prevent collapse, uplift or sliding off the footing systems? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Anchorage systems
	

	
		Bracing systems
	

	
		Connecting structural elements together
	




1. [bookmark: _Ref531355745]Which Australian Standard outlines the requirements of high wind areas?

	Answer
	AS/NZS 1170.2:2021 Structural design actions Wind actions
	



1. [bookmark: _Ref427232597]The acceleration coefficient is a number which indicates the expected severity of the earthquake ground movement. Which Australian Standard should be referenced for this information?

	Answer
	The two different areas are categorised by an acceleration coefficient  (as determined under AS1170.4 and as outlined in the NCC) which is:
Equal to 0.12 but less than 0.15
0.15 or greater
	



1. [bookmark: _Ref531355751]True or False (Tick your response): Where the acceleration coefficient is greater than 0.15, there are additional NCC requirements than where the acceleration coefficient is 0.12.

	Answer
		True 
	
	
	
		False 
	
	





1. [bookmark: _Ref531355987]Which of the following areas require specific compliance in alpine areas? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Access bridges
	

	
		Access for emergency vehicles
	

	
		External doorways
	

	
		External ramps
	




1. [bookmark: _Ref531355991]Identify the Volume and Parts of the NCC that relate to each of the following areas for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Topic
	Classes 1 and 10
	Classes 2 to 9
	
	
	Bushfire
	Part 3.10.5
	G5
	

	
	High wind
	Part 3.0.3
	Specification B1.2Design of buildings in cyclonic areas
	

	
	Earthquake
	Part 3.10.2
	Part B1Structural provisions 
	

	
	Alpine area
	Part 3.10.4 Construction in alpine areas
	Part B1Structural provisions
	

	
	New technologies
	NA
	NA
	




1. [bookmark: _Ref427232821][bookmark: _Ref531356004]How are emerging building technologies and methods assessed in the National Construction Code? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Using verification methods
	

	
		With ‘deemed to satisfy’ provisions
	

	
		With documentary evidence
	





1. [bookmark: _Ref531356217]True or False (Tick your response): Footings should be set out in accordance with the building plan.

	Answer
		True 
	
	
	
		False 
	
	




1. [bookmark: _Ref531356194]Name three (3) different types of footing systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Concrete slab floors, Steel screw piers , Timber

	Concrete, Steel, Timber

	




1. [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to footings (including damp coursing and provision of termite barriers) for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
		Volume 2 -3.2.5 Footing and slab construction &  3.1.4.3 Termite management systems
	


  
	Volume 1 Part B1 points VI & XV
	




1. [bookmark: _Ref531356170]For each of the following identify two (2) Australian Standards that relate to footings.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
		AS 2870 and AS/NZS 2904
	 Please note that the text box to the right for classes 2 to 9 isn’t functioning so please treat the following answer as my response for this as I am  unable to type in the other part of this table. 

Classes 2 to 9 
My answer for this item is AS 3600 Reinforced concrete design. & AS 2159-1995 Piling  



	
	





1. [bookmark: _Ref531356390]Name two (2) materials that may be used for damp proof coursing.

	Answer
	horizontal barrier,  Builders Black Plastic 
	



1. [bookmark: _Ref531356392]Name two (2) termite resistant materials.

	Answer
	Woven stainless Steel,  flexible PVC flashing. 
	



1. [bookmark: _Ref531356575]Name three (3) different types of floor systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Concrete Slab on Grade,  Platform floor ,Timber flooring on stumps bearers and joists,
	Suspended slab, steel floor, panel systems.  
	




1. [bookmark: _Ref427235728]What should be considered when constructing a floor system?

	Answer
	When constructing the floor system it is important to take into consideration the type of flooring, the laying of pipes and reinforcement.
	



1. [bookmark: _Ref531356610]Which Australian Standard is referenced in Volumes 1 and 2 of the NCC regarding the requirements for slabs and footings?

	Answer
	AS 2870
	



1. [bookmark: _Ref531356630]Name three (3) different types of materials used for wall systems or structures falling under Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Cavity Brick, Concrete Block, Timber and lightweight cladding
	Tilt panel, Earth walls,  Steel frame with compressed panel cladding
	




1. [bookmark: _Ref531356612]Identify the Volume and Parts of the NCC that relate to masonry wall systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Part 3.3.5Masonry veneer
	B1.4
	




1. [bookmark: _Ref531356616]Which Australian Standard is referenced in Volumes 1 and 2 of the NCC regarding masonry structures?

	Answer
	AS 3700
	



1. [bookmark: _Ref427577558][bookmark: _Ref531356640][bookmark: _Ref427237033]Explain the purpose of bracing. 

	Answer
	Bracing is attached to studs to provide lateral support to wall framing. Metal straps, timber or sheet bracing can be used for bracing.
	



1. [bookmark: _Ref531357045]Explain the purpose of fixings and tie-downs. 

	Answer
	To join the structural elements of the roof to the walls and the walls to the floor to prevent them from blowing off in a cyclone. 
	



1. [bookmark: _Ref531331115]Which Australian Standard relates to timber frames, bracing and fixings?

	Answer
	AS 1684 Residential Timber Framed Construction is a four-part Australian Standard covering design criteria, building practices, tie-downs, bracing and span tables for timber framing members. It is also referred to as the Timber Framing Code.
	



1. [bookmark: _Ref531357052]For the Australian Standard in Q66. which part relates to cyclonic areas?

	Answer
	Part 1
	



1. [bookmark: _Ref531357065]Which of the following should be observed when checking the quality of the frame (whether, factory pre-cut and pre-nailed, factory pre-cut and assembled on site, or cut and assembled on site)? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Fixings must be protected from corrosion
	

	
		Fixings must be protected from termites
	

	
		Provision has been made for plumbing services and fixtures
	

	
		Tie downs and nominal nailing must both be present
	

	
		Top and bottom plates have a tight fit on studs
	

	
		Top plate is to be reinforced when rafters land on top of plates
	

	
		Walls are tied together
	

	
		Walls are plumb
	

	
		Walls are square
	



1. [bookmark: _Ref531357185]True or False (Tick your response): Sarking is a substitute for cladding and is regarded as the principal means of weatherproofing.

	Answer
		True 
	
	
	
		False 
	
	




1. [bookmark: _Ref427237737]What is flashing?

	Answer
	Flashings are used at corners and vertical joints and around openings to ensure that water is prevented from penetrating the wall frame cavity. As flashing does not extend fully behind the cladding, non-permeable materials may be used.
	



1. [bookmark: _Ref531357196]Identify the Volume and Parts of the NCC that relate to wall cladding material requirements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Part 3.5 
	Specification J1.2
	




1. [bookmark: _Ref531357076]True or False (Tick your response): Timber can stand greater stresses than brickwork.

	Answer
		True 
	
	
	
		False 
	
	




1. [bookmark: _Ref531357077]True or False (Tick your response): Individual timber boards for cladding should be nailed together at the overlap.

	Answer
		True 
	
	
	
		False 
	
	




1. [bookmark: _Ref531357461]When should flashing materials be fixed to plywood cladding? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		After the cladding is fixed
	

	
		Before the cladding is fixed
	

	
		While the cladding is being fixed
	

	
		At any convenient time
	




1. [bookmark: _Ref531357463]What is the purpose of articulation joints? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		They allow for shrinkage in a building
	

	
		They tie the brickwork to the frame
	

	
		They allow for movement in a building
	

	
		They seal the cavities 
	




1. [bookmark: _Ref531357466]When is the most appropriate time for the rough-in to occur for a brick veneer building constructed on a concrete slab Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Before brickwork
	

	
		After brickwork
	

	
		After plasterboard
	

	
		Any time
	




1. [bookmark: _Ref531357473]Apart from plumbing and electrical, name four (4) other services that should be considered at rough-in.

	Answer
	Mechanical ventilation, Data, automation and building management system, security. 
	


1. [bookmark: _Ref531357478]Identify the Volume and Parts of the NCC that relate to window installation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Part 3.6
	F1.13
	




1. [bookmark: _Ref531357506]Name two (2) Australian Standards that relate to the installation of windows. 

	Answer
	AS 1288, AS 2047
	



1. [bookmark: _Ref531357537]What is the purpose of a window schedule? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		To help work out the appropriate type of window
	

	
		To work out the appropriate opening size of windows
	

	
		To work out whether to use a timber or aluminium frame
	

	
		To work out the height of a window
	




1. [bookmark: _Ref531357490]Identify the Volume and Parts of the NCC that relate to door installation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	3.6.4.1 Doors
	Specification C3.4 Point 2 Fire Doors, Point 3 Smoke doors.
	




1. [bookmark: _Ref427238214][bookmark: _Ref531357492]What Australian Standard must the design of a timber roof truss adhere to?

	Answer
	AS 1720 Part 5

	



1. [bookmark: _Ref427583793][bookmark: _Ref531357772]What is a roof system? Name three (3) roof types.

	Answer
	Types of roof systems include:
Gable
Hip
Skillion



	



1. [bookmark: _Ref531357774]True or False (Tick your response): Roof trusses can be modified on site to suite different needs.

	Answer
		True 
	
	
	
		False 
	
	




1. [bookmark: _Ref427584594]Devise a checklist for ensuring the quality of an installed roof frame.

	Answer
	Truss layout plan
Manufacturer's specifications for tie-downs, bracings and lateral stability
Roof truss certification
Adequacy of supporting structure
Dimension, overall width and length of wall for fit
Support to girder trusses
Plumb and spacings
All tie-downs and fixings
Location of specialised trusses
Trusses have not been modified on-site
Eave overhangs
Trimming to manhole.


	



1. [bookmark: _Ref531357779]Devise a checklist for ensuring the quality of an installed roof truss.

	Answer
	
· Adequacy of supporting structure
· Dimension, overall width and length of wall for fit
· Adequacy of supporting structure
· Dimension, overall width and length of wall for fit
· Adequacy of supporting structure
· Dimension, overall width and length of wall for fit
· Eave overhangs


	



1. [bookmark: _Ref531357807]Name three (3) roof cladding materials.

	Answer
	Roof cladding materials include:
Brick veneer
Tiles (concrete, clay, metal)
Sheeting

	



1. [bookmark: _Ref427583809]What pitch of roof should roof tiles be applied? Are there exceptions?

	Answer
	Roof tiles can generally be used on roofs of 15º or greater pitch, however, some materials and methods of manufacture require 25º or greater pitch.
	




1. [bookmark: _Ref531358032]When installing corrugated metal roof sheeting, which is the preferred direction of laying sheets to improve side lap effectiveness for minimising leakage? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Away from the prevailing weather
	

	
		Towards the north
	

	
		Towards the prevailing weather
	




1. [bookmark: _Ref531358025]True or False (Tick your response): Sarking is advisable under any roof.

	Answer
		True 
	
	
	
		False 
	
	




1. [bookmark: _Ref531358038]What Australian Standard relates to sarking?

	Answer
	AS/NZS 4256
	



1. [bookmark: _Ref531358043]Name three (3) items that may require roof penetration. 

	Answer
	Mech vent to bathrooms, skylights, supports for flyover roofing for patios. 
	



1. [bookmark: _Ref531358046]Identify the sections/parts of NCC Volume 1 that relate to the installation of skylights.

	Answer
	J1.4 Roof lights
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	PRACTICAL ASSESSMENT INSTRUCTIONS

103. The following practical assessment will require the Participant to complete work related activities.
104. The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
105. Please fill in the details below – providing your name, signature and date of assessment.
1. The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
106. The Assessor may substitute a Practical Task with an alternate task of equal value.
1. Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Callum Quinn

	
	

	Participant signature
	
	
	

	Date
	1/12/2021



	Assessor name
	Chris Abbott

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1
		
	Task 2
		



	ASSESSOR COMMENTS

	


CPCCBC4010B Apply structural principles to residential low rise constructions

	Practical Task 1

	Description of task:
A suitable observer is to verify the participant’s ability to apply structural principles to the erection and demolition of a low rise residential structure (Classes 1 and 10).

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
107. Photographic evidence of projects, including detailed descriptions of all structural elements 
108. Documentation from a project structurally designed; for example a garage, small extension, etc. including: 
1. A copy of the plans and/or specifications 
2. Identification of site classification, uplift forces, wind ratings, 
3. Component selection methods – for example; BCA references, Australian Standard references

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Plans, computer, suitable work area appropriate to the construction process. 

	Assessment of task

	Name of participant:
	Callum Quinn

	Name of observer:
	Damien Carroll

	Role of observer 
(Confirm suitability to sign)
	Direct Supervisor as senior estimator

	Email address of observer
	damien.carroll@murphybuilders.com.au

	Signature of observer:
	
	Date:
	1/12/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. Provide comments if left unticked.

	1 Apply structural principles to planning

	1. [bookmark: _Ref530725761]Identify main structural principles that apply to the erection or demolition of the structure.
	
	1. [bookmark: _Ref530725767]Describe structural performance in terms of the effect of section properties on various materials. 
	
	1. [bookmark: _Ref530725780]Explain structural performance characteristics of the slabs, floors, beams, columns and retaining walls – and apply to the planning of the construction work. 
	
	1. [bookmark: _Ref530725785]Coordinate demolition of existing structures in accordance with safe work practices, legislative, environmental and planning requirements. 
	
	2 Structural integrity of buildings

	Q1.  [bookmark: _Ref530725788]Consult relevant industry professionals to provide advice regarding the design process and structural integrity of the proposed building – using language and concepts appropriate to cultural differences (including non-verbal communication). 
	
	Q2.  [bookmark: _Ref530725791]Collect and analyse project documentation to assist with the analysis of plans and specifications. 
	
	Q3.  [bookmark: _Ref530725796]Analyse project documentation for compliance with National Construction Code requirements for bushfire, high wind, earthquake and alpine environments.
	
	Q4.  [bookmark: _Ref530725800]Assess new and emerging building technologies, techniques and materials for application to the construction process and their compliance with National Construction Code requirements and Australian standards.
	
	Q5.  [bookmark: _Ref530725804]Conduct pre-commencement site inspection to confirm analysis. 
	
	3 Footing system

	2.7A.  [bookmark: _Ref530725808]Set out footings in accordance with building plans.
	
	2.7B.  [bookmark: _Ref530725812]Assess structural integrity of the footings specified in the plans for compliance with relevant codes and accepted industry construction principles. 
	
	2.7C.  [bookmark: _Ref530725816]Lay footings specified in building’s plan, checking for compliance with project documentation. 
	
	2.7D.  [bookmark: _Ref530725822]Plan, implement and check damp coursing, provision of termite barriers and other relevant techniques in accordance with codes, standards and industry practice. 
	
	4 Floor system

	1.3A.  [bookmark: _Ref530725827]Assess concrete slab or bearers and joists specified in building plan for structural integrity and compliance with relevant codes and accepted industry construction principles.
	
	1.3B.  [bookmark: _Ref530725949]Supervise laying of floor system specified in building’s plan, checking for compliance with project documentation. 
	
	5 Structural and non-structural wall systems

	2.1A.  [bookmark: _Ref530725953]Identify and analyse technical construction principles and performance of materials to be used in the construction in the planning of the building and construction project. 
	
	2.1B.  [bookmark: _Ref530725957]Plan, implement and check application of bracing requirements, tie-downs, tolerance, allowances and fixing and installation of components for compliance with relevant Australian standards, codes and manufacturer specifications. 
	
	2.1C.  [bookmark: _Ref530725961]Select structural timber members for low rise buildings to conform to AS1684 requirements. 
	
	2.1D.  [bookmark: _Ref530725966]Put processes in place to ensure quality of the frame – whether factory pre-cut and pre-nailed, factory pre-cut and assembled on site, or cut and assembled on site. 
	
	2.1E.  [bookmark: _Ref530725969]Attach and check vapour permeable sarking or a waterproof membrane relevant to the construction method. 
	
	6 Roof system

	2.2A.  [bookmark: _Ref530725974]Assess structural integrity of roof system components specified in building plan for compliance with relevant codes and accepted industry construction principles. 
	
	2.2B.  [bookmark: _Ref530725980]Plan, implement and check erection of roof trusses in accordance with requirements of building plan, type of roof being construction, relevant codes and accepted industry construction principles. 
	
	2.2C.  [bookmark: _Ref530725983]Put processes in place to ensure quality of the manufactured roof trusses or hand-cut roof system. 
	
	2.2D.  [bookmark: _Ref530725987]Plan roof sarking and cladding and supervise installation for compliance with codes, standards and industry practice.  
	
	7 External wall cladding

	2.3A.  [bookmark: _Ref530725992]Assess structural performance of cladding to be used for bracing in the frame construction for compliance with relevant codes, manufacturer specifications and accepted industry construction principles. 
	
	2.3B.  [bookmark: _Ref530725996]Supervise installation of cladding as specified in building plan, and check for compliance with standards and accepted industry construction principles. 
	
	2.3C.  [bookmark: _Ref530725999]Supervise installation of windows and external doors to ensure compliance with relevant codes, manufacturer specifications and accepted industry construction principles. 
	
	The Participant’s performance was:  Satisfactory     Not Satisfactory


	OBSERVER COMMENTS

	Quite a number of the tenders Callum works on , are design and construct. As such detailed cost planning and pricing must be conducted with very little to no structural detail. As such Callum has to apply his understanding of the structural principles that engineers are likely to apply to each built he must apply these assumptions to items such as footing systems, slab design, sub floor, wall frame and roof details. Each system and likely design decision greatly effects the actual cost of the build. Without an good understanding of these principles he would not be able to effectively perform in his current role.  



This page is intentionally blank

CPCCBC4011B Apply structural principles to commercial low rise constructions

	Practical Task 2

	Description of task:
A suitable observer is to verify the participant’s ability to apply structural principles to the erection and demolition of a low rise commercial structure (Classes 2 to 9 with a gross floor area not exceeding 2000m2, but not including Type A or Type B construction). 

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include:
113. Photographic evidence of projects, including detailed descriptions of all structural elements
114. Documentation from a commercial works structurally designed; including: 
1. A copy of the plans and/or specifications 
2. Identification of site classification, uplift forces, wind ratings
3. Component selection methods – for example; BCA references, Australian Standard references

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Plans, computer, suitable work area appropriate to the construction process. 

	Assessment of task

	Name of participant:
	Callum Quinn

	Name of observer:
	Damien Carroll

	Role of observer 
(Confirm suitability to sign)
	Direct Supervisor as senior estimator

	Email address of observer
	damien.carroll@murphybuilders.com.au

	Signature of observer:
	
	Date:
	22/11/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. Provide comments if left unticked.

	1 Apply structural principles to planning

	1. [bookmark: _Ref530737028]Identify main structural principles that apply to the erection or demolition of the structure.
	
	1. [bookmark: _Ref530737033]Describe structural performance in terms of the effect of section properties on various materials. 
	
	1. [bookmark: _Ref530737038]Explain structural performance characteristics of the slabs, beams, columns and retaining walls – and apply to the planning of the construction work. 
	
	1. [bookmark: _Ref530737043]Coordinate demolition of existing structures in accordance with safe work practices, legislative, environmental and planning requirements. 
	
	2 Structural integrity of buildings

	1. [bookmark: _Ref530737047]Consult relevant industry professionals to provide advice regarding the design process and structural integrity of the proposed building – using language and concepts appropriate to cultural differences (including non-verbal communication). 
	
	1. [bookmark: _Ref530737050]Collect and analyse project documentation to assist with the analysis of plans and specifications. 
	
	1. [bookmark: _Ref530737054]Analyse project documentation for compliance with National Construction Code requirements for bushfire, high wind, earthquake and alpine environments.
	
	1. [bookmark: _Ref530737058]Assess new and emerging building technologies, techniques and materials for application to the construction process and their compliance with National Construction Code requirements and Australian standards.
	
	1. [bookmark: _Ref530737062]Conduct pre-commencement site inspection to confirm analysis. 
	
	3 Footing system

	1. [bookmark: _Ref530737066]Set out footing systems in accordance with building plans.
	
	1. [bookmark: _Ref530737070]Assess structural integrity of the footings specified in the plans for compliance with relevant codes and accepted industry construction principles. 
	
	1. [bookmark: _Ref530737073]Lay footings specified in building’s plan, checking for compliance with project documentation. 
	
	1. [bookmark: _Ref530737076]Plan, implement and check damp coursing, provision of termite barriers and other relevant techniques in accordance with codes, standards and industry practice. 
	
	4 Floor system

	1. [bookmark: _Ref530737080]Assess floor system components specified in building plan for structural integrity and compliance with relevant codes and accepted industry construction principles.
	
	1. [bookmark: _Ref530737083]Supervise laying of structural floor system specified in building’s plan, checking for compliance with project documentation. 
	
	5 Structural wall systems and wall cladding systems

	1. [bookmark: _Ref530737087]Identify and analyse technical construction principles and performance characteristics of structural wall systems and wall cladding systems in the planning of the building and construction project. 
	
	1. [bookmark: _Ref530737091]Identify, implement and check processes for erecting wall systems and wall cladding systems for compliance with manufacturer specifications and relevant Australian standards and codes. 
	
	1. [bookmark: _Ref530737095]Identify and implement building plans and relevant standards and codes to ensure appropriate allowances were made for relevant services to be installed. 
	
	1. [bookmark: _Ref530737100]Install windows and external doors in compliance with relevant codes, manufacturer specifications and accepted industry construction principles. 
	
	6 Structural roof systems and roof cladding systems 

	1. [bookmark: _Ref530737103]Assess structural integrity of the structural roof system and roof cladding system components specified in the building’s plan for compliance with relevant codes and accepted industry construction principles. 
	
	1. [bookmark: _Ref530737107]Plan and implement and check construction of roof system and roof cladding system (including details of service penetrations, skylights and roof ventilators) according to building plan’s requirements, type of roof being constructed, relevant codes and accepted industry construction principles. 
	
	1. [bookmark: _Ref530737112]Put processes in place to ensure quality of finished roof system. 
	
	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS

	Quite a number of the tenders Callum works on, are design and construct. As such detailed cost planning and pricing must be conducted with very little to no structural detail. As such Callum has to apply his understanding of the structural principles that engineers are likely to apply to each built he must apply these assumptions to items such as footing systems, slab design, sub floor, wall frame and roof details. Each system and likely design decision greatly effect the actual cost of the build. Without an good understanding of these principles he would not be able to effectively perform in his current role. 

In relation to the commercial builds in particular the Callum has worked on he has had hands on experience with suspended slabs, cost saving alternatives, retaining wall deletions with batter replacements, zone of influence, structural fire treatments. 
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