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16 October 2020

Lockyer Valley Regional Council
26 Railway Street
GATTON QLD 4343

ATTENTION:  CHRIS GODDARD

Dear Chris

RE: 	TENDER SUBMISSION FOR GATTON SHIRE HALL UPGRADE WORKS
	
Thank you for the opportunity to present our tender price for the Gatton Shire Hall Upgrade Works.  

With Toowoomba being our home base for over 24 years, McNab has delivered countless local projects for which we have established a strong, reputable and professional local subcontractor and supplier base which we are able to use on this project.  

Having delivered key refurbishment projects in the Toowoomba area, we understand the importance of keeping these facilities operational and minimising disruptions to daily operations which we achieve through collaborative planning with all stakeholders and establishing relationships through constant communication. 

We look forward to the opportunity of delivering your project.  Our tender price is based upon the following qualifications:

We also offer that peace of mind of being ‘locals’.  With our office being just a short 36km from site, a large percentage of our Toowoomba workforce being Gatton and Lockyer Valley residents combined with a trusted subcontractor and supplier local network we offer a guarantee of a collaborative project team who are deeply connected to creating a positive project outcome for you. 

OUR TENDER PRICE (EXCL GST)

GATTON SHIRE HALL UPGRADE WORKS					$1,608,880.00

This price is based upon the tender clarifications overleaf.  

We look forward to the opportunity of working with to deliver the Gatton Shire Hall Upgrade Works.  Should you require additional information or tender clarification, please feel free to contact me on 07 3252 6900.
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Yours sincerely,


Sean Snowden
Estimating & Design Manager



[image: ][image: ]
[image: ]

[image: ]
[image: ]
CLARIFICATIONS

McNab have allowed a Provisional Sum of $2,000.00 (ex GST) for materials and labour for Scope of Works 5B for Roof rectification as detailed on drawing B.140, due to unknown extent. 
To prevent damage to the pavers around the Bar Extension, we have allowed to remove a wider section of pavers around this area. Salvaged pavers will then be relayed to edge of building and gardens to make good.  
We have allowed to install plastic and sheet plywood to various areas of the auditorium timber floor to provide protection from damage during the works. 
Our tender price for stainless steel joinery to the kitchen refurbishment is based on Option 1 only with the coldroom doorway being installed (therefore, no stainless steel bench and shelf to the western wall).
We note that a geotechnical report was not provided with tender documents therefore we have only allowed for backhoe piers to the Bar Extension as per the sizes detailed on structural drawing S03.
We have allowed for a full width motorised roller shutter to the bar servery (door hardware specification only states manual roller shutter).
McNab advise that we have allowed for an alternative aluminium suite (Ezial 150mm centre glaze frame in lieu of GJames 475 series) to be installed which allows the aluminium assemblies for the Eastern Courtyard doors/windows to be full height (3000mm high) without the need for a head at 2400mm high. We also advise that the acoustic requirements for these assemblies will not likely be achieved, which was also advised by GJames.  
We have allowed for painting of new and disturbed areas only (not the full internal or external areas of the building).
We have assumed there are no concrete slabs under the existing paved areas including the courtyard and bar extension.
We have allowed to machine excavate the pavers to the existing courtyard and bar extension areas. Undamaged pavers will then be stacked/stockpiled for reuse or handover to the LVRC. No allowance is made to hand remove pavers. 
We have not priced “Cold Room Option 2” as no structural drawings and architectural details have been provided as part of the tender documents to allow pricing. This area of the building is likely to be on mainly filled materials, therefore the footing and slab system under coldroom option 2 is likely to be on bored piers to support this option. As this is not a D&C project, we have not priced this option   
Due to the uncertainty of some asbestos locations detailed in the provided Asbestos Management Plan, McNab have allowed a Provisional sum of $2,500.00 (ex GST) for asbestos removal and air monitoring (if required) to remove and dispose of any Asbestos Containing Materials including the roof parapet sheeting identified on drawing B.140. 
McNab advise that we have not allowed to provide a temporary site office and amenities facilities for the project. To minimise costs, we have allowed to utilise a suitable area within the building for our office (to be agreed) and we would use the existing toilets on site. We would maintain all areas in a clean and tidy condition and make good, should any damage occur. 
McNab take no responsibility for galvanic or bi-metallic corrosion issues in the future due to incompatibility of materials in the roof replacement works (zincalume/colourbond to galvanised roofing products). 
McNab have not allowed for underfloor heating and waterproofing to kitchen coldroom (option 1). Site inspection revealed this coldroom would be installed over the timber flooring, however we are unsure as to what the underfloor substrate under this area is. Subfloor heating may be required if this is a timber suspended floor. We have allowed to install FC underlay sheeting prior to the insulation floor panel being installed. A 75mm thick concrete wear slab is then installed over the insulated floor panel. No allowance is made to strengthen the existing floor structure to carry the loads imposed by the concrete wearing slab, cold room and loaded contents.
We have allowed for 6mm villaboard wall linings in accordance with drawings (not 9mm as detailed in linings specification).
We have not allowed for any underlays to the proposed carpet tile areas in the Foyer as these tiles have a suitable backing material as part of the tile and are allowed to be directly stuck to the substrate floor. 
We have not allowed for structural strengthening of the existing roof structure to take loads for new roof mounted mechanical plant. Required new plant deck platforms have been allowed only in a manner similar to existing roof mounted units.
Please note our preliminaries have been divided across all tasks in the price breakup.  If any part of the works is deleted/reduced, McNab reserves the right to re-negotiate our final tender price.
We confirm we will comply with the Training Policy (TPAS) as described in Section 8 of the RFT and Contract AS 2124.
 


EXCLUSIONS 

Our tender submission excludes the following:
Latent conditions.
Stainless steel corner guards as nil mentioned on drawings. 
Skate deterrent systems. 
To remove any adhesives under existing floor coverings. 
To waterproof the kitchen and bar floors as these are not considered wet areas under the Australian Standards.
To divert any existing services to allow for excavations for footings, slab works, etc. We have allowed to explore and locate existing services in conjunction with council consultants.
CCTV, security access and control systems.
NBN pathways, equipment and infrastructure.  
Electrical supply authority fees and charges. 
Plumbing applications and approvals. We have allowed for council inspection fees. 
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Level 1, 12 Neil Street, Toowoomba Qld 4350
PO Box 2304, Toowoomba Qld 4350

(07) 4620 0700
info@mcnab.net.au

mcnab.net.au
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