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CPCCBC4001A 
Apply building codes and standards to the construction process for low rise building projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4001A Apply building codes and standards to the construction process for low rise building projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	[bookmark: _Ref396827952]Participant Name
	Tess Veldink




	Task
	Assessment Results 

	Theory Exam
	þ Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	Myles Walder

	Assessor Signature
	
	Unit Competence Determination Date
	23/03/2021
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CPCCBC4001A 
Apply building codes and standards to the construction process for low rise building projects

	THEORY EXAM INSTRUCTIONS

1. This exam will occur under standard assessment conditions.
1. An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
2. Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
3. Please fill in the details below, providing your name, signature and date of assessment.
1. Your signature acknowledges that this is your own work.
4. Assessors are to complete marking in pen of a different colour to the Participant.
5. If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
1. If a Participant changes their response in writing, they must put their initials next to the written change.
2. If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Tess Veldink1

	
	

	Participant signature
	
	
	

	Date
	16/02/2021



	Assessor name
	Myles Walder

	
	

	Assessor signature
	
	
	

	Date
	23/03/2021




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	38
	38
	Satisfactory
	Not Yet Satisfactory

	
	
	þ
	


	ASSESSOR COMMENTS

	Question 14 – You have referenced an Australian Standard not the correct Act/ legislation


[bookmark: _Ref5882211]A Performance Solution must abide by which of the following? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	¨
	
	þ	Be assessed according to one or more of the Assessment Methods
	

	
	¨	Go beyond the requirements of Deemed-to-Satisfy Provisions
	

	
	þ	Comply with the Performance Requirements
	




[bookmark: _Ref5882213]True or False (Tick your response): The Performance Requirements of the National Construction Code can be achieved by using a Performance Solution, a Deemed-to-Satisfy Solution, or a combination of both.

	Answer
	þ	True 
	
	þ
	
		False 
	
	




[bookmark: _Ref5882215]True or False (Tick your response): The term ‘Performance Solution’ in the NCC was formerly known as ‘Alternative Solution’.

	Answer
	þ	True 
	
	þ
	
		False 
	
	




[bookmark: _Ref5882219]Where a Performance Solution has been proposed, which of the following documentation should be prepared and retained? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	þ
	
	þ	Details of the relevant Performance Requirements 
	

	
	þ	Assessment Methods used to establish compliance with the relevant Performance requirements
	

	
	þ	Details of any Expert Judgement relied upon
	

	
	þ	Details of any tests of calculations used to determine compliance with the Performance Requirements
	

	
	þ	Details of any Standards or other information which were relied upon
	





[bookmark: _Ref5950292]True or False (Tick your response): Where a Deemed-to-Satisfy solution has been proposed, all relevant plans/specifications should be retained.

	Answer
	þ	True 
	
	þ
	
		False 
	
	




[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that outline the Assessment Methods used to determine whether a Performance Solution or a Deemed-to-Satisfy Solution complies with the Performance Requirements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	þ
	
	Volume 2 Part 1.0 Application – 1.0.9 Assessment methods
	Volume 1 Part A0 Application – A0.5 Assessment methods

	




[bookmark: _Ref536106146]Identify the Australian Standard that relates to artificial lighting needed for safe movement, as noted in the NCC.

	Answer
	AS/NZS 1680.0
	þ



[bookmark: _Ref5782698]Identify the Volume and Parts of the NCC that outline the requirements for artificial lighting needed for safe movement for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	þ
	
	Volume 2 Part 2.4 – F2.4.4 Light B
	Volume 1 Section J energy efficiency  Part J6
	





[bookmark: _Ref5882620]Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to lighting:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements ____________ to ____________ are satisfied by complying with F4.12
F4.1
Fp4.5
FP4.1

1. ____________ to ____________; and Part G6

1. For a building containing an occupiable outdoor area, ____________; and 
1. for farm buildings and farm sheds, ____________. 
Part H3

Where a Performance Solution is proposed, the relevant Performance Requirements must be determined in accordance with ____________ and ____________ as applicable. A2.4 (3)
A2.2 (3)


	Answer
	

	þ



[bookmark: _Ref422743346][bookmark: _Ref531682593]Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to light:

Where an alternative light system is proposed as a Performance Requirement to that described in ____________, that proposal must comply with – P2.4.4
Part 3.8.4

1. Performance Requirement ____________; and 
1. the relevant Performance Requirements determined in accordance with ____________ and ____________ as applicable.A2.4(3)
A2.2 (3)


	Answer
	

	þ



[bookmark: _Ref5882637]Identify the Australian Standard that relates to each of the listed types of fire fighting equipment, as noted in the NCC.

	Answer
	Equipment
	Australian Standard
	þ
	
	Fire hydrants
	AS 2419 C2.12
	

	
	Fire hose reels
	AS 2441 E1.4
	

	
	Portable fire extinguishers
	AS 2444 E1.6
	

	
	Smoke alarms
	AS 3786 E2.2a
	



[bookmark: _Ref5882646]For each of the listed types of fire fighting equipment, identify whether they are required by the NCC (if so, identify the relevant Part).

	Answer
	Equipment
	Volume 1
	Volume 2
	þ
	
	Fire hydrants
	Part E1 Fire fighting equipment E1.3
	
	

	
	Fire hose reels
	Part E1 Fire fighting equipment E1.3
	
	

	
	Portable fire extinguishers
	Part E1 Fire fighting equipment E1.6
	
	

	
	Smoke alarms
	E2.2a Smoke detection and alarm systems
	3.7 Fire Safety – 3.7.2 smoke alarms
	




[bookmark: _Ref531682022]Identify the applicable Act in your jurisdiction that outlines the requirements for smoke alarm installation in domestic dwellings. 
Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	þ
	
	Building Fire Safety (Domestic Smoke Alarms) Legislation Amendment Regulation 2016 

	1. A smoke alarm must be installed in each bedroom of the domestic dwelling, in a place that complies with section 13AD. 
2. (2)  Each smoke alarm must— 
1. (a)  comply with AS 3786–2014; and 
2. (b)  contain a photoelectric sensor; and 
3. (c)  not also contain an ionisation sensor; and 
4. (d)  be hardwired to the domestic dwelling’s electricity supply; and 
5. (e)  be interconnected to every other smoke alarm installed in the dwelling. 
3. (3)  A smoke alarm (the first smoke alarm) is interconnected to another smoke alarm if— 
1. (a)  the first smoke alarm sounds an alert if the other smoke alarm is activated because its sensor detects smoke; and 
2. (b)  the other smoke alarm sounds an alert if the first smoke alarm is activated because its sensor detects smoke. 
(4)  Subsections (1) and (2) do not apply to a sole-occupancy unit in a class 2 building if a smoke detection system that complies with the BCA, specification E2.2a, clause 4 has been installed in the domestic dwelling. 
(5) If the BCA is inconsistent with this section, this section prevails to the extent of the inconsistency. 

	





[bookmark: _Ref5883662]Identify the applicable Act in your jurisdiction that outlines the requirements for testing smoke alarms in domestic dwellings. 
Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Building Fire Safety (Domestic Smoke Alarms) Legislation Amendment Regulation 2016, clause 5 

	 04RAA When smoke alarm operates when tested 
1. (1)  A smoke alarm operates when tested if it operates when tested in a way required under subsection (3).
2. (2)  Also, a smoke alarm powered by a battery that is 19 capable of being replaced operates when tested 
if—
(a) the battery in the smoke alarm is replaced
(b) after the battery is replaced, the smoke 24 alarm operates when tested in the way 25 required under subsection (3)
A smoke alarm installed in a domestic dwelling must be tested as follows— 
(a) for an alarm that can be tested by pressing a  button or other device to indicate whether  the alarm is capable of detecting smoke—by pressing the button or other device; 
(b) otherwise— 
1. (i)  by being tested by the owner of the  dwelling in the way stated in the manufacturer’s instructions; or 
2. (ii)  by being tested by a tenant of the dwelling in the way stated in the information statement.

	




[bookmark: _Ref5952975]Identify the applicable Act in your jurisdiction that outlines what must occur if smoke alarm in a domestic dwelling does not operate upon testing and when any rectification must occur. Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	þ
	
	Clause 8  Replacement of s 104RC (Lessor must replace smoke
alarm) 
  
	1. he owner of a domestic dwelling must replace a 26 smoke alarm in the dwelling under this section 27 within 10 years after the day the smoke alarm was 28 manufactured. 29 
Maximum penalty—5 penalty units. 30 
2. (2)  Also, if a smoke alarm in a domestic dwelling 31 does not operate when tested, the owner of the 32 dwelling must immediately replace the smoke 33 alarm under this section. 
Maximum penalty—5 penalty units. 

	




[bookmark: _Ref5883528]In observation of NCC Volume 2, identify three (3) aspects which should be checked with regards to smoke alarms.

	Answer
	Connected to the consumer main power where consumers power is supplied to the building, be interconnected where there is more than one alarm and comply with the correct Australian standard
	þ




[bookmark: _Ref5883676]Must all smoke alarms be interconnected in domestic dwellings? Explain your response with reference to legislation.

	Answer
	A 10-year phased rollout of interconnected photoelectric smoke alarms in Queensland will happen over three specific periods starting from 1 January 2017.
· From 1 January 2017: In all new dwellings and substantially renovated dwellings (this applies to building applications submitted from 1 January 2017).
· From 1 January 2022: In all domestic dwellings leased and sold.
· From 1 January 2027: In all other domestic dwellings

	þ



[bookmark: _Ref5883539]Fill in the blanks for the definition of fire compartments, referring to Volume 1 of the NCC:

Fire compartment means – 
1. The total space of a building; or
1. When referred to in –
1. The Performance Requirements – any part of a building separated from the remainder by ____________ to fire such as _____________ and/or ____________ having an appropriate resistance to the spread of fire with any ____________ adequately protected; orfloors
walls
barriers
floors

1. The Deemed-to-Satisfy Provisions – any part of a building separated from the remainder by ____________ and/or ____________ each having an ____________ not less than that required for a fire ____________ for that type of construction and where all ____________ in the ____________ construction are protected in accordance with the DtS Provisions of the relevant Part. wall
openings
FRL
floors
walls
Separating 


	Answer
	
	þ



[bookmark: _Ref5787153]Identify the Volume and Parts of the NCC that outline the requirements for fire compartmentation and separation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	þ
	
	Volume 2 Part 3.7 Fire Safety. 3.7.1 Fire separation 
	Volume 1 part C3 Protection of opening C3.1 Application of part
	



[bookmark: _Ref5885739]Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to fire compartmentation and separation:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements ____________ to ____________ are satisfied by complying with C2.14
C2.1
C1.14
C1.1
CP9
CP1

1. ____________ to ____________, ____________ to ____________ and ____________ to ____________; and C3.1

Part G3
C3.17

1. in a building containing an atrium, ____________; and Part H1

1. for additional requirements for Class 9b buildings, ____________; and Part H3

1. for farm sheds, ____________. 
Where a Performance Solution is proposed, the relevant Performance Requirements must be determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)


	Answer
	

	þ



[bookmark: _Ref5885741]Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to fire separation:

Where an alternative fire separation design is proposed as a Performance Solution to that described in Part ____________ that proposal must comply with Performance Requirement ____________; and the relevant Performance Requirements determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)
P2.3.1
3.7.2


	Answer
	

	þ



[bookmark: _Ref5885751]Identify the Australian Standard referenced in NCC Volume 1 with regards to compartmentation and separation for electricity supply systems.

	Answer
	AS/NZS 3013

	þ




[bookmark: _Ref5886137]Identify the Volume and Parts of the NCC that outline the level of fire resistance required for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	þ
	
	Volume 2 Part 1.2, 1.2.3 Fire resistance of building elements
	Volume 1 Section C Part C1, C1.1 Fire resisting construction 
	




[bookmark: _Ref5951761]In a building’s specifications, an FRL is stated as being 90 / 60 / -. 
If exposed to a standard fire test, how many minutes can you expect this building element to last for the criteria listed below? 

	Answer
	Minutes
	Criteria
	þ
	
	) – no requirements
	Insulation
	

	
	60
	Integrity
	

	
	90
	Structural adequacy
	




[bookmark: _Ref5886138]Fill in the blanks: 
According to NCC Volume 1, an electricity substation located within a building must be separated from any other part of the building by construction having an FRL of no less than ____ / ____ / ____ and have any doorway in that construction protected with a self-closing fire door having an FRL of not less than ____ / ____ / ____. 120

120

120
-
30
120


	Answer
	

	þ



[bookmark: _Ref5886140]Fill in the blanks: According to NCC Volume 2, if an electrical wire or cable penetrates a separating wall, the service and building element at the penetration must be identical with a prototype assembly which has been tested and achieve an FRL of not less than ____ / ____ / ____. -
60
60


	Answer
	

	þ




[bookmark: _Ref5886711]Identify the applicable Act in your jurisdiction that outlines the occupier’s requirements for maintaining prescribed fire safety installations (e.g. fire doors). Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	þ
	
	Building Fire Safety Regulation 2008. Part 5 Prescribed fire safety installation

	This section applies to a person carrying out maintenance of a prescribed fire safety installation. 
The person must carry out the maintenance of the installation in compliance with QDC, part MP6.1. 
Maximum penalty—30 penalty units. 
This section applies if a person who is carrying out, or has carried out, maintenance of a prescribed fire safety installation for a building, becomes aware, or ought reasonably to be aware, of a critical defect in the installation. 
 The person must give the occupier of the building a notice about the defect in the approved form (a critical defect notice) within 24 hours after the person carries out the maintenance of the installation. 
Maximum penalty—30 penalty units. 

	




[bookmark: _Ref5958063]Identify the applicable Regulation in your jurisdiction that outlines the timeframes in which repair or corrective action must be taken when maintaining prescribed fire safety installations. Briefly identify the requirements. 

	Answer
	Regulation name and section(s)
	Requirements
	þ
	
	Building Fire Safety Regulation 2008.Part 5 division 3 obligations of occupiers 
	1. Subsection (4) applies if the record of maintenance for a prescribed fire safety installation for a building shows that repair or other corrective action is required for the installation. 
2. (4)  The occupier of the building must ensure the repair is carried out or the corrective action is taken no later than 1 month after the maintenance of the installation was carried out, unless the occupier has a reasonable excuse. 

	




[bookmark: _Ref5886716]NCC Volume 1 outlines that fire doors must be fitted with smoke seals and the assembly must be tested in accordance with Australian Standards. To which classes of building does this specification apply?

	Answer
	Class 5 or 6 buildings 
	þ



[bookmark: _Ref5886719]Do all fire doors require tags? Explain your response with reference to legislation.

	Answer
	Buildings approved after 1 April 1976 under the Building Act 1975 all require tags to be fitted to the fire doors.

Fire doors need to be tagged in accordance with AS/NZS 1905.1. the information on the tag includes: 
· The component standard – AS/NZS 1905.1 
· Fire resistant Level (FRL) – e.g. -/60/30 
· Manufacturer’s name (Company name) 
· Applicant’s name 
· Certifier (Company name) 
· Door tag number 
· Year of manufacturing 


	þ


[bookmark: _Ref5886882]Match the building classifications and their descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Classification
	Answers
	Description
	
	
	1
	Class 1
	1 - E 
	A
	A non-habitable building or structure.
	

	
	2
	Class 2
	2 - H   
	B
	A laboratory or a building in which a handicraft or process for the production, assembling, altering, repairing, packing, finishing or cleaning of goods or produce is carried on for trade, sale or gain.
	

	
	3
	Class 3
	3 - C   
	C
	A residential building other than Class 1 or 2 which is a common place of long term transient living for a number of unrelated persons. 
	

	
	4
	Class 4
	4 - D   
	D
	A dwelling in a building that is Class 5, 6, 7, 8 or 9 if it is the only dwelling in the building. 
	

	
	5
	Class 5
	5 - F   
	E
	May be a single dwelling or a boarding house, guest hose or hostel with a floor area less than 300m2.
	

	
	6
	Class 6
	6 - G  
	F
	An office building used for professional or commercial purposes, excluding buildings of Class 6, 7, 8 or 9.
	

	
	7
	Class 7
	7 - I   
	G
	A shop or other building for the sale of goods by retail or the supply of services direct to the public.
	

	
	8
	Class 8
	8 - B   
	H
	A building containing 2 or more sole-occupancy units, each being a separate dwelling. 
	

	
	9
	Class 9
	9 - J   
	I
	A building which is a carpark or fore storage/display of goods or produce for sale by wholesale. 
	

	
	10
	Class 10
	10 - A   
	J
	A building of a public nature.
	




[bookmark: _Ref5886883]What class of building would shops, restaurants and cafes belong to?

	Answer
	Class 6
	þ



[bookmark: _Ref5886885]What class of building would a general medical practitioner’s office belong to?

	Answer
	Class 5
	þ




[bookmark: _Ref423946303]True or False (Tick your response): At the design stage, it may not be clear who the final tenant will be (or how they will be using their tenancy), so as long as the design meets the minimum requirements of all the classifications, it could be used for any of the purposes.

	Answer
	þ	True 
	
	þ
	
		False 
	
	




[bookmark: _Ref531681692]Where parts of a building have different purposes, the classification of Class 1 may apply to the whole building if not more than what percentage of the floor area is used for a purpose which is a different classification? Tick your response.

	Answer
	Choice
	Possible Answers
	þ
	
		5%
	

	
	þ	10%
	

	
		25%
	

	
		50%
	




[bookmark: _Ref5965263]The NCC aims to ensure structures appropriately withstand normal forces. Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definitions
	þ
	
	1
	Bending
	1 - B
	A
	A force which shortens or crushes.
	

	
	2
	Compression
	2 - A
	B
	A fore which stretches and squashes at the same time.
	

	
	3
	Shear
	3 - F
	C
	A force which tries to pull something apart.
	

	
	4
	Strain
	4 - D
	D
	Intensity of the internally distributed forces that resist a change in the form of a body.
	

	
	5
	Stress
	5 - E
	E
	Physical change in the dimensions of a structure that results from applying a load.
	

	
	6
	Tension
	6 - C
	F
	Created where two opposite forces try to cut, tear or rip something in two.
	





[bookmark: _Ref5965264]True or False (Tick your response): When a beam is loaded, the top is compressed and the bottom is in tension.

	Answer
	þ	True 
	
	þ
	
		False 
	
	




[bookmark: _Ref5965265]True or False (Tick your response): When a cantilever is loaded, the top surface is in tension and the bottom is in compression.

	Answer
	þ	True 
	
	þ
	
		False 
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	PRACTICAL ASSESSMENT INSTRUCTIONS

19. The following practical assessment will require the Participant to complete work related activities.
20. The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
21. Please fill in the details below – providing your name, signature and date of assessment.
1. The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
22. The Assessor may substitute a Practical Task with an alternate task of equal value.
1. Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Tess Veldink

	
	

	Participant signature
	
	
	

	Date
	2/03/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	2/03/2021





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4001A
Apply building codes and standards to the construction process for low rise building projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to access, interpret and apply relevant building codes and standards. 
23. Occasion 1: Construction classified as Class 1 and 10 construction
24. Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. 

Evidence to be submitted may include: 
25. Documented evidence of determining a compliant solution on a project including: 
1. Correspondence such as letters, emails, and records of other communications
2. Certifier reports, instructions
26. Other compliance documentation for a project including: 
1. Council or private certifier inspection reports 
2. Structural inspection certificates 
3. Occupation certificates

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Drawings and specifications, National Construction Code, Australian Standards, Relevant legislation.

	Assessment of task

	Name of participant:
	Tess Veldink

	Name of observer:
	

	Role of observer 
(Confirm suitability to sign)
	

	Email address of observer
	

	Signature of observer:
	
	Date:
	2/03/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Access and interpret codes and standards

	Q1.  [bookmark: _Ref531596182][bookmark: _Ref5621987]Identify relevant performance requirements from the National Construction Code that apply to individual projects described as low rise.
	þ	þ
	Q2.  [bookmark: _Ref531596194]Determine requirements of relevant National Construction Code deemed-to-satisfy (DTS) provisions.
	þ	þ
	Q3.  [bookmark: _Ref5621994]Access and interpret requirements of relevant Australian standards referenced in the National Construction Code. 
	þ	þ
	2 Classify buildings

	1. [bookmark: _Ref531596197][bookmark: _Ref5621997]Determine the nature of building according to its use and arrangement.
	þ	þ
	1. [bookmark: _Ref5622001]Apply National Construction Code criteria to determine the defined classification. 
	þ	þ
	1. [bookmark: _Ref5622021]Identify and interpret National Construction Code requirements for multiple classification.
	þ	þ
	3 Solutions for compliance

	1. [bookmark: _Ref5622025]Determine range of criteria to ensure that construction methods comply with National Construction Code performance requirements. 
	þ	þ
	1. [bookmark: _Ref531596223][bookmark: _Ref5622028]In accordance with company policy and procedures, discuss and propose alternative solutions to a design or construction problem that complied with National Construction Code requirements, considering basic design principles and the behaviour of materials and structures under stress, strain, compression, bending or combined actions.
	þ	þ
	1. [bookmark: _Ref5622031]Identify and document performance-based solutions in accordance with National Construction Code requirements.
	þ	þ
	1. [bookmark: _Ref5622034]Analyse and apply assessment methods referenced in the National Construction Code to determine whether a building solution complied with performance requirements or DTS provision. 
	þ	þ
	1. [bookmark: _Ref5622037]Identify and complete relevant documentation in accordance with National Construction Code requirements. 
	þ	þ
	1. [bookmark: _Ref535842459]Effectively communicate using the following methods:
36. Language/concepts appropriate to cultural differences
37. Non-verbal communication
	þ	þ
	4 Fire protection requirements 

	1. [bookmark: _Ref531596228]Identify and apply passive and active fire control elements for low rise buildings, as required by the National Construction Code and other legislation (including WHS requirements). 
	þ	þ
	1. [bookmark: _Ref5622050]Determine level of fire resistance required for the construction of various low rise buildings.
	þ	þ
	1. [bookmark: _Ref5622053]Check existing buildings for compliance with passive and active fire protection requirements, in accordance with National Construction Code requirements.
	þ	þ
	The Participant’s performance was: þ Satisfactory     Not Satisfactory



	OBSERVER COMMENTS

	Both occasions discussed and applied building codes to different occasions associated with NCC volume 1 and 2. The first occasion was a residential house with a termite issue and the second occasion was a shopping centre not exceeding 2000m2 with a parents/changing room not containing a changing table. Both occasions used email and meeting minutes are correspondence, included certifiers reports, plans included in occasion 2 and occasion one had a compliance certificate. The practical used correct terminology and effective communication when references the NCC and used many non-verbals to get information across.

Access and interpret codes and standards
The first part of both occasions was an introduction to what the NCC is and performance requirement. This section was discussed in detail as it set up what was to be discussed later on. DTS and performance solutions was explained and the assessment method.

Classify Buildings
The next part was an sub introduction to the NCC and how buildings are classified. The nature and criteria of the chosen buildings for each occasion was discussed in detail to give background.

Solution of Compliance
In this section it highlighted the important to fully understand the project before working on it to ensure you are complying with the NCC requirements. A problem situation was then discussed in detail giving an overview, performance solution, final design and the benefits. Occasion 1 discussed a termite issue and occasion 2 discussed a parent room issue. Both performance solutions referenced the NCC volumes.

A certificate from occasion 1 was referenced which showed what type of performance based solution was used. Occasion 2 didn’t have a certificate but explained the solution used. Both occasions discussed the different assessment methods and which one the occasion used. 

Keeping the relevant information and duplicating it  was touched on explaining the importance in case the builder needs to refer back in case of inspections.

Fire Protection Requirements

The importance of the fire safety requirements was explained along with the different fire safety measure in a house and shopping centre. An active and passive system chart was included which both occasions made reference to. The FRL was explained with a diagram and the was referred back to each occasion. To finish off the role of a building certifier was touched on and his importance in the building industry was referenced.  
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