Progress Inspection checklist template
	Inspector name:
	Rick
	Date
	15/02/2024

	Site location
	Rockpool Pelican Waters

	
	

	Trade being inspected
	Ceilings & Partitions ITP




[bookmark: _GoBack]Area preparation
1 Grid lines and datum point identified and pinned. 					Y/N
2 Concrete Rectification complete including corrects falls in wet areas. 			Y/N
3 Door/ window openings water proofed. (Photos and spec sheet required). 		Y/N
4 Sub Sills Installed. 									Y/N
Fire walls If Applicable
1 Firewall Pre sheet - service trade sign off acknowledged.			 HOLD POINT
2 Metal door frames installed and fire rated (checked ready for fitting of doors) 		Y/N
3 Fire wall sheeting complete as per approved system. 				Y/N
4 Fire Wall setting complete 								Y/N
5 Fire wall mastic complete								Y/N
6 Fire walls complete and ready for McNab inspection. 			HOLD POINT
Service trades
1 Electrical, comms and security services installed as per latest plan ready to sheet	Y/N
2 Plumbing services installed as per current plan ready to sheet			Y/N
3 Mechanical services installed as per current plan ready to sheet			Y/N
Wall framing and sheeting
1 Set -out in accordance with the latest plans and specifications. 			Y/N
2 Studs /Nogs (Min 18mm thick) installed for Joinery, fittings & fixtures- (Photos showing dimensions). 									Y/N
3 Access panels located and trimmed. 						Y/N
4 Positive framing to all internals. 							Y/N
5 Framing complete for all service penetrations.					Y/N
6 Box Studs/ timber infills installed to door frame openings. 				Y/N
7 All door openings are correct size, plumb and level. 					Y/N
8 Ceiling Heights as per plans including bulkheads.					Y/N
9 All ceiling frame members avoid lighting locations.					Y/N
10 All service trades signed ITP off ready to sheet				HOLD POINT
11 Pre sheet inspection With McNab.						HOLD POINT
12 Insulation installed as documented.							Y/N
13 Correct sheet type as per specification.						Y/N
14 Stud & ceiling adhesive applied as per specification.					Y/N
15 Fixed in accordance with manufactures recommendations.				Y/N
16 All Services brought through sheeting.						Y/N
17 Bulkheads installed true and plumb.							Y/N
18 Expansion Joints considered and installed in areas where there is potential for cracking and at required intervals.								Y/N
19 Area left clean and excess materials removed.					Y/N
20 Inspection with McNab ahead of the painter. 					HOLD POINT

