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Documentation of design and construction (suitability or evidence of suitability)
	Project Name: Inala Hotel

	Project address: Cnr of Rudd St &, Freeman Rd
Inala QLD 4077
	Site Plan attached: yes

	Prepared by: Michael Trott

	Date: 10/01/25

	Description of project:
Construction of pub/hotel


	Site Classification/s:
Mostly rock or very stable soil with little or no ground movement due to moisture changes.

	Documentation of design and construction (suitability or evidence of suitability)

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earthworks
	AS 3798 - Guidelines for Earthworks for Commercial and Residential Developments

	N/A

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earth retaining structures
	AS 4678 - Earth-retaining Structures

	N/A

	Drainage
	NCC Volume 1 Section F, AS/NZS 3500.3 Plumbing and Drainage

	N/A

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Termite risk management
	AS 3660.1 Termite Management

	Physical barrier system applied


	Materials
	NCC Volume 1 Section B - Structural Provisions

	N/A

	Footings and slabs

	Site classification

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Footings and slabs
	AS 2870 - Residential Slabs and Footings

	Standard design for Class M soil


	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Moisture Barrier
	AS 2870 - Damp-proofing under slabs

	Polyethylene sheeting applied


	Materials
	NCC Volume 1 Section B - Structural Provisions

	Reinforced concrete to 28 MPa


	Concrete and reinforcement

	Concrete and reinforcement
	NCC / Australian Standards requirements
	Compliant Performance solution

	Concrete and reinforcement
	AS 3600 - Concrete Structures

	Reinforced with F72 mesh


	Materials
	AS/NZS 4671 - Steel Reinforcing Materials

	Tied reinforcement to comply


	Masonry

	Masonry
	NCC / Australian Standards requirements
	Compliant Performance solution

	Masonry
	AS 3700 - Masonry Structures

	Compliant masonry walls


	Moisture Barrier
	AS 3700 - Damp-proofing

	Damp-proof course applied


	Materials
	NCC Volume 1 Section B - Structural Provisions

	Standard masonry units used


	Framing/Structure

	Framing/Structure
	NCC / Australian Standards requirements
	Compliant Performance solution

	Framing
	AS 1684 - Residential Timber Framing Code

	Engineered timber applied


	Materials
	AS 1720 - Timber Structures

	Grade verified


	Roof and Wall Cladding

	Roof and wall cladding
	NCC / Australian Standards requirements
	Compliant Performance solution

	Roof and wall cladding
	AS 1562.1 - Design and Installation of Sheet Roof and Wall Cladding

	Metal cladding for durability


	Materials
	NCC Volume 1 Section B - Structural Provisions

	Compliant cladding materials


	Glazing

	Glazing
	NCC / Australian Standards requirements
	Compliant Performance solution

	Glazing
	AS 1288 - Glass in Buildings - Selection and Installation

	Safety glazing applied


	Materials
	NCC Volume 1 Section B - Structural Provisions

	Laminated glass used where required


	Fire Safety

	Fire Safety
	NCC / Australian Standards requirements
	Compliant Performance solution

	Fire Safety
	NCC Volume 1 Part C1 - Fire Resistance and Stability

	Fire-rated walls installed


	
	
	

	
	
	

	Access/Stairs/Lifts/Ramps

	Access/Stairs/Lifts/Ramps
	NCC / Australian Standards requirements
	Compliant Performance solution

	Access
	AS 1428.1 - Design for Access and Mobility

	Ramp slope compliant


	
	
	

	Materials
	NCC Volume 1 Section D - Access and Egress

	Durable finishes applied


	Ancillary Provisions

	Ancillary Provisions
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	NCC Volume 1 Section G

	N/A

	
	
	

	
	
	

	Energy Efficiency

	Energy Efficiency
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	NCC Volume 1 Section J - Energy Efficiency

	Insulated roofing and walls applied


	
	
	

	
	
	

	Health and Safety

	· Compliance with NCC Work Health and Safety provisions ensured.
· Materials conform to Australian Standards for durability and safety.




	Consultation

	Engineers
Architects
Fire engineers
Local authorities

	Policies

	

	Procedures

	

	Issues to be addressed and consultation

	Issue
	Who to consult
	Improvements for consideration
	Feedback following consideration
	Supporting Resources
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