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Documentation of design and construction (suitability or evidence of suitability)
	Project Name: Rockpool Pelican waters

	Project address: 17 Spitfire banks Drive
	Site Plan attached: 

	Prepared by: Ric

	Date: 9/11/2023

	Description of project:
150 Room Aged care facility

	Site Classification/s:
Class 9c

	Documentation of design and construction (suitability or evidence of suitability)

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earthworks
	Part 3.2 Earth works

	3.2.1 Un-retained bulk earth works – site cut and fill

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earth retaining structures
	3.1.2 earth retaining structures
	a. Performance RequirementP2.1.1; and
a. The relevant Performance Requirements determined in accordance with A2.2(3) and A2.4(3) as applicable.


	Drainage
	3.3 Drainage    
	3.3 Drainage – 3.3.1 Application
                         3.3.2 Drainage requirements
                         3.3.3 Surface drainage
                         3.3.4 Subsoil drainage
                         3.3.5 Stormwater drainage    
                         


	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Termite risk management
	3.4 Termite risk management

	3.4.1 Requirements for termite management systems
3.4.2 Termite management system
3.4.3 Durable notice

	Materials
	Steel Aluminium, other metals
 Concrete, Masonry, fibre re-enforced cement,
Timber-naturally termite resistance in accordance with Appendix C AS3660.1.  
Timber- preservative in accordance with Appendix D AS3660.1.
	Fibre crete into ground footings.
Removed load bearing block walls and installed structural steel columns to hold up roof frame loads.
[bookmark: _GoBack]

	Footings and slabs

	Site classification: 

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Footings and slabs
	4.1 Scope and application of section 4



4.2 Footing, slab and  associated elements
	4.1.1 Scope
4.1.2 Applications
4.1.3 Explanation of terms

4.2.1 to 4.2.22

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Moisture Barrier
	Part 4.2 Footings, slabs and associated elements
	4.2.8 Vapour barriers

	Materials
	0.2 mm nominal thickness polyethylene film; and medium impact resistant, determined in accordance with criteria specified in clause 5.3.3.3 of AS 2870.(3)A vapour barrier must be branded continuously “AS 2870 Concrete underlay, 0.2 mm Medium impact resistance”.(4)Installation: A vapour barrier must be installed as follows: Lap not less than 200 mm at all joints. Tape or seal with a close-fitting sleeve around all service penetrations. Fully seal where punctured (unless for service penetrations) with additional polyethylene film and tape.
	

	Concrete and reinforcement

	Concrete and reinforcement
	NCC / Australian Standards requirements
	Compliant Performance solution

	Concrete and reinforcement
	Part 4.2 Footings, slabs and associated elements - 


	
	4.2.10 concrete


	Materials
	Concrete must comply with AS 3600; and—have a strength at 28 days of not less than 20 MPa (denoted as N20 grade); and have a 20 mm maximum nominal aggregate size; and have a nominal 100 mm slump. Water must not be added to the mix to increase the slump to a value in excess of that specified. Concrete must be placed, compacted and cured in accordance with good building practice.
	

	Masonry

	Masonry
	NCC / Australian Standards requirements
	Compliant Performance solution

	Masonry
	5.1.1 Scope and application of Section 5
5.1.2 Application
	Part 5.2 Masonry veneer  52.1 - 5.2.6,
Part 5.3 Cavity masonry  5.3.1 - 5.3.7, 
Part 5.4 Unreinforced single leaf masonry   5.4.1 – 5.4.5, 
Part 5.5 Isolated piers   5.5.1 – 5.5.6
Part 5.6 Masonry components and accessories    5.6.1 – 5.6.8, 
Part 5.7 Weatherproofing of masonry   5.7.1 – 5.7.6

	Moisture Barrier
	Part 5.7 Weatherproofing of masonry
	Part 5.7 Weatherproofing of masonry   5.7.1 – 5.7.6

	Materials
	A material that complies with AS/NZS 2904; or embossed black polyethylene film of high impact resistance and low slip, with a nominal thickness of 0.5 mm prior to embossing, and comply with clause 7.6 of AS/NZS 2904; or polyethylene coated metal, that has an aluminium core of not less than 0.1 mm thick, is coated both sides with bitumen adhesive enclosed in polyethylene film of not less than 0.1 mm thick on each face, and has a nominal total thickness of not less than 0.5 mm prior to embossing; or bitumen impregnated materials of not less than 2.5 mm thick, that comply with clause 7.5 of AS/NZS 2904; or termite sheet materials complying with Part 3.4 (with no penetrations) serving the purpose of a damp-proof course and/or flashing that is continuous through the wall or pier.
	

	Framing/Structure

	Framing/Structure
	NCC / Australian Standards requirements
	Compliant Performance solution

	Framing
	Part 6.1 Scope and application of Section 6
6.1.1 Scope
6.1.2 Application
	Part 6.2 Subfloor ventilation 
6.2.1 Subfloor ventilation

Part 6.3 Structural steel members
6.3.1 to 6.3.9

	Materials
	Structural steel members may be used as follows: Bearers supporting a timber floor or non-loadbearing stud wall — in accordance with 6.3.3.Strutting beams supporting roof and ceiling loads — in accordance with 6.3.4.Lintels supporting roof, ceiling, and frame and timber floor— in accordance with 6.3.5.Columns— in accordance with 6.3.6.
	

	Roof and Wall Cladding

	Roof and wall cladding
	NCC / Australian Standards requirements
	Compliant Performance solution

	Roof and wall cladding
	Part 7.1 Scope and application of Section 7
7.1.1 Scope
7.1.2 Application
	Part 7.2 Sheet roofing 7.2.1 – 7.2.8
Part 7.3 Roof tiles and shingles 7.3.1 – 7.3.6
Part 7.4 Gutters and downpipes 7.4.1 – 7.4.7
Part 7.5 Timber and composite wall cladding -
7.5.1 – 7.5.8

	Materials
	Fasteners
Galvanized or zinc/aluminium sheet metal
Machine-folded sheet metal sections
Fasteners for flashings and capping (must comply with 7.2.5.)
Fascia
Downpipe and fixing clips, guttering
Selected Roof tiles and shingles.
	

	Glazing

	Glazing
	NCC / Australian Standards requirements
	Compliant Performance solution

	Glazing
	Part 8.1 Scope and application of Section 8
8.1.1 Scope
8.1.2 Application
	Part 8.2 Windows and external glazed doors 8.2.1 – 8.2.2
Part 8.3 Glass 8.3.1 – 8.3.3
Part 8.4 Glazing human impact 8.4.1 – 8.4.8

	Materials
	Appropriate glazing specified for job.
3 mm monolithic annealed glass, the maximum area must not be more than 0.85 m2.
Glazing used in areas where the potential for human impact could occur must comply with the appropriate provisions listed in Part 8.4.
Glazing used in the perimeter of buildings and supported on all sides must comply with the appropriate provisions listed in 8.3.3.
	

	Fire Safety

	Fire Safety
	NCC / Australian Standards requirements
	Compliant Performance solution

	Fire Safety
	Part 9.1 Scope and application of Section 9
9.1.1 Scope
9.1.2 Application
	Part 9.2 Fire separation of external walls  9.2.1 – 9.2.10
Part 9.3 Fire protection of separating walls and floors  9.3.1 - 9.3.4
Part 9.4 Fire protection of garage top dwellings  9.4.1 -9.4.2
Part 9.5 Smoke alarms and evacuation lighting  9.5.1 – 9.5.5

	
	
	

	
	
	

	Access/Stairs/Lifts/Ramps

	Access/Stairs/Lifts/Ramps
	NCC / Australian Standards requirements
	Compliant Performance solution

	Access
	Part 11.1 Scope and application of Section 11
11.1.1 Scope
11.1.2 Application
	Part 11.2 Stairway and ramp construction 11.2.1 – 11.2.6
Part 11.3 Barriers and handrails 11.3.1 – 11.3.8

	
	
	

	Materials
	Timber, Glass, Steel, aluminium, Metal, Composite 
	

	Ancillary Provisions

	Ancillary Provisions
	NCC / Australian Standards requirements
	Compliant Performance solution

	Ancillary Provisions
	Part 12.1 Scope and application of Section 12
12.1.1 Scope
12.1.2 Application
	Part 12.2 Construction in alpine areas 12.2.1 – 12.2.4
Part 12.3 Attachment of framed decks and balconies to external walls of buildings using a waling plate –12.3.1 – 12.3.4
Part 12.4 Heating appliances, fireplaces, chimneys and flues  12.4.1 – 12.4.5


	
	
	

	
	
	

	Energy Efficiency

	Energy Efficiency
	NCC / Australian Standards requirements
	Compliant Performance solution

	Energy Efficiency
	Part 13.1 Scope and application of Section 13
13.1.1 Scope
13.1.2 Application
	Part 13.2 Building fabric 13.2.1 – 13.2.7
Part 13.3 External glazing 13.3.1 – 13.3.4
Part 13.4 Building sealing 13.4.1 – 13.4.7
Part 13.5 Ceiling fans 13.5.1 – 13.5.2
Part 13.6 Whole-of-home energy usage 13.6.1 – 13.6.2
Part 13.7 Services 13.7.1 – 13.7.9


	
	
	

	Health and Safety
	Part 10.1 Scope and application of Section 10
10.1.1 Scope
10.1.2 Application
	Part 10.2 Wet area waterproofing 10.2.1 – 10.2.32
Part 10.3 Room heights 10.3.1
Part 10.4 Facilities 10.4.1 – 10.4.2
Part 10.5 Light 10.5.1 – 10.5.2
Part 10.6 Ventilation 10.6.1 – 10.6.3
Part 10.7 Sound insulation 10.7.1 – 10.7.8
Part 10.8 Condensation management 10.8.1 – 10.8.3

	Health and Safety

	



	Consultation

	Consultation is the cornerstone of the Australian Building Codes Board's (ABCB) commitment to maintaining a contemporary and relevant National Construction Code (NCC). The consultation process also relates to our CodeMark Australia and WaterMark product certification schemes. This hub is a place for you to find and participate in consultations that interest you

	Policies

	As a general user of the National Construction Code (NCC), you will likely only need one particular volume:
· Volume One for commercial construction;  
· Volume Two, for residential housing; or
· Volume Three for plumbing and drainage.
The Deemed-to-Satisfy Solutions within the NCC are the parts of the code you will likely need for your project. 
It’s important to remember however, that while the NCC sets out the legal requirements for construction of a house, building or plumbing and drainage installation, it’s the state or territory legislation that give it legal effect.
State and territory regulation
The NCC is given legal effect through building or plumbing legislation set out by your state or territory government, or other statutory authority. These Acts and Regulations set out the legal framework and administration mechanisms for the NCC, to support the design and construction of buildings and plumbing and drainage systems.
The dates of adoption of the NCC are determined by State and Territory building or plumbing administrations.


	Procedures

	Administrative requirements
Administration requirements typically covered in your state or territory legislation include:
· Plan submission and approval procedures
· Issue of permits
· Inspections and audits
· Provision of evidentiary certificates
· Issue of certificates
· Review and enforcement of standards
· Fees and charges
In some jurisdictions, some of these administrative requirements may be undertaken by your local government.


	Issues to be addressed and consultation

	Issue
	Who to consult
	Improvements for consideration
	Feedback following consideration
	Supporting Resources

	Render cracking
	Render Subbie
	Render no thicker than 7mm unless hi-build used to bulk up before final finish coat
	Subbie agreed and changes were made
	Consult NCC

	Render cracking over 4 meters
	Render Subbie
	Construction movement joint filled with flexible closed cell polyethylene.
Flexible sealant in coursing line of render. Proprietary bead used both sides of joint and rendered to the bead.
	Subbie agreed and changes were made
	Consult NCC

	Bathroom floor ties drummy
	Tile Subbie
	Rip up Tiles, identify effected area in bedding.
Repair and relay
	Tile subbie agreed and rectified defect
	Consult NCC

	Feature Stone cladding is heavier than quoted. Maybe too heavy for glue
	Tile Subbies
	Heavy steel angle used
To support part of the weight, changed to recommend adhesive   
	After consultation all parties  agreed and rectified issue
	Consult NCC

	Hot water not being delivered to each level of building
	Plumber
	Upgrade of Pump system to better handle requirements
	Plumber agreed and changes were made
	Consult NCC

	Gap between wall and downpipe would allow water to penetrate under waterproofing on deck 
	Waterproof Subbie
	Carry waterproofing up wall and seal behind downpipe/wall so water cannot penetrate under waterproofing membrane
	All parties agreed and rectified issue
	Consult NCC
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