CONTRACT TITLE:  

LOCATION:  

DRAWING NUMBERS:

SITE SPECIFIC DOCUMENT NUMBER:   

NO.
ITEM
INSPECTION
STANDARD
INSPECT BY
Y / N
NA
COMMENTS
1
Check set out of penetrations
Drawing/Spec
A




2
Check location and set out and design of pipe work and council approved plans
Drawing/Spec
A




3
Check fall and coordinate with other trades
Drawing/Spec
AS3500.2
A


4
Check type material –pipe clips, jointing method 
Drawing/Spec 
AS3500.2
A



5
Visual inspection prior to welding, glue or final connection

A


6
Check fire rating any penetrations

ITP/ CC /F.R.
AS1530.4, AS4072, BCA 3.12, C3.15
A/W


7
Test pipe work
Water 
AS3500.2
A




Air 
AS3500.2
A 


8
Pipe ID / Tape
Spec
AS3500.2
A/W



9
Inspection- Council- Other statutory authority

A



Photos attached





KEY  A= CC INSPECTION  W= CLIENT WITNESS POINT H= HOLD POINT G=GCCC
Supervisors Confirmation of Satisfactory Inspection
Checklist completed by:
Name: 
Signature:

Date: ___/___/___

