Jeremy Tydd
CPCCBC4012 Read and interpret plans and specifications

Any documentation or photographic evidence in support of reading and interpreting plans and specifications (e.g. any modifications that the candidate has applied to existing project plans, environmental plans, plans/drawings and specifications)
10X75mmx250mm plate has been added in on top of the posts for the beams to be bolted to make the structure stronger. This can be seen in the attached photos 
All structural steel works is in accordance with AS4100, AS1418, AS/NZS1554
C1 Members are 100x 5mm SHS Columns, these are the two large posts holding the structure up on the outside.
C2 members are 76x4.5 mm CHS  and there is 4 off them the are able to be a little smaller as there is 4, as 76mm sits on the top plate of the house a lot neater. 
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GENERAL NOTES

9.
10.
1t
12
13,
14,

15.

'ALL PROFESSIONAL ACTIVITIES TO BE IN ACCORDANCE WITH THE RELEVANT SECTIONS OF THE; QUEENSLAND BULDING ACT,
'QUEENSLAND WORKPLACE HEALTH AND SAFETY ACT AND CODES, CODES OF PRACTICE, NATIONAL CONSTRUCTION CODE AND
AUSTRALIAN STANDARDS AS WELL AS ACCEPTED INDUSTRY BEST PRACTICES AND THESE STRUCTURAL DRAWINGS.

ALL PROFESSIONAL ACTIVITIES TO BE PERFORMED IN A SAFE AND RESPONSIBLE MANNER BY SUITABLY QUALIFIED AND LICENSED
'SUB CONTRACTORS AND CONTRACTORS,

SAFETY IN DESIGN HAS BEEN CONSIDERED FOR ALL PHASES OF THIS PROJECT AND THE RELATED RISKS HAVE BEEN DEEMED TO BE
TYPICAL OF THIS PROJECT. DUE CAUTION AND CARE TO BE EXHIBITED AT ALL TIMES.

IT IS THE CONTRACTOR'S RESPONSIBILITY TO ENSURE THE STRUCTURE IS MAINTAINED IN A STABLE CONDITION DURNG
CONSTRUCTION WITH SUFFICIENT TEMPORARY BRACING.

'DONOT SCALE OFF THESE DRAWINGS. I IN DOUBT ASK.

THESE STRUCTURAL DRAWINGS HAVE BEEN BASED ON THE BEST INFORMATION AVAILABLE DURING THE DESIGN PROCESS
HOWEVER ALL EXISTING STRUCTURAL ELEMENTS SHOULD BE VERIFIED BY THE CONTRACTOR PRIOR TO COMMENCING WORKS. ANY
DISCREPANCIES SHALL BE REFERRED TO CQ STRUCTURAL ENGINEERING.

THESE STRUCTURAL DRAWINGS SHALL BE READ IN CONJUNCTION WITH ALL OTHER CONSULTANTS DRAWINGS AND SPECIFICATIONS
FOR RELEVANT INFORMATION. ANY DISCREPANCIES SHALL BE REFERRED TO THE CQ STRUCTURAL ENGINEERING PRIOR TO
COMMENCING RELEVANT WORKS.

AL TERMITE MANAGEMENT AND WATERPROOFING SHALL BE IN ACCORDANCE WITH ARCHITECT'S SPECIFICATIONS, THE RELEVANT
AUSTRALIAN STANDARDS AND ACCEPTED INDUSTRY PRACTICES. TERMITE MANAGEMENT SHALL NOT PREVENT CONNECTION OF
STRUCTURAL ELEMENTS.

ALL SET OUT, LEVELS AND DIMENSIONS SHALL BE IN ACCORDANCE WITH THE ARCHITECT'S DRAWINGS.

DIMENSIONS IN THESE STRUCTURAL DRAWINGS WILL TYPICALLY BE IN MILLIMETRES AND LEVELS IN METRES.

ALL DETALLS IN THE STRUCTURAL DRAWINGS TAKE PRECEDENCE OVER THESE SPECIFICATION NOTES, ANY DISCREPANCIES SHALL
BE REFERRED TO THE CQ STRUCTURAL ENGINEERING FOR CLARIFICATION.

ALLOW FOR MOVEMENT IN THE FOUNDATION MATERIALS BY FOLLOWING THE RELEVANT CONSULTANT'S AND MANUFACTURER'S
DETAILS AND SPECIFICATIONS REGARDING ARTICULATION OF ALL CLADDING, LININGS, SERVICES AND FINISHES.

ALL PROPRIETARY PRODUCTS ARE TO BE USED, APPLIED ANDIOR INSTALLED IN ACCORDANCE WITH MANUFACTURER'S
'SPECIFICATIONS, DETAILS AND GUIDELINES,

LOCATION OF ALL EXISTING IN-GROUND AND ABOVE GROUND SERVICES TO BE CONFIRMED BY THE CONTRACTOR. ALL EXISTING.
'SERVICES SHOWN IN THESE DRAWINGS ARE INDICATIVE ONLY.

ANY DEVIATIONS OR ALTERATIONS TO THESE DRAWINGS SHALL BE APPROVED BY CQ STRUCTURAL ENGINEERING.

DESIGN DATA

'SOUND STRUCTURAL ENGINEERING JUDGEMENT, APPLICATION OF ACCEPTED STRUCTURAL ENGINEERING PRINCIPLES AND THE
RELEVANT SECTIONS OF THE QUEENSLAND BUILDING ACT, NATIONAL CONSTRUCTION CODE, AUSTRALIAN STANDARDS AND
MANUFACTURER'S PUBLICATIONS HAVE BEEN CONSIDERED IN THE PREPARATION OF THESE STRUCTURAL DRAWINGS,
THE FOLLOWING UNIFORMLY DISTRIBUTED/CONCENTRATED ACTIONS AND PARAMETERS HAVE BEEN ASSESSED AS APPROPRIATE
FOR THIS PROJECT.
21 IMPOSED ACTIONS

211, ROOF-025KPAAND 1.4KN

22. WINDLOADS
221, STRUCTURAL IMPORTANCE LEVEL 2
222 REGIONC

223 TERRAN CATEGORY 2
224, WIND DIRECTION MULTIPLIER (M) 0.9/1.0

225 TERRANHEIGHT MULTIPLIER (Mcar) 091

226, SHIELDING MULTIPLIER (M) 1.0

227 CLIMATE CHANGE MULTIPLIER (M) 105

228 TOPOGRAPHICAL MULTIPLIER (Mr) 1.0

229, FREE ROOFS ARE PARTIALLY BLOCKED UNDER
2210, EQUIVALENT AS4055 WIND CLASSIFICATION C2

STRUCTURAL STEEL WORKS

'ALL STRUCTURAL STEEL WORKS SHALL BE IN ACCORDANCE WITH AS4100, AS1418, ASINZS1554, AS 1627, ASNZS2312, AS3828,
ASINZS4500, ASINZS5131 AND THESE STRUCTURAL ENGINEERING DRAWINGS.

CONTRACTOR TO PROVIDE ACRS CERTIFICATES FOR ALL STRUCTURAL STEEL AND FABRICATED STRUCTURAL STEEL.

ALL STRUCTURAL STEEL SHOP DRAWINGS SHALL BE SUBMITTED TO CQ STRUCTURAL ENGINEERING FOR APPROVAL.
STRUCTURAL STEEL SHALL COMPLY WITH,

4.1, SQUARE HOLLOW SECTIONS - GRADE 350MPA TO ASNZS1163

42, RECTANGULAR HOLLOW SECTIONS - GRADE 350MPA TO ASINZS1163

43, PLATE - GRADE 350MPA TO ASINZS3678

BOLTS, NUTS AND WASHERS ARE TO COMPLY WITH

51. 4.6/ BOLT- GRADE 4.6 COMMERCIAL TOAS1111 AND AS1112

ALL STRUCTURAL STEEL WELDING SHALL COMPLY WITH AS1554 AND SHALL BE COMPLETE BY AN EXPERIENCED AND QUALIFIED
WELDER. ALL WELDS ARE TO BE 6MM CONTINUOUS FILLET WELD UNO. ALL ELECTRODES TO BE E48XX. FLAME CUT EDGES TO BE.
‘GROUND SMOOTH. REMOVE SHARP EDGES AND BURRS. ALL WELD SPLATTER TO BE REMOVED.

SURFACE PREPARATION SHALL BE CLASS 25 ABRASIVE BLAST CLEAN GENERALLY WITH INTERMEDIATE AND TOP COATS TO
ARCHITECT' DETALLS. CORROSION PROTECTION OF STRUCTURAL STEEL SHALL BE:

7.1, EPOXY PRIMER - INTERNATIONAL PROTECTIVE COATINGS INTERZING £2 OR SIMILAR. MIN 70uM THICK.

INSTALL NON-SHRINK CEMENTITIOUS GROUT UNDER ALL BASE PLATES.

STRUCTURAL STEEL WORKS SHALL COMPLY WITH;

9.1, AL STRUCTURAL STEEL ENCASED IN CONCRETE SHALL HAVE RUST INHIBITING SEALANT (BITUMINOUS SEALANT OR SIMILAR).
92. FABRICATE ALL CLEATS FROM 10MM FLAT BAR.

93. GRIND ALL SHARP EDGES AND CORNERS SMOOTH.

94. AL CHS, RHS AND SHS MEMBERS SHALL BE SEALED WITH 3MM PLATES.

95. BOLTS SHALL BE M16 4 6/5. ALL EXTERNAL BOLTS SHALL BE GALVANISED.

Member Schedule
C1 - 100x5 SHS Column.
C2 - 76x4.5 CHS Stub Column or
similar proprietary flyover bracket.
Space evenly to match existing

trusses

B1 - 150x100x4 RHS Beam.
B2 - 170x63 LVL Beam - Sheet
with FC sheeting and full seal.
~—> Span direction of 125 Solarspan
panel. Fix in accordance with
manufacturer's details. 5 degree

pitch nominal

EB (V) - Existing beam under

#14 Tek screw
with cyclone cap
into each rib

I |

Slab/Footing Plan

Solarspal P

10 Cap plate
1/10 Gusset
both sides

4/M16 Studs
Plug welded

concrete

Existing
concrete
thickening

Existing
concrete slab

Existing

1200 Max

7000 Max

<—><

1200 Max

e

Existing
roof line

4800 Max
Roof Framing Plan

Type 17 - #14 Screw
with cyclone cap into
each rib. Min 200 long.
Pre drill into timber

8 Cap plate
2/M10 bolts
Recess into B2 as required

Dektite or similar

8 Cleat plate
2/M10 bolts




