Metal Roofing ITP Pelican Waters
Pre Roof													Response Type
Certified EDGE PROTECTION and safety systems are installed and complete with handover certificate received. 
Attach sign off.												Hold Point
Check colours, profiles, material thicknesses against project specification: Attach photos of delivery docket. 
Photos of delivery dockets.											Yes/No
Insulation meets the R value as stated in section J report. Attach Documents.						Yes/No
Facia has been packed with water resistant product to stop facia from oil canning. Photos				Yes/No
Confirm Combustible products are not used under metal cladding/ sheeting. Check BA conditions and/or with certifier.
Email 													Yes/No

Roofing Contractor	
Safety wire is completed and installed to AS/NZS 4389 and HB39:2015 section 4.4. Attach photos of loop ties.		 Yes/No
Confirm no insulation crosses tops of fire walls and underside is neat and tidy. Photos					Yes/No
Box gutter support brackets, laps, under/over sealing – installed as per design. Photos					Yes/No
All swarf is cleaned of daily.											Yes/No
Sheets are the same length and have the correct overhang into gutter (250mm). 					Yes/No
Expansion Joints installed in accordance with the project documentation and HB39:2015 section 7.7 check minimum 250mm overlap, additional purlins installed and trays turned up/down.								Yes/No
All sheet laps are correct as per AS 1562.1 section 4.5 laps to be 250mm based on a roof pitch below 15%.			Yes/No
All sheets have been correctly turned up under flashings and turned down into gutter. Photos				Yes/No
All screws have neo seals installed in a straight line and not overtightened with correct colour fixings. Photos 		Yes/No
Apron flashings turned up minimum 100mm and the hanging flashing/ over flashing 50mm min and 25mm away from soaker gutter or apron. Photos													Yes/No
Barge/ parapet capping/ flashings installed as per HB39-2015. Section 8.7. Photos					Yes/No
Ridge capping’s are to be scribed and cut neat and tidy. Photos							Yes/No
All decktite’s/ pan flashings installed over a rib and are to be under and over sealed. Installed as per manufacturer’s installation guide. Documents and photos											Yes/No
Any roof repairs have been completed in accordance with the manufacturer’s specifications. Photos			Yes/No

McNab/ Subcontractor Inspection /Sign off
Inspect roof and gutters to confirm all swarf removed, gutters and roof cleaned of rubbish. All joints under and over sealed, no damage to sheets, sarking and insulation is neat and tidy, etc. Photos								Yes/No
[bookmark: _GoBack]Roof has been videoed and water tested before safety handrail / edge protection has been removed.			Hold Point

Safety System
Anchor safety system installed as per AS 1891.4 – 2009 – Industrial fall arrest system 					Yes/No
All anchor points installed as per plan and signed off with tag attached. 						Yes/No
All material removed from roof and gutters including swarf, screws and material.					Yes/No
							
