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CPCCBC4010B 
Apply structural principles to residential low rise constructions

CPCCBC4011B
APPLY STRUCTURAL PRINCIPLES TO COMMERCIAL LOW RISE CONSTRUCTIONS

	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.



	[bookmark: _Ref531082936]Participant name
	Haydn Morriss

	

	

	Participant signature
	



	Assessor name
	

	

	

	Assessor signature
	



	Date
	2/01/2019



	Number of questions
	Number of questions answered correctly
	Satisfactory?

	93
	
	Yes
	No

	
	
		

	ASSESSOR COMMENTS

	


What is the most important aspect in the design of buildings? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Aesthetics
	

	
		Cost
	

	
		Location
	

	
		Stability
	




[bookmark: _Ref531083005]Where can the definitive properties of materials used in the building industry be found? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Australian Standards
	

	
		Building journals
	

	
		Practical learning on the job
	

	
		Textbooks on building
	




[bookmark: _Ref427229923]Which industry professional would you contact for structural advice? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Architect
	

	
		Draftsperson
	

	
		Engineer
	

	
		Quantity surveyor
	




[bookmark: _Ref531353369]Which industry professional would you contact for the preparation of working drawings? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Building surveyor
	

	
		Draftsperson
	

	
		Quantity surveyor
	



[bookmark: _Ref427229919]Briefly describe the role of an architect.

	Answer
	The role of an architect is to design buildings that comply with various codes and legislations. They also help with setting a budget for the building construction
	



[bookmark: _Ref427229924]What is the difference between a building surveyor and a land surveyor?

	Answer
	Building surveyors provide professional advice on property and construction. They ensure buildings comply with building codes and assess building plans submitted for approval. Land surveyors assess surrounding landscape for the purpose of development. They set up building lines and conduct boundary surveys. 
	



[bookmark: _Ref427229926][bookmark: _Ref531353386]Which industry professional would you contact for matters relating to cost? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Architect
	

	
		Building surveyor
	

	
		Engineer
	

	
		Quantity surveyor
	



[bookmark: _Ref531353744]A land surveyor is to reinstate survey pegs. Which of the following documents would the surveyor need? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Title
	

	
		Contour plans
	

	
		Project specifications
	




[bookmark: _Ref531353745]When preparing a trench a builder digs through a gas pipe which was not shown on the plans. Which report should be used to prove the mistake was not the builder’s? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Engineer’s drawings
	

	
		Condition report
	

	
		Soil report
	




[bookmark: _Ref427230180][bookmark: _Ref531353749]Which two (2) of the following can be determined from the contour report? Tick your responses.

	Answer
	Choice
	Possible Answers
	
	
		Extent of cut and fill
	

	
		Height of retaining walls
	

	
		Location of trees
	

	
		Location of windows
	




[bookmark: _Ref531353759]The customer has requested a glass balcony. Which document would the builder refer to for information on structural members? 
Tick your response. 

	Answer
	Choice
	Possible Answers
	
	
		Building specifications
	

	
		Condition report
	

	
		Engineering report
	



[bookmark: _Ref427230170][bookmark: _Ref531353761]The builder is planning a project and requires information on the location of fixtures and fittings, windows and doors. Which plans show this information? Tick your response. 

	Answer
	Choice
	Possible Answers
	
	
		Cross sections
	

	
		Floor plans
	

	
		Footing designs
	




[bookmark: _Ref427230166][bookmark: _Ref531353766]After an inspection, the client believes that what was installed is different to what they had chosen in the contract. What document details the materials the builder was meant to use? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Building specifications
	

	
		Plan of the subdivision
	

	
		Site plan
	




[bookmark: _Ref427579066][bookmark: _Ref531353770]What key pieces of information can be found on a site plan? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Location of street frontage
	

	
		Location of proposed building
	

	
		North point
	




[bookmark: _Ref427230177]What is the purpose of a footing design?

	Answer
	The purpose of footing design to ensure loads are distributed  on the foundation below whilst complying with AS 2879 – 2006.
	



[bookmark: _Ref531354185]Why would a pre-commencement site inspection be conducted? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		To ensure all contract documentation clearly reflects the actual site
	

	
		It allows the supervisor to get some fresh air
	

	
		To ensure that the client actually owns the property
	

	
		So that levels can be taken to check the slope of the site
	




[bookmark: _Ref531082938]What are the dead loads in a building? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		All stationary materials
	

	
		Permanent materials
	

	
		Roofing materials
	

	
		Use for which the building is intended
	




[bookmark: _Ref531082940]What is the formula for calculating a dead load?

	Answer
	Dead load = Volume of member x Unit weight of materials
	



[bookmark: _Ref531082941]What are the live loads in a building? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Loads arising from the function of the structure
	

	
		Loads due to rain
	

	
		Loads due to wind
	

	
		Utility services
	





Refer to the table shown below to respond to Q20. to Q21.  These values are used to calculate live loads using the formula: Area of floor x Live load rating.

	Live loads for floors as per building usage
	Uniformly distributed load (kPa or kN/m²)

	Houses
	1.5

	Flats, motel bedrooms, apartments
	2.0

	Offices
	3.0

	Workshops
	5.0

	Parking, vehicle >2.5t
	5.0

	Hospitals, school assembly areas with fixed seating
	3.0

	Dance halls, bars, lounges
	5.0




[bookmark: _Ref481992592]Calculate the live load of a guest house measuring 23m x 8m. 
Show your calculations.

	Answer
	23.0m x 8.0m = 184m2
Live load rating of guest house =1.5kPa
184m2 x 1.5kPa = 276kN
	



[bookmark: _Ref427215838]Calculate the live load of a commercial office premises floor measuring 33m x 11m. Show your calculations.

	Answer
	33.0m x 11.0m = 363m2
Live load rating for office premises = 3kPa
363m2 x 1.5kPa = 544.50kN

	



Please refer to the information below in responding to Q22. to Q25. 

 (
There is a building 21
m
 long x 10
m
 wide x 8
m
 high with a 25
⁰
 pitched gable roof. The rafter line on the metal clad roof measures 5.5
m
 on the rafter line
 (
from the fascia/gutter line up to the ridge line
)
.
The wind load is calculated as 
Area of 
surface
 x 
W
ind load rate
.
 
The wind load rates are as follows:
Windward wall is 21 metres long x 8 metres high with a wind load rate of +1.5KN/m²; 
Leeward wall 
is 
21 metres long x 8 metres high with a wind load rate of -0.8kN/m²; 
Windward roof with a wind load rate of +0.8kN/m²; and 
Leeward roof with a wind load rate of -1.5kN/m²
)


[bookmark: _Ref427218342]What is the wind load of the windward wall? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-252kN
	

	
		134.4kN
	

	
		252kN
	

	
		86.4kN
	




[bookmark: _Ref427218344]What is the wind load for the leeward wall? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-134.4kN
	

	
		-94.2kN
	

	
		252kN
	

	
		134.4kN
	




[bookmark: _Ref427218346]What is the wind load for the leeward roof? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		-173.25kN
	

	
		92.4kN
	

	
		173.25kN
	

	
		-134.4kN
	




[bookmark: _Ref427057362]What is the wind load for the windward roof? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		252kN
	

	
		-92.4kN
	

	
		-252kN
	

	
		92.4kN
	





[bookmark: _Ref427217924]Explain the term ‘load path’ in reference to a building.

	Answer
	Load path is the direction each consecutive load will pass through to each of its members.Starting from the highest point going down to the lowest. 
	



[bookmark: _Ref427219307]Forces are represented as vectors and have three (3) properties. 
Name these properties.

	Answer
	Magnitude, direction and position.
	



[bookmark: _Ref427219642]Name five (5) structural members that a building may consist of.

	Answer
	Bearers
Trusses
Loading bearing walls
Floor
Wind bracing
	


[bookmark: _Ref427219933]What should be considered when determining the shape and type of material to use?

	Answer
	It’s strength, toughness, hardness, brittleness, ductility and malleability.
	



[bookmark: _Ref427220471]Match the mechanical properties and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Mechanical properties
	Answers
	Definitions
	
	
	1
	Brittleness
	1 - G
	A
	The resistance the structural member is able to offer the load that will just cause fracture. 
	

	
	2
	Elasticity 
	2 - C
	B
	The resistance to a fracture point of a material by repeated bending or twisting after yield point has passed.
	

	
	3
	Ductility
	3 - E
	C
	Present if a material deforms with loading and then returns to its original shape when the loads are removed.
	

	
	4
	Hardness 
	4 - H
	D
	If a material deforms when loaded and does not return to its original shape when the load is removed, causing permanent deformation. 
	

	
	5
	Malleability
	5 - F
	E
	Enables a material to be drawn out in the direction of its length. 
	

	
	6
	Plasticity
	6 - D
	F
	Can be hammered or otherwise worked into various shapes.
	

	
	7
	Strength
	7 - A
	G
	Causes material to break or snap off without any noticeable lengthening. 
	

	
	8
	Toughness
	8 - B
	H
	The degree of resistance to indentation or abrasion. 
	




[bookmark: _Ref427220295]Match the beam types and descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Beam type
	Answers
	Description
	
	
	1
	Cantilevered 
	1 - A
	A
	Overhang their supports.
	

	
	2
	Continuously supported
	2 - C
	B
	Supported at each end only.
	

	
	3
	Simply supported
	3 - B
	C
	Supported by 3+ support points. 
	



[bookmark: _Ref427225888]Match the column considerations and explanations by writing the appropriate letter next to each number in the centre column.

	Answer
	Column consideration
	Answers
	Explanation
	
	
	1
	Axially loaded column
	1 - A
	A
	The load is central to the centre of gravity axis. 
	

	
	2
	Buckling
	2 - E
	B
	The load is off-centre, resulting in bending and compressing stress being applied to the column.
	

	
	3
	End fixity and effective length
	3 - C
	C
	The rigid connection to other members at the top and bottom affects the way a column buckles.
	

	
	4
	Non-axially loaded column
	4 - B
	D
	[bookmark: _GoBack]Affects the maximum load a column can be allowed to support.
	

	
	5
	Slenderness ratio
	5 - D
	E
	Occurs at the weakness axis unless a lateral restraint is used to prevent it. 
	




[bookmark: _Ref427224602]Explain how a column is in compression.

	Answer
	A column is in compression as it bears the force of a load.  
	



[bookmark: _Ref427225635]Explain the letters ‘CHS’ and ‘SHS’ with reference to columns.

	Answer
	CHS – Circular hollow section is the most efficient shape for a column
SHS – Square hollow section is the second most efficient shape
	



[bookmark: _Ref427227379]Match the retaining wall types and descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Retaining wall
	Answers
	Description
	
	
	1
	Cantilevered retaining wall
	1 - B
	A
	Leans into the excavated soil and constructed at an angle between 45 and 80 degrees. Typically constructed from brickwork or pre-cast interlocking concrete units. 
	

	
	2
	Gravity retaining wall
	2 - C
	B
	Relies upon the correct placement of steel reinforcement and varying thickness of concrete to resist the soil pressure. 
	

	
	3
	Inclined retaining wall
	3 - A
	C
	Relies on its own weight to resist soil forces. Typically constructed from stone, brickwork or concrete. 
	




[bookmark: _Ref427227493]What is a ground level concrete slab floor?

	Answer
	It is a concrete floor that is poured directly into excavated trenches and relies on the existing ground for support.
	



[bookmark: _Ref427227808]What should you consider when selecting the type of slab floor?

	Answer
	The moisture content of the soil must be taken into consideration as the slab can become damaged from the ground moisture
	



[bookmark: _Ref531355302]True or False (Tick your response): Concrete slab floors are popular in the construction of structures because they take less time to construct.

	Answer
		True 
	
	
	
		False 
	
	





[bookmark: _Ref427228752]Match the following slab structural performance terms with the descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Description
	
	
	1
	Foundation movement
	1 - C
	A
	Placed along the perimeter of the slab. Design is influenced by the reactivity of the soils. 
	

	
	2
	Slab bending
	2 - B
	B
	Movement is classified as dishing or doming. 
	

	
	3
	Stiffening beams
	3 - A
	C
	Addressed by regulating the moisture content of the soil.
	




[bookmark: _Ref531355427]Which of these terms relate to a roof truss? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Chord, knee, web
	

	
		Spider, pitch, chord
	

	
		Ankle, heel, tar
	

	
		Web, heel, pitch
	




[bookmark: _Ref427229422][bookmark: _Ref531008635]What are important considerations when undertaking demolition work? Describe relevant legislation, regulations and/or Codes of Practice relating to planning requirements, environmental standards, and safe work practices.

	Answer
	Method of demolition
Fencing and hoardings needed
Protection of existing buildings
The order in which the structure will be demolished
Whether traffic control is necessary
Ensure required licences have been obtained and if a demolition permit is needed.
Any hazardous materials that relevant authorities need to be advised of.


The Demolition Code of Practice 2013 and Work Health and Safety Regulations 2011 must be adhered to.
	


[bookmark: _Ref531355335]When demolition is being undertaken, which of the following items must be checked daily? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		All boundaries are secured against unlawful entry
	

	
		All hazardous materials are removed or covered as required by OHS legislation
	

	
		All openings and elevated free edges are properly guarded
	

	
		All potential fire and safety hazards are eliminated and disconnected services are secured
	

	
		Asbestos is left on the nature strip for the garbage pickup
	

	
		Demolished materials have not been left on any floor or structure if their weight exceeds the safe carrying capacity of the floor or structure
	

	
		Emergency access routes are clear of debris
	

	
		Footpaths and public access are clear of demolished materials
	

	
		Neighbours have been notified not to hang out their washing
	

	
		No structure or part of a structure is left in such a condition that it may become dangerous, such as collapse due to wind or vibration
	

	
		Partly demolished elements are stabilised and loose materials are secured against bad weather
	

	
		Signs and balloons are in place for the garage sale
	

	
		Tell the demolisher to take a long lunch break as you don't need supervision
	

	
		Temporary hoardings, bracing, shoring and propping is tight and secure and in place as required to protect both workers and public
	




[bookmark: _Ref531355737]Identify two (2) requirements under the NCC with regards to construction in bushfire prone areas?

	Answer
	The requirements vary depending on the risk category that is determined, for BAL 29 post, stumps, columns etc must be constructed from bush fire resistant timber or non-combustible material. External wall cladding must be Bushfire resisting timber and sarking. 
	



[bookmark: _Ref427231195]What does AS3959 refer to?

	Answer
	AS3959 refers to the Construction of buildings in bushfire prone areas.
	



[bookmark: _Ref531355744]Which of the following can assist with providing sufficient restraint to transfer wind forces to the ground to prevent collapse, uplift or sliding off the footing systems? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Anchorage systems
	

	
		Bracing systems
	

	
		Connecting structural elements together
	




[bookmark: _Ref531355745]Which Australian Standard outlines the requirements of high wind areas?

	Answer
	AS 1170.2
	



[bookmark: _Ref427232597]The acceleration coefficient is a number which indicates the expected severity of the earthquake ground movement. Which Australian Standard should be referenced for this information?

	Answer
	AS 1170.4
	



[bookmark: _Ref531355751]True or False (Tick your response): Where the acceleration coefficient is greater than 0.15, there are additional NCC requirements than where the acceleration coefficient is 0.12.

	Answer
		True 
	
	
	
		False 
	
	





[bookmark: _Ref531355987]Which of the following areas require specific compliance in alpine areas? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Access bridges
	

	
		Access for emergency vehicles
	

	
		External doorways
	

	
		External ramps
	




[bookmark: _Ref531355991]Identify the Volume and Parts of the NCC that relate to each of the following areas for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Topic
	Classes 1 and 10
	Classes 2 to 9
	
	
	Bushfire
	Vol 2 Part 3.7.4
	Vol 1 Part G5
	

	
	High wind
	Vol 2 Part 3.10.1
	Vol 1 Part B1.2 
	

	
	Earthquake
	Vol 2 Part 3.10.2
	Vol 1 Part B1.2  
	

	
	Alpine area
	Vol 2 Part 3.7.5
	Vol 1 Part G4
	

	
	New technologies
	Vol 2 Parts 1.0.5 + 1.2
	Vol 1 Part A2
	




[bookmark: _Ref427232821][bookmark: _Ref531356004]How are emerging building technologies and methods assessed in the National Construction Code? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Using verification methods
	

	
		With ‘deemed to satisfy’ provisions
	

	
		With documentary evidence
	





[bookmark: _Ref531356217]True or False (Tick your response): Footings should be set out in accordance with the building plan.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531356194]Name three (3) different types of footing systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Stumps
Concrete slabs
Pier and Beam
	Concrete slabs
Drilled or driven piles
Reinforced concrete piers and beams
	




[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to footings (including damp coursing and provision of termite barriers) for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Vol 2 Parts 3.1 & 3.2
	Vol 1 Parts B1.4, F1.9 F1.10
	




[bookmark: _Ref531356170]For each of the following identify two (2) Australian Standards that relate to footings.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	AS 2870 AS1684
	AS/NZS 2904 AS3660
	





[bookmark: _Ref531356390]Name two (2) materials that may be used for damp proof coursing.

	Answer
	Aluminium and impact resistant plastic
	



[bookmark: _Ref531356392]Name two (2) termite resistant materials.

	Answer
	Steel and concrete
	



[bookmark: _Ref531356575]Name three (3) different types of floor systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Concrete slab
Bearers and joists

	Concrete slab
Brick bases
Engineered timber products 
	




[bookmark: _Ref427235728]What should be considered when constructing a floor system?

	Answer
	The type of flooring, the laying of pipes and reinforcement. Is the flooring system a concrete slab or require bearers and joists.
	



[bookmark: _Ref531356610]Which Australian Standard is referenced in Volumes 1 and 2 of the NCC regarding the requirements for slabs and footings?

	Answer
	AS2870
	



[bookmark: _Ref531356630]Name three (3) different types of materials used for wall systems or structures falling under Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Cavity brick
Concrete block
Timber
	Composite walls
Earth walls
Framed walls incorporating timber
	




[bookmark: _Ref531356612]Identify the Volume and Parts of the NCC that relate to masonry wall systems for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Vol 2 Part 3.3.1
	Vol 1 B1.4
	




[bookmark: _Ref531356616]Which Australian Standard is referenced in Volumes 1 and 2 of the NCC regarding masonry structures?

	Answer
	AS3700
	



[bookmark: _Ref427577558][bookmark: _Ref531356640][bookmark: _Ref427237033]Explain the purpose of bracing. 

	Answer
	Bracing enables framework to resist horizontal forces 
	



[bookmark: _Ref531357045]Explain the purpose of fixings and tie-downs. 

	Answer
	Fixings are necessary to ensure the structural adequacy for various framing members. Tie downs fixings provide for structural connections to resist uplift and shear forces in the floor, wall and roof framing.
	



[bookmark: _Ref531331115]Which Australian Standard relates to timber frames, bracing and fixings?

	Answer
	AS1684.2
	



[bookmark: _Ref531357052]For the Australian Standard in Q66. which part relates to cyclonic areas?

	Answer
	AS1684.3
	



[bookmark: _Ref531357065]Which of the following should be observed when checking the quality of the frame (whether, factory pre-cut and pre-nailed, factory pre-cut and assembled on site, or cut and assembled on site)? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Fixings must be protected from corrosion
	

	
		Fixings must be protected from termites
	

	
		Provision has been made for plumbing services and fixtures
	

	
		Tie downs and nominal nailing must both be present
	

	
		Top and bottom plates have a tight fit on studs
	

	
		Top plate is to be reinforced when rafters land on top of plates
	

	
		Walls are tied together
	

	
		Walls are plumb
	

	
		Walls are square
	



[bookmark: _Ref531357185]True or False (Tick your response): Sarking is a substitute for cladding and is regarded as the principal means of weatherproofing.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref427237737]What is flashing?

	Answer
	Flashings are used at corners and vertical joints and around openings to ensure that water does not enter wall frame cavity.
	



[bookmark: _Ref531357196]Identify the Volume and Parts of the NCC that relate to wall cladding material requirements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Vol 2 Part 3.5.3  
	Vol 1 Part J1.2
	




[bookmark: _Ref531357076]True or False (Tick your response): Timber can stand greater stresses than brickwork.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531357077]True or False (Tick your response): Individual timber boards for cladding should be nailed together at the overlap.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531357461]When should flashing materials be fixed to plywood cladding? 
Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		After the cladding is fixed
	

	
		Before the cladding is fixed
	

	
		While the cladding is being fixed
	

	
		At any convenient time
	




[bookmark: _Ref531357463]What is the purpose of articulation joints? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		They allow for shrinkage in a building
	

	
		They tie the brickwork to the frame
	

	
		They allow for movement in a building
	

	
		They seal the cavities 
	




[bookmark: _Ref531357466]When is the most appropriate time for the rough-in to occur for a brick veneer building constructed on a concrete slab Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Before brickwork
	

	
		After brickwork
	

	
		After plasterboard
	

	
		Any time
	




[bookmark: _Ref531357473]Apart from plumbing and electrical, name four (4) other services that should be considered at rough-in.

	Answer
	Communication sysytems
Extractive vacuum system
Smoke control & containment systems
Ducting for heating & cooling
	


[bookmark: _Ref531357478]Identify the Volume and Parts of the NCC that relate to window installation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Vol 2 Part 3.6
	Vol 1 B1.4, F1.13 J3.4
	




[bookmark: _Ref531357506]Name two (2) Australian Standards that relate to the installation of windows. 

	Answer
	AS1288
AS2047
	



[bookmark: _Ref531357537]What is the purpose of a window schedule? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		To help work out the appropriate type of window
	

	
		To work out the appropriate opening size of windows
	

	
		To work out whether to use a timber or aluminium frame
	

	
		To work out the height of a window
	




[bookmark: _Ref531357490]Identify the Volume and Parts of the NCC that relate to door installation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Vol2 Part 3.6.4.1
	Vol1 D2.19
	




[bookmark: _Ref427238214][bookmark: _Ref531357492]What Australian Standards must the design of a timber roof truss adhere to?

	Answer
	AS 1720.1
	



[bookmark: _Ref427583793][bookmark: _Ref531357772]What is a roof system? Name three (3) roof types.

	Answer
	A roof system is a structure that forms the roof of a building.
3 roof sytems are –
Gable
Hip
Skillion
	



[bookmark: _Ref531357774]True or False (Tick your response): Roof trusses can be modified on site to suite different needs.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref427584594]Devise a checklist for ensuring the quality of an installed roof frame.

	Answer
	Rise & pitch of roof against plan
Correct propping of ridge, hips, valleys, rafters and under purlins at correct centres
Adequate collar ties
Line of rafter, hips and valleys
Support to strutting beams
Fascia and barge boards
All tie-downs and fixings
Ceiling joist and alignment with rafters
Hanging beams
Trimmers for location
Trimming to manhole

	



[bookmark: _Ref531357779]Devise a checklist for ensuring the quality of an installed roof truss.

	Answer
	Truss layout plan
Manufacturers specs for tie-downs, bracings and lateral stability
Roof truss certification
Adequacy of supporting structure
Dimension, overall width and length of wall for fit
Support to girder trusses
Plumb and spacings
All tie-downs and fixings
Location of specialised trusses
Trusses have not been modified on-site
Eave overhangs
Trimming to manhole
	



[bookmark: _Ref531357807]Name three (3) roof cladding materials.

	Answer
	Tiles
Shingles
Roof sheeting
	



[bookmark: _Ref427583809]What pitch of roof should roof tiles be applied? Are there exceptions?

	Answer
	15 degrees or greater
There are exceptions for some materials and methods of manufacture to be greater than 25 degrees
	




[bookmark: _Ref531358032]When installing corrugated metal roof sheeting, which is the preferred direction of laying sheets to improve side lap effectiveness for minimising leakage? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Away from the prevailing weather
	

	
		Towards the north
	

	
		Towards the prevailing weather
	




[bookmark: _Ref531358025]True or False (Tick your response): Sarking is advisable under any roof.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531358038]What Australian Standard relates to sarking?

	Answer
	AS/NZS 4256
	



[bookmark: _Ref531358043]Name three (3) items that may require roof penetration. 

	Answer
	Ducts, plumbing and electrical services
	



[bookmark: _Ref531358046]Identify the sections/parts of NCC Volume 1 that relate to the installation of skylights.

	Answer
	Section J and Part F4
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