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CPCCBC4001A 
Apply building codes and standards to the construction process for low rise building projects


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	Karl Lemiszczuk
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	Date
	Click here to enter a date.




	Number of questions
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	35
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	[bookmark: _Ref396827952]ASSESSOR COMMENTS

	


[bookmark: _Ref423932567]The diagram below represents an external house wall, shows part of roof and eave and a window in the wall and the vertical boundary line fence is shown a prescribed measurement of 900mm from the house wall to allow light from the sun to reach the window. 

[image: ]

What type of regulation could allow a lesser distance to be used if appropriate justification was provided?

In what document/s might you find the appropriate information?

	Answer
	Performance Based Regs could allow a lessor distance. U can get a performance based document from the ABCB to demonstrate your building system or material meets legislative requirements.
	



[bookmark: _Ref423933353]In regard to the above 900mm distance from house wall to boundary fence and in using or referencing performance-based regulations in the BCA what else should you be aware of and consider? 

	Answer
	You must consider the dimensions comply with Part 3.7.1 Fire separation, Parts 3.7.1.3 an 3.7.1.5. Figures 3.7.1.2, 3.7.1.3 require FRL (fire resistance level of 60/60/60. So this consideration must take into account the FRL of the external wall for opening window  located near the boundary. Also dimensions between external walls an boundaries may be subjected to local councils planning laws.
	


[bookmark: _Ref423934890]Who has responsibility for producing and maintaining The Building Code of Australia (BCA) and who is it done on behalf of? 

	Answer
	Australian Building codes Board, ABCB on behalf of the Commonwealth Government.
	



[bookmark: _Ref423934988]Fill in the missing words to complete the following two sentences. 
provisions
technical

a. The BCA is a uniform set of ___________ ______________ for the __________ and ______________ of buildings and other structures throughout Australia. design
construction
document
Performance-based

b. It is a ______________________ ________________ that is referenced so that your building system or material can demonstrate that it meets certain performance requirements in order to meet __________________ ____________________.legislative
requirements


	Answer
	
	



[bookmark: _Ref423935105]What is the principal goal of the Building Code of Australia (BCA)?

	Answer
	BCA’s goal is to enable the achievement of nationally consistent, minimum necessary standards of safety, health, amenity and sustainability objectives.
	



[bookmark: _Ref423935280]How many volumes are there in the BCA and to what do the volumes refer?

	Answer
	There are two BCA volumes:
Volume One: 
Class 2 – 9 buildings
Access requirements for people with a disability in Class 1b and 10a buildings
Certain Class 10b structures including access requirements for people with a disability in class 10b swimming pools
Volume Two: 
Class 1 and 10a buildings
Certain Class 10b structures (other than access requirements for people with a disability in Class 10b
Class 10c
	


[bookmark: _Ref423935639]Explain the BCA performance requirements for low rise projects from the diagram below.
[image: ]

	Answer
	A ‘Performance requirement’ is defined as the level of performance which a Building Solution must meet.
A0.5 Meeting the Performance Requirements.
Compliance with the Performance Requirements can only be achieved by:
A-Complying with the deemed-to-satisfy provisions
B-Formulating an alternative solution which:
i-Complies with the Performance Requirements
ii-Is shown to be equivalent to the deemed-to-satisfy provisions
iii-A combination of (a) and (b)
	


[bookmark: _Ref423936447]What is the intent of the ‘Relevant Performance Requirements’ in the BCA?

	Answer
	The intent of the ‘Relevant Performance Requirements’ is to set out the method of determining the appropriate Performance Requirements to be used when an Alternative Solution is used to prove that a Building Solution complies with the BCA.
	



[bookmark: _Ref423936842]Building solutions set out the means of achieving compliance with the performance requirements. The BCA provides for two methods that can be followed to develop a building solution. Explain these two methods.

	Answer
	Deemed to satisfy provisions. These include examples of materials, components, design factors, and construction methods which, if used, will result in compliance with the performance requirements of the BCA. An example of a deemed-to-satisfy provision in the BCA is a ceiling height must not be less than 2.4 metres in a habitable room.

Alternative solutions. The key to the performance-based BCA is that there is no obligation to adopt any particular material, component, design factor or construction method. An approval authority may still issue an approval if a building proposal differs in whole or in part from deemed-to-satisfy provisions described in the BCA and if it can be demonstrated that the design complies with the relevant performance requirements 
	



[bookmark: _Ref423937248]The deemed-to-satisfy building solution establishes a clear and concise process for compliance for a builder, building surveyor or the like (building certifier) who does not want to develop a new means of achieving performance requirements; what does ‘deemed-to-satisfy’ mean?

	Answer
	Deemed to satisfy means the aim to achieve a minimum acceptable standard for construction.
	


[bookmark: _Ref423937619]Write an example of a ‘deemed-to-satisfy’ provision for a class 1 building including deemed-to-satisfy requirements for kitchen, bathroom, laundry and sanitary facilities.

Nominate where you found the information in the BCA.

	Answer
	From BCA Volume two, F2.4.3 Facilities
A Class 1 building is to be provided with suitable-
(a) space and facilities for personal hygiene; and
(b) space and facilities for laundering; and
(c) space and facilities for the preparation and cooking of food.

The performance requirement for this provision is:
(a) Suitable sanitary facilities for personal hygiene must be provided in a
convenient location within or outside the Class 1 building appropriate to the
function or use of the building.
(b) Any sanitary facilities for personal hygiene must be-
(i) within the building; or
(ii) grouped elsewhere on the allotment in a convenient location.
(c) Laundering facilities or space for laundering facilities must be provided in a
convenient location within the building or elsewhere on the allotment,
appropriate to the function or use of the building.
(d) A food preparation facility must be provided which includes-
(i) a means for food rinsing, utensil washing and waste water disposal;
and
(ii) a means for cooking food; and
(iii) a space for food preparation

Building Solution:
The deem to satisfy provision responds to the performance requirement as outlined. If an alternate approach is proposed, it must adequately address the performance requirements. In responding to the performance requirements the deemed to satisfy option aims to achieve a minimum acceptable standard for construction.

	


[bookmark: _Ref423937984]Who and what is Standards Australia?

	Answer
	Standards Australia is Australia’s peak Standards body, recognised through a Memorandum of Understanding with the Commonwealth Government. 
It is an independent, non-government, not-for-profit organisation. In consultation with government, business, industry, community, academia and consumers, Standards Australia develops internationally aligned Australian Standards and related publications to help ensure the safety, reliability and performance of a range of products, services and systems.

	



[bookmark: _Ref423937985]What are Australian Standards?

	Answer
	“Standards are published documents setting out specifications and procedures designed to ensure products, services and systems are safe, reliable and consistently perform the way they were intended to. 
They establish a common language which defines quality and safety criteria.”
	


[bookmark: _Ref423939945]The classification of a building or part of a building is determined by the purpose for which it is designed, constructed or adapted to be used. Please summarise the 10 building classifications below.

	Answer
	Class
	Summary
	
	
	1
	One or more buildings which in association constitute: a. Class 1a – a single dwelling b. Class 1b – boarding house, hostel
	

	
	2
	A building containing 2 or more sole-occupancy units each being a separate dwelling
	

	
	3
	A residential building, other than a building of class 1 or 2, which is a common place of long term or transient living for a number of unrelated persons (E.g.: boarding house, school, hotel)
	

	
	4
	A dwelling in a building that is Class 5, 6, 7, 8 or 9 if it is the only dwelling in the building
	

	
	5
	An office building used for professional or commercial purposes, excluding buildings of Class 6, 7, 8 or 9
	

	
	6
	A shop or other building for the sale of goods by retail or the supply of services direct to the public
	

	
	7
	A building which is Class 7a (a car park) or class 7b (for storage or display of goods or produce for sale)
	

	
	8
	A laboratory or building for the production, assembling, altering, repairing, packing, finishing or cleaning of goods for sale
	

	
	9
	A building of a public nature: Class 9a – health-care building, Class 9b – an assembly building, Class 9c – aged care building
	

	
	10
	A non-habitable building or structure: Class 10a – non-habitable building, Class 10b – fence, mast, pool, Class 10c - Shelter
	




[bookmark: _Ref423940316]Other than the 10 BCA building classifications (A3.2), there are also multiple classifications (A3.3) where each part of a building is classified separately. 

Where would you find a full list of Past A3 classification of Buildings and Structures?

	Answer
	PART A3 CLASSIFICATION OF BUILDINGS AND STRUCTURES, can be found within the Building Codes Australia,
	



[bookmark: _Ref423946303]True or False (Tick your response): If a building or part of a building has more than one classification applying to the whole building or part in accordance with, that building or part must comply with all the relevant provisions of the BCA for each classification.

	Answer
	☒	True 
	
	
	
	☐	False 
	
	




[bookmark: _Ref423941205]Familiarity with plans and specifications for a project when interpreting a building solution and therefore trying to interpret clauses and other referenced documents in the BCA is important.

What do plans and specifications include?

	Answer
	The plans and spec may include, Floor level plans, Elevation plans, Sectional Drawings and all specifications. 
	



[bookmark: _Ref423941402]You must have a clear picture of the building to be constructed and be able to identify the criteria that you will need to compare to the Deemed-To-Satisfy (DTS). What is it you must also consider when constructing complex buildings?

	Answer
	In complex buildings, you will find that requirements of one BCA clause may have an impact on the requirements of another.
	




[bookmark: _Ref423941611]Complete the missing words from the sentence below and explain the difference between these points. 
mandatory

BCA Performance Requirements are _________________ and Deemed-to-Satisfy provisions are ______________. optional


	Answer
	BCA provides a ‘recipe’ that can be used to comply with the performance requirements and that these acceptable ‘recipes’ are called ‘Deemed-to-satisfy’ provisions. Therefore a DTS provision is Optional.
	 




[bookmark: _Ref423941845]What is a Building Solution?

	Answer
	Building Solution means a solution which complies with the Performance Requirements and is-
(a) an Alternative Solution; or
(b) a solution which complies with the Deemed-to-Satisfy Provisions; or
(c) a combination of (a) and (b).
	



[bookmark: _Ref423942068]Referring to the BCA, what are the objectives of Section C Fire Resistance?

	Answer
	The Objective of this Section in the BCA is to—
(a)	 safeguard people from illness or injury due to a fire in a building; and
(b)	 safeguard occupants from illness or injury while evacuating a building during a fire; and
(c)	 facilitate the activities of emergency services personnel; and
(d)	 avoid the spread of fire between buildings; and
(e)	 protect other property from physical damage caused by structural failure of a building as a result of fire.
	



[bookmark: _Ref423942460]Why is it necessary to identify and document performance-based solutions?

	Answer
	It is necessary to identify and document performance-based solutions in order to:
comply with organisational quality procedures and processes
apply and interpret relevant documentation and codes
accurately apply National and State and Territory OHS requirements relating to construction workplace
identify faults and problems impacting on OHS and proposing appropriate action to rectify
	



[bookmark: _Ref423942735]In the context of the Building Code of Australia what are Assessment Methods used to determine?

	Answer
	Assessment Methods are used to determine whether a Building Solution complies with the relevant BCA Performance Requirements. A Building Solution can be achieved through complying with the Deemed-to-Satisfy Provisions, or by using an Alternative Solution to achieve the Performance Requirements. Approval of Alternate Solutions can use the following assessments, evidence of suitability, Verification methods, comparison with the DTS Provisions or Expert Judgement.
	



[bookmark: _Ref423943044]Explain the importance of maintaining detailed documentation for a building project.

	Answer
	It is important that you maintain a detailed level of documentation to ensure that the building is compliant and can pass assessment.
The ability to refer to detailed documentation provides a vital reference tool required for inspections of key building elements, this ensures they are not inadvertently overlooked.
	


[bookmark: _Ref423943211]With regard to detailed documentation what are some of the documents that must be provided and maintained by contractors?

	Answer
	ITP’s
	



[bookmark: _Ref423943524]Other than the Builder maintaining detailed documentation, who will also have responsibility to resolve and correct errors for any ambiguity identified in the plans?

	Answer
	A building Certifier has to carefully check the details of the plan against the applicable standards and codes.
	



[bookmark: _Ref423943842]The threat of an accidental fire in a building and to prevent it are important to understanding fire and taking all steps to prevent or confine fire and to prevent fire spreading within the structure as well as to adjoining or adjacent buildings. 

In this regard Fire Protection Systems are paramount and are subject to?

	Answer
	Building regulations
Fire regulations
Insurance company requirements
Local government requirements
Other regulatory authorities
	



[bookmark: _Ref423943887]Briefly explain the following fire definitions:

	Answer
	Term
	Explanation
	
	
	Fire
	Fire is the rapid oxidation of a gas, liquid or solid substance accompanied by the release of heat and light. Chemically, fire represents an exothermic or heat-producing reaction.
	

	
	Passive Fire Protection
	Passive fire protection is an integral component of the three components of structural fire protection and fire safety in a building.
Passive fire protection attempts to contain fires or slow the spread, through the use of fire resistant walls, floors and doors.
	

	
	Active Fire Protection
	Active fire protection is an integral part of fire protection and is characterised by items and systems which require a certain amount of motion and response in order to work (eg: fire sprinkler system or fire detection devices).
	



[bookmark: _Ref423944362]The purpose of fire protection is to: 
1. Prevent/reduce the possibility of fire and 
2. Reduce the spread of fire within and around a building

Name the two categories or systems that provide measurement and arrangements for fire protection.

	Answer
	Active Systems-
Portable fire extinguishers
Fire hydrants/hose reels
Sprinkler systems
Smoke detection and alarm systems
Passsive Systems-
Fire isolated stairs and passageways
Fire resistant materials (walls, roofs, openings)
Fire doors
Fire curtains
Fire rated ceilings
Fire stop collars (in floor slabs)


	



[bookmark: _Ref423944529]With respect to the general level of fire protection explain separately the terms ‘Fire Load’ and ‘Fire Load Density’?

	Answer
	Fire load refers to the amount of potential heat that can be liberated during the fire of the combustible contents of a given enclosure. It is expressed as a numerical value represented as kJ/kg (kilojoule per kilogram) or as MJ/kg (megajoules per kilogram).

Fire load density is the fire load of a given enclosure or building divided by floor area. It is expressed as fire load per unit area of floor space (the greater the fire load the more severe the fire).

	


[bookmark: _Ref423944839]Using Volume 2 of the BCA respond to the following:
a) Where in the BCA would you look to find requirements for building in bushfire prone areas for Class 1 and 10 buildings? 
b) Where in the BCA would you look to find requirements for building in bushfire prone areas for Class 2-9 buildings? 
c) What Australian Standard must be complied with to satisfy the Deemed to Satisfy Provisions for construction of Class 2 and 3 buildings in bushfire prone areas?

	Answer
	a)
	PART 3.7.4 BUSHFIRE AREAS page 289 onwards
	 

	
	b)
	Volume 1
Section C Fire Resistance
Part C1 Fire Resistance and Stability P93
Part C2 Compartmentation and Separation P100
Part C3 Protection of openings P109
	

	
	c)
	A0.10
	




[bookmark: _Ref423945259]What is a Fire Safety Schedule and its relationship to the approval of development of a class 2 – 9 building?

	Answer
	List all the essential fire safety measures that should be installed in the building and the performance standard to which each of these measures must be capable of operating.
	



[bookmark: _Ref423945523]What are building certifiers responsible for?

	Answer
	Are responsible for ensuring specific compliance is achieved and they do this by conducting visual inspections.
	



[bookmark: _Ref423945524]What are building certifiers not responsible for?

	Answer
	Building Ceritfiers are not responsible for the quality of workmanship within the construction process…
	



[bookmark: _Ref423945635]Where in the BCA would you determine the level of fire resistance required for the construction of buildings?

	Answer
	For fire-resisting construction between Class 1 buildings see Part 3.7.1
[bookmark: _GoBack]Fire Resistants section C Volume 1..
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