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CPCCBC4012B 
Read and interpret plans and specifications


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Ante Begic

	

	

	Participant signature
	



	Assessor name
	

	

	

	Assessor signature
	



	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Satisfactory?

	87
	
	Yes
	No

	
	
		

	ASSESSOR COMMENTS

	


Plans and specifications are used to inform which of the following processes? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Building contracts
	

	
		Development applications 
	

	
		Estimation
	

	
		Planning
	

	
		Supervisory tasks
	

	
		Tenders
	




[bookmark: _Ref532191033]Which compass direction is always shown on plans and drawings?

	Answer
	North
	



[bookmark: _Ref427670124]What information is provided on a location plan?

	Answer
	Shows a site on a particular street

	



[bookmark: _Ref427670125]What detail does a site or block plan contain?

	Answer
	Provides specific detail of the block on which a development is proposed
· Site boundaries
· Street frontage name etc

	


[bookmark: _Ref427670660]What do floor plans identify?

	Answer
	Shows detail of the proposed structure, such as rooms, positions of fixtures, floor coverings, levels, room names and internal sizes..

	



[bookmark: _Ref427671793]What is a landscape plan and what information might it provide?

	Answer
	Shows details of plants, paths, garden layouts and retaining walls
	



[bookmark: _Ref427670661]What are elevation views? What do they provide to the plan reader?

	Answer
	View of the proposed structure from its sides (i.e. from north, south, east and west). 
Each side is what is you will see when standing in front of the wall

	



[bookmark: _Ref427670662]What is a section?

	Answer
	The section is a view of the house after it has been cut vertically at some point. You will be able to see overall height, floor to ceiling height, construction details etc.
	



[bookmark: _Ref427670664]What are detailed drawings?

	Answer
	A drawing, at relatively large scale, of a part of a building, machine, etc., with dimensions or other information for use in construction
	



[bookmark: _Ref427671414]What are specifications?

	Answer
	A detailed description of the design and materials used to make something
Key features included within building specifications include:

· Levels and survey information
· Materials lists
· Performance data and material technical data
· Schedules of quantities & Stress, load and bearing calculations

	




[bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	ACRYL
	Acrylic
	

	
	AS
	Australian Standard
	

	
	ASSD
	Assumed Datum
	

	
	B
	Basin
	

	
	BN
	Bull Nose
	

	
	BTH
	Bath
	

	
	BWK
	Brickwork
	

	
	CB
	Concrete Block
	

	
	CF
	Concrete floor
	

	
	CG
	Clear Glass
	

	
	CJ
	Ceiling Joint
	

	
	CORR
	Corrugated
	

	
	CWT
	Cold Water Tank
	

	
	DG
	Double Glazing
	

	
	DH
	Double Hung
	

	
	DPC
	Damp Proof Course
	

	
	DSB
	Distribution Switch Board
	

	
	DW
	Dishwasher
	

	
	EJ
	Expansion Joint
	

	
	FPBD
	Fibrous Plaster Board
	

	
	FFL
	Finished Floor Level
	

	
	FHR
	Fire Hose Reel
	

	
	GPO
	General Purpose Outlet
	

	
	HBD
	Hardboard
	

	
	HTR
	Heater
	

	
	HWD
	Hardwood
	




[bookmark: _Ref427675022]Name each of the drawing symbol images shown in the table below.

	Answer
	Name
	Image
	
	
	Cavity Brick
	[image: Wall - Cavity brick]
	

	
	Brick Veneer
	[image: Wall - Brick veneer]
	

	
	Wall timber stud
	[image: Wall - Timber stud]
	

	
	In cavity Windows
	[image: Window - In cavity wall]
	

	
	Windows in cavity wall

	[image: Window - In single wall]
	

	
	Hinged Door
	[image: Door - Swing single]
	

	
	Double Hinged Door
	[image: Door - Swing double]
	

	
	 Sliding Door into pocket
	[image: Door - Sliding into pocket]
	

	
	External Sliding door exposed on wall
	[image: Door - Sliding exposed on wall]
	

	
	Socket outlet
	[image: Socket outlet (power) - general]
	





[bookmark: _Ref427733304]Identify what the following window symbols represent on elevations.

	Answer
	Item
	Drawing
	
	
	Hinged at Side
	[image: ]
	

	
	Hinged at top
	[image: ]
	

	
	Sliding Horizontally
	[image: ]
	

	
	Fixed
	[image: ]
	




[bookmark: _Ref532192707]What does a clouded area on a plan indicate?






	Answer
	On plans, revisions or amendments are represented by a clouded area
	



[bookmark: _Ref532192900]An amendment to specifications could relate to which of the following? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Contact details of all construction crew members
	

	
		Materials or products used
	

	
		Methods of carrying out specified work
	





Refer to the title block below to respond to Q16. to Q18. 
[image: ]
Source: http://www.dtwd.wa.gov.au/sites/default/files/teachingproducts/BC1934_CCBY.PDF 

[bookmark: _Ref531861864]On what date was an amendment made to the window details?

	Answer
	05/10/2011 & 08/11/2011
	



[bookmark: _Ref532193187]True or False (Tick your response): Details of the window in Q16. should also be reflected in the specifications and confirmed with the client.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531862015]What amendment occurred on 08/11/2011?

	Answer
	Bed 3 Robe Deleted
	




Refer to the site plan below to respond to Q19. to Q26. 

[image: Site plan for a block of land showing existing building and proposed residence plus other detail]

[bookmark: _Ref531861219]What structure is being built on this site? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Residence
	

	
		Road
	

	
		Shed
	

	
		Water meter
	




[bookmark: _Ref532193598]What is the Lot number of this site?

	Answer
	Lot 16
	



[bookmark: _Ref532193601]What is the size of this lot?

	Answer
	3653m2
	



[bookmark: _Ref532193617]Is the shed at the north-east of the proposed structure to be removed or retained? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Removed
	

	
		Retained
	




[bookmark: _Ref532193558]True or False (Tick your response): The sewer is at the eastern boundary of the property.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref532193550]True or False (Tick your response): The driveway is located to the south of the proposed property.

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref532193569]What size is the easement on the eastern boundary of the site?

	Answer
	5m
	



[bookmark: _Ref531861509]True or False (Tick your response): The stormwater drain is constructed from PVC pipe.

	Answer
		True 
	
	
	
		False 
	
	




Refer to the contour plan below to respond to Q27. to Q28. 

[image: contourplan]

[bookmark: _Ref531872622]What is the level at the northernmost point of the site?

	Answer
	3.94
	



[bookmark: _Ref532193453]Which end of the site has the lowest level? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		East
	

	
		West
	



Refer to the sectional drawing below to respond to Q29. to Q49. 

[image: cross_section]
[bookmark: _Ref427660755][bookmark: _Ref532194571]Give a brief description about the building from the detail available in the sectional drawing. Is it the same structure proposed in Q19. to Q26.?

	Answer
	Residential building with 4 bedrooms. It is the same structure proposed in Q19 to Q26 WD9733
	



[bookmark: _Ref427733756]Who is the client?

	Answer
	H&M Smith
	



[bookmark: _Ref427733757]Where is this project to be built?

	Answer
	Lot 16 Glenvalley Road
	



[bookmark: _Ref427733759]What are the contact details for the draftsman?

	Answer
	Joe Foreman

0413113113
	



[bookmark: _Ref427733761]What sheet number is this drawing?

	Answer
	Sheet 5 of 7
	



[bookmark: _Ref427660519][bookmark: _Ref427733762]What timber is required for loading and non-load bearing walls?

	Answer
	45 x 90 Pine for load bearing
35 x 90 Pine for non load bearing
	


[bookmark: _Ref427733763]What spacing is recommended for common studs?

	Answer
	600 max spacing Every truss straped to wall
	



[bookmark: _Ref427733765]What type of roof truss is to be installed?

	Answer
	Gang rail roof trusses at 900 spacing
	



[bookmark: _Ref427733766]What centres are the trusses positioned at?

	Answer
	900
	



[bookmark: _Ref427733769]What size are the veranda posts?

	Answer
	90 x 90
	



[bookmark: _Ref427733771]What timber species are the veranda posts to come from?

	Answer
	DAR Oregon
	



[bookmark: _Ref427733773]What pitch is the roof?

	Answer
	30 degrees
	



[bookmark: _Ref427733774]What size are the noggings and at what spacing?

	Answer
	1350 max spacing
35 x 70
	



[bookmark: _Ref427733776]What size are the ceiling joists?

	Answer
	HJ 240 joists
	


[bookmark: _Ref427733778]What timber is used for roof battens and what spacing?

	Answer
	FG Pine 900 max spacing
	



[bookmark: _Ref427733780]What thickness is the plasterboard sheeting?

	Answer
	10mm
	



[bookmark: _Ref427733781]What type of flooring is to be installed?

	Answer
	15mm plywood flooring
	



[bookmark: _Ref427733783]What is the roof cladding material?

	Answer
	Colorbond corrugated metal roofing
	



[bookmark: _Ref427733784]Where will you find information about the footings?

	Answer
	Engineers Drawing
	



[bookmark: _Ref427733786]What do the letters ‘DAR’ refer when timber ordering?

	Answer
	Dressed All Round
	



[bookmark: _Ref427662218]Explain what ‘240 x 63 LVL’ refers to on the sectional drawing. What do the letters ‘LVL’ refer to?

	Answer
	Laminated Veneer Lumber. It is the starting joist between verandah and family room
	


Refer to the drawing below to respond to Q50. to Q65. 

[image: ]

[bookmark: _Ref427663500]What is the number of the drawing?

	Answer
	02
	



[bookmark: _Ref427734104]What is the Job Number?

	Answer
	00R-112
	



[bookmark: _Ref427734106]What is the scale of the drawing?

	Answer
	1:100
	



[bookmark: _Ref427733995]What does the drawing show?

	Answer
	North / East / West / South Elevation Views and a section view of a residential building
	



[bookmark: _Ref427734110]Which view shows the front of the house?

	Answer
	East Elevation
	



[bookmark: _Ref427734113]How many motor vehicles can be parked in the garage?

	Answer
	2
	



[bookmark: _Ref427734114]What are the window and doors made from?

	Answer
	Aluminium Framed Windows and Doors frames / Timber Door
	



[bookmark: _Ref427734116]What is the size of the eaves?

	Answer
	450
	


[bookmark: _Ref427734119]What are the eaves lined with?

	Answer
	HardiFlex
	



[bookmark: _Ref427734120]What type of roof structure is the roof built from?

	Answer
	Timber Framed Roof Truss
	



[bookmark: _Ref532197046]Which Clause of the NCC should be read for more detail about roof structure in Q59. ?

	Answer
	Code Reference clause
	



[bookmark: _Ref532197154]Which Australian Standard should be read for more detail about the roof structure in Q59. ?

	Answer
	AS 1720
	



[bookmark: _Ref427734122]What is the roof cladding materials made from?

	Answer
	Concrete Roof Tiles
	



[bookmark: _Ref532197156]Which Clause of the NCC should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	NCC Volume 2 Part 3.5.1.0 and 3.5.1.2
	



[bookmark: _Ref532197157]Which Australian Standard should be read for more detail about the roof cladding materials in Q62. ?

	Answer
	AS 2049
	



[bookmark: _Ref427663512]What is the roof pitch?

	Answer
	22.5
	



[bookmark: _Ref531871432]Identify one (1) regulatory body you may need to submit plans to for approval?

	Answer
	City Council
	



[bookmark: _Ref532197251]Briefly describe the approval process and timeframes for an approval through the regulatory body in Q66. 

	Answer
	From 6 days to 3 month process
	



[bookmark: _Ref427673788]What is a prime cost (PC) item? Give an example.

	Answer
	An amount of money included in a contract sum to purchase a specified item such as tiles, taps, doors or bathroom fittings
An agreed estimated amount is included at contract signing but the specific products are not selected until a later stage
A builder must estimate the cost of such items at or above the lowest amount these items could reasonably cost.
For example if a client selects a more expensive door than allowed by the PC item, say a $500 door compared with a $440 PC amount, a variation will be required to cover the additional $60.  If the PC item varies, so will the final contract sum.
	



[bookmark: _Ref427673790]What is a provisional sum (PS) item? Give an example.

	Answer
	An amount of money included in contract sum to cover work and/or materials, not detailed when entering the contract
Typically builders will include a PS for site work costs
The builder is legally required to take reasonable steps to ensure an accurate site works cost estimate but unforeseen events mean that the provisional sum is exceeded which is added to the contract sum

For example a building site may seem sandy and clean with minimal siteworks required, however, there may be large limestone rocks/tree trunks concealed below the surface which only emerge once siteworks commence, causing cost overrun.


	


Refer to the Bill of Quantities below to respond to Q70. to Q76. 

[image: ]
[image: ]

Source: http://organizedbuilders.com.au/sites/default/files/BOQ-Summary.pdf 



[bookmark: _Ref531867328]True or False (Tick your response): This Bill of Quantities represents a job for a two-storey house.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref532199102]Identify two (2) materials being used for the floors?

	Answer
	Tile and timber, carpet, vinyl
	



[bookmark: _Ref532199110]True or False (Tick your response): A landscaper has been contracted for this job.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref532199056]How much does the contracted plasterer cost?

	Answer
	12900
	



[bookmark: _Ref532199058]How much do the kitchen appliances cost?

	Answer
	2700
	



[bookmark: _Ref532199060]What percentage of the total cost does the fixing stage represent of the building contract?

	Answer
	[bookmark: _GoBack]23
	



[bookmark: _Ref531866973]What percentage of the total cost does the completion stage represent of the building contract?

	Answer
	17
	


Refer to the Purchase Order below to respond to Q77. to Q82. 

[image: ]
Source: http://organizedbuilders.com.au/sites/default/files/Databuild-Bill-of-Quantities.pdf 

[bookmark: _Ref531874116]How many Pine F5 90 x 45 studs (2.4m long) are required?

	Answer
	100
	



[bookmark: _Ref532199470]If the material in Q77. increased in cost to $2.75 each, what would be the total cost for this material?

	Answer
	275
	



[bookmark: _Ref532199474]How many sheet of ply are required in total (i.e. all sizes)?

	Answer
	13
	



[bookmark: _Ref531874121]What material has the highest total cost?

	Answer
	Pine 90 x 45 mgp10 (long Lengths)
	



[bookmark: _Ref531874448]How many metres are required of the material in Q80. ?

	Answer
	322.5m
	



[bookmark: _Ref531874565]What beam is identified as being a better option than F17?

	Answer
	E14
	




Refer to the labour chart below to respond to Q83. to Q86. 

[image: ]
Source: https://www.archsd.gov.hk/media/89170/sor2013_vol1_builders_works_2013_11_04.pdf 



[bookmark: _Ref531873766]Based on the hourly rates given, which is the least expensive trade to contract?

	Answer
	Asphalter (Road construction)
	



[bookmark: _Ref532199773]If the trade in Q83. were to be contracted for two (2) hours’ work, how much would this cost?

	Answer
	214.80
	



[bookmark: _Ref531873865]Based on the hourly rates given, which is the most expensive trade to contract?

	Answer
	Bar Bender & Fixer
	



[bookmark: _Ref531873882]If the trade in Q85. were to be contracted for six (6) hours’ work, how much would this cost?

	Answer
	1285.85
	



[bookmark: _Ref531691201]Name the building legislation (Act and Regulations) that apply within your jurisdiction and should be referenced when reading plans and building contracts.

	Answer
	Home Building Act 1989
Home Building Regulation 2014
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