Interim Test Report – Timber framing 
Site address:									
Date:										
Site Supervisor:									
Signature:									
The purpose of this report is to ensure critical aspects of the construction points are adhered to in accordance with AS16 Timber framing and the National Construction Code Volume 2 – Part 3.4.3 Timber framing

	Item
	Checkpoint
	Notes

	Sub – floor framing
	☐ Member sizes and spacings
☐ Minimum clearances to ground levels
☐ Sub – Floor bracing
☐ Provisions for sub – floor ventilation
☐ Termite protection
☐ Ground grading
	

	Lower floor wall framing
	☐ Member sizes and spacing
☐ Bracing
☐ Tie – down and point – load locations
	

	Upper floor wall framing
	☐ Wall framing elements to slab or upper levels of multi-storey construction should be checked to ensure member sizes and spacings, bracing, tie-down and point-load requirements comply with the building development approval
	

	Floor framing and flooring
	 ☐ Member sizes and spacings
☐ Diaphragm bracing and blocking
☐ Water proof / resistant flooring to wet areas
	

	Insulation for energy efficiency requirements (if applicable)
	☐ Insulation or sarking to external wall framing
☐ Roof/ceiling insulation
	


	Structural walls (masonry)
	☐  Tie-down points and lateral bracing elements
☐  Core filling (if relevant)
☐  Sizes, lateral support.
	

	Roof and ceiling framing
	☐  Member sizes and spacings
☐  Cross-bracing and tie-down
☐  Point-loads supported
☐  Location and fixing of truss binders
☐  Batten fixing and joint location (sheet roofs).
	



